(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 17)
    (no_connects 1)
    (area 134.956499 94.316499 185.083501 144.443501)
    (thickness 1.6002)
    (drawings 4)
    (tracks 80)
    (zones 0)
    (modules 6)
    (nets 22)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (grid_origin 160.02 119.38)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /Anode)
  (net 4 /Din)
  (net 5 "Net-(J1-Pad3)")
  (net 6 /HV6)
  (net 7 /HV5)
  (net 8 /HV10)
  (net 9 /HV4)
  (net 10 /HV9)
  (net 11 /HV3)
  (net 12 /HV8)
  (net 13 /HV2)
  (net 14 /HV7)
  (net 15 /HV1)
  (net 16 "Net-(J1-Pad5)")
  (net 17 "Net-(J1-Pad1)")
  (net 18 "Net-(J1-Pad15)")
  (net 19 "Net-(LED1-Pad1-DO)")
  (net 20 "Net-(NX1-PadA)")
  (net 21 "Net-(NX1-PadA1)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net /Anode)
    (add_net /Din)
    (add_net /HV1)
    (add_net /HV10)
    (add_net /HV2)
    (add_net /HV3)
    (add_net /HV4)
    (add_net /HV5)
    (add_net /HV6)
    (add_net /HV7)
    (add_net /HV8)
    (add_net /HV9)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(LED1-Pad1-DO)")
    (add_net "Net-(NX1-PadA)")
    (add_net "Net-(NX1-PadA1)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AE37366)
    (at 156.337 119.38 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.413 0.127 180) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 2.413 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm (layer F.Cu) (tedit 5A3B14FF)
    (at 170.18 99.38 270)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 270) (layer F.SilkS) hide)
    (fp_text value Nixie (at 1.27 22.65 270) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV6))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV5))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV10))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV4))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV9))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV3))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV8))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HV2))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /HV7))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /HV1))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Din))
    (pad 17 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole oval (at 2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adafruit:adafruit-LED3535 (layer F.Cu) (tedit 5AE37384)
    (at 159.92348 119.39524)
    (attr smd)
    (fp_text reference LED1 (at 3.175 -0.254 90) (layer F.SilkS) hide)
    (fp_text value WS2812BSK6812MINI (at 0.127 2.54) (layer F.SilkS) hide)
    (pad 1-DO smd rect (at 1.74752 0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(LED1-Pad1-DO)"))
    (pad 2-GN smd rect (at 1.74752 -0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3-DI smd rect (at -1.74752 -0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 /Din))
    (pad 4-VD smd rect (at -1.74752 0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module logos:mermaid_l (layer B.Cu) (tedit 0)
    (at 163.322 134.62 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module mynixies:mynixies-ZM1042-8331 (layer F.Cu) (tedit 5AE36B14)
    (at 160.02 119.53494)
    (descr "SOCKET WITH D-SUB SOCKETS")
    (tags "SOCKET WITH D-SUB SOCKETS")
    (attr virtual)
    (fp_text reference NX1 (at 0.127 -15.26794) (layer F.SilkS))
    (fp_text value ZM1042MILLMAX8331 (at 0.5588 0.61468) (layer F.SilkS) hide)
    (fp_text user 2 (at 5.0038 -3.6195) (layer F.SilkS))
    (fp_text user 3 (at 6.32206 -1.01854) (layer F.SilkS))
    (fp_text user 4 (at 6.2103 1.59258) (layer F.SilkS))
    (fp_text user 5 (at 4.70916 4.07162) (layer F.SilkS))
    (fp_text user 6 (at 2.64668 5.59054) (layer F.SilkS))
    (fp_text user 7 (at -2.15138 5.4229) (layer F.SilkS))
    (fp_text user 8 (at -4.4323 4.02844) (layer F.SilkS))
    (fp_text user 9 (at -5.77342 1.61798) (layer F.SilkS))
    (fp_text user 0 (at -5.80136 -1.1303) (layer F.SilkS))
    (fp_text user A (at -2.32918 -5.40258) (layer F.SilkS))
    (fp_text user A (at 0.30734 -5.92328) (layer F.SilkS))
    (fp_text user IV (at 0.33528 6.10362) (layer F.SilkS))
    (fp_text user 1 (at -4.73202 -3.70078) (layer F.SilkS))
    (pad 0 thru_hole circle (at -8.18896 -1.8669) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 8 /HV10))
    (pad 1 thru_hole circle (at -6.5659 -5.23494) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 15 /HV1))
    (pad 2 thru_hole circle (at 6.5659 -5.23494) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 13 /HV2))
    (pad 3 thru_hole circle (at 8.18896 -1.8669) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 11 /HV3))
    (pad 4 thru_hole circle (at 8.18896 1.8669) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 9 /HV4))
    (pad 5 thru_hole circle (at 6.5659 5.23494) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 7 /HV5))
    (pad 6 thru_hole circle (at 3.6449 7.56666) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 6 /HV6))
    (pad 7 thru_hole circle (at -3.6449 7.56666) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 14 /HV7))
    (pad 8 thru_hole circle (at -6.5659 5.23494) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 12 /HV8))
    (pad 9 thru_hole circle (at -8.18896 1.8669) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 10 /HV9))
    (pad A thru_hole circle (at 0 -8.39978) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 20 "Net-(NX1-PadA)"))
    (pad A1 thru_hole circle (at -3.6449 -7.56666) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 21 "Net-(NX1-PadA1)"))
    (pad IV thru_hole circle (at 0 8.39978) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AE37390)
    (at 161.29 107.95)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 3.429 0.127) (layer F.SilkS) hide)
    (fp_text value 8K2 (at 0.127 -1.524) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(NX1-PadA1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /Anode))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text NEO3535 (at 159.893 122.301 360) (layer F.SilkS))
  (gr_text "Mill-Max\n8331-0-15-15-18-27-10-0" (at 159.893 108.458) (layer B.SilkS))
  (gr_text "nixies.us\nZM1040, ZM1042,\nZ566, Z5660M,\nZ522M, Z5220M,\nLC-631" (at 161.92 137.58) (layer B.Mask))
  (gr_circle (center 160.02 119.38) (end 135.02 119.38) (layer Edge.Cuts) (width 0.127))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 190.02 89.38) (xy 130.02 89.38) (xy 130.02 149.38) (xy 190.02 149.38)
      )
    )
  )
)
