<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="20.6375" y1="13.97" x2="-7.62" y2="13.97" width="0" layer="20"/>
<wire x1="-7.62" y1="13.97" x2="-8.255" y2="13.335" width="0" layer="20" curve="90"/>
<wire x1="-8.255" y1="13.335" x2="-8.255" y2="-1.27" width="0" layer="20"/>
<wire x1="-8.255" y1="-1.27" x2="-7.62" y2="-1.905" width="0" layer="20" curve="90"/>
<wire x1="-7.62" y1="-1.905" x2="20.32" y2="-1.905" width="0" layer="20"/>
<wire x1="20.32" y1="-1.905" x2="20.955" y2="-1.27" width="0" layer="20" curve="90"/>
<wire x1="20.955" y1="-1.27" x2="20.955" y2="13.6525" width="0" layer="20"/>
<wire x1="20.955" y1="13.6525" x2="20.6375" y2="13.97" width="0" layer="20" curve="90"/>
<text>-</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>GND</text>
<text>VCC</text>
<text>TX</text>
<text>RX</text>
<text>GND</text>
<text>ESP-01</text>
<text>P</text>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="EVQ-Q2">
</package>
<package name="SOT23-W">
<description>&lt;b&gt;SOT23&lt;/b&gt; - Wave soldering</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="2X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_LONGPADS">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-BEC">
<description>TO-236 ITT Intermetall</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP2" library="pinhead" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="Q3" library="adafruit" package="SOT23-W" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="M0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="R3" library="adafruit" package="M0805" value="2k">
<attribute name="NAME"/>
</element>
<element name="R2" library="adafruit" package="M0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X02_LONGPADS" value="M02PTH3"/>
<element name="GND" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="VCC" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="adafruit" package="2X04" value="">
<attribute name="VALUE"/>
</element>
<element name="PNP" library="transistor" package="SOT23-BEC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="NPN" library="transistor" package="SOT23-BEC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="M0805" value="2k">
<attribute name="NAME"/>
</element>
<element name="SW2" library="adafruit" package="EVQ-Q2" value="SPST_TACT-EVQQ2"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP2" pad="1"/>
<contactref element="JP5" pad="1"/>
<contactref element="GND" pad="TP"/>
<contactref element="JP3" pad="7"/>
<contactref element="NPN" pad="E"/>
<contactref element="SW2" pad="B"/>
<contactref element="SW2" pad="B'"/>
</signal>
<signal name="N$4">
<contactref element="JP2" pad="2"/>
<contactref element="Q3" pad="3"/>
<contactref element="VCC" pad="TP"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP3" pad="6"/>
<contactref element="JP3" pad="3"/>
<contactref element="PNP" pad="E"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="JP2" pad="3"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="JP2" pad="4"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="N$5">
<contactref element="Q3" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="Q3" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="NPN" pad="C"/>
<contactref element="SW2" pad="A"/>
<contactref element="SW2" pad="A'"/>
</signal>
<signal name="N$7">
<contactref element="JP3" pad="5"/>
<contactref element="R4" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
<signal name="N$8">
<contactref element="NPN" pad="B"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R3" pad="1"/>
<contactref element="PNP" pad="C"/>
</signal>
<signal name="N$13">
<contactref element="PNP" pad="B"/>
<contactref element="R4" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
