(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 6)
    (zones 0)
    (modules 9)
    (nets 3)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
  )
  (module ICComponents:logo (layer F.Cu) (tedit 0)
    (at -27 0)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module ICComponents:1mmMountingHole (layer F.Cu) (tedit 5E209F5B)
    (at -37 8.5)
    (fp_text reference REF** (at 0 1.7526) (layer Dwgs.User))
    (fp_text value 1mmMountingHole (at 0 -1.3716) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1 1) (drill 1) (layers *.Cu *.Mask))
  )
  (module ICComponents:1mmMountingHole (layer F.Cu) (tedit 5E209F5B)
    (at 37 8.5)
    (fp_text reference REF** (at 0 1.7526) (layer Dwgs.User))
    (fp_text value 1mmMountingHole (at 0 -1.3716) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1 1) (drill 1) (layers *.Cu *.Mask))
  )
  (module ICComponents:1mmMountingHole (layer F.Cu) (tedit 5E209F5B)
    (at -37 -8.5)
    (fp_text reference REF** (at 0 1.7526) (layer Dwgs.User))
    (fp_text value 1mmMountingHole (at 0 -1.3716) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1 1) (drill 1) (layers *.Cu *.Mask))
  )
  (module ICComponents:1mmMountingHole (layer F.Cu) (tedit 5E209F5B)
    (at 37 -8.5)
    (fp_text reference REF** (at 0 1.7526) (layer Dwgs.User))
    (fp_text value 1mmMountingHole (at 0 -1.3716) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1 1) (drill 1) (layers *.Cu *.Mask))
  )
  (module ICComponents:4-40MountingHole (layer F.Cu) (tedit 5E20A43E)
    (at -31 15)
    (fp_text reference J4 (at -0.0254 5.1308) (layer Dwgs.User))
    (fp_text value VFrish (at 0.0508 -4.7752) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 2.3) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole circle (at 2.3 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole circle (at -2.3 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.3) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
  )
  (module ICComponents:4-40MountingHole (layer F.Cu) (tedit 5E20A43E)
    (at -31 -15)
    (fp_text reference J3 (at -0.0254 5.1308) (layer Dwgs.User))
    (fp_text value VCath (at 0.0508 -4.7752) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 2.3) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 2.3 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at -2.3 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.3) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
  )
  (module ICComponents:4-40MountingHole (layer F.Cu) (tedit 5E20A43E)
    (at 31 15)
    (fp_text reference J2 (at -0.0254 5.1308) (layer Dwgs.User))
    (fp_text value VFrish (at 0.0508 -4.7752) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 2.3) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole circle (at 2.3 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole circle (at -2.3 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.3) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
  )
  (module ICComponents:4-40MountingHole (layer F.Cu) (tedit 5E20A43E)
    (at 31 -15)
    (fp_text reference J1 (at -0.0254 5.1308) (layer Dwgs.User))
    (fp_text value VCath (at 0.0508 -4.7752) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 2.3) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 2.3 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at -2.3 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.3) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
  )
  (gr_text "IC Window Pane v1\nAdam Anthony 1/16/20" (at 27 0) (layer F.SilkS))
  (gr_line (start -15 15) (end -15 -15) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 15 15) (end -15 15) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 15 -15) (end 15 15) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -15 -15) (end 15 -15) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -38.5 23) (end -38.5 -23) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 38.5 23) (end -38.5 23) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 38.5 -23) (end 38.5 23) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -38.5 -23) (end 38.5 -23) (layer Edge.Cuts) (width 0.05))
)
