<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="66.802" y1="50.546" x2="108.946" y2="50.546" width="0" layer="20"/>
<wire x1="108.946" y1="50.546" x2="108.946" y2="77.14" width="0" layer="20"/>
<wire x1="108.946" y1="77.14" x2="66.802" y2="77.14" width="0" layer="20"/>
<wire x1="66.802" y1="77.14" x2="66.802" y2="50.546" width="0" layer="20"/>
<text>Q2</text>
<text>L1</text>
<text>D2</text>
<text>Ch 2</text>
<text>Ch 1</text>
<text>2018</text>
<text>T. Kircher</text>
<text>DANGER</text>
<text>HIGH VOLTAGE</text>
<text>HIGH VOLTAGE</text>
<text>DANGER</text>
</plain>
<libraries>
<library name="thomas_library">
<description>Dr. K's collection of Eagle CAD footprints for projects</description>
<packages>
<package name="0805">
<description>This 0805 (2012 metric) footprint has 1.0mm x 1.2mm pads, with a 1.2mm gap. Specification from Panasonic. Verified 8/15/2011</description>
</package>
<package name="1206">
<description>This 1206 (3216 metric) footprint has 1.25mm x 1.5mm pads, with a 2.2mm gap. Specification from Panasonic. Verified 8/15/2011</description>
</package>
<package name="DO-219AB">
</package>
<package name="SOIC8">
<description>&lt;b&gt;SOIC-8&lt;/b&gt; CASE 751-07&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC34164-D.PDF&lt;p&gt;
&lt;b&gt;D (R-PDSO-G8)&lt;/b&gt;PLATIC SMALL-OUTLINE PACKAGE&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/tlc27l2.pdf</description>
</package>
<package name="1200LRS">
</package>
<package name="SOT-23A">
<description>This SOT-23A footprint has 1.0mm x 0.6mm pin pads, 0.95mm spacing, and 2.7mm diameter. Verified 8/15/2011</description>
</package>
<package name="TO-252">
</package>
<package name="3362P">
</package>
<package name="TP">
<description>This is a large test point</description>
</package>
</packages>
</library>
<library name="logo">
<description>&lt;b&gt;Electronic and CadSoft EAGLE logos&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="ESD_10.00">
<description>&lt;b&gt;Logo ESD 10 mm&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Medium - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="thomas_library" package="0805" value="1nF">
<attribute name="NAME"/>
</element>
<element name="C2" library="thomas_library" package="1206" value="10nF">
<attribute name="NAME"/>
</element>
<element name="C3" library="thomas_library" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="thomas_library" package="1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="D1" library="thomas_library" package="0805" value="1N914">
<attribute name="NAME"/>
</element>
<element name="D2" library="thomas_library" package="DO-219AB" value="VS-1EFU06-M3"/>
<element name="IC1" library="thomas_library" package="SOIC8" value="TLC555">
<attribute name="NAME"/>
</element>
<element name="L1" library="thomas_library" package="1200LRS" value="10mH"/>
<element name="Q1" library="thomas_library" package="SOT-23A" value="MMBT3904">
<attribute name="NAME"/>
</element>
<element name="Q2" library="thomas_library" package="TO-252" value="KSC5502"/>
<element name="R1" library="thomas_library" package="0805" value="330">
<attribute name="NAME"/>
</element>
<element name="R2" library="thomas_library" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R3" library="thomas_library" package="0805" value="220k">
<attribute name="NAME"/>
</element>
<element name="R4" library="thomas_library" package="0805" value="100k">
<attribute name="NAME"/>
</element>
<element name="R5" library="thomas_library" package="3362P" value="10"/>
<element name="R6" library="thomas_library" package="1206" value="10">
<attribute name="NAME"/>
</element>
<element name="R7" library="thomas_library" package="1206" value="4.7M">
<attribute name="NAME"/>
</element>
<element name="R8" library="thomas_library" package="1206" value="4.7M">
<attribute name="NAME"/>
</element>
<element name="TP1" library="thomas_library" package="TP" value="TP"/>
<element name="TP2" library="thomas_library" package="TP" value="TP"/>
<element name="U$14" library="logo" package="ESD_10.00" value=""/>
<element name="U$15" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
</elements>
<signals>
<signal name="N$2">
<contactref element="R4" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="R4" pad="2"/>
<contactref element="L1" pad="P3"/>
<contactref element="IC1" pad="8"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="6"/>
<contactref element="R5" pad="P$3"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="1"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="D1" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R5" pad="P$1"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="N$5">
<contactref element="Q1" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="Q2" pad="P$2"/>
</signal>
<signal name="N$7">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="7"/>
<contactref element="Q2" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="R7" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="D2" pad="P$2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R7" pad="2"/>
<contactref element="TP1" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="D2" pad="P$1"/>
<contactref element="Q2" pad="P$3"/>
<contactref element="L1" pad="P1"/>
</signal>
<signal name="N$13">
<contactref element="R8" pad="2"/>
<contactref element="TP2" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
