(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 60)
    (no_connects 0)
    (area 121.792999 59.562999 153.797001 118.237001)
    (thickness 1.6)
    (drawings 52)
    (tracks 265)
    (zones 0)
    (modules 32)
    (nets 36)
  )
  (page USLetter)
  (title_block
    (title "OSH Park Badge")
    (company www.MakersBox.us)
    (comment 1 "K. Olsen")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (user_trace_width 2.032)
    (trace_clearance 0.1524)
    (zone_clearance 1)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.254)
    (edge_width 0.254)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 1 0.5)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 1.00076)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 210.82 95.25)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /VBAT)
  (net 3 /D10)
  (net 4 /D11)
  (net 5 /D12)
  (net 6 /D13)
  (net 7 /D8)
  (net 8 /D4)
  (net 9 /D3)
  (net 10 "Net-(P3-Pad2)")
  (net 11 "Net-(P3-Pad1)")
  (net 12 "Net-(P4-Pad2)")
  (net 13 "Net-(P4-Pad1)")
  (net 14 "Net-(P5-Pad2)")
  (net 15 "Net-(P6-Pad2)")
  (net 16 "Net-(P3-Pad3)")
  (net 17 "Net-(P3-Pad4)")
  (net 18 "Net-(P4-Pad3)")
  (net 19 "Net-(P4-Pad4)")
  (net 20 /A4)
  (net 21 /A5)
  (net 22 /A0)
  (net 23 /A1)
  (net 24 /D6)
  (net 25 /D5)
  (net 26 "Net-(D2-Pad2)")
  (net 27 "Net-(D3-Pad2)")
  (net 28 "Net-(D4-Pad2)")
  (net 29 "Net-(D5-Pad2)")
  (net 30 /D9)
  (net 31 /A2)
  (net 32 /A3)
  (net 33 /3V3)
  (net 34 /D2)
  (net 35 /D1)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /3V3)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /D1)
    (add_net /D10)
    (add_net /D11)
    (add_net /D12)
    (add_net /D13)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D8)
    (add_net /D9)
    (add_net /VBAT)
    (add_net GND)
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P6-Pad2)")
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 59FAAA0B)
    (at 139.7 82.55 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 3.81 1.27 180) (layer F.SilkS) hide)
    (fp_text value 1uF (at -1.905 0.254 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VBAT))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:PHOTOTRANS (layer F.Cu) (tedit 59FA9756)
    (at 149.86 114.935 90)
    (descr LTR-4206)
    (tags "PHOTOTRANS NPN")
    (fp_text reference Q2 (at 0 2.54 270) (layer F.SilkS) hide)
    (fp_text value OPTO_NPN (at 0.35921 0.35921 180) (layer F.SilkS) hide)
    (fp_text user E (at -1.9 2 90) (layer F.SilkS))
    (fp_text user C (at 2.1 2.1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole circle (at 1.27 0 135) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /A2))
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:PHOTOTRANS (layer F.Cu) (tedit 59FA9731)
    (at 149.86 62.865 90)
    (descr LTR-4206)
    (tags "PHOTOTRANS NPN")
    (fp_text reference Q1 (at 0 2.54 270) (layer F.SilkS) hide)
    (fp_text value OPTO_NPN (at 0.35921 0.35921 180) (layer F.SilkS) hide)
    (fp_text user E (at -1.9 2 90) (layer F.SilkS))
    (fp_text user C (at 2.1 2.1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole circle (at 1.27 0 135) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A5))
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-18_W7.62mm (layer F.Cu) (tedit 59FBD34C)
    (at 142.24 107.95 180)
    (descr "18-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 2.54 10.16 270) (layer F.SilkS) hide)
    (fp_text value ULN2803 (at 5.08 10.16 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 /D10))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 /D11))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 /D12))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /D13))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 /D6))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 /D5))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 /D4))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 /D3))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 10 thru_hole oval (at 7.62 20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VBAT))
    (pad 11 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P4-Pad4)"))
    (pad 12 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P4-Pad3)"))
    (pad 13 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P4-Pad2)"))
    (pad 14 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P4-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P3-Pad4)"))
    (pad 16 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P3-Pad3)"))
    (pad 17 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P3-Pad2)"))
    (pad 18 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P3-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-18_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module library:JST_B5B-XH-A (layer F.Cu) (tedit 59CB0C0C)
    (at 124.46 109.22 90)
    (descr "JST XH series connector, JST_B5B-XH-A")
    (tags "connector jst xh")
    (fp_text reference P3 (at 3.81 -1.27 90) (layer F.SilkS))
    (fp_text value RIGHT_STEPPER (at 5.08 2.54 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P3-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P3-Pad3)"))
    (pad 4 thru_hole circle (at 7.5 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P3-Pad4)"))
    (pad 5 thru_hole circle (at 10 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VBAT))
    (model ./kicad-jst-xh.3dshapes/JST_B5B-XH-A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937007874 0.3937007874 0.3937007874))
      (rotate (xyz 0 0 0))
    )
  )
  (module library:JST_B5B-XH-A (layer F.Cu) (tedit 59CB0BD4)
    (at 124.46 93.98 90)
    (descr "JST XH series connector, JST_B5B-XH-A")
    (tags "connector jst xh")
    (fp_text reference P4 (at 3.81 -1.27 90) (layer F.SilkS))
    (fp_text value LEFT_STEPPER (at 5.08 2.54 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P4-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P4-Pad3)"))
    (pad 4 thru_hole circle (at 7.5 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P4-Pad4)"))
    (pad 5 thru_hole circle (at 10 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VBAT))
    (model ./kicad-jst-xh.3dshapes/JST_B5B-XH-A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937007874 0.3937007874 0.3937007874))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Lego_Pad (layer F.Cu) (tedit 59BB65C9)
    (at 125.73 114.3)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -1.27) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:Lego_Pad (layer F.Cu) (tedit 59BB65D8)
    (at 143.51 114.3)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -1.27) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:Lego_Pad (layer F.Cu) (tedit 59BB65F8)
    (at 143.51 63.5)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -1.27) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:Lego_Pad (layer F.Cu) (tedit 59BB65E8)
    (at 125.73 63.5)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -1.27) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D7.5_L11.2_P2.5 (layer F.Cu) (tedit 59FAAA19)
    (at 137.16 70.485 180)
    (descr "Radial Electrolytic Capacitor Diameter 7.5mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 0 -2.54 180) (layer F.SilkS) hide)
    (fp_text value 100uF (at -2.667 4.064 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VBAT))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D7.5_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 59CB0C53)
    (at 137.16 78.105 180)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C2 (at 0 -1.27 180) (layer F.SilkS) hide)
    (fp_text value 10uF (at -2.286 -0.254 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VBAT))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12 (layer F.Cu) (tedit 59BB62B7)
    (at 144.78 110.49 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -2.54 180) (layer Dwgs.User) hide)
    (fp_text value TRINKET_LEFT (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /D9))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /D10))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /D11))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /D12))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /D13))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A0))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A1))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /A2))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /A3))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A4))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A5))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12 (layer F.Cu) (tedit 59BB62C4)
    (at 129.54 110.49 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -2.54 180) (layer Dwgs.User) hide)
    (fp_text value TRINKET_RIGHT (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VBAT))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /3V3))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /D8))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /D6))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /D5))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /D4))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /D3))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /D2))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /D1))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 59FAA408)
    (at 142.24 76.2 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0 7.62 270) (layer F.SilkS) hide)
    (fp_text value SERVO (at 0 8.89 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /D8))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VBAT))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:SW_Micro_SPST (layer F.Cu) (tedit 59BB6BCA)
    (at 134.62 63.5)
    (tags "Switch Micro SPST")
    (fp_text reference SW1 (at 2.286 -1.778) (layer F.SilkS) hide)
    (fp_text value SPST (at 2.54 -1.905) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P6-Pad2)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VBAT))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_Micro_SPST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.33 0.33 0.33))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 59BB6A7D)
    (at 137.16 116.205 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at 2.54 1.27 360) (layer F.SilkS) hide)
    (fp_text value "A5 - A1" (at 0 2.54 360) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A0))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A1))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:MadeInOregonRev25 (layer F.Cu) (tedit 0)
    (at 138.43 102.235 90)
    (fp_text reference VAL (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value MadeInOregonRev25 (at 0 0 90) (layer F.SilkS) hide)
  )
  (module myFootPrints:MB225rev (layer F.Cu) (tedit 0)
    (at 138.43 109.22 90)
    (fp_text reference VAL (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value MB225rev (at 0 0 90) (layer F.SilkS) hide)
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol (layer F.Cu) (tedit 59FAA9A9)
    (at 128.016 68.072 270)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P5 (at 2.032 -2.286 270) (layer F.SilkS) hide)
    (fp_text value BATT1 (at 1.75 6 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol (layer F.Cu) (tedit 59FAA99C)
    (at 128.016 75.438 270)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P6 (at 1.778 -2.286 270) (layer F.SilkS) hide)
    (fp_text value BATT2 (at 1.75 6 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P6-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P5-Pad2)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 59FA9767)
    (at 149.86 111.125 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D2 (at 1.27 0.635 90) (layer F.SilkS) hide)
    (fp_text value IR_LED (at 1.3 -2.9 90) (layer F.Fab))
    (fp_text user K (at -3.81 -1.27 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 59FA977B)
    (at 149.86 74.295 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D3 (at 1.27 1.27 90) (layer F.SilkS) hide)
    (fp_text value IR_LED (at 1.3 -2.9 90) (layer F.Fab))
    (fp_text user K (at 1.27 -1.27 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 59FA976F)
    (at 149.86 106.045 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D4 (at 1.27 1.27 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.3 -2.9 90) (layer F.Fab))
    (fp_text user K (at -3.81 -1.27 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(D4-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 59FA9785)
    (at 149.86 69.215 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D5 (at 1.27 1.27 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.3 -2.9 90) (layer F.Fab))
    (fp_text user K (at -3.81 1.27 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(D5-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 5664956A)
    (at 148.59 97.79 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R2 (at 0 -1.905 270) (layer F.Fab))
    (fp_text value 100 (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 30 /D9))
    (pad 2 thru_hole circle (at 3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 26 "Net-(D2-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 5664956A)
    (at 148.59 80.01 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R3 (at 0 -1.905 90) (layer F.Fab))
    (fp_text value 100 (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 20 /A4))
    (pad 2 thru_hole circle (at 3.175 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 27 "Net-(D3-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 5664956A)
    (at 151.13 97.79 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R4 (at 0 -1.905 270) (layer F.Fab))
    (fp_text value 330 (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 34 /D2))
    (pad 2 thru_hole circle (at 3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 28 "Net-(D4-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 5664956A)
    (at 151.13 80.01 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R5 (at 0 -1.905 90) (layer F.Fab))
    (fp_text value 330 (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 35 /D1))
    (pad 2 thru_hole circle (at 3.175 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 29 "Net-(D5-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 59FA8CC2)
    (at 132.334 102.362 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R6 (at 0 -1.905 270) (layer F.Fab))
    (fp_text value 10K (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 33 /3V3))
    (pad 2 thru_hole circle (at 3.175 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 31 /A2))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 59FA8CE6)
    (at 132.334 85.852 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R7 (at 0 -1.905 90) (layer F.Fab))
    (fp_text value 10K (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 33 /3V3))
    (pad 2 thru_hole circle (at 3.175 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 21 /A5))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:SW_PUSH_SMALL (layer F.Cu) (tedit 57A15124)
    (at 149.86 88.9 90)
    (fp_text reference SW2 (at 0 0 90) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 2 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 3.25 -2.25 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 32 /A3))
    (pad 2 thru_hole circle (at 3.25 2.25 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at -3.25 -2.25 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 32 /A3))
    (pad 2 thru_hole circle (at -3.25 2.25 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (gr_text "Darlington Array" (at 139.7 98.425 90) (layer F.SilkS))
  (gr_text + (at 136.525 76.2) (layer B.SilkS))
  (gr_text + (at 136.525 68.58) (layer B.SilkS))
  (gr_text + (at 147.955 71.12) (layer B.SilkS))
  (gr_text + (at 147.955 66.04) (layer B.SilkS))
  (gr_text + (at 147.955 102.87) (layer B.SilkS))
  (gr_text + (at 147.955 107.95) (layer B.SilkS))
  (gr_text A5 (at 147.32 64.135 90) (layer F.SilkS))
  (gr_text D1 (at 147.32 69.215 90) (layer F.SilkS))
  (gr_text D18 (at 147.32 74.295 90) (layer F.SilkS))
  (gr_text D2 (at 147.32 106.045 90) (layer F.SilkS))
  (gr_text D9 (at 147.32 111.76 90) (layer F.SilkS))
  (gr_text A2 (at 147.32 116.84 90) (layer F.SilkS))
  (gr_line (start 148.59 59.69) (end 149.86 59.69) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 148.59 118.11) (end 149.86 118.11) (angle 90) (layer Edge.Cuts) (width 0.254))
  (dimension 8 (width 0.3) (layer Dwgs.User)
    (gr_text "8.000 mm" (at 159.17 71.25 90) (layer Dwgs.User))
    (feature1 (pts (xy 135.82 67.25) (xy 160.52 67.25)))
    (feature2 (pts (xy 135.82 75.25) (xy 160.52 75.25)))
    (crossbar (pts (xy 157.82 75.25) (xy 157.82 67.25)))
    (arrow1a (pts (xy 157.82 67.25) (xy 158.406421 68.376504)))
    (arrow1b (pts (xy 157.82 67.25) (xy 157.233579 68.376504)))
    (arrow2a (pts (xy 157.82 75.25) (xy 158.406421 74.123496)))
    (arrow2b (pts (xy 157.82 75.25) (xy 157.233579 74.123496)))
  )
  (dimension 17.78 (width 0.3) (layer Dwgs.User)
    (gr_text "0.7000 in" (at 134.62 54.53) (layer Dwgs.User))
    (feature1 (pts (xy 143.51 63.5) (xy 143.51 53.18)))
    (feature2 (pts (xy 125.73 63.5) (xy 125.73 53.18)))
    (crossbar (pts (xy 125.73 55.88) (xy 143.51 55.88)))
    (arrow1a (pts (xy 143.51 55.88) (xy 142.383496 56.466421)))
    (arrow1b (pts (xy 143.51 55.88) (xy 142.383496 55.293579)))
    (arrow2a (pts (xy 125.73 55.88) (xy 126.856504 56.466421)))
    (arrow2b (pts (xy 125.73 55.88) (xy 126.856504 55.293579)))
  )
  (gr_text + (at 147.955 107.95) (layer F.SilkS))
  (gr_text + (at 147.955 102.87) (layer F.SilkS))
  (gr_text + (at 136.525 76.2) (layer F.SilkS))
  (gr_text + (at 136.525 68.58) (layer F.SilkS))
  (gr_text + (at 147.955 66.04) (layer F.SilkS))
  (gr_text + (at 147.955 71.12) (layer F.SilkS))
  (gr_text LED (at 152.4 74.93 90) (layer F.SilkS))
  (gr_text IR (at 152.4 69.215 90) (layer F.SilkS))
  (gr_text LED (at 152.4 102.87 90) (layer F.SilkS))
  (gr_text IR (at 152.4 108.585 90) (layer F.SilkS))
  (gr_line (start 143.51 59.69) (end 148.59 59.69) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 143.51 118.11) (end 148.59 118.11) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 153.67 114.3) (end 153.67 63.5) (angle 90) (layer Edge.Cuts) (width 0.254))
  (dimension 58.42 (width 0.3) (layer Dwgs.User)
    (gr_text "2.3000 in" (at 111.68 88.9 90) (layer Dwgs.User))
    (feature1 (pts (xy 123.19 59.69) (xy 110.33 59.69)))
    (feature2 (pts (xy 123.19 118.11) (xy 110.33 118.11)))
    (crossbar (pts (xy 113.03 118.11) (xy 113.03 59.69)))
    (arrow1a (pts (xy 113.03 59.69) (xy 113.616421 60.816504)))
    (arrow1b (pts (xy 113.03 59.69) (xy 112.443579 60.816504)))
    (arrow2a (pts (xy 113.03 118.11) (xy 113.616421 116.983496)))
    (arrow2b (pts (xy 113.03 118.11) (xy 112.443579 116.983496)))
  )
  (dimension 50.8 (width 0.3) (layer Dwgs.User)
    (gr_text "2.0000 in" (at 116.76 88.9 270) (layer Dwgs.User))
    (feature1 (pts (xy 125.73 114.3) (xy 115.41 114.3)))
    (feature2 (pts (xy 125.73 63.5) (xy 115.41 63.5)))
    (crossbar (pts (xy 118.11 63.5) (xy 118.11 114.3)))
    (arrow1a (pts (xy 118.11 114.3) (xy 117.523579 113.173496)))
    (arrow1b (pts (xy 118.11 114.3) (xy 118.696421 113.173496)))
    (arrow2a (pts (xy 118.11 63.5) (xy 117.523579 64.626504)))
    (arrow2b (pts (xy 118.11 63.5) (xy 118.696421 64.626504)))
  )
  (gr_text A0 (at 140.335 116.84) (layer F.SilkS))
  (gr_text A1 (at 129.54 116.84) (layer F.SilkS))
  (gr_text "BATT_1 BATT_2" (at 130.302 73.406 90) (layer F.SilkS))
  (gr_text "Ver 0.2\nNov 2017" (at 138.43 86.36 90) (layer B.SilkS))
  (gr_text "Trinket Robot Shield" (at 127 95.25 90) (layer B.SilkS))
  (dimension 25.4 (width 0.3) (layer Dwgs.User)
    (gr_text "1.00 in" (at 134.62 50.72) (layer Dwgs.User))
    (feature1 (pts (xy 147.32 60.96) (xy 147.32 49.37)))
    (feature2 (pts (xy 121.92 60.96) (xy 121.92 49.37)))
    (crossbar (pts (xy 121.92 52.07) (xy 147.32 52.07)))
    (arrow1a (pts (xy 147.32 52.07) (xy 146.193496 52.656421)))
    (arrow1b (pts (xy 147.32 52.07) (xy 146.193496 51.483579)))
    (arrow2a (pts (xy 121.92 52.07) (xy 123.046504 52.656421)))
    (arrow2b (pts (xy 121.92 52.07) (xy 123.046504 51.483579)))
  )
  (gr_text GND (at 134.62 113.03) (layer F.SilkS))
  (gr_text "S + -" (at 144.78 73.66 90) (layer F.SilkS))
  (gr_line (start 143.51 59.69) (end 125.73 59.69) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 121.92 66.04) (end 121.92 63.5) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 121.92 114.3) (end 121.92 113.03) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 125.73 118.11) (end 143.51 118.11) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_arc (start 149.86 114.3) (end 153.67 114.3) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_arc (start 125.73 114.3) (end 125.73 118.11) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_arc (start 149.86 63.5) (end 149.86 59.69) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_arc (start 125.73 63.5) (end 121.92 63.5) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_text "-  +   -  +" (at 123.19 73.025 270) (layer F.SilkS))
  (gr_text "OFF       ON" (at 134.62 60.96 180) (layer F.SilkS))
  (gr_line (start 121.92 113.03) (end 121.92 66.04) (angle 90) (layer Edge.Cuts) (width 0.254))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.82 119.25) (xy 120.82 119.25) (xy 120.82 59.25) (xy 153.82 59.25)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.82 121.25) (xy 119.82 121.25) (xy 119.82 57.25) (xy 154.82 57.25)
      )
    )
  )
)
