(kicad_pcb (version 20170919) (host pcbnew "(2017-09-19 revision dddaa7e69)-makepkg")
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 3538)
    (zones 0)
    (modules 124)
    (nets 287)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 GND.Cu power)
    (2 PWR.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.127)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (trace_clearance 0.1016)
    (zone_clearance 0.127)
    (zone_45_only no)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (user_via 0.762 0.508)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 25.4 120.65)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U6-Pad44)")
  (net 2 "Net-(U6-Pad43)")
  (net 3 "Net-(U6-Pad42)")
  (net 4 "Net-(U6-Pad25)")
  (net 5 "Net-(U6-Pad24)")
  (net 6 "Net-(U6-Pad23)")
  (net 7 "Net-(U6-Pad22)")
  (net 8 "Net-(U6-Pad21)")
  (net 9 "Net-(U6-Pad2)")
  (net 10 "Net-(U6-Pad1)")
  (net 11 GND)
  (net 12 +3V3)
  (net 13 "/CPU Memory/~CS0")
  (net 14 "/CPU Memory/~CS1")
  (net 15 /CPU/~CS3)
  (net 16 "Net-(U7-Pad44)")
  (net 17 "Net-(U7-Pad43)")
  (net 18 "Net-(U7-Pad42)")
  (net 19 "Net-(U7-Pad25)")
  (net 20 "Net-(U7-Pad24)")
  (net 21 "Net-(U7-Pad23)")
  (net 22 "Net-(U7-Pad22)")
  (net 23 "Net-(U7-Pad21)")
  (net 24 "Net-(U7-Pad2)")
  (net 25 "Net-(U7-Pad1)")
  (net 26 "Net-(U16-Pad44)")
  (net 27 "Net-(U16-Pad43)")
  (net 28 "Net-(U16-Pad42)")
  (net 29 /A18)
  (net 30 /A17)
  (net 31 /A16)
  (net 32 /A15)
  (net 33 /~RD)
  (net 34 /D7)
  (net 35 /D6)
  (net 36 /D5)
  (net 37 /D4)
  (net 38 /A14)
  (net 39 /A13)
  (net 40 /A12)
  (net 41 /A11)
  (net 42 /A10)
  (net 43 "Net-(U16-Pad25)")
  (net 44 "Net-(U16-Pad24)")
  (net 45 "Net-(U16-Pad23)")
  (net 46 "Net-(U16-Pad22)")
  (net 47 "Net-(U16-Pad21)")
  (net 48 /A9)
  (net 49 /A8)
  (net 50 /A7)
  (net 51 /A6)
  (net 52 /A5)
  (net 53 /~WR)
  (net 54 /D3)
  (net 55 /D2)
  (net 56 /D1)
  (net 57 /D0)
  (net 58 /A4)
  (net 59 /A3)
  (net 60 /A2)
  (net 61 /A1)
  (net 62 /A0)
  (net 63 "Net-(U16-Pad2)")
  (net 64 "Net-(U16-Pad1)")
  (net 65 "Net-(U17-Pad1)")
  (net 66 "Net-(U17-Pad2)")
  (net 67 "/CPU Memory/~CS2")
  (net 68 "Net-(U17-Pad21)")
  (net 69 "Net-(U17-Pad22)")
  (net 70 "Net-(U17-Pad23)")
  (net 71 "Net-(U17-Pad24)")
  (net 72 "Net-(U17-Pad25)")
  (net 73 "Net-(U17-Pad42)")
  (net 74 "Net-(U17-Pad43)")
  (net 75 "Net-(U17-Pad44)")
  (net 76 "Net-(U8-Pad44)")
  (net 77 "Net-(U8-Pad43)")
  (net 78 "Net-(U8-Pad42)")
  (net 79 "Net-(U8-Pad25)")
  (net 80 "Net-(U8-Pad24)")
  (net 81 "Net-(U8-Pad23)")
  (net 82 "Net-(U8-Pad22)")
  (net 83 "Net-(U8-Pad21)")
  (net 84 "Net-(U8-Pad2)")
  (net 85 "Net-(U8-Pad1)")
  (net 86 "Net-(U9-Pad1)")
  (net 87 "Net-(U9-Pad2)")
  (net 88 "Net-(U9-Pad21)")
  (net 89 "Net-(U9-Pad22)")
  (net 90 "Net-(U9-Pad23)")
  (net 91 "Net-(U9-Pad24)")
  (net 92 "Net-(U9-Pad25)")
  (net 93 "Net-(U9-Pad42)")
  (net 94 "Net-(U9-Pad43)")
  (net 95 "Net-(U9-Pad44)")
  (net 96 "Net-(D1-Pad1)")
  (net 97 "Net-(C4-Pad1)")
  (net 98 /LED_A)
  (net 99 "/Graphics Controller/R0")
  (net 100 "/Graphics Controller/R1")
  (net 101 "/Graphics Controller/R2")
  (net 102 "/Graphics Controller/R3")
  (net 103 "/Graphics Controller/R4")
  (net 104 "/Graphics Controller/R5")
  (net 105 "/Graphics Controller/R6")
  (net 106 "/Graphics Controller/R7")
  (net 107 "/Graphics Controller/G0")
  (net 108 "/Graphics Controller/G1")
  (net 109 "/Graphics Controller/G2")
  (net 110 "/Graphics Controller/G3")
  (net 111 "/Graphics Controller/G4")
  (net 112 "/Graphics Controller/G5")
  (net 113 "/Graphics Controller/G6")
  (net 114 "/Graphics Controller/G7")
  (net 115 "/Graphics Controller/B0")
  (net 116 "/Graphics Controller/B1")
  (net 117 "/Graphics Controller/B2")
  (net 118 "/Graphics Controller/B3")
  (net 119 "/Graphics Controller/B4")
  (net 120 "/Graphics Controller/B5")
  (net 121 "/Graphics Controller/B6")
  (net 122 "/Graphics Controller/B7")
  (net 123 "/Graphics Controller/DCLK")
  (net 124 "/Graphics Controller/HSYNC")
  (net 125 "/Graphics Controller/VSYNC")
  (net 126 "/Graphics Controller/DEN")
  (net 127 "Net-(J3-Pad35)")
  (net 128 "Net-(J3-Pad37)")
  (net 129 "Net-(J3-Pad38)")
  (net 130 "Net-(J3-Pad39)")
  (net 131 "Net-(J3-Pad40)")
  (net 132 "Net-(C2-Pad1)")
  (net 133 "Net-(BT1-Pad1)")
  (net 134 "Net-(C58-Pad1)")
  (net 135 /CLK1)
  (net 136 "Net-(U18-Pad3)")
  (net 137 /CLK0)
  (net 138 /CLK2)
  (net 139 "Net-(L3-Pad1)")
  (net 140 +1V2)
  (net 141 "Net-(D2-Pad3)")
  (net 142 /LED_PWM)
  (net 143 "Net-(D2-Pad2)")
  (net 144 "Net-(R15-Pad1)")
  (net 145 "Net-(C56-Pad1)")
  (net 146 "Net-(D3-Pad2)")
  (net 147 "Net-(C17-Pad1)")
  (net 148 "Net-(C18-Pad1)")
  (net 149 "/Graphics Controller/SS_B")
  (net 150 "Net-(R8-Pad2)")
  (net 151 "Net-(D4-Pad1)")
  (net 152 "/Graphics Controller/SCK")
  (net 153 /RESET)
  (net 154 /~WAIT)
  (net 155 /CPU_RESET)
  (net 156 /INT)
  (net 157 /~MREQ)
  (net 158 /~IOREQ)
  (net 159 /~BUSREQ)
  (net 160 /~BUSACK)
  (net 161 /A23)
  (net 162 /A22)
  (net 163 /A21)
  (net 164 /A20)
  (net 165 /A19)
  (net 166 "/Graphics Controller/SDO")
  (net 167 "/Graphics Controller/SDI")
  (net 168 "Net-(J4-Pad4)")
  (net 169 "Net-(J4-Pad3)")
  (net 170 "Net-(J4-Pad1)")
  (net 171 "Net-(C49-Pad1)")
  (net 172 "Net-(C53-Pad1)")
  (net 173 "Net-(C49-Pad2)")
  (net 174 "Net-(U12-Pad21)")
  (net 175 /CPU/L_RI1)
  (net 176 /CPU/L_RXD1)
  (net 177 "Net-(U12-Pad18)")
  (net 178 /CPU/L_CTS1)
  (net 179 /CPU/L_DSR1)
  (net 180 /CPU/L_DCD1)
  (net 181 /CPU/L_TXD1)
  (net 182 /CPU/L_RTS1)
  (net 183 /CPU/L_DTR1)
  (net 184 /CPU/R_DTR1)
  (net 185 /CPU/R_RTS1)
  (net 186 /CPU/R_TXD1)
  (net 187 /CPU/R_DCD1)
  (net 188 /CPU/R_DSR1)
  (net 189 /CPU/R_CTS1)
  (net 190 /CPU/R_RI1)
  (net 191 /CPU/R_RXD1)
  (net 192 "Net-(C54-Pad1)")
  (net 193 "Net-(C50-Pad2)")
  (net 194 "Net-(C50-Pad1)")
  (net 195 "Net-(C48-Pad1)")
  (net 196 "Net-(C48-Pad2)")
  (net 197 "Net-(C52-Pad1)")
  (net 198 /CPU/R_RXD0)
  (net 199 /CPU/R_RI0)
  (net 200 /CPU/R_CTS0)
  (net 201 /CPU/R_DSR0)
  (net 202 /CPU/R_DCD0)
  (net 203 /CPU/R_TXD0)
  (net 204 /CPU/R_RTS0)
  (net 205 /CPU/R_DTR0)
  (net 206 /CPU/L_DTR0)
  (net 207 /CPU/L_RTS0)
  (net 208 /CPU/L_TXD0)
  (net 209 /CPU/L_DCD0)
  (net 210 /CPU/L_DSR0)
  (net 211 /CPU/L_CTS0)
  (net 212 "Net-(U11-Pad18)")
  (net 213 /CPU/L_RXD0)
  (net 214 /CPU/L_RI0)
  (net 215 "Net-(U11-Pad21)")
  (net 216 "Net-(C47-Pad2)")
  (net 217 "Net-(C51-Pad1)")
  (net 218 "Net-(C47-Pad1)")
  (net 219 /CPU/MISO)
  (net 220 /CPU/MOSI)
  (net 221 /CPU/SCK)
  (net 222 "Net-(U4-Pad133)")
  (net 223 "Net-(C17-Pad2)")
  (net 224 "Net-(U4-Pad109)")
  (net 225 "Net-(U4-Pad77)")
  (net 226 "Net-(U4-Pad58)")
  (net 227 "Net-(C18-Pad2)")
  (net 228 "Net-(U4-Pad51)")
  (net 229 "Net-(U4-Pad50)")
  (net 230 "Net-(U4-Pad36)")
  (net 231 "Net-(U4-Pad35)")
  (net 232 "/Graphics Controller/GPU_D7")
  (net 233 "/Graphics Controller/GPU_D6")
  (net 234 "/Graphics Controller/GPU_D5")
  (net 235 "/Graphics Controller/GPU_D4")
  (net 236 "/Graphics Controller/GPU_D3")
  (net 237 "/Graphics Controller/GPU_D2")
  (net 238 "/Graphics Controller/GPU_D1")
  (net 239 "/Graphics Controller/GPU_D0")
  (net 240 "/Graphics Controller/GPU_A18")
  (net 241 "/Graphics Controller/GPU_A17")
  (net 242 "/Graphics Controller/GPU_A16")
  (net 243 "/Graphics Controller/GPU_A15")
  (net 244 "/Graphics Controller/GPU_A14")
  (net 245 "/Graphics Controller/GPU_A13")
  (net 246 "/Graphics Controller/GPU_A12")
  (net 247 "/Graphics Controller/GPU_A11")
  (net 248 "/Graphics Controller/GPU_A10")
  (net 249 "/Graphics Controller/GPU_A9")
  (net 250 "/Graphics Controller/GPU_A8")
  (net 251 "/Graphics Controller/GPU_A7")
  (net 252 "/Graphics Controller/GPU_A6")
  (net 253 "/Graphics Controller/GPU_A5")
  (net 254 "/Graphics Controller/GPU_A4")
  (net 255 "/Graphics Controller/GPU_A3")
  (net 256 "/Graphics Controller/GPU_A2")
  (net 257 "/Graphics Controller/GPU_A1")
  (net 258 "/Graphics Controller/GPU_A0")
  (net 259 "Net-(U10-Pad100)")
  (net 260 "Net-(U10-Pad93)")
  (net 261 "Net-(U10-Pad92)")
  (net 262 "Net-(U10-Pad89)")
  (net 263 "Net-(U10-Pad88)")
  (net 264 "Net-(U10-Pad86)")
  (net 265 "Net-(U10-Pad66)")
  (net 266 "Net-(U10-Pad65)")
  (net 267 "Net-(U10-Pad64)")
  (net 268 "Net-(U10-Pad63)")
  (net 269 "Net-(U10-Pad62)")
  (net 270 "Net-(C57-Pad1)")
  (net 271 "Net-(U10-Pad55)")
  (net 272 "Net-(U10-Pad49)")
  (net 273 "Net-(F1-Pad1)")
  (net 274 "Net-(J5-Pad0)")
  (net 275 "Net-(J6-Pad0)")
  (net 276 "Net-(J2-Pad3)")
  (net 277 "/Graphics Controller/~GPU_OE")
  (net 278 "/Graphics Controller/~GPU_WE")
  (net 279 "/Graphics Controller/~GPU_CS1")
  (net 280 "/Graphics Controller/~GPU_CS0")
  (net 281 "/Graphics Controller/~GPU_CS2")
  (net 282 "/Graphics Controller/~GPU_CS3")
  (net 283 "Net-(R17-Pad2)")
  (net 284 "Net-(R16-Pad2)")
  (net 285 "Net-(R13-Pad2)")
  (net 286 "Net-(C55-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1016)
    (trace_width 0.25)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A17)
    (add_net /A18)
    (add_net /A19)
    (add_net /A2)
    (add_net /A20)
    (add_net /A21)
    (add_net /A22)
    (add_net /A23)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /CLK0)
    (add_net /CLK1)
    (add_net /CLK2)
    (add_net "/CPU Memory/~CS0")
    (add_net "/CPU Memory/~CS1")
    (add_net "/CPU Memory/~CS2")
    (add_net /CPU/L_CTS0)
    (add_net /CPU/L_CTS1)
    (add_net /CPU/L_DCD0)
    (add_net /CPU/L_DCD1)
    (add_net /CPU/L_DSR0)
    (add_net /CPU/L_DSR1)
    (add_net /CPU/L_DTR0)
    (add_net /CPU/L_DTR1)
    (add_net /CPU/L_RI0)
    (add_net /CPU/L_RI1)
    (add_net /CPU/L_RTS0)
    (add_net /CPU/L_RTS1)
    (add_net /CPU/L_RXD0)
    (add_net /CPU/L_RXD1)
    (add_net /CPU/L_TXD0)
    (add_net /CPU/L_TXD1)
    (add_net /CPU/MISO)
    (add_net /CPU/MOSI)
    (add_net /CPU/R_CTS0)
    (add_net /CPU/R_CTS1)
    (add_net /CPU/R_DCD0)
    (add_net /CPU/R_DCD1)
    (add_net /CPU/R_DSR0)
    (add_net /CPU/R_DSR1)
    (add_net /CPU/R_DTR0)
    (add_net /CPU/R_DTR1)
    (add_net /CPU/R_RI0)
    (add_net /CPU/R_RI1)
    (add_net /CPU/R_RTS0)
    (add_net /CPU/R_RTS1)
    (add_net /CPU/R_RXD0)
    (add_net /CPU/R_RXD1)
    (add_net /CPU/R_TXD0)
    (add_net /CPU/R_TXD1)
    (add_net /CPU/SCK)
    (add_net /CPU/~CS3)
    (add_net /CPU_RESET)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net "/Graphics Controller/B0")
    (add_net "/Graphics Controller/B1")
    (add_net "/Graphics Controller/B2")
    (add_net "/Graphics Controller/B3")
    (add_net "/Graphics Controller/B4")
    (add_net "/Graphics Controller/B5")
    (add_net "/Graphics Controller/B6")
    (add_net "/Graphics Controller/B7")
    (add_net "/Graphics Controller/DCLK")
    (add_net "/Graphics Controller/DEN")
    (add_net "/Graphics Controller/G0")
    (add_net "/Graphics Controller/G1")
    (add_net "/Graphics Controller/G2")
    (add_net "/Graphics Controller/G3")
    (add_net "/Graphics Controller/G4")
    (add_net "/Graphics Controller/G5")
    (add_net "/Graphics Controller/G6")
    (add_net "/Graphics Controller/G7")
    (add_net "/Graphics Controller/GPU_A0")
    (add_net "/Graphics Controller/GPU_A1")
    (add_net "/Graphics Controller/GPU_A10")
    (add_net "/Graphics Controller/GPU_A11")
    (add_net "/Graphics Controller/GPU_A12")
    (add_net "/Graphics Controller/GPU_A13")
    (add_net "/Graphics Controller/GPU_A14")
    (add_net "/Graphics Controller/GPU_A15")
    (add_net "/Graphics Controller/GPU_A16")
    (add_net "/Graphics Controller/GPU_A17")
    (add_net "/Graphics Controller/GPU_A18")
    (add_net "/Graphics Controller/GPU_A2")
    (add_net "/Graphics Controller/GPU_A3")
    (add_net "/Graphics Controller/GPU_A4")
    (add_net "/Graphics Controller/GPU_A5")
    (add_net "/Graphics Controller/GPU_A6")
    (add_net "/Graphics Controller/GPU_A7")
    (add_net "/Graphics Controller/GPU_A8")
    (add_net "/Graphics Controller/GPU_A9")
    (add_net "/Graphics Controller/GPU_D0")
    (add_net "/Graphics Controller/GPU_D1")
    (add_net "/Graphics Controller/GPU_D2")
    (add_net "/Graphics Controller/GPU_D3")
    (add_net "/Graphics Controller/GPU_D4")
    (add_net "/Graphics Controller/GPU_D5")
    (add_net "/Graphics Controller/GPU_D6")
    (add_net "/Graphics Controller/GPU_D7")
    (add_net "/Graphics Controller/HSYNC")
    (add_net "/Graphics Controller/R0")
    (add_net "/Graphics Controller/R1")
    (add_net "/Graphics Controller/R2")
    (add_net "/Graphics Controller/R3")
    (add_net "/Graphics Controller/R4")
    (add_net "/Graphics Controller/R5")
    (add_net "/Graphics Controller/R6")
    (add_net "/Graphics Controller/R7")
    (add_net "/Graphics Controller/SCK")
    (add_net "/Graphics Controller/SDI")
    (add_net "/Graphics Controller/SDO")
    (add_net "/Graphics Controller/SS_B")
    (add_net "/Graphics Controller/VSYNC")
    (add_net "/Graphics Controller/~GPU_CS0")
    (add_net "/Graphics Controller/~GPU_CS1")
    (add_net "/Graphics Controller/~GPU_CS2")
    (add_net "/Graphics Controller/~GPU_CS3")
    (add_net "/Graphics Controller/~GPU_OE")
    (add_net "/Graphics Controller/~GPU_WE")
    (add_net /INT)
    (add_net /LED_A)
    (add_net /LED_PWM)
    (add_net /RESET)
    (add_net /~BUSACK)
    (add_net /~BUSREQ)
    (add_net /~IOREQ)
    (add_net /~MREQ)
    (add_net /~RD)
    (add_net /~WAIT)
    (add_net /~WR)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C47-Pad1)")
    (add_net "Net-(C47-Pad2)")
    (add_net "Net-(C48-Pad1)")
    (add_net "Net-(C48-Pad2)")
    (add_net "Net-(C49-Pad1)")
    (add_net "Net-(C49-Pad2)")
    (add_net "Net-(C50-Pad1)")
    (add_net "Net-(C50-Pad2)")
    (add_net "Net-(C51-Pad1)")
    (add_net "Net-(C52-Pad1)")
    (add_net "Net-(C53-Pad1)")
    (add_net "Net-(C54-Pad1)")
    (add_net "Net-(C55-Pad1)")
    (add_net "Net-(C56-Pad1)")
    (add_net "Net-(C57-Pad1)")
    (add_net "Net-(C58-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D2-Pad3)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad35)")
    (add_net "Net-(J3-Pad37)")
    (add_net "Net-(J3-Pad38)")
    (add_net "Net-(J3-Pad39)")
    (add_net "Net-(J3-Pad40)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J5-Pad0)")
    (add_net "Net-(J6-Pad0)")
    (add_net "Net-(L3-Pad1)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(U10-Pad100)")
    (add_net "Net-(U10-Pad49)")
    (add_net "Net-(U10-Pad55)")
    (add_net "Net-(U10-Pad62)")
    (add_net "Net-(U10-Pad63)")
    (add_net "Net-(U10-Pad64)")
    (add_net "Net-(U10-Pad65)")
    (add_net "Net-(U10-Pad66)")
    (add_net "Net-(U10-Pad86)")
    (add_net "Net-(U10-Pad88)")
    (add_net "Net-(U10-Pad89)")
    (add_net "Net-(U10-Pad92)")
    (add_net "Net-(U10-Pad93)")
    (add_net "Net-(U11-Pad18)")
    (add_net "Net-(U11-Pad21)")
    (add_net "Net-(U12-Pad18)")
    (add_net "Net-(U12-Pad21)")
    (add_net "Net-(U16-Pad1)")
    (add_net "Net-(U16-Pad2)")
    (add_net "Net-(U16-Pad21)")
    (add_net "Net-(U16-Pad22)")
    (add_net "Net-(U16-Pad23)")
    (add_net "Net-(U16-Pad24)")
    (add_net "Net-(U16-Pad25)")
    (add_net "Net-(U16-Pad42)")
    (add_net "Net-(U16-Pad43)")
    (add_net "Net-(U16-Pad44)")
    (add_net "Net-(U17-Pad1)")
    (add_net "Net-(U17-Pad2)")
    (add_net "Net-(U17-Pad21)")
    (add_net "Net-(U17-Pad22)")
    (add_net "Net-(U17-Pad23)")
    (add_net "Net-(U17-Pad24)")
    (add_net "Net-(U17-Pad25)")
    (add_net "Net-(U17-Pad42)")
    (add_net "Net-(U17-Pad43)")
    (add_net "Net-(U17-Pad44)")
    (add_net "Net-(U18-Pad3)")
    (add_net "Net-(U4-Pad109)")
    (add_net "Net-(U4-Pad133)")
    (add_net "Net-(U4-Pad35)")
    (add_net "Net-(U4-Pad36)")
    (add_net "Net-(U4-Pad50)")
    (add_net "Net-(U4-Pad51)")
    (add_net "Net-(U4-Pad58)")
    (add_net "Net-(U4-Pad77)")
    (add_net "Net-(U6-Pad1)")
    (add_net "Net-(U6-Pad2)")
    (add_net "Net-(U6-Pad21)")
    (add_net "Net-(U6-Pad22)")
    (add_net "Net-(U6-Pad23)")
    (add_net "Net-(U6-Pad24)")
    (add_net "Net-(U6-Pad25)")
    (add_net "Net-(U6-Pad42)")
    (add_net "Net-(U6-Pad43)")
    (add_net "Net-(U6-Pad44)")
    (add_net "Net-(U7-Pad1)")
    (add_net "Net-(U7-Pad2)")
    (add_net "Net-(U7-Pad21)")
    (add_net "Net-(U7-Pad22)")
    (add_net "Net-(U7-Pad23)")
    (add_net "Net-(U7-Pad24)")
    (add_net "Net-(U7-Pad25)")
    (add_net "Net-(U7-Pad42)")
    (add_net "Net-(U7-Pad43)")
    (add_net "Net-(U7-Pad44)")
    (add_net "Net-(U8-Pad1)")
    (add_net "Net-(U8-Pad2)")
    (add_net "Net-(U8-Pad21)")
    (add_net "Net-(U8-Pad22)")
    (add_net "Net-(U8-Pad23)")
    (add_net "Net-(U8-Pad24)")
    (add_net "Net-(U8-Pad25)")
    (add_net "Net-(U8-Pad42)")
    (add_net "Net-(U8-Pad43)")
    (add_net "Net-(U8-Pad44)")
    (add_net "Net-(U9-Pad1)")
    (add_net "Net-(U9-Pad2)")
    (add_net "Net-(U9-Pad21)")
    (add_net "Net-(U9-Pad22)")
    (add_net "Net-(U9-Pad23)")
    (add_net "Net-(U9-Pad24)")
    (add_net "Net-(U9-Pad25)")
    (add_net "Net-(U9-Pad42)")
    (add_net "Net-(U9-Pad43)")
    (add_net "Net-(U9-Pad44)")
  )
  (net_class power ""
    (clearance 0.127)
    (trace_width 0.254)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V2)
    (add_net +3V3)
    (add_net GND)
  )
  (module footprints:EVP-AK (layer B.Cu) (tedit 5A00AA8D)
    (at 25.654 99.822 180)
    (fp_text reference SW2 (at -1.016 4.064 90) (layer B.SilkS))
    (fp_text value NMI (at 2 0 90) (layer B.Fab))
    (pad 0 smd rect (at -1.9 0 180) (size 1.1 1.4) (drill (offset -0.55 0)) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -2.3 -1.4 180) (size 1.1 0.7) (layers B.Cu B.Paste B.Mask)
      (net 285 "Net-(R13-Pad2)"))
    (pad 1 smd rect (at -2.3 1.4 180) (size 1.1 0.7) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 0 smd rect (at 0 -2.3 180) (size 1.35 0.4) (drill (offset -0.675 0.2)) (layers B.Cu B.Paste B.Mask))
    (pad 0 smd rect (at -0.95 -1.85 180) (size 0.4 0.4) (drill (offset 0.2 0.2)) (layers B.Cu B.Paste B.Mask))
    (pad 0 smd rect (at 0 -2.3 180) (size 0.65 1.15) (drill (offset -0.325 0.575)) (layers B.Cu B.Paste B.Mask))
    (pad 0 smd rect (at -0.95 1.85 180) (size 0.4 0.4) (drill (offset 0.2 -0.2)) (layers B.Cu B.Paste B.Mask))
    (pad 0 smd rect (at 0 2.3 180) (size 0.65 1.15) (drill (offset -0.325 -0.575)) (layers B.Cu B.Paste B.Mask))
    (pad 0 smd rect (at 0 2.3 180) (size 1.35 0.4) (drill (offset -0.675 -0.2)) (layers B.Cu B.Paste B.Mask))
    (pad 0 thru_hole circle (at -0.95 -1.85 180) (size 0.8 0.8) (drill 0.55) (layers *.Cu *.Mask))
    (pad 0 thru_hole circle (at -0.95 1.85 180) (size 0.8 0.8) (drill 0.55) (layers *.Cu *.Mask))
  )
  (module footprints:EVP-AK (layer B.Cu) (tedit 5A00AA8D)
    (at 25.654 109.982 180)
    (fp_text reference SW1 (at -1.016 4.064 90) (layer B.SilkS))
    (fp_text value RESET (at 2 0 90) (layer B.Fab))
    (pad 0 smd rect (at -1.9 0 180) (size 1.1 1.4) (drill (offset -0.55 0)) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -2.3 -1.4 180) (size 1.1 0.7) (layers B.Cu B.Paste B.Mask)
      (net 153 /RESET))
    (pad 1 smd rect (at -2.3 1.4 180) (size 1.1 0.7) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 0 smd rect (at 0 -2.3 180) (size 1.35 0.4) (drill (offset -0.675 0.2)) (layers B.Cu B.Paste B.Mask))
    (pad 0 smd rect (at -0.95 -1.85 180) (size 0.4 0.4) (drill (offset 0.2 0.2)) (layers B.Cu B.Paste B.Mask))
    (pad 0 smd rect (at 0 -2.3 180) (size 0.65 1.15) (drill (offset -0.325 0.575)) (layers B.Cu B.Paste B.Mask))
    (pad 0 smd rect (at -0.95 1.85 180) (size 0.4 0.4) (drill (offset 0.2 -0.2)) (layers B.Cu B.Paste B.Mask))
    (pad 0 smd rect (at 0 2.3 180) (size 0.65 1.15) (drill (offset -0.325 -0.575)) (layers B.Cu B.Paste B.Mask))
    (pad 0 smd rect (at 0 2.3 180) (size 1.35 0.4) (drill (offset -0.675 -0.2)) (layers B.Cu B.Paste B.Mask))
    (pad 0 thru_hole circle (at -0.95 -1.85 180) (size 0.8 0.8) (drill 0.55) (layers *.Cu *.Mask))
    (pad 0 thru_hole circle (at -0.95 1.85 180) (size 0.8 0.8) (drill 0.55) (layers *.Cu *.Mask))
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 33.528 101.6)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R14 (at 0 1.85) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 286 "Net-(C55-Pad1)"))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 285 "Net-(R13-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 33.528 96.52 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C55 (at 0 1.75 180) (layer B.SilkS))
    (fp_text value 2.2uF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 286 "Net-(C55-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 33.528 99.06 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R13 (at -3.302 0 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 285 "Net-(R13-Pad2)"))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 33.528 111.506 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 153 /RESET))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:DB9 (layer B.Cu) (tedit 59FDD3A1)
    (at 175.26 70.358 270)
    (fp_text reference J6 (at 0 13.335 270) (layer B.SilkS))
    (fp_text value "COM B" (at 0 2.54 270) (layer B.Fab))
    (pad 1 thru_hole rect (at -5.49 10.93 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 187 /CPU/R_DCD1))
    (pad 0 thru_hole circle (at -12.5 9.51 270) (size 5 5) (drill 3.15) (layers *.Cu *.Mask)
      (net 275 "Net-(J6-Pad0)"))
    (pad 2 thru_hole circle (at -2.75 10.93 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 191 /CPU/R_RXD1))
    (pad 3 thru_hole circle (at -0.01 10.93 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 186 /CPU/R_TXD1))
    (pad 4 thru_hole circle (at 2.73 10.93 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 184 /CPU/R_DTR1))
    (pad 5 thru_hole circle (at 5.47 10.93 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 6 thru_hole circle (at -4.12 8.09 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 188 /CPU/R_DSR1))
    (pad 7 thru_hole circle (at -1.38 8.09 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 185 /CPU/R_RTS1))
    (pad 8 thru_hole circle (at 1.36 8.09 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 189 /CPU/R_CTS1))
    (pad 9 thru_hole circle (at 4.1 8.09 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 190 /CPU/R_RI1))
    (pad 0 thru_hole circle (at 12.5 9.51 270) (size 5 5) (drill 3.15) (layers *.Cu *.Mask)
      (net 275 "Net-(J6-Pad0)"))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 59FE8FAC)
    (at 158.75 117.475)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK3 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 59FE8FB0)
    (at 158.75 57.277)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK2 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 59FE8FA1)
    (at 28.575 57.277)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK1 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 59FE8FA6)
    (at 28.575 117.475)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK4 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Fuse_Holders_and_Fuses:Fuse_SMD1206_HandSoldering (layer F.Cu) (tedit 0)
    (at 44.066 64.135)
    (descr "Fuse, Sicherung, SMD1206, Littlefuse-Wickmann 433 Series, Hand Soldering,")
    (tags "Fuse Sicherung SMD1206 Littlefuse-Wickmann 433 Series Hand Soldering ")
    (attr smd)
    (fp_text reference F1 (at 0.199 -2.44) (layer F.SilkS))
    (fp_text value 5A (at -0.15 2.5) (layer F.Fab))
    (pad 2 smd rect (at 2.09 0 90) (size 2.03 2.65) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at -2.09 0 90) (size 2.03 2.65) (layers F.Cu F.Paste F.Mask)
      (net 273 "Net-(F1-Pad1)"))
  )
  (module Connectors:Barrel_Jack_CUI_PJ-036AH-SMT (layer B.Cu) (tedit 59B0DEC6)
    (at 35.4 83.82 90)
    (descr "Surface-mount DC Barrel Jack, http://www.cui.com/product/resource/pj-036ah-smt.pdf")
    (tags "Power Jack SMT")
    (attr smd)
    (fp_text reference J2 (at -4.5 5.75 90) (layer B.SilkS))
    (fp_text value 5VDC (at 0 -11.25 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad "" np_thru_hole circle (at 0 -7 90) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad 3 smd rect (at 6.45 -3.2 90) (size 3.9 6.2) (layers B.Cu B.Paste B.Mask)
      (net 276 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at -6.45 -3.2 90) (size 3.9 6.2) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at 0.7 5.8 90) (size 3.3 4.4) (layers B.Cu B.Paste B.Mask)
      (net 273 "Net-(F1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Barrel_Jack_CUI_PJ-036AH-SMT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SRP1770TA (layer B.Cu) (tedit 59F4DCEC)
    (at 70.736 63.5)
    (fp_text reference L1 (at 6.35 9.906) (layer B.SilkS))
    (fp_text value 68uH (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -6 0) (size 4 12.5) (drill (offset -2 0)) (layers B.Cu B.Paste B.Mask)
      (net 96 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 6 0) (size 4 12.5) (drill (offset 2 0)) (layers B.Cu B.Paste B.Mask)
      (net 97 "Net-(C4-Pad1)"))
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 141.605 91.313 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C65 (at -3.81 -0.762 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 139.573 89.027 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R17 (at -0.254848 1.81088 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 283 "Net-(R17-Pad2)"))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_IDC:IDC-Header_2x05_Pitch2.54mm_Angled (layer B.Cu) (tedit 59DE1F47)
    (at 78.74 116.84 270)
    (descr "10 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference J4 (at -2.286 -5.08 180) (layer B.SilkS))
    (fp_text value PGM (at 6.105 -16.51 270) (layer B.Fab))
    (fp_text user %R (at 8.805 -5.08 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 2.54 -10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 149 "/Graphics Controller/SS_B"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 152 "/Graphics Controller/SCK"))
    (pad 8 thru_hole oval (at 2.54 -7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 166 "/Graphics Controller/SDO"))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 167 "/Graphics Controller/SDI"))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 153 /RESET))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 155 /CPU_RESET))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 168 "Net-(J4-Pad4)"))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 169 "Net-(J4-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 170 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_IDC.3dshapes/IDC-Header_2x05_Pitch2.54mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 102.74 96.48 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C17 (at 3.75 0 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 147 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 223 "Net-(C17-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 38.1292 105.13 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C30 (at 1.2 -1.8 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 102.74 98.98 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C22 (at 3.75 0 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 223 "Net-(C17-Pad2)"))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 147 "Net-(C17-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 106.24 94.23)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C20 (at -0.25 -3) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 98.74 94.23 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C19 (at 0 2.75 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 102.24 113.08 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C18 (at 0.75 -2 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 148 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 227 "Net-(C18-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 92.19 112.78 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C16 (at 1.75 1.75 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 92.19 97.28 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C15 (at 0 -1.75 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 92.19 107.28 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C14 (at 3 0 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 140 +1V2))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 111.54 96.53 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C13 (at -3.7 0.55 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 111.54 106.03 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C12 (at -4 0 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 111.54 100.03 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C11 (at -3.75 0 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 111.54 103.53 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C10 (at -3.75 0 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 140 +1V2))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 67.54 85.78 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C9 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 98 /LED_A))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 125.9208 91.07 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at -3 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 140 +1V2))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 110.49 92.48 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C21 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 140 +1V2))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 110.99 113.58 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C23 (at -3 0 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 97.99 113.58 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C24 (at -3 0.25 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 105.482 115.33)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C25 (at -0.0085 2.526) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 95.49 113.58 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C26 (at -3 -0.5 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 140 +1V2))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 102.24 110.58 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C27 (at 3.75 0.25 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 148 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 227 "Net-(C18-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 95.79 99.28 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C28 (at -1.476 -2.572 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 29.9292 105.13)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C29 (at 3.8528 0.026) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 45.9292 105.13)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C31 (at 1.4 1.8) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 111.06 77.62 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C61 (at 1.6 -1.8 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 86.86 77.62)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C62 (at 1.4 1.8) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 95.06 77.62 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C63 (at 0.8 -1.8 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 151.638 64.69)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C64 (at 3.81 0) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 145.669 76.835 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C59 (at 3.8 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 77.47 76.835 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C8 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 61.9292 105.13)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C33 (at 1.4 1.8) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 70.1292 105.13 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C34 (at 1.4 -1.8 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 77.9292 105.13)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C35 (at 1.4 1.8) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 86.1292 105.13 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C36 (at 1.4 -1.8 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 135.09 99.53 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C37 (at -0.15 -1.85 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 135.09 105.03 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C38 (at 0 1.75 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 138.04 110.93 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C39 (at 0.05 -1.75 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 143.44 110.93 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C40 (at -0.05 -1.75 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 147.14 108.28 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C41 (at 0.25 -1.75 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 147.14 102.53 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C42 (at 0.25 -1.75 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 141.49 95.13 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C43 (at -3.65 0 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 54.1292 105.13 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C32 (at 1.4 -1.8 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 151.89 107.705 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C45 (at 2.93 0.383 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 151.89 95.355 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C46 (at 2.925 0 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 151.89 113.555 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C47 (at -3.285 -0.125 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 216 "Net-(C47-Pad2)"))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 218 "Net-(C47-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 102.86 77.62)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C60 (at 1.4 1.8) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 66.675 76.2 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 156.845 75.565 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 136.74 95.13 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C44 (at 3.8 0 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 142.494 104.902 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C58 (at 0 1.75 180) (layer B.SilkS))
    (fp_text value 2.2uF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 134 "Net-(C58-Pad1)"))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 147.955 114.3)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C57 (at 3.937 0.762) (layer F.SilkS))
    (fp_text value 18pF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 270 "Net-(C57-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 147.955 117.475)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C56 (at 3.81 0.127) (layer F.SilkS))
    (fp_text value 18pF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(C56-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 157.09 100.555 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C54 (at -3.9 0.325 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 192 "Net-(C54-Pad1)"))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 154.49 100.555 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C53 (at -3.9 0 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 172 "Net-(C53-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 156.718 107.696 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C52 (at 3.048 0 -180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 197 "Net-(C52-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 154.305 109.601 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C51 (at 3.81 0 -90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 217 "Net-(C51-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 159.69 100.555 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C50 (at 3.9 0 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 194 "Net-(C50-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 193 "Net-(C50-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 151.89 100.555 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C49 (at -0.975 -1.95 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 173 "Net-(C49-Pad2)"))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 171 "Net-(C49-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 120.08 91.005 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at -3.065 0.0908 180) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 160.274 109.474 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C48 (at -3.302 0 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 196 "Net-(C48-Pad2)"))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 195 "Net-(C48-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_1210 (layer F.Cu) (tedit 58307C54)
    (at 122.93 90.055 270)
    (descr "Resistor SMD 1210, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference L3 (at 3.015 0.0092) (layer F.SilkS))
    (fp_text value 2.2uH (at 0 2.7 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 140 +1V2))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(L3-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer B.Cu) (tedit 59959803)
    (at 36.83 56.515)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at -3.175 0) (layer B.SilkS))
    (fp_text value PWR (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 146 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer B.Cu) (tedit 59959803)
    (at 70.485 116.84)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 0 -1.905) (layer B.SilkS))
    (fp_text value RUN (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 151 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 155 /CPU_RESET))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 149.225 109.855 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R15 (at -3.683 -0.127 270) (layer F.SilkS))
    (fp_text value 220R (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(C56-Pad1)"))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(R15-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 104.232 101.839)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at -3.302 0) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 149 "/Graphics Controller/SS_B"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 111.54 108.53 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at -3.5 0 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 150 "Net-(R8-Pad2)"))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 95.85 106.411 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at -2.75 0.1) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.95 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 152 "/Graphics Controller/SCK"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 65.405 116.84 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R11 (at 0 1.905) (layer B.SilkS))
    (fp_text value 22R (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 151 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 106.49 97.73 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0.553 -2.06) (layer B.SilkS))
    (fp_text value 100R (at 0 -1.95 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 147 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 64.516 116.332 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R16 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 284 "Net-(R16-Pad2)"))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 71.628 82.042)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 10k (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 142 /LED_PWM))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 61.214 84.582 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value "1R75 1%" (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 98 /LED_A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 36.703 62.23)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at -3.175 0) (layer B.SilkS))
    (fp_text value 2k2 (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 146 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 95.758 118.028)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 3.302 0.254) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 155 /CPU_RESET))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 105.99 111.58 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at -1.5 -2 90) (layer B.SilkS))
    (fp_text value 100R (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 148 "Net-(C18-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 140.716 107.442)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R12 (at -3.556 -0.508) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 154 /~WAIT))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:DB9 (layer B.Cu) (tedit 59FDD3A1)
    (at 175.26 104.14 270)
    (fp_text reference J5 (at 0 13.335 270) (layer B.SilkS))
    (fp_text value "COM A" (at 0 2.54 270) (layer B.Fab))
    (pad 0 thru_hole circle (at 12.5 9.51 270) (size 5 5) (drill 3.15) (layers *.Cu *.Mask)
      (net 274 "Net-(J5-Pad0)"))
    (pad 9 thru_hole circle (at 4.1 8.09 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 199 /CPU/R_RI0))
    (pad 8 thru_hole circle (at 1.36 8.09 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 200 /CPU/R_CTS0))
    (pad 7 thru_hole circle (at -1.38 8.09 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 204 /CPU/R_RTS0))
    (pad 6 thru_hole circle (at -4.12 8.09 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 201 /CPU/R_DSR0))
    (pad 5 thru_hole circle (at 5.47 10.93 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 4 thru_hole circle (at 2.73 10.93 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 205 /CPU/R_DTR0))
    (pad 3 thru_hole circle (at -0.01 10.93 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 203 /CPU/R_TXD0))
    (pad 2 thru_hole circle (at -2.75 10.93 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 198 /CPU/R_RXD0))
    (pad 0 thru_hole circle (at -12.5 9.51 270) (size 5 5) (drill 3.15) (layers *.Cu *.Mask)
      (net 274 "Net-(J5-Pad0)"))
    (pad 1 thru_hole rect (at -5.49 10.93 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 202 /CPU/R_DCD0))
  )
  (module footprints:TSOPII-44 (layer F.Cu) (tedit 59CBFC90)
    (at 85.26 69.22)
    (fp_text reference U17 (at 6.14 -1.57) (layer F.SilkS))
    (fp_text value SRAM-512k (at 5.5 18.6) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U17-Pad1)"))
    (pad 2 smd rect (at 0 0.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(U17-Pad2)"))
    (pad 3 smd rect (at 0 1.6) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 62 /A0))
    (pad 4 smd rect (at 0 2.4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 61 /A1))
    (pad 5 smd rect (at 0 3.2) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 60 /A2))
    (pad 6 smd rect (at 0 4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 59 /A3))
    (pad 7 smd rect (at 0 4.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 58 /A4))
    (pad 8 smd rect (at 0 5.6) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 67 "/CPU Memory/~CS2"))
    (pad 9 smd rect (at 0 6.4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 57 /D0))
    (pad 10 smd rect (at 0 7.2) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 56 /D1))
    (pad 11 smd rect (at 0 8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 12 smd rect (at 0 8.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 13 smd rect (at 0 9.6) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 55 /D2))
    (pad 14 smd rect (at 0 10.4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 54 /D3))
    (pad 15 smd rect (at 0 11.2) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 53 /~WR))
    (pad 16 smd rect (at 0 12) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 52 /A5))
    (pad 17 smd rect (at 0 12.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 51 /A6))
    (pad 18 smd rect (at 0 13.6) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 50 /A7))
    (pad 19 smd rect (at 0 14.4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 49 /A8))
    (pad 20 smd rect (at 0 15.2) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 48 /A9))
    (pad 21 smd rect (at 0 16) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U17-Pad21)"))
    (pad 22 smd rect (at 0 16.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U17-Pad22)"))
    (pad 23 smd rect (at 11.4108 16.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U17-Pad23)"))
    (pad 24 smd rect (at 11.4108 16) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U17-Pad24)"))
    (pad 25 smd rect (at 11.4108 15.2) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U17-Pad25)"))
    (pad 26 smd rect (at 11.4108 14.4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 42 /A10))
    (pad 27 smd rect (at 11.4108 13.6) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 41 /A11))
    (pad 28 smd rect (at 11.4108 12.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 40 /A12))
    (pad 29 smd rect (at 11.4108 12) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 39 /A13))
    (pad 30 smd rect (at 11.4108 11.2) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 38 /A14))
    (pad 31 smd rect (at 11.4108 10.4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 37 /D4))
    (pad 32 smd rect (at 11.4108 9.6) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 36 /D5))
    (pad 33 smd rect (at 11.4108 8.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 34 smd rect (at 11.4108 8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 35 smd rect (at 11.4108 7.2) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 35 /D6))
    (pad 36 smd rect (at 11.4108 6.4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 34 /D7))
    (pad 37 smd rect (at 11.4108 5.6) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 33 /~RD))
    (pad 38 smd rect (at 11.4108 4.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 32 /A15))
    (pad 39 smd rect (at 11.4108 4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 31 /A16))
    (pad 40 smd rect (at 11.4108 3.2) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 30 /A17))
    (pad 41 smd rect (at 11.4108 2.4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 29 /A18))
    (pad 42 smd rect (at 11.4108 1.6) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U17-Pad42)"))
    (pad 43 smd rect (at 11.4108 0.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U17-Pad43)"))
    (pad 44 smd rect (at 11.4108 0) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U17-Pad44)"))
  )
  (module SMD_Packages:PLCC-32 (layer B.Cu) (tedit 0)
    (at 142.875 78.105 90)
    (descr "Support CMS Plcc 32 pins")
    (tags "CMS Plcc")
    (attr smd)
    (fp_text reference U15 (at 1 12) (layer B.SilkS))
    (fp_text value SST39LF040-55-4C-NHE (at 7.9 0.2) (layer B.Fab))
    (pad 1 smd rect (at 0 6.985 90) (size 0.762 2.032) (layers B.Cu B.Paste B.Mask)
      (net 29 /A18))
    (pad 2 smd rect (at -1.27 6.985 90) (size 0.762 2.032) (layers B.Cu B.Paste B.Mask)
      (net 31 /A16))
    (pad 3 smd rect (at -2.54 6.985 90) (size 0.762 2.032) (layers B.Cu B.Paste B.Mask)
      (net 32 /A15))
    (pad 4 smd rect (at -3.81 6.985 90) (size 0.762 2.032) (layers B.Cu B.Paste B.Mask)
      (net 40 /A12))
    (pad 5 smd rect (at -5.715 5.08 90) (size 2.032 0.762) (layers B.Cu B.Paste B.Mask)
      (net 50 /A7))
    (pad 6 smd rect (at -5.715 3.81 90) (size 2.032 0.762) (layers B.Cu B.Paste B.Mask)
      (net 51 /A6))
    (pad 7 smd rect (at -5.715 2.54 90) (size 2.032 0.762) (layers B.Cu B.Paste B.Mask)
      (net 52 /A5))
    (pad 8 smd rect (at -5.715 1.27 90) (size 2.032 0.762) (layers B.Cu B.Paste B.Mask)
      (net 58 /A4))
    (pad 9 smd rect (at -5.715 0 90) (size 2.032 0.762) (layers B.Cu B.Paste B.Mask)
      (net 59 /A3))
    (pad 10 smd rect (at -5.715 -1.27 90) (size 2.032 0.762) (layers B.Cu B.Paste B.Mask)
      (net 60 /A2))
    (pad 11 smd rect (at -5.715 -2.54 90) (size 2.032 0.762) (layers B.Cu B.Paste B.Mask)
      (net 61 /A1))
    (pad 12 smd rect (at -5.715 -3.81 90) (size 2.032 0.762) (layers B.Cu B.Paste B.Mask)
      (net 62 /A0))
    (pad 13 smd rect (at -5.715 -5.08 90) (size 2.032 0.762) (layers B.Cu B.Paste B.Mask)
      (net 57 /D0))
    (pad 14 smd rect (at -3.81 -6.985 90) (size 0.762 2.032) (layers B.Cu B.Paste B.Mask)
      (net 56 /D1))
    (pad 15 smd rect (at -2.54 -6.985 90) (size 0.762 2.032) (layers B.Cu B.Paste B.Mask)
      (net 55 /D2))
    (pad 16 smd rect (at -1.27 -6.985 90) (size 0.762 2.032) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 17 smd rect (at 0 -6.985 90) (size 0.762 2.032) (layers B.Cu B.Paste B.Mask)
      (net 54 /D3))
    (pad 18 smd rect (at 1.27 -6.985 90) (size 0.762 2.032) (layers B.Cu B.Paste B.Mask)
      (net 37 /D4))
    (pad 19 smd rect (at 2.54 -6.985 90) (size 0.762 2.032) (layers B.Cu B.Paste B.Mask)
      (net 36 /D5))
    (pad 20 smd rect (at 3.81 -6.985 90) (size 0.762 2.032) (layers B.Cu B.Paste B.Mask)
      (net 35 /D6))
    (pad 21 smd rect (at 5.715 -5.08 90) (size 2.032 0.762) (layers B.Cu B.Paste B.Mask)
      (net 34 /D7))
    (pad 22 smd rect (at 5.715 -3.81 90) (size 2.032 0.762) (layers B.Cu B.Paste B.Mask)
      (net 13 "/CPU Memory/~CS0"))
    (pad 23 smd rect (at 5.715 -2.54 90) (size 2.032 0.762) (layers B.Cu B.Paste B.Mask)
      (net 42 /A10))
    (pad 24 smd rect (at 5.715 -1.27 90) (size 2.032 0.762) (layers B.Cu B.Paste B.Mask)
      (net 33 /~RD))
    (pad 25 smd rect (at 5.715 0 90) (size 2.032 0.762) (layers B.Cu B.Paste B.Mask)
      (net 41 /A11))
    (pad 26 smd rect (at 5.715 1.27 90) (size 2.032 0.762) (layers B.Cu B.Paste B.Mask)
      (net 48 /A9))
    (pad 27 smd rect (at 5.715 2.54 90) (size 2.032 0.762) (layers B.Cu B.Paste B.Mask)
      (net 49 /A8))
    (pad 28 smd rect (at 5.715 3.81 90) (size 2.032 0.762) (layers B.Cu B.Paste B.Mask)
      (net 39 /A13))
    (pad 29 smd rect (at 5.715 5.08 90) (size 2.032 0.762) (layers B.Cu B.Paste B.Mask)
      (net 38 /A14))
    (pad 30 smd rect (at 3.81 6.985 90) (size 0.762 2.032) (layers B.Cu B.Paste B.Mask)
      (net 30 /A17))
    (pad 31 smd rect (at 2.54 6.985 90) (size 0.762 2.032) (layers B.Cu B.Paste B.Mask)
      (net 53 /~WR))
    (pad 32 smd rect (at 1.27 6.985 90) (size 0.762 2.032) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
  )
  (module footprints:Molex-0541044031 locked (layer B.Cu) (tedit 59F54176)
    (at 55.99 85.28 180)
    (fp_text reference J3 (at -11.955 0.825 180) (layer B.SilkS))
    (fp_text value LCD (at 0.11 -3.186 180) (layer B.Fab))
    (pad 1 smd rect (at -9.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 2 smd rect (at -9.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 98 /LED_A))
    (pad 3 smd rect (at -8.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 4 smd rect (at -8.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 5 smd rect (at -7.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 99 "/Graphics Controller/R0"))
    (pad 6 smd rect (at -7.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 100 "/Graphics Controller/R1"))
    (pad 7 smd rect (at -6.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 101 "/Graphics Controller/R2"))
    (pad 8 smd rect (at -6.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 102 "/Graphics Controller/R3"))
    (pad 9 smd rect (at -5.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 103 "/Graphics Controller/R4"))
    (pad 10 smd rect (at -5.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 104 "/Graphics Controller/R5"))
    (pad 11 smd rect (at -4.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 105 "/Graphics Controller/R6"))
    (pad 12 smd rect (at -4.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 106 "/Graphics Controller/R7"))
    (pad 13 smd rect (at -3.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 107 "/Graphics Controller/G0"))
    (pad 14 smd rect (at -3.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 108 "/Graphics Controller/G1"))
    (pad 15 smd rect (at -2.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 109 "/Graphics Controller/G2"))
    (pad 16 smd rect (at -2.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 110 "/Graphics Controller/G3"))
    (pad 17 smd rect (at -1.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 111 "/Graphics Controller/G4"))
    (pad 18 smd rect (at -1.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 112 "/Graphics Controller/G5"))
    (pad 19 smd rect (at -0.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 113 "/Graphics Controller/G6"))
    (pad 20 smd rect (at -0.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 114 "/Graphics Controller/G7"))
    (pad 21 smd rect (at 0.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 115 "/Graphics Controller/B0"))
    (pad 22 smd rect (at 0.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 116 "/Graphics Controller/B1"))
    (pad 23 smd rect (at 1.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 117 "/Graphics Controller/B2"))
    (pad 24 smd rect (at 1.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 118 "/Graphics Controller/B3"))
    (pad 25 smd rect (at 2.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 119 "/Graphics Controller/B4"))
    (pad 26 smd rect (at 2.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 120 "/Graphics Controller/B5"))
    (pad 27 smd rect (at 3.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 121 "/Graphics Controller/B6"))
    (pad 28 smd rect (at 3.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 122 "/Graphics Controller/B7"))
    (pad 29 smd rect (at 4.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 30 smd rect (at 4.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 123 "/Graphics Controller/DCLK"))
    (pad 31 smd rect (at 5.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 32 smd rect (at 5.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 124 "/Graphics Controller/HSYNC"))
    (pad 33 smd rect (at 6.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 125 "/Graphics Controller/VSYNC"))
    (pad 34 smd rect (at 6.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 126 "/Graphics Controller/DEN"))
    (pad 35 smd rect (at 7.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 127 "Net-(J3-Pad35)"))
    (pad 36 smd rect (at 7.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 37 smd rect (at 8.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 128 "Net-(J3-Pad37)"))
    (pad 38 smd rect (at 8.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 129 "Net-(J3-Pad38)"))
    (pad 39 smd rect (at 9.25 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 130 "Net-(J3-Pad39)"))
    (pad 40 smd rect (at 9.75 0 180) (size 0.3 1.5) (drill (offset 0 0.75)) (layers B.Cu B.Paste B.Mask)
      (net 131 "Net-(J3-Pad40)"))
    (pad "" smd rect (at -10.65 -0.9 180) (size 2.4 2.4) (drill (offset -1.2 -1.2)) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at 10.65 -0.9 180) (size 2.4 2.4) (drill (offset 1.2 -1.2)) (layers B.Cu B.Paste B.Mask))
  )
  (module Housings_QFP:TQFP-144_20x20mm_Pitch0.5mm locked (layer F.Cu) (tedit 58CC9A48)
    (at 102.74 104.78)
    (descr "P/PG-TQFP-144-2, -3, -7 (see MAXIM 21-0087.PDF and 90-0144.PDF)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U4 (at -12 -11) (layer F.SilkS))
    (fp_text value iCE40-HX4K-TQ144 (at 0 12.275) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 144 smd rect (at -8.75 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 126 "/Graphics Controller/DEN"))
    (pad 143 smd rect (at -8.25 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 125 "/Graphics Controller/VSYNC"))
    (pad 142 smd rect (at -7.75 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 124 "/Graphics Controller/HSYNC"))
    (pad 141 smd rect (at -7.25 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 123 "/Graphics Controller/DCLK"))
    (pad 140 smd rect (at -6.75 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 139 smd rect (at -6.25 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 122 "/Graphics Controller/B7"))
    (pad 138 smd rect (at -5.75 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 121 "/Graphics Controller/B6"))
    (pad 137 smd rect (at -5.25 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 120 "/Graphics Controller/B5"))
    (pad 136 smd rect (at -4.75 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 119 "/Graphics Controller/B4"))
    (pad 135 smd rect (at -4.25 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 118 "/Graphics Controller/B3"))
    (pad 134 smd rect (at -3.75 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 117 "/Graphics Controller/B2"))
    (pad 133 smd rect (at -3.25 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(U4-Pad133)"))
    (pad 132 smd rect (at -2.75 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 131 smd rect (at -2.25 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 130 smd rect (at -1.75 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 116 "/Graphics Controller/B1"))
    (pad 129 smd rect (at -1.25 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 115 "/Graphics Controller/B0"))
    (pad 128 smd rect (at -0.75 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 114 "/Graphics Controller/G7"))
    (pad 127 smd rect (at -0.25 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 223 "Net-(C17-Pad2)"))
    (pad 126 smd rect (at 0.25 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(C17-Pad1)"))
    (pad 125 smd rect (at 0.75 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 113 "/Graphics Controller/G6"))
    (pad 124 smd rect (at 1.25 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 112 "/Graphics Controller/G5"))
    (pad 123 smd rect (at 1.75 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 122 smd rect (at 2.25 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 111 "/Graphics Controller/G4"))
    (pad 121 smd rect (at 2.75 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 110 "/Graphics Controller/G3"))
    (pad 120 smd rect (at 3.25 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 109 "/Graphics Controller/G2"))
    (pad 119 smd rect (at 3.75 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 108 "/Graphics Controller/G1"))
    (pad 118 smd rect (at 4.25 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 107 "/Graphics Controller/G0"))
    (pad 117 smd rect (at 4.75 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 106 "/Graphics Controller/R7"))
    (pad 116 smd rect (at 5.25 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 105 "/Graphics Controller/R6"))
    (pad 115 smd rect (at 5.75 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 104 "/Graphics Controller/R5"))
    (pad 114 smd rect (at 6.25 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 103 "/Graphics Controller/R4"))
    (pad 113 smd rect (at 6.75 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 102 "/Graphics Controller/R3"))
    (pad 112 smd rect (at 7.25 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 101 "/Graphics Controller/R2"))
    (pad 111 smd rect (at 7.75 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 140 +1V2))
    (pad 110 smd rect (at 8.25 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 100 "/Graphics Controller/R1"))
    (pad 109 smd rect (at 8.75 -10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(U4-Pad109)"))
    (pad 108 smd rect (at 10.55 -8.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 107 smd rect (at 10.55 -8.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 99 "/Graphics Controller/R0"))
    (pad 106 smd rect (at 10.55 -7.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 62 /A0))
    (pad 105 smd rect (at 10.55 -7.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 61 /A1))
    (pad 104 smd rect (at 10.55 -6.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 60 /A2))
    (pad 103 smd rect (at 10.55 -6.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 102 smd rect (at 10.55 -5.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 59 /A3))
    (pad 101 smd rect (at 10.55 -5.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 58 /A4))
    (pad 100 smd rect (at 10.55 -4.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 99 smd rect (at 10.55 -4.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 /A5))
    (pad 98 smd rect (at 10.55 -3.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 /A6))
    (pad 97 smd rect (at 10.55 -3.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 /A7))
    (pad 96 smd rect (at 10.55 -2.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 /A8))
    (pad 95 smd rect (at 10.55 -2.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 /A9))
    (pad 94 smd rect (at 10.55 -1.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 /A10))
    (pad 93 smd rect (at 10.55 -1.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 /A11))
    (pad 92 smd rect (at 10.55 -0.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 140 +1V2))
    (pad 91 smd rect (at 10.55 -0.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 /A12))
    (pad 90 smd rect (at 10.55 0.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 /A13))
    (pad 89 smd rect (at 10.55 0.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 88 smd rect (at 10.55 1.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 /A14))
    (pad 87 smd rect (at 10.55 1.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 /A15))
    (pad 86 smd rect (at 10.55 2.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 85 smd rect (at 10.55 2.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 /A16))
    (pad 84 smd rect (at 10.55 3.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 /A17))
    (pad 83 smd rect (at 10.55 3.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /A18))
    (pad 82 smd rect (at 10.55 4.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 165 /A19))
    (pad 81 smd rect (at 10.55 4.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 164 /A20))
    (pad 80 smd rect (at 10.55 5.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 161 /A23))
    (pad 79 smd rect (at 10.55 5.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 162 /A22))
    (pad 78 smd rect (at 10.55 6.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 163 /A21))
    (pad 77 smd rect (at 10.55 6.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 225 "Net-(U4-Pad77)"))
    (pad 76 smd rect (at 10.55 7.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 /D0))
    (pad 75 smd rect (at 10.55 7.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /D1))
    (pad 74 smd rect (at 10.55 8.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 /D2))
    (pad 73 smd rect (at 10.55 8.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 54 /D3))
    (pad 72 smd rect (at 8.75 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 71 smd rect (at 8.25 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 149 "/Graphics Controller/SS_B"))
    (pad 70 smd rect (at 7.75 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 152 "/Graphics Controller/SCK"))
    (pad 69 smd rect (at 7.25 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 68 smd rect (at 6.75 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 167 "/Graphics Controller/SDI"))
    (pad 67 smd rect (at 6.25 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 166 "/Graphics Controller/SDO"))
    (pad 66 smd rect (at 5.75 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 153 /RESET))
    (pad 65 smd rect (at 5.25 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 155 /CPU_RESET))
    (pad 64 smd rect (at 4.75 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 142 /LED_PWM))
    (pad 63 smd rect (at 4.25 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 /D4))
    (pad 62 smd rect (at 3.75 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 /D5))
    (pad 61 smd rect (at 3.25 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 /D6))
    (pad 60 smd rect (at 2.75 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 /D7))
    (pad 59 smd rect (at 2.25 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 58 smd rect (at 1.75 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(U4-Pad58)"))
    (pad 57 smd rect (at 1.25 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 56 smd rect (at 0.75 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 158 /~IOREQ))
    (pad 55 smd rect (at 0.25 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 157 /~MREQ))
    (pad 54 smd rect (at -0.25 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(C18-Pad1)"))
    (pad 53 smd rect (at -0.75 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(C18-Pad2)"))
    (pad 52 smd rect (at -1.25 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 156 /INT))
    (pad 51 smd rect (at -1.75 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 228 "Net-(U4-Pad51)"))
    (pad 50 smd rect (at -2.25 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 229 "Net-(U4-Pad50)"))
    (pad 49 smd rect (at -2.75 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 137 /CLK0))
    (pad 48 smd rect (at -3.25 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 /~RD))
    (pad 47 smd rect (at -3.75 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 53 /~WR))
    (pad 46 smd rect (at -4.25 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 45 smd rect (at -4.75 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 154 /~WAIT))
    (pad 44 smd rect (at -5.25 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 160 /~BUSACK))
    (pad 43 smd rect (at -5.75 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 159 /~BUSREQ))
    (pad 42 smd rect (at -6.25 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 282 "/Graphics Controller/~GPU_CS3"))
    (pad 41 smd rect (at -6.75 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 281 "/Graphics Controller/~GPU_CS2"))
    (pad 40 smd rect (at -7.25 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 140 +1V2))
    (pad 39 smd rect (at -7.75 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 279 "/Graphics Controller/~GPU_CS1"))
    (pad 38 smd rect (at -8.25 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 280 "/Graphics Controller/~GPU_CS0"))
    (pad 37 smd rect (at -8.75 10.55 90) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 258 "/Graphics Controller/GPU_A0"))
    (pad 36 smd rect (at -10.55 8.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 230 "Net-(U4-Pad36)"))
    (pad 35 smd rect (at -10.55 8.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 231 "Net-(U4-Pad35)"))
    (pad 34 smd rect (at -10.55 7.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 240 "/Graphics Controller/GPU_A18"))
    (pad 33 smd rect (at -10.55 7.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 241 "/Graphics Controller/GPU_A17"))
    (pad 32 smd rect (at -10.55 6.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 257 "/Graphics Controller/GPU_A1"))
    (pad 31 smd rect (at -10.55 6.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 256 "/Graphics Controller/GPU_A2"))
    (pad 30 smd rect (at -10.55 5.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 29 smd rect (at -10.55 5.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 255 "/Graphics Controller/GPU_A3"))
    (pad 28 smd rect (at -10.55 4.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 254 "/Graphics Controller/GPU_A4"))
    (pad 27 smd rect (at -10.55 4.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 140 +1V2))
    (pad 26 smd rect (at -10.55 3.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 242 "/Graphics Controller/GPU_A16"))
    (pad 25 smd rect (at -10.55 3.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 239 "/Graphics Controller/GPU_D0"))
    (pad 24 smd rect (at -10.55 2.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 243 "/Graphics Controller/GPU_A15"))
    (pad 23 smd rect (at -10.55 2.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 277 "/Graphics Controller/~GPU_OE"))
    (pad 22 smd rect (at -10.55 1.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 232 "/Graphics Controller/GPU_D7"))
    (pad 21 smd rect (at -10.55 1.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 233 "/Graphics Controller/GPU_D6"))
    (pad 20 smd rect (at -10.55 0.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 238 "/Graphics Controller/GPU_D1"))
    (pad 19 smd rect (at -10.55 0.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 234 "/Graphics Controller/GPU_D5"))
    (pad 18 smd rect (at -10.55 -0.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 237 "/Graphics Controller/GPU_D2"))
    (pad 17 smd rect (at -10.55 -0.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 235 "/Graphics Controller/GPU_D4"))
    (pad 16 smd rect (at -10.55 -1.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 236 "/Graphics Controller/GPU_D3"))
    (pad 15 smd rect (at -10.55 -1.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 278 "/Graphics Controller/~GPU_WE"))
    (pad 14 smd rect (at -10.55 -2.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 13 smd rect (at -10.55 -2.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 12 smd rect (at -10.55 -3.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 244 "/Graphics Controller/GPU_A14"))
    (pad 11 smd rect (at -10.55 -3.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 245 "/Graphics Controller/GPU_A13"))
    (pad 10 smd rect (at -10.55 -4.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 246 "/Graphics Controller/GPU_A12"))
    (pad 9 smd rect (at -10.55 -4.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 253 "/Graphics Controller/GPU_A5"))
    (pad 8 smd rect (at -10.55 -5.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 252 "/Graphics Controller/GPU_A6"))
    (pad 7 smd rect (at -10.55 -5.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 247 "/Graphics Controller/GPU_A11"))
    (pad 6 smd rect (at -10.55 -6.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 5 smd rect (at -10.55 -6.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 4 smd rect (at -10.55 -7.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 251 "/Graphics Controller/GPU_A7"))
    (pad 3 smd rect (at -10.55 -7.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 248 "/Graphics Controller/GPU_A10"))
    (pad 2 smd rect (at -10.55 -8.25) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 250 "/Graphics Controller/GPU_A8"))
    (pad 1 smd rect (at -10.55 -8.75) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 249 "/Graphics Controller/GPU_A9"))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-144_20x20mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:TSOPII-44 locked (layer F.Cu) (tedit 59CBFC90)
    (at 87.74 113.53 180)
    (fp_text reference U9 (at 5.6692 18.31 180) (layer F.SilkS))
    (fp_text value SRAM-512k (at 5.5 -2 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U9-Pad1)"))
    (pad 2 smd rect (at 0 0.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(U9-Pad2)"))
    (pad 3 smd rect (at 0 1.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 258 "/Graphics Controller/GPU_A0"))
    (pad 4 smd rect (at 0 2.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 257 "/Graphics Controller/GPU_A1"))
    (pad 5 smd rect (at 0 3.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 256 "/Graphics Controller/GPU_A2"))
    (pad 6 smd rect (at 0 4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 255 "/Graphics Controller/GPU_A3"))
    (pad 7 smd rect (at 0 4.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 254 "/Graphics Controller/GPU_A4"))
    (pad 8 smd rect (at 0 5.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 282 "/Graphics Controller/~GPU_CS3"))
    (pad 9 smd rect (at 0 6.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 239 "/Graphics Controller/GPU_D0"))
    (pad 10 smd rect (at 0 7.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 238 "/Graphics Controller/GPU_D1"))
    (pad 11 smd rect (at 0 8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 12 smd rect (at 0 8.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 13 smd rect (at 0 9.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 237 "/Graphics Controller/GPU_D2"))
    (pad 14 smd rect (at 0 10.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 236 "/Graphics Controller/GPU_D3"))
    (pad 15 smd rect (at 0 11.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 278 "/Graphics Controller/~GPU_WE"))
    (pad 16 smd rect (at 0 12 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 253 "/Graphics Controller/GPU_A5"))
    (pad 17 smd rect (at 0 12.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 252 "/Graphics Controller/GPU_A6"))
    (pad 18 smd rect (at 0 13.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 251 "/Graphics Controller/GPU_A7"))
    (pad 19 smd rect (at 0 14.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 250 "/Graphics Controller/GPU_A8"))
    (pad 20 smd rect (at 0 15.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 249 "/Graphics Controller/GPU_A9"))
    (pad 21 smd rect (at 0 16 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(U9-Pad21)"))
    (pad 22 smd rect (at 0 16.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(U9-Pad22)"))
    (pad 23 smd rect (at 11.4108 16.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(U9-Pad23)"))
    (pad 24 smd rect (at 11.4108 16 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(U9-Pad24)"))
    (pad 25 smd rect (at 11.4108 15.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(U9-Pad25)"))
    (pad 26 smd rect (at 11.4108 14.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 248 "/Graphics Controller/GPU_A10"))
    (pad 27 smd rect (at 11.4108 13.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 247 "/Graphics Controller/GPU_A11"))
    (pad 28 smd rect (at 11.4108 12.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 246 "/Graphics Controller/GPU_A12"))
    (pad 29 smd rect (at 11.4108 12 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 245 "/Graphics Controller/GPU_A13"))
    (pad 30 smd rect (at 11.4108 11.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 244 "/Graphics Controller/GPU_A14"))
    (pad 31 smd rect (at 11.4108 10.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 235 "/Graphics Controller/GPU_D4"))
    (pad 32 smd rect (at 11.4108 9.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 234 "/Graphics Controller/GPU_D5"))
    (pad 33 smd rect (at 11.4108 8.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 34 smd rect (at 11.4108 8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 35 smd rect (at 11.4108 7.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 233 "/Graphics Controller/GPU_D6"))
    (pad 36 smd rect (at 11.4108 6.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 232 "/Graphics Controller/GPU_D7"))
    (pad 37 smd rect (at 11.4108 5.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 277 "/Graphics Controller/~GPU_OE"))
    (pad 38 smd rect (at 11.4108 4.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 243 "/Graphics Controller/GPU_A15"))
    (pad 39 smd rect (at 11.4108 4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 242 "/Graphics Controller/GPU_A16"))
    (pad 40 smd rect (at 11.4108 3.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 241 "/Graphics Controller/GPU_A17"))
    (pad 41 smd rect (at 11.4108 2.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 240 "/Graphics Controller/GPU_A18"))
    (pad 42 smd rect (at 11.4108 1.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(U9-Pad42)"))
    (pad 43 smd rect (at 11.4108 0.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(U9-Pad43)"))
    (pad 44 smd rect (at 11.4108 0 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(U9-Pad44)"))
  )
  (module Battery_Holders:Keystone_1058_1x2032-CoinCell (layer F.Cu) (tedit 589EE147)
    (at 40.64 80.645 315)
    (descr http://www.keyelco.com/product-pdf.cfm?p=14028)
    (tags "Keystone type 1058 coin cell retainer")
    (attr smd)
    (fp_text reference BT1 (at 0 7.62 315) (layer F.SilkS))
    (fp_text value RTC_BAT (at 0 -9.398001 315) (layer F.Fab))
    (pad 2 smd rect (at 14.680001 0 315) (size 2.54 3.51) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -14.680001 0 315) (size 2.54 3.51) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(BT1-Pad1)"))
  )
  (module Capacitors_THT:CP_Radial_D10.0mm_P5.00mm (layer B.Cu) (tedit 597BC7C2)
    (at 99.822 60.96)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C5 (at 2.5 6.31) (layer B.SilkS))
    (fp_text value 100uF (at 2.5 -6.31) (layer B.Fab))
    (fp_text user %R (at 2.5 0) (layer B.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D10.0mm_P5.00mm (layer B.Cu) (tedit 597BC7C2)
    (at 51.051 60.96)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C2 (at -2.032 -4.826) (layer B.SilkS))
    (fp_text value 100uF (at 2.5 -6.31) (layer B.Fab))
    (fp_text user %R (at 2.5 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 132 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D10.0mm_P5.00mm (layer B.Cu) (tedit 597BC7C2)
    (at 63.246 77.978 180)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C4 (at 2.54 6.223 180) (layer B.SilkS))
    (fp_text value 1000uF (at 2.5 -6.31 180) (layer B.Fab))
    (fp_text user %R (at 2.5 0 180) (layer B.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 97 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_DS26_d2.0mm_l6.0mm_Horizontal (layer F.Cu) (tedit 58CD3077)
    (at 144.78 114.935 270)
    (descr "Crystal THT DS26 6.0mm length 2.0mm diameter http://www.microcrystal.com/images/_Product-Documentation/03_TF_metal_Packages/01_Datasheet/DS-Series.pdf")
    (tags ['DS26'])
    (fp_text reference Y1 (at 0 9.525 90) (layer F.SilkS))
    (fp_text value 32.768kHz (at 3.47 1.625) (layer F.Fab))
    (fp_text user %R (at 1 4.75) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.9 0 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 145 "Net-(C56-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 270 "Net-(C57-Pad1)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_DS26_d2.0mm_l6.0mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123F (layer F.Cu) (tedit 587F7769)
    (at 67.276 65.024 270)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D1 (at -0.127 -1.905 270) (layer F.SilkS))
    (fp_text value 1N5822 (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at -0.127 -1.905 270) (layer F.Fab))
    (pad 2 smd rect (at 1.4 0 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.4 0 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-100_14x14mm_Pitch0.5mm (layer F.Cu) (tedit 58CC9A46)
    (at 139.24 103.03)
    (descr "LQFP100: plastic low profile quad flat package; 100 leads; body 14 x 14 x 1.4 mm (see NXP sot407-1_po.pdf and sot407-1_fr.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U10 (at -8.25 -8.15) (layer F.SilkS))
    (fp_text value ez80L92 (at 0 9.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 100 smd rect (at -6 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 259 "Net-(U10-Pad100)"))
    (pad 99 smd rect (at -5.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 98 smd rect (at -5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 97 smd rect (at -4.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 96 smd rect (at -4 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 95 smd rect (at -3.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 220 /CPU/MOSI))
    (pad 94 smd rect (at -3 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 219 /CPU/MISO))
    (pad 93 smd rect (at -2.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 260 "Net-(U10-Pad93)"))
    (pad 92 smd rect (at -2 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 261 "Net-(U10-Pad92)"))
    (pad 91 smd rect (at -1.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 221 /CPU/SCK))
    (pad 90 smd rect (at -1 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 156 /INT))
    (pad 89 smd rect (at -0.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 262 "Net-(U10-Pad89)"))
    (pad 88 smd rect (at 0 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 263 "Net-(U10-Pad88)"))
    (pad 87 smd rect (at 0.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 86 smd rect (at 1 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 264 "Net-(U10-Pad86)"))
    (pad 85 smd rect (at 1.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 135 /CLK1))
    (pad 84 smd rect (at 2 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 83 smd rect (at 2.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 175 /CPU/L_RI1))
    (pad 82 smd rect (at 3 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 180 /CPU/L_DCD1))
    (pad 81 smd rect (at 3.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 179 /CPU/L_DSR1))
    (pad 80 smd rect (at 4 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 183 /CPU/L_DTR1))
    (pad 79 smd rect (at 4.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 178 /CPU/L_CTS1))
    (pad 78 smd rect (at 5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 182 /CPU/L_RTS1))
    (pad 77 smd rect (at 5.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 176 /CPU/L_RXD1))
    (pad 76 smd rect (at 6 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 181 /CPU/L_TXD1))
    (pad 75 smd rect (at 7.9 -6) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 214 /CPU/L_RI0))
    (pad 74 smd rect (at 7.9 -5.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 209 /CPU/L_DCD0))
    (pad 73 smd rect (at 7.9 -5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 210 /CPU/L_DSR0))
    (pad 72 smd rect (at 7.9 -4.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 206 /CPU/L_DTR0))
    (pad 71 smd rect (at 7.9 -4) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 211 /CPU/L_CTS0))
    (pad 70 smd rect (at 7.9 -3.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 207 /CPU/L_RTS0))
    (pad 69 smd rect (at 7.9 -3) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 213 /CPU/L_RXD0))
    (pad 68 smd rect (at 7.9 -2.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 208 /CPU/L_TXD0))
    (pad 67 smd rect (at 7.9 -2) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 66 smd rect (at 7.9 -1.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 265 "Net-(U10-Pad66)"))
    (pad 65 smd rect (at 7.9 -1) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 266 "Net-(U10-Pad65)"))
    (pad 64 smd rect (at 7.9 -0.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 267 "Net-(U10-Pad64)"))
    (pad 63 smd rect (at 7.9 0) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 268 "Net-(U10-Pad63)"))
    (pad 62 smd rect (at 7.9 0.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 269 "Net-(U10-Pad62)"))
    (pad 61 smd rect (at 7.9 1) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 60 smd rect (at 7.9 1.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(C58-Pad1)"))
    (pad 59 smd rect (at 7.9 2) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(R15-Pad1)"))
    (pad 58 smd rect (at 7.9 2.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 270 "Net-(C57-Pad1)"))
    (pad 57 smd rect (at 7.9 3) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 56 smd rect (at 7.9 3.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 55 smd rect (at 7.9 4) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 271 "Net-(U10-Pad55)"))
    (pad 54 smd rect (at 7.9 4.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 160 /~BUSACK))
    (pad 53 smd rect (at 7.9 5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 159 /~BUSREQ))
    (pad 52 smd rect (at 7.9 5.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 286 "Net-(C55-Pad1)"))
    (pad 51 smd rect (at 7.9 6) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 155 /CPU_RESET))
    (pad 50 smd rect (at 6 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 154 /~WAIT))
    (pad 49 smd rect (at 5.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 272 "Net-(U10-Pad49)"))
    (pad 48 smd rect (at 5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 53 /~WR))
    (pad 47 smd rect (at 4.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 33 /~RD))
    (pad 46 smd rect (at 4 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 157 /~MREQ))
    (pad 45 smd rect (at 3.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 158 /~IOREQ))
    (pad 44 smd rect (at 3 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 43 smd rect (at 2.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 42 smd rect (at 2 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 34 /D7))
    (pad 41 smd rect (at 1.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 35 /D6))
    (pad 40 smd rect (at 1 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 36 /D5))
    (pad 39 smd rect (at 0.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 37 /D4))
    (pad 38 smd rect (at 0 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 54 /D3))
    (pad 37 smd rect (at -0.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 55 /D2))
    (pad 36 smd rect (at -1 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 56 /D1))
    (pad 35 smd rect (at -1.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 57 /D0))
    (pad 34 smd rect (at -2 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 33 smd rect (at -2.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 32 smd rect (at -3 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 15 /CPU/~CS3))
    (pad 31 smd rect (at -3.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 67 "/CPU Memory/~CS2"))
    (pad 30 smd rect (at -4 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 14 "/CPU Memory/~CS1"))
    (pad 29 smd rect (at -4.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 13 "/CPU Memory/~CS0"))
    (pad 28 smd rect (at -5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 161 /A23))
    (pad 27 smd rect (at -5.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 162 /A22))
    (pad 26 smd rect (at -6 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 163 /A21))
    (pad 25 smd rect (at -7.9 6) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 164 /A20))
    (pad 24 smd rect (at -7.9 5.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 165 /A19))
    (pad 23 smd rect (at -7.9 5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 29 /A18))
    (pad 22 smd rect (at -7.9 4.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 30 /A17))
    (pad 21 smd rect (at -7.9 4) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 31 /A16))
    (pad 20 smd rect (at -7.9 3.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 32 /A15))
    (pad 19 smd rect (at -7.9 3) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 18 smd rect (at -7.9 2.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 17 smd rect (at -7.9 2) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 38 /A14))
    (pad 16 smd rect (at -7.9 1.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 39 /A13))
    (pad 15 smd rect (at -7.9 1) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 40 /A12))
    (pad 14 smd rect (at -7.9 0.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 41 /A11))
    (pad 13 smd rect (at -7.9 0) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 42 /A10))
    (pad 12 smd rect (at -7.9 -0.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 48 /A9))
    (pad 11 smd rect (at -7.9 -1) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 49 /A8))
    (pad 10 smd rect (at -7.9 -1.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 50 /A7))
    (pad 9 smd rect (at -7.9 -2) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 51 /A6))
    (pad 8 smd rect (at -7.9 -2.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 7 smd rect (at -7.9 -3) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 6 smd rect (at -7.9 -3.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 52 /A5))
    (pad 5 smd rect (at -7.9 -4) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 58 /A4))
    (pad 4 smd rect (at -7.9 -4.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 59 /A3))
    (pad 3 smd rect (at -7.9 -5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 60 /A2))
    (pad 2 smd rect (at -7.9 -5.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 61 /A1))
    (pad 1 smd rect (at -7.9 -6) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 62 /A0))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/LQFP-100_14x14mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIJ-8_5.3x5.3mm_Pitch1.27mm (layer B.Cu) (tedit 58CC8F64)
    (at 139.5 90.455)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U13 (at -6.35 -0.254) (layer B.SilkS))
    (fp_text value W25Q128FWSIG (at 0 -3.68) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -3.65 1.905) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 2 smd rect (at -3.65 0.635) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 219 /CPU/MISO))
    (pad 3 smd rect (at -3.65 -0.635) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 283 "Net-(R17-Pad2)"))
    (pad 4 smd rect (at -3.65 -1.905) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 5 smd rect (at 3.65 -1.905) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 220 /CPU/MOSI))
    (pad 6 smd rect (at 3.65 -0.635) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 221 /CPU/SCK))
    (pad 7 smd rect (at 3.65 0.635) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 283 "Net-(R17-Pad2)"))
    (pad 8 smd rect (at 3.65 1.905) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIJ-8_5.3x5.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIJ-8_5.3x5.3mm_Pitch1.27mm (layer B.Cu) (tedit 58CC8F64)
    (at 102.04 106.03 180)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U5 (at 3.818 3.368 180) (layer B.SilkS))
    (fp_text value W25Q16JVSSIQ (at 0 -3.68 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 8 smd rect (at 3.65 1.905 180) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 7 smd rect (at 3.65 0.635 180) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 150 "Net-(R8-Pad2)"))
    (pad 6 smd rect (at 3.65 -0.635 180) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 152 "/Graphics Controller/SCK"))
    (pad 5 smd rect (at 3.65 -1.905 180) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 166 "/Graphics Controller/SDO"))
    (pad 4 smd rect (at -3.65 -1.905 180) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 3 smd rect (at -3.65 -0.635 180) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 150 "Net-(R8-Pad2)"))
    (pad 2 smd rect (at -3.65 0.635 180) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 167 "/Graphics Controller/SDI"))
    (pad 1 smd rect (at -3.65 1.905 180) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 149 "/Graphics Controller/SS_B"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIJ-8_5.3x5.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-28_4.4x9.7mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 154.415 107.38 180)
    (descr "TSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot361-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U11 (at -5.275 3.575 180) (layer F.SilkS))
    (fp_text value MAX3243ECPWR (at 0 5.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2.85 -4.225 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(C48-Pad1)"))
    (pad 2 smd rect (at -2.85 -3.575 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(C48-Pad2)"))
    (pad 3 smd rect (at -2.85 -2.925 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(C52-Pad1)"))
    (pad 4 smd rect (at -2.85 -2.275 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 198 /CPU/R_RXD0))
    (pad 5 smd rect (at -2.85 -1.625 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 199 /CPU/R_RI0))
    (pad 6 smd rect (at -2.85 -0.975 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 200 /CPU/R_CTS0))
    (pad 7 smd rect (at -2.85 -0.325 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 201 /CPU/R_DSR0))
    (pad 8 smd rect (at -2.85 0.325 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 202 /CPU/R_DCD0))
    (pad 9 smd rect (at -2.85 0.975 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 203 /CPU/R_TXD0))
    (pad 10 smd rect (at -2.85 1.625 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 204 /CPU/R_RTS0))
    (pad 11 smd rect (at -2.85 2.275 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 205 /CPU/R_DTR0))
    (pad 12 smd rect (at -2.85 2.925 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 206 /CPU/L_DTR0))
    (pad 13 smd rect (at -2.85 3.575 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 207 /CPU/L_RTS0))
    (pad 14 smd rect (at -2.85 4.225 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 208 /CPU/L_TXD0))
    (pad 15 smd rect (at 2.85 4.225 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 209 /CPU/L_DCD0))
    (pad 16 smd rect (at 2.85 3.575 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 210 /CPU/L_DSR0))
    (pad 17 smd rect (at 2.85 2.925 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 211 /CPU/L_CTS0))
    (pad 18 smd rect (at 2.85 2.275 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(U11-Pad18)"))
    (pad 19 smd rect (at 2.85 1.625 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 213 /CPU/L_RXD0))
    (pad 20 smd rect (at 2.85 0.975 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 214 /CPU/L_RI0))
    (pad 21 smd rect (at 2.85 0.325 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 215 "Net-(U11-Pad21)"))
    (pad 22 smd rect (at 2.85 -0.325 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 23 smd rect (at 2.85 -0.975 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 24 smd rect (at 2.85 -1.625 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 216 "Net-(C47-Pad2)"))
    (pad 25 smd rect (at 2.85 -2.275 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 26 smd rect (at 2.85 -2.925 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 27 smd rect (at 2.85 -3.575 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 217 "Net-(C51-Pad1)"))
    (pad 28 smd rect (at 2.85 -4.225 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(C47-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-28_4.4x9.7mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-28_4.4x9.7mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 154.415 95.03 180)
    (descr "TSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot361-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U12 (at 0.745 6.13 180) (layer F.SilkS))
    (fp_text value MAX3243ECPWR (at 0 5.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 28 smd rect (at 2.85 -4.225 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 171 "Net-(C49-Pad1)"))
    (pad 27 smd rect (at 2.85 -3.575 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 172 "Net-(C53-Pad1)"))
    (pad 26 smd rect (at 2.85 -2.925 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 25 smd rect (at 2.85 -2.275 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 24 smd rect (at 2.85 -1.625 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(C49-Pad2)"))
    (pad 23 smd rect (at 2.85 -0.975 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 22 smd rect (at 2.85 -0.325 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 21 smd rect (at 2.85 0.325 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 174 "Net-(U12-Pad21)"))
    (pad 20 smd rect (at 2.85 0.975 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 175 /CPU/L_RI1))
    (pad 19 smd rect (at 2.85 1.625 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 176 /CPU/L_RXD1))
    (pad 18 smd rect (at 2.85 2.275 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(U12-Pad18)"))
    (pad 17 smd rect (at 2.85 2.925 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 178 /CPU/L_CTS1))
    (pad 16 smd rect (at 2.85 3.575 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 179 /CPU/L_DSR1))
    (pad 15 smd rect (at 2.85 4.225 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 180 /CPU/L_DCD1))
    (pad 14 smd rect (at -2.85 4.225 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 181 /CPU/L_TXD1))
    (pad 13 smd rect (at -2.85 3.575 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 182 /CPU/L_RTS1))
    (pad 12 smd rect (at -2.85 2.925 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 183 /CPU/L_DTR1))
    (pad 11 smd rect (at -2.85 2.275 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 /CPU/R_DTR1))
    (pad 10 smd rect (at -2.85 1.625 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 185 /CPU/R_RTS1))
    (pad 9 smd rect (at -2.85 0.975 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 186 /CPU/R_TXD1))
    (pad 8 smd rect (at -2.85 0.325 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 187 /CPU/R_DCD1))
    (pad 7 smd rect (at -2.85 -0.325 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 188 /CPU/R_DSR1))
    (pad 6 smd rect (at -2.85 -0.975 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 189 /CPU/R_CTS1))
    (pad 5 smd rect (at -2.85 -1.625 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 190 /CPU/R_RI1))
    (pad 4 smd rect (at -2.85 -2.275 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 191 /CPU/R_RXD1))
    (pad 3 smd rect (at -2.85 -2.925 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(C54-Pad1)"))
    (pad 2 smd rect (at -2.85 -3.575 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(C50-Pad2)"))
    (pad 1 smd rect (at -2.85 -4.225 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(C50-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-28_4.4x9.7mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_12x12mm_h6mm (layer B.Cu) (tedit 5990349B)
    (at 77.47 79.375 270)
    (descr "Choke, SMD, 12x12mm 6mm height")
    (tags "Choke SMD")
    (attr smd)
    (fp_text reference L4 (at -1.27 7.112 270) (layer B.SilkS))
    (fp_text value 10uH (at 0 -7.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 4.95 0 270) (size 2.9 5.4) (layers B.Cu B.Paste B.Mask)
      (net 141 "Net-(D2-Pad3)"))
    (pad 1 smd rect (at -4.95 0 270) (size 2.9 5.4) (layers B.Cu B.Paste B.Mask)
      (net 132 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_12x12mm_h6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_12x12mm_h8mm (layer B.Cu) (tedit 5990349C)
    (at 88.646 61.595)
    (descr "Choke, SMD, 12x12mm 8mm height")
    (tags "Choke SMD")
    (attr smd)
    (fp_text reference L2 (at 8.128 5.969) (layer B.SilkS))
    (fp_text value 22uH (at 0 -7.6) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 4.95 0) (size 2.9 5.4) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 1 smd rect (at -4.95 0) (size 2.9 5.4) (layers B.Cu B.Paste B.Mask)
      (net 97 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_12x12mm_h8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Oscillators:Oscillator_SMD_EuroQuartz_XO91-4pin_7.0x5.0mm (layer F.Cu) (tedit 58CD3345)
    (at 156.21 69.85 90)
    (descr "Miniature Crystal Clock Oscillator EuroQuartz XO91 series, http://cdn-reichelt.de/documents/datenblatt/B400/XO91.pdf, 7.0x5.0mm^2 package")
    (tags "SMD SMT crystal oscillator")
    (attr smd)
    (fp_text reference X1 (at 0 -4.1 90) (layer F.SilkS))
    (fp_text value 50MHz (at 0 4.1 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd rect (at -2.5 -2.1 90) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 3 smd rect (at 2.5 -2.1 90) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(U18-Pad3)"))
    (pad 2 smd rect (at 2.5 2.1 90) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -2.5 2.1 90) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Oscillators.3dshapes/Oscillator_SMD_EuroQuartz_XO91-4pin_7.0x5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x25_Pitch1.27mm_SMD (layer B.Cu) (tedit 59650537)
    (at 125.73 60.96 270)
    (descr "surface-mounted straight pin header, 2x25, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x25 1.27mm double row")
    (attr smd)
    (fp_text reference J1 (at 0 16.935 270) (layer B.SilkS))
    (fp_text value Expansion (at 0 -16.935 270) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 50 smd rect (at 1.95 -15.24 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 49 smd rect (at -1.95 -15.24 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 48 smd rect (at 1.95 -13.97 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 140 +1V2))
    (pad 47 smd rect (at -1.95 -13.97 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 153 /RESET))
    (pad 46 smd rect (at 1.95 -12.7 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 154 /~WAIT))
    (pad 45 smd rect (at -1.95 -12.7 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 156 /INT))
    (pad 44 smd rect (at 1.95 -11.43 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 53 /~WR))
    (pad 43 smd rect (at -1.95 -11.43 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 33 /~RD))
    (pad 42 smd rect (at 1.95 -10.16 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 157 /~MREQ))
    (pad 41 smd rect (at -1.95 -10.16 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 158 /~IOREQ))
    (pad 40 smd rect (at 1.95 -8.89 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 159 /~BUSREQ))
    (pad 39 smd rect (at -1.95 -8.89 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 160 /~BUSACK))
    (pad 38 smd rect (at 1.95 -7.62 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 138 /CLK2))
    (pad 37 smd rect (at -1.95 -7.62 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 36 smd rect (at 1.95 -6.35 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 34 /D7))
    (pad 35 smd rect (at -1.95 -6.35 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 35 /D6))
    (pad 34 smd rect (at 1.95 -5.08 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 36 /D5))
    (pad 33 smd rect (at -1.95 -5.08 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 37 /D4))
    (pad 32 smd rect (at 1.95 -3.81 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 54 /D3))
    (pad 31 smd rect (at -1.95 -3.81 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 55 /D2))
    (pad 30 smd rect (at 1.95 -2.54 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 56 /D1))
    (pad 29 smd rect (at -1.95 -2.54 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 57 /D0))
    (pad 28 smd rect (at 1.95 -1.27 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 161 /A23))
    (pad 27 smd rect (at -1.95 -1.27 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 162 /A22))
    (pad 26 smd rect (at 1.95 0 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 25 smd rect (at -1.95 0 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 163 /A21))
    (pad 24 smd rect (at 1.95 1.27 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 164 /A20))
    (pad 23 smd rect (at -1.95 1.27 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 165 /A19))
    (pad 22 smd rect (at 1.95 2.54 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 29 /A18))
    (pad 21 smd rect (at -1.95 2.54 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 30 /A17))
    (pad 20 smd rect (at 1.95 3.81 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 31 /A16))
    (pad 19 smd rect (at -1.95 3.81 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 32 /A15))
    (pad 18 smd rect (at 1.95 5.08 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 38 /A14))
    (pad 17 smd rect (at -1.95 5.08 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 39 /A13))
    (pad 16 smd rect (at 1.95 6.35 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 40 /A12))
    (pad 15 smd rect (at -1.95 6.35 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 41 /A11))
    (pad 14 smd rect (at 1.95 7.62 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 42 /A10))
    (pad 13 smd rect (at -1.95 7.62 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 12 smd rect (at 1.95 8.89 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 48 /A9))
    (pad 11 smd rect (at -1.95 8.89 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 49 /A8))
    (pad 10 smd rect (at 1.95 10.16 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 50 /A7))
    (pad 9 smd rect (at -1.95 10.16 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 51 /A6))
    (pad 8 smd rect (at 1.95 11.43 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 52 /A5))
    (pad 7 smd rect (at -1.95 11.43 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 58 /A4))
    (pad 6 smd rect (at 1.95 12.7 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 59 /A3))
    (pad 5 smd rect (at -1.95 12.7 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 60 /A2))
    (pad 4 smd rect (at 1.95 13.97 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 61 /A1))
    (pad 3 smd rect (at -1.95 13.97 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 62 /A0))
    (pad 2 smd rect (at 1.95 15.24 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.95 15.24 270) (size 2.4 0.74) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x25_Pitch1.27mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 61.722 81.28 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D2 (at 2.794 0 180) (layer F.SilkS))
    (fp_text value BAT54 (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(D2-Pad3)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 98 /LED_A))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 66.548 81.026)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U3 (at 0 -2.54) (layer F.SilkS))
    (fp_text value FAN5333BSX (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(D2-Pad3)"))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 3 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 98 /LED_A))
    (pad 4 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 142 /LED_PWM))
    (pad 5 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 116.205 89.58)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U2 (at -1.35 -2.85) (layer F.SilkS))
    (fp_text value TPS62262 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(L3-Pad1)"))
    (pad 4 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 140 +1V2))
    (pad 3 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6_Handsoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 149.86 66.04 90)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference U18 (at 0 -2.9 90) (layer F.SilkS))
    (fp_text value PL133-37TC (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 -0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 135 /CLK1))
    (pad 2 smd rect (at -1.35 0 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 3 smd rect (at -1.35 0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(U18-Pad3)"))
    (pad 4 smd rect (at 1.35 0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 138 /CLK2))
    (pad 6 smd rect (at 1.35 -0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 137 /CLK0))
    (pad 5 smd rect (at 1.35 0 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6_Handsoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 58.748 116.84)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference U14 (at 4.064 0) (layer F.SilkS))
    (fp_text value SN74LVC1G3157DBVR (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.35 0) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(BT1-Pad1)"))
    (pad 6 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 284 "Net-(R16-Pad2)"))
    (pad 4 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(C58-Pad1)"))
    (pad 3 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 284 "Net-(R16-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-263-5_TabPin3 (layer B.Cu) (tedit 590079C0)
    (at 46.606 72.39 180)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-5-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-5 TO-263-5 SOT-426")
    (attr smd)
    (fp_text reference U1 (at 9.649 4.953 180) (layer B.SilkS))
    (fp_text value LM2576S-3.3 (at 0 -6.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 3 smd rect (at 0.95 -2.775 180) (size 4.55 5.25) (layers B.Cu B.Paste)
      (net 11 GND))
    (pad 3 smd rect (at 5.8 2.775 180) (size 4.55 5.25) (layers B.Cu B.Paste)
      (net 11 GND))
    (pad 3 smd rect (at 0.95 2.775 180) (size 4.55 5.25) (layers B.Cu B.Paste)
      (net 11 GND))
    (pad 3 smd rect (at 5.8 -2.775 180) (size 4.55 5.25) (layers B.Cu B.Paste)
      (net 11 GND))
    (pad 3 smd rect (at 3.375 0 180) (size 9.4 10.8) (layers B.Cu B.Mask)
      (net 11 GND))
    (pad 5 smd rect (at -5.775 -3.4 180) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 4 smd rect (at -5.775 -1.7 180) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 97 "Net-(C4-Pad1)"))
    (pad 3 smd rect (at -5.775 0 180) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 2 smd rect (at -5.775 1.7 180) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 96 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -5.775 3.4 180) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 132 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-263-5_TabPin3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:TSOPII-44 locked (layer F.Cu) (tedit 59CBFC90)
    (at 71.74 113.53 180)
    (fp_text reference U8 (at 5.6692 18.31 180) (layer F.SilkS))
    (fp_text value SRAM-512k (at 5.5 -2 180) (layer F.Fab))
    (pad 44 smd rect (at 11.4108 0 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U8-Pad44)"))
    (pad 43 smd rect (at 11.4108 0.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U8-Pad43)"))
    (pad 42 smd rect (at 11.4108 1.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U8-Pad42)"))
    (pad 41 smd rect (at 11.4108 2.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 240 "/Graphics Controller/GPU_A18"))
    (pad 40 smd rect (at 11.4108 3.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 241 "/Graphics Controller/GPU_A17"))
    (pad 39 smd rect (at 11.4108 4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 242 "/Graphics Controller/GPU_A16"))
    (pad 38 smd rect (at 11.4108 4.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 243 "/Graphics Controller/GPU_A15"))
    (pad 37 smd rect (at 11.4108 5.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 277 "/Graphics Controller/~GPU_OE"))
    (pad 36 smd rect (at 11.4108 6.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 232 "/Graphics Controller/GPU_D7"))
    (pad 35 smd rect (at 11.4108 7.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 233 "/Graphics Controller/GPU_D6"))
    (pad 34 smd rect (at 11.4108 8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 33 smd rect (at 11.4108 8.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 32 smd rect (at 11.4108 9.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 234 "/Graphics Controller/GPU_D5"))
    (pad 31 smd rect (at 11.4108 10.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 235 "/Graphics Controller/GPU_D4"))
    (pad 30 smd rect (at 11.4108 11.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 244 "/Graphics Controller/GPU_A14"))
    (pad 29 smd rect (at 11.4108 12 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 245 "/Graphics Controller/GPU_A13"))
    (pad 28 smd rect (at 11.4108 12.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 246 "/Graphics Controller/GPU_A12"))
    (pad 27 smd rect (at 11.4108 13.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 247 "/Graphics Controller/GPU_A11"))
    (pad 26 smd rect (at 11.4108 14.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 248 "/Graphics Controller/GPU_A10"))
    (pad 25 smd rect (at 11.4108 15.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U8-Pad25)"))
    (pad 24 smd rect (at 11.4108 16 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U8-Pad24)"))
    (pad 23 smd rect (at 11.4108 16.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U8-Pad23)"))
    (pad 22 smd rect (at 0 16.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U8-Pad22)"))
    (pad 21 smd rect (at 0 16 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U8-Pad21)"))
    (pad 20 smd rect (at 0 15.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 249 "/Graphics Controller/GPU_A9"))
    (pad 19 smd rect (at 0 14.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 250 "/Graphics Controller/GPU_A8"))
    (pad 18 smd rect (at 0 13.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 251 "/Graphics Controller/GPU_A7"))
    (pad 17 smd rect (at 0 12.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 252 "/Graphics Controller/GPU_A6"))
    (pad 16 smd rect (at 0 12 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 253 "/Graphics Controller/GPU_A5"))
    (pad 15 smd rect (at 0 11.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 278 "/Graphics Controller/~GPU_WE"))
    (pad 14 smd rect (at 0 10.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 236 "/Graphics Controller/GPU_D3"))
    (pad 13 smd rect (at 0 9.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 237 "/Graphics Controller/GPU_D2"))
    (pad 12 smd rect (at 0 8.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 11 smd rect (at 0 8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 10 smd rect (at 0 7.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 238 "/Graphics Controller/GPU_D1"))
    (pad 9 smd rect (at 0 6.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 239 "/Graphics Controller/GPU_D0"))
    (pad 8 smd rect (at 0 5.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 281 "/Graphics Controller/~GPU_CS2"))
    (pad 7 smd rect (at 0 4.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 254 "/Graphics Controller/GPU_A4"))
    (pad 6 smd rect (at 0 4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 255 "/Graphics Controller/GPU_A3"))
    (pad 5 smd rect (at 0 3.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 256 "/Graphics Controller/GPU_A2"))
    (pad 4 smd rect (at 0 2.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 257 "/Graphics Controller/GPU_A1"))
    (pad 3 smd rect (at 0 1.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 258 "/Graphics Controller/GPU_A0"))
    (pad 2 smd rect (at 0 0.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U8-Pad2)"))
    (pad 1 smd rect (at 0 0 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U8-Pad1)"))
  )
  (module footprints:TSOPII-44 (layer F.Cu) (tedit 59CBFC90)
    (at 101.26 69.22)
    (fp_text reference U16 (at 5.8108 -1.6) (layer F.SilkS))
    (fp_text value SRAM-512k (at 5.5 18.6) (layer F.Fab))
    (pad 44 smd rect (at 11.4108 0) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U16-Pad44)"))
    (pad 43 smd rect (at 11.4108 0.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U16-Pad43)"))
    (pad 42 smd rect (at 11.4108 1.6) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U16-Pad42)"))
    (pad 41 smd rect (at 11.4108 2.4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 29 /A18))
    (pad 40 smd rect (at 11.4108 3.2) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 30 /A17))
    (pad 39 smd rect (at 11.4108 4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 31 /A16))
    (pad 38 smd rect (at 11.4108 4.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 32 /A15))
    (pad 37 smd rect (at 11.4108 5.6) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 33 /~RD))
    (pad 36 smd rect (at 11.4108 6.4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 34 /D7))
    (pad 35 smd rect (at 11.4108 7.2) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 35 /D6))
    (pad 34 smd rect (at 11.4108 8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 33 smd rect (at 11.4108 8.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 32 smd rect (at 11.4108 9.6) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 36 /D5))
    (pad 31 smd rect (at 11.4108 10.4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 37 /D4))
    (pad 30 smd rect (at 11.4108 11.2) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 38 /A14))
    (pad 29 smd rect (at 11.4108 12) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 39 /A13))
    (pad 28 smd rect (at 11.4108 12.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 40 /A12))
    (pad 27 smd rect (at 11.4108 13.6) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 41 /A11))
    (pad 26 smd rect (at 11.4108 14.4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 42 /A10))
    (pad 25 smd rect (at 11.4108 15.2) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U16-Pad25)"))
    (pad 24 smd rect (at 11.4108 16) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U16-Pad24)"))
    (pad 23 smd rect (at 11.4108 16.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U16-Pad23)"))
    (pad 22 smd rect (at 0 16.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U16-Pad22)"))
    (pad 21 smd rect (at 0 16) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U16-Pad21)"))
    (pad 20 smd rect (at 0 15.2) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 48 /A9))
    (pad 19 smd rect (at 0 14.4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 49 /A8))
    (pad 18 smd rect (at 0 13.6) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 50 /A7))
    (pad 17 smd rect (at 0 12.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 51 /A6))
    (pad 16 smd rect (at 0 12) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 52 /A5))
    (pad 15 smd rect (at 0 11.2) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 53 /~WR))
    (pad 14 smd rect (at 0 10.4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 54 /D3))
    (pad 13 smd rect (at 0 9.6) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 55 /D2))
    (pad 12 smd rect (at 0 8.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 11 smd rect (at 0 8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 10 smd rect (at 0 7.2) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 56 /D1))
    (pad 9 smd rect (at 0 6.4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 57 /D0))
    (pad 8 smd rect (at 0 5.6) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 14 "/CPU Memory/~CS1"))
    (pad 7 smd rect (at 0 4.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 58 /A4))
    (pad 6 smd rect (at 0 4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 59 /A3))
    (pad 5 smd rect (at 0 3.2) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 60 /A2))
    (pad 4 smd rect (at 0 2.4) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 61 /A1))
    (pad 3 smd rect (at 0 1.6) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 62 /A0))
    (pad 2 smd rect (at 0 0.8) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U16-Pad2)"))
    (pad 1 smd rect (at 0 0) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U16-Pad1)"))
  )
  (module footprints:TSOPII-44 (layer F.Cu) (tedit 59CBFC90)
    (at 39.74 113.53 180)
    (fp_text reference U6 (at 6 18.31 180) (layer F.SilkS))
    (fp_text value SRAM-512k (at 5.5 -2 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U6-Pad1)"))
    (pad 2 smd rect (at 0 0.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U6-Pad2)"))
    (pad 3 smd rect (at 0 1.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 258 "/Graphics Controller/GPU_A0"))
    (pad 4 smd rect (at 0 2.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 257 "/Graphics Controller/GPU_A1"))
    (pad 5 smd rect (at 0 3.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 256 "/Graphics Controller/GPU_A2"))
    (pad 6 smd rect (at 0 4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 255 "/Graphics Controller/GPU_A3"))
    (pad 7 smd rect (at 0 4.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 254 "/Graphics Controller/GPU_A4"))
    (pad 8 smd rect (at 0 5.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 280 "/Graphics Controller/~GPU_CS0"))
    (pad 9 smd rect (at 0 6.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 239 "/Graphics Controller/GPU_D0"))
    (pad 10 smd rect (at 0 7.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 238 "/Graphics Controller/GPU_D1"))
    (pad 11 smd rect (at 0 8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 12 smd rect (at 0 8.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 13 smd rect (at 0 9.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 237 "/Graphics Controller/GPU_D2"))
    (pad 14 smd rect (at 0 10.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 236 "/Graphics Controller/GPU_D3"))
    (pad 15 smd rect (at 0 11.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 278 "/Graphics Controller/~GPU_WE"))
    (pad 16 smd rect (at 0 12 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 253 "/Graphics Controller/GPU_A5"))
    (pad 17 smd rect (at 0 12.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 252 "/Graphics Controller/GPU_A6"))
    (pad 18 smd rect (at 0 13.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 251 "/Graphics Controller/GPU_A7"))
    (pad 19 smd rect (at 0 14.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 250 "/Graphics Controller/GPU_A8"))
    (pad 20 smd rect (at 0 15.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 249 "/Graphics Controller/GPU_A9"))
    (pad 21 smd rect (at 0 16 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U6-Pad21)"))
    (pad 22 smd rect (at 0 16.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U6-Pad22)"))
    (pad 23 smd rect (at 11.4108 16.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U6-Pad23)"))
    (pad 24 smd rect (at 11.4108 16 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U6-Pad24)"))
    (pad 25 smd rect (at 11.4108 15.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U6-Pad25)"))
    (pad 26 smd rect (at 11.4108 14.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 248 "/Graphics Controller/GPU_A10"))
    (pad 27 smd rect (at 11.4108 13.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 247 "/Graphics Controller/GPU_A11"))
    (pad 28 smd rect (at 11.4108 12.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 246 "/Graphics Controller/GPU_A12"))
    (pad 29 smd rect (at 11.4108 12 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 245 "/Graphics Controller/GPU_A13"))
    (pad 30 smd rect (at 11.4108 11.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 244 "/Graphics Controller/GPU_A14"))
    (pad 31 smd rect (at 11.4108 10.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 235 "/Graphics Controller/GPU_D4"))
    (pad 32 smd rect (at 11.4108 9.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 234 "/Graphics Controller/GPU_D5"))
    (pad 33 smd rect (at 11.4108 8.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 34 smd rect (at 11.4108 8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 35 smd rect (at 11.4108 7.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 233 "/Graphics Controller/GPU_D6"))
    (pad 36 smd rect (at 11.4108 6.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 232 "/Graphics Controller/GPU_D7"))
    (pad 37 smd rect (at 11.4108 5.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 277 "/Graphics Controller/~GPU_OE"))
    (pad 38 smd rect (at 11.4108 4.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 243 "/Graphics Controller/GPU_A15"))
    (pad 39 smd rect (at 11.4108 4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 242 "/Graphics Controller/GPU_A16"))
    (pad 40 smd rect (at 11.4108 3.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 241 "/Graphics Controller/GPU_A17"))
    (pad 41 smd rect (at 11.4108 2.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 240 "/Graphics Controller/GPU_A18"))
    (pad 42 smd rect (at 11.4108 1.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U6-Pad42)"))
    (pad 43 smd rect (at 11.4108 0.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U6-Pad43)"))
    (pad 44 smd rect (at 11.4108 0 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(U6-Pad44)"))
  )
  (module footprints:TSOPII-44 locked (layer F.Cu) (tedit 59CBFC90)
    (at 55.74 113.53 180)
    (fp_text reference U7 (at 5.7 18.31 180) (layer F.SilkS))
    (fp_text value SRAM-512k (at 5.5 -2 180) (layer F.Fab))
    (pad 44 smd rect (at 11.4108 0 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U7-Pad44)"))
    (pad 43 smd rect (at 11.4108 0.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U7-Pad43)"))
    (pad 42 smd rect (at 11.4108 1.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U7-Pad42)"))
    (pad 41 smd rect (at 11.4108 2.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 240 "/Graphics Controller/GPU_A18"))
    (pad 40 smd rect (at 11.4108 3.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 241 "/Graphics Controller/GPU_A17"))
    (pad 39 smd rect (at 11.4108 4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 242 "/Graphics Controller/GPU_A16"))
    (pad 38 smd rect (at 11.4108 4.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 243 "/Graphics Controller/GPU_A15"))
    (pad 37 smd rect (at 11.4108 5.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 277 "/Graphics Controller/~GPU_OE"))
    (pad 36 smd rect (at 11.4108 6.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 232 "/Graphics Controller/GPU_D7"))
    (pad 35 smd rect (at 11.4108 7.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 233 "/Graphics Controller/GPU_D6"))
    (pad 34 smd rect (at 11.4108 8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 33 smd rect (at 11.4108 8.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 32 smd rect (at 11.4108 9.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 234 "/Graphics Controller/GPU_D5"))
    (pad 31 smd rect (at 11.4108 10.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 235 "/Graphics Controller/GPU_D4"))
    (pad 30 smd rect (at 11.4108 11.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 244 "/Graphics Controller/GPU_A14"))
    (pad 29 smd rect (at 11.4108 12 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 245 "/Graphics Controller/GPU_A13"))
    (pad 28 smd rect (at 11.4108 12.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 246 "/Graphics Controller/GPU_A12"))
    (pad 27 smd rect (at 11.4108 13.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 247 "/Graphics Controller/GPU_A11"))
    (pad 26 smd rect (at 11.4108 14.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 248 "/Graphics Controller/GPU_A10"))
    (pad 25 smd rect (at 11.4108 15.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U7-Pad25)"))
    (pad 24 smd rect (at 11.4108 16 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U7-Pad24)"))
    (pad 23 smd rect (at 11.4108 16.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U7-Pad23)"))
    (pad 22 smd rect (at 0 16.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U7-Pad22)"))
    (pad 21 smd rect (at 0 16 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U7-Pad21)"))
    (pad 20 smd rect (at 0 15.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 249 "/Graphics Controller/GPU_A9"))
    (pad 19 smd rect (at 0 14.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 250 "/Graphics Controller/GPU_A8"))
    (pad 18 smd rect (at 0 13.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 251 "/Graphics Controller/GPU_A7"))
    (pad 17 smd rect (at 0 12.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 252 "/Graphics Controller/GPU_A6"))
    (pad 16 smd rect (at 0 12 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 253 "/Graphics Controller/GPU_A5"))
    (pad 15 smd rect (at 0 11.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 278 "/Graphics Controller/~GPU_WE"))
    (pad 14 smd rect (at 0 10.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 236 "/Graphics Controller/GPU_D3"))
    (pad 13 smd rect (at 0 9.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 237 "/Graphics Controller/GPU_D2"))
    (pad 12 smd rect (at 0 8.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 11 smd rect (at 0 8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 10 smd rect (at 0 7.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 238 "/Graphics Controller/GPU_D1"))
    (pad 9 smd rect (at 0 6.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 239 "/Graphics Controller/GPU_D0"))
    (pad 8 smd rect (at 0 5.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 279 "/Graphics Controller/~GPU_CS1"))
    (pad 7 smd rect (at 0 4.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 254 "/Graphics Controller/GPU_A4"))
    (pad 6 smd rect (at 0 4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 255 "/Graphics Controller/GPU_A3"))
    (pad 5 smd rect (at 0 3.2 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 256 "/Graphics Controller/GPU_A2"))
    (pad 4 smd rect (at 0 2.4 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 257 "/Graphics Controller/GPU_A1"))
    (pad 3 smd rect (at 0 1.6 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 258 "/Graphics Controller/GPU_A0"))
    (pad 2 smd rect (at 0 0.8 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U7-Pad2)"))
    (pad 1 smd rect (at 0 0 180) (size 1.5174 0.477) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U7-Pad1)"))
  )
  (gr_text "Z80 Computer\nRev 0\n© 2017 Alex French" (at 89.154 90.424) (layer B.SilkS))
  (gr_text "5VDC\nCNTR +" (at 29.21 68.58 270) (layer B.SilkS))
  (gr_text EXPANSION (at 125.73 56.134) (layer B.SilkS))
  (gr_text NMI (at 29.972 99.822 270) (layer B.SilkS))
  (dimension 133.35 (width 0.3) (layer Dwgs.User)
    (gr_text "5.2500 in" (at 92.075 141.05) (layer Dwgs.User))
    (feature1 (pts (xy 158.75 120.65) (xy 158.75 142.4)))
    (feature2 (pts (xy 25.4 120.65) (xy 25.4 142.4)))
    (crossbar (pts (xy 25.4 139.7) (xy 158.75 139.7)))
    (arrow1a (pts (xy 158.75 139.7) (xy 157.623496 140.286421)))
    (arrow1b (pts (xy 158.75 139.7) (xy 157.623496 139.113579)))
    (arrow2a (pts (xy 25.4 139.7) (xy 26.526504 140.286421)))
    (arrow2b (pts (xy 25.4 139.7) (xy 26.526504 139.113579)))
  )
  (gr_text RESET (at 30.226 109.982 270) (layer B.SilkS))
  (gr_text "COM A" (at 161.29 92.075 90) (layer B.SilkS))
  (gr_text "COM B" (at 161.29 83.185 90) (layer B.SilkS))
  (gr_text CDONE (at 69.215 119.38) (layer B.SilkS))
  (gr_text PWR (at 41.656 56.642) (layer B.SilkS))
  (dimension 149.86 (width 0.3) (layer Dwgs.User)
    (gr_text "5.9000 in" (at 100.33 134.699999) (layer Dwgs.User))
    (feature1 (pts (xy 175.26 120.65) (xy 175.26 136.049999)))
    (feature2 (pts (xy 25.4 120.65) (xy 25.4 136.049999)))
    (crossbar (pts (xy 25.4 133.349999) (xy 175.26 133.349999)))
    (arrow1a (pts (xy 175.26 133.349999) (xy 174.133496 133.93642)))
    (arrow1b (pts (xy 175.26 133.349999) (xy 174.133496 132.763578)))
    (arrow2a (pts (xy 25.4 133.349999) (xy 26.526504 133.93642)))
    (arrow2b (pts (xy 25.4 133.349999) (xy 26.526504 132.763578)))
  )
  (dimension 66.675 (width 0.3) (layer Dwgs.User)
    (gr_text "2.6250 in" (at 1.19 87.3125 90) (layer Dwgs.User))
    (feature1 (pts (xy 25.4 53.975) (xy -0.16 53.975)))
    (feature2 (pts (xy 25.4 120.65) (xy -0.16 120.65)))
    (crossbar (pts (xy 2.54 120.65) (xy 2.54 53.975)))
    (arrow1a (pts (xy 2.54 53.975) (xy 3.126421 55.101504)))
    (arrow1b (pts (xy 2.54 53.975) (xy 1.953579 55.101504)))
    (arrow2a (pts (xy 2.54 120.65) (xy 3.126421 119.523496)))
    (arrow2b (pts (xy 2.54 120.65) (xy 1.953579 119.523496)))
  )
  (dimension 59.944 (width 0.3) (layer Dwgs.User)
    (gr_text "2.3600 in" (at 18.97 116.078 90) (layer Dwgs.User))
    (feature1 (pts (xy 25.4 86.106) (xy 17.62 86.106)))
    (feature2 (pts (xy 25.4 146.05) (xy 17.62 146.05)))
    (crossbar (pts (xy 20.32 146.05) (xy 20.32 86.106)))
    (arrow1a (pts (xy 20.32 86.106) (xy 20.906421 87.232504)))
    (arrow1b (pts (xy 20.32 86.106) (xy 19.733579 87.232504)))
    (arrow2a (pts (xy 20.32 146.05) (xy 20.906421 144.923496)))
    (arrow2b (pts (xy 20.32 146.05) (xy 19.733579 144.923496)))
  )
  (dimension 30.48 (width 0.3) (layer Dwgs.User)
    (gr_text "1.2000 in" (at 40.64 127) (layer Dwgs.User))
    (feature1 (pts (xy 55.88 120.57) (xy 55.88 128.35)))
    (feature2 (pts (xy 25.4 120.57) (xy 25.4 128.35)))
    (crossbar (pts (xy 25.4 125.65) (xy 55.88 125.65)))
    (arrow1a (pts (xy 55.88 125.65) (xy 54.753496 126.236421)))
    (arrow1b (pts (xy 55.88 125.65) (xy 54.753496 125.063579)))
    (arrow2a (pts (xy 25.4 125.65) (xy 26.526504 126.236421)))
    (arrow2b (pts (xy 25.4 125.65) (xy 26.526504 125.063579)))
  )
  (gr_line (start 25.4 120.65) (end 25.4 53.975) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.26 120.65) (end 25.4 120.65) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.26 53.975) (end 175.26 120.65) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 25.4 53.975) (end 175.26 53.975) (layer Edge.Cuts) (width 0.15))
  (zone (net 11) (net_name GND) (layer GND.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25.4 120.65) (xy 25.4 53.975) (xy 175.26 53.975) (xy 175.26 120.65)
      )
    )
  )
  (zone (net 12) (net_name +3V3) (layer PWR.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25.4 120.65) (xy 25.4 53.975) (xy 175.26 53.975) (xy 175.26 120.65)
      )
    )
  )
)
