(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 46)
    (tracks 608)
    (zones 0)
    (modules 144)
    (nets 69)
  )
  (page A4)
  (title_block
    (title MMDVM_HS_Hat)
    (date 2018-06-05)
    (rev 1.6)
    (company DB9MAT+DF2ET)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.9 1.7)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 169.6 112.9)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/opt/MMDVM_HS_Hat/gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C4-Pad1)")
  (net 3 +3V3)
  (net 4 "Net-(C8-Pad1)")
  (net 5 "Net-(C11-Pad1)")
  (net 6 NRST)
  (net 7 "Net-(C18-Pad1)")
  (net 8 "Net-(C18-Pad2)")
  (net 9 COS_LED)
  (net 10 PTT_LED)
  (net 11 DMR_LED)
  (net 12 DSTAR_LED)
  (net 13 P25_LED)
  (net 14 YSF_LED)
  (net 15 RF)
  (net 16 SWDIO)
  (net 17 TXD)
  (net 18 RXD)
  (net 19 DISP_TXD)
  (net 20 DISP_RXD)
  (net 21 BOOT0)
  (net 22 CLKOUT)
  (net 23 DATAIN)
  (net 24 DATAOUT)
  (net 25 SLE)
  (net 26 SDATA)
  (net 27 SREAD)
  (net 28 SCLK)
  (net 29 "Net-(C1-Pad1)")
  (net 30 "Net-(C4-Pad2)")
  (net 31 "Net-(C5-Pad1)")
  (net 32 "Net-(C6-Pad1)")
  (net 33 "Net-(C10-Pad1)")
  (net 34 "Net-(C11-Pad2)")
  (net 35 "Net-(C12-Pad1)")
  (net 36 "Net-(C13-Pad1)")
  (net 37 "Net-(C14-Pad1)")
  (net 38 "Net-(C15-Pad2)")
  (net 39 "Net-(C20-Pad2)")
  (net 40 "Net-(C21-Pad2)")
  (net 41 "Net-(C23-Pad2)")
  (net 42 "Net-(R2-Pad1)")
  (net 43 "Net-(R10-Pad2)")
  (net 44 CE)
  (net 45 SWCLK)
  (net 46 +5V)
  (net 47 SERVICE)
  (net 48 "Net-(D1-Pad2)")
  (net 49 "Net-(R3-Pad1)")
  (net 50 "Net-(R8-Pad2)")
  (net 51 "Net-(R9-Pad2)")
  (net 52 "Net-(D2-Pad2)")
  (net 53 "Net-(D3-Pad2)")
  (net 54 "Net-(D4-Pad2)")
  (net 55 "Net-(D5-Pad2)")
  (net 56 "Net-(D6-Pad2)")
  (net 57 "Net-(D7-Pad2)")
  (net 58 "Net-(D8-Pad2)")
  (net 59 "Net-(C27-Pad1)")
  (net 60 "Net-(AE1-Pad1)")
  (net 61 SCL)
  (net 62 SDA)
  (net 63 "Net-(PI1-Pad38)")
  (net 64 VDD)
  (net 65 "Net-(D9-Pad2)")
  (net 66 NXDN_LED)
  (net 67 "Net-(L6-Pad2)")
  (net 68 "Net-(L6-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net BOOT0)
    (add_net CE)
    (add_net CLKOUT)
    (add_net COS_LED)
    (add_net DATAIN)
    (add_net DATAOUT)
    (add_net DISP_RXD)
    (add_net DISP_TXD)
    (add_net DMR_LED)
    (add_net DSTAR_LED)
    (add_net GND)
    (add_net NRST)
    (add_net NXDN_LED)
    (add_net "Net-(AE1-Pad1)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C23-Pad2)")
    (add_net "Net-(C27-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(L6-Pad1)")
    (add_net "Net-(L6-Pad2)")
    (add_net "Net-(PI1-Pad38)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net P25_LED)
    (add_net PTT_LED)
    (add_net RF)
    (add_net RXD)
    (add_net SCL)
    (add_net SCLK)
    (add_net SDA)
    (add_net SDATA)
    (add_net SERVICE)
    (add_net SLE)
    (add_net SREAD)
    (add_net SWCLK)
    (add_net SWDIO)
    (add_net TXD)
    (add_net VDD)
    (add_net YSF_LED)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module MMDVM:Logo_silk_CC-BY-NC-SA_5x2mm (layer F.Cu) (tedit 0)
    (at 192.2 114.15)
    (descr "CC BY-NC-SA logo, 5x2mm")
    (fp_text reference G*** (at 0.2 -0.7) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.2 0.2) (layer F.SilkS) hide)
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5A6987B8)
    (at 210.3 122.2 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R19 (at 1.7 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at -2.54 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(D9-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 66 NXDN_LED))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 5A698776)
    (at 213.3 122.2 180)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D9 (at 1.6 0 180) (layer F.SilkS))
    (fp_text value blue (at 0 1.4 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(D9-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 175.1 122.75)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 213.75 134.75)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 167.6 113)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 188.75 127.75)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 202.5 127.25)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 202.5 123)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 197.5 123)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 208 114.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 174.75 114.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 191.5 129)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 185.25 118.25)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 184.5 120.25)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 218.75 117.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 218.75 119.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 201.05 117.75)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 194 118.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 210 130.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 204.75 135)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 195 131.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 195 135.1)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 195.5 129)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 181 130)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 171.25 134.75)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 171.25 131.25)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 190.45 112.45)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 177.25 116.25)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 185 112.75)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 171.05 122.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 168.75 122.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 166 122.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 171 126.25)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 171 124.75)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 168.75 125.75)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 167.5 124.75)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 165.5 124.75)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 164 125.25)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 163 126.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 163 122.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 163 120.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 163 118.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 163 116.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 163 114.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 163 112.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 185 129.75)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 197 127.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 182.6 126.6)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 181.4 126.6)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 180.2 126.6)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 179 126.6)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 182.6 125.4)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 181.4 125.4)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 180.2 125.4)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 179 125.4)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 182.6 124.2)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 181.4 124.2)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 180.2 124.2)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 179 124.2)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 182.6 123)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 181.4 123)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 180.2 123)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 179 123)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4711)
    (at 168.75 124.15 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 0.95 -0.95 90) (layer F.SilkS))
    (fp_text value 6p8 (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D49C5)
    (at 172.6 121)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at -1.6 0) (layer F.SilkS))
    (fp_text value 10n (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D49DE)
    (at 172.6 119.75)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at -1.6 0) (layer F.SilkS))
    (fp_text value 220p (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591C4706)
    (at 172.6 123.65 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at -1.65 -0.05 180) (layer F.SilkS))
    (fp_text value 10p (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591C4718)
    (at 172.6 124.85 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at -1.65 0 180) (layer F.SilkS))
    (fp_text value 4p7 (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4CC8)
    (at 172.6 127.4 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 1.45 0 270) (layer F.SilkS))
    (fp_text value 6p8 (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591C4697)
    (at 172.6 130 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at 0 -1 180) (layer F.SilkS))
    (fp_text value 10n (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4B2D)
    (at 172.6 118.5 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at 1.55 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D47C5)
    (at 175 121.05 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at -0.1 -0.9 180) (layer F.SilkS))
    (fp_text value 10n (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 597859F7)
    (at 177.2 130)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at 1.8 0) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4C38)
    (at 175 118.5 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C11 (at 0 1.1 180) (layer F.SilkS))
    (fp_text value 22n (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A9E9CA3)
    (at 178.7 116.45 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C12 (at 1.9 0 90) (layer F.SilkS))
    (fp_text value 470p (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A9E9CA7)
    (at 180.05 116.45 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C13 (at 1.9 0 90) (layer F.SilkS))
    (fp_text value 15n (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4D23)
    (at 181.3 118.7 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C14 (at 1.9 0 90) (layer F.SilkS))
    (fp_text value 1n (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A9E9CAD)
    (at 182.65 116.4 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C15 (at -1.9 0 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C15-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591C2AEE)
    (at 205.5 133.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C16 (at -1.8 0 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 NRST))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A9E9CB2)
    (at 183.85 116.4 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C17 (at 1.9 0.05 90) (layer F.SilkS))
    (fp_text value 10n (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591C41E2)
    (at 186.6 119.05 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C18 (at -2.05 0 180) (layer F.SilkS))
    (fp_text value 22p (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C18-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4A5C)
    (at 190.85 116.7 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C19 (at -0.05 -1 270) (layer F.SilkS))
    (fp_text value 10n (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591C3FF6)
    (at 186.6 125.55 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C20 (at 0.1 -0.95 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C20-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4A84)
    (at 195 133.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C21 (at -0.1 -1 90) (layer F.SilkS))
    (fp_text value 20p (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C21-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591C402B)
    (at 186.6 124.15 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C22 (at -1.85 -0.35 180) (layer F.SilkS))
    (fp_text value 10n (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591C2AE9)
    (at 204 133.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C23 (at 1.8 0 90) (layer F.SilkS))
    (fp_text value 20p (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C23-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4A8D)
    (at 193.04 128.05 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C24 (at 0 -1.038 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4A77)
    (at 206 121 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C25 (at 1.95 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4A71)
    (at 196.7 118.25 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C26 (at -0.05 -1.2 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 5994589F)
    (at 215.8 113.75 180)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 1.55 0.05 180) (layer F.SilkS))
    (fp_text value red (at 0 1.4 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 47 SERVICE))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 59945898)
    (at 213.3 112.6 180)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 1.6 0 180) (layer F.SilkS))
    (fp_text value green (at 0 1.4 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 599458A5)
    (at 213.3 115 180)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 1.6 0 180) (layer F.SilkS))
    (fp_text value yellow (at 0 1.4 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 599458AA)
    (at 215.8 116.2 180)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 1.6 0 180) (layer F.SilkS))
    (fp_text value red (at 0 1.4 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 599458AF)
    (at 213.3 117.4 180)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at 1.6 0 180) (layer F.SilkS))
    (fp_text value green (at 0 1.4 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 599458B5)
    (at 215.8 118.6 180)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D6 (at 1.6 0 180) (layer F.SilkS))
    (fp_text value yellow (at 0 1.4 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 599458B9)
    (at 213.3 119.8 180)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D7 (at 1.6 0 180) (layer F.SilkS))
    (fp_text value amber (at 0 1.4 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connectors:SMA_THT_Jack_Straight (layer F.Cu) (tedit 591D5CFC)
    (at 166.5 131.25)
    (descr "SMA pcb through hole jack")
    (tags "SMA THT Jack Straight")
    (fp_text reference P3 (at 0 -2.45) (layer F.SilkS))
    (fp_text value SMA (at 0 5) (layer F.Fab))
    (fp_text user %R (at 0 -5) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (net 59 "Net-(C27-Pad1)"))
    (model ${KIPRJMOD}/libraries/sma_straight_32k101-400l5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591D4A94)
    (at 193.04 126.05 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at -0.01 1 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 BOOT0))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(PI1-Pad38)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591C46CC)
    (at 172.6 128.7 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 1.45 0 90) (layer F.SilkS))
    (fp_text value 1k1 (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 59785986)
    (at 178.7 118.7 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 1 -0.9 90) (layer F.SilkS))
    (fp_text value 560 (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591D4AF8)
    (at 180 118.7 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at -1.6 1.1 90) (layer F.SilkS))
    (fp_text value 270 (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591D4D28)
    (at 207.2 133.5 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 1.6 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 NRST))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 597858EA)
    (at 186.6 120.3 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at -1.8 -0.05 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 CLKOUT))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591C2AFE)
    (at 186.6 121.6 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R9 (at -1.9 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 DATAIN))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 597858F2)
    (at 186.6 122.9 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R10 (at -2.05 0) (layer F.SilkS))
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 DATAOUT))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 59785A46)
    (at 210.3 112.6 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R11 (at 1.65 -0.05 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 59785A5D)
    (at 210.3 115 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R12 (at 1.65 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 COS_LED))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 59785ACC)
    (at 210.3 116.2 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R13 (at 1.6 0.05 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at -2.54 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 PTT_LED))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 59785AFB)
    (at 210.3 117.4 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R14 (at 1.65 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at -2.54 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(D5-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 DSTAR_LED))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 59785B33)
    (at 210.3 118.6 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R15 (at 1.7 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at -2.54 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 DMR_LED))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 59785B64)
    (at 210.3 119.8 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R16 (at 1.7 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at -2.54 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(D7-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 YSF_LED))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 59785B4C)
    (at 210.3 121 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R17 (at 1.7 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at -2.54 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(D8-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 P25_LED))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 59785B15)
    (at 210.3 113.8)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R18 (at -1.65 0) (layer F.SilkS))
    (fp_text value 1k (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at -2.54 0) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_B3U-1000P (layer F.Cu) (tedit 5A7D9535)
    (at 210.7 133.4)
    (descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, without Boss")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 0 180) (layer F.SilkS))
    (fp_text value DNI (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at -1.7 0) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 6 NRST))
    (pad 2 smd rect (at 1.7 0) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/libraries/smd_push.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.5 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-48-1EP_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 591D4C16)
    (at 180.79375 124.89375)
    (descr "UK Package; 48-Lead Plastic QFN (7mm x 7mm); (see Linear Technology QFN_48_05-08-1704.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 1.60625 4.70625) (layer F.SilkS))
    (fp_text value ADF7021 (at 0 4.75) (layer F.Fab))
    (pad 1 smd rect (at -3.4 -2.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at -3.4 -2.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C11-Pad2)"))
    (pad 3 smd rect (at -3.4 -1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 4 smd rect (at -3.4 -1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C4-Pad1)"))
    (pad 5 smd rect (at -3.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C5-Pad1)"))
    (pad 7 smd rect (at -3.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C6-Pad1)"))
    (pad 8 smd rect (at -3.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R2-Pad1)"))
    (pad 9 smd rect (at -3.4 1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 10 smd rect (at -3.4 1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R3-Pad1)"))
    (pad 11 smd rect (at -3.4 2.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C10-Pad1)"))
    (pad 12 smd rect (at -3.4 2.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at -2.75 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at 0.75 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 23 smd rect (at 2.25 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at 2.75 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 CE))
    (pad 25 smd rect (at 3.4 2.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 SLE))
    (pad 26 smd rect (at 3.4 2.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 SDATA))
    (pad 27 smd rect (at 3.4 1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 SREAD))
    (pad 28 smd rect (at 3.4 1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 SCLK))
    (pad 29 smd rect (at 3.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 30 smd rect (at 3.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 31 smd rect (at 3.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C20-Pad2)"))
    (pad 32 smd rect (at 3.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 33 smd rect (at 3.4 -1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 34 smd rect (at 3.4 -1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R10-Pad2)"))
    (pad 35 smd rect (at 3.4 -2.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R9-Pad2)"))
    (pad 36 smd rect (at 3.4 -2.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R8-Pad2)"))
    (pad 37 smd rect (at 2.75 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 38 smd rect (at 2.25 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C18-Pad2)"))
    (pad 40 smd rect (at 1.25 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 41 smd rect (at 0.75 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C15-Pad2)"))
    (pad 42 smd rect (at 0.25 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C14-Pad1)"))
    (pad 43 smd rect (at -0.25 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 44 smd rect (at -0.75 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(L6-Pad2)"))
    (pad 45 smd rect (at -1.25 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 46 smd rect (at -1.75 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(L6-Pad1)"))
    (pad 47 smd rect (at -2.25 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C11-Pad1)"))
    (pad 49 smd rect (at 1.93125 1.93125) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 1.93125 0.64375) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 1.93125 -0.64375) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 1.93125 -1.93125) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 1.93125) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 0.64375) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 -0.64375) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 -1.93125) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 1.93125) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 0.64375) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 -0.64375) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 -1.93125) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 1.93125) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 0.64375) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 -0.64375) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 -1.93125) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 200 125 90)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U2 (at 0 -0.102 180) (layer F.SilkS))
    (fp_text value STM32F103C8T6 (at 0 6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 2 smd rect (at -4.35 -2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 SERVICE))
    (pad 3 smd rect (at -4.35 -1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 CE))
    (pad 4 smd rect (at -4.35 -1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C21-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C23-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 NRST))
    (pad 8 smd rect (at -4.35 0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 10 smd rect (at -4.35 1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -4.35 2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -4.35 2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 DISP_TXD))
    (pad 13 smd rect (at -2.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 DISP_RXD))
    (pad 14 smd rect (at -2.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 P25_LED))
    (pad 19 smd rect (at 0.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 YSF_LED))
    (pad 20 smd rect (at 0.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 21 smd rect (at 1.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 25 smd rect (at 4.35 2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 DSTAR_LED))
    (pad 26 smd rect (at 4.35 2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 DMR_LED))
    (pad 27 smd rect (at 4.35 1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 PTT_LED))
    (pad 28 smd rect (at 4.35 1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 COS_LED))
    (pad 29 smd rect (at 4.35 0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 66 NXDN_LED))
    (pad 30 smd rect (at 4.35 0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 TXD))
    (pad 31 smd rect (at 4.35 -0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 RXD))
    (pad 32 smd rect (at 4.35 -0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 33 smd rect (at 4.35 -1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 34 smd rect (at 4.35 -1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 37 smd rect (at 2.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 CLKOUT))
    (pad 39 smd rect (at 1.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 DATAIN))
    (pad 40 smd rect (at 1.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 DATAOUT))
    (pad 41 smd rect (at 0.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 SCLK))
    (pad 42 smd rect (at 0.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 SDATA))
    (pad 43 smd rect (at -0.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 SREAD))
    (pad 44 smd rect (at -0.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 SLE))
    (pad 46 smd rect (at -1.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 47 smd rect (at -2.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/LQFP-48_7x7mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_3225-4pin_3.2x2.5mm (layer F.Cu) (tedit 591D4BA2)
    (at 186.75 116 180)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference X1 (at 0 2.15 180) (layer F.SilkS))
    (fp_text value TCXO (at 0 2.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0.85 180) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 1.1 0.85 180) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 -0.85 180) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C18-Pad1)"))
    (pad 4 smd rect (at -1.1 -0.85 180) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (model ${KIPRJMOD}/libraries/crystal_xrcgb.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.7 1.7 1.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_Abracon_ABM3-2pin_5.0x3.2mm (layer F.Cu) (tedit 597859A6)
    (at 199.45 133)
    (descr "Abracon Miniature Ceramic Smd Crystal ABM3 http://www.abracon.com/Resonators/abm3.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 0.05 0) (layer F.SilkS))
    (fp_text value 8MHz (at 0 2.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.05 0) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C21-Pad2)"))
    (pad 2 smd rect (at 2.05 0) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C23-Pad2)"))
    (model ${KIPRJMOD}/libraries/crystal_smd_5x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 599458C2)
    (at 215.8 121 180)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D8 (at 1.6 0 180) (layer F.SilkS))
    (fp_text value red (at 0 1.4 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(D8-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 59785B83)
    (at 174.9 130)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0.4 -1 180) (layer F.SilkS))
    (fp_text value 3k8 (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5978596F)
    (at 175 119.8 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at -1.6 0.05 180) (layer F.SilkS))
    (fp_text value 3r9 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C11-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C8-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pizero:RPI-Zero-RASPBERRYPI_BASTELSTUBE_V13_RASPI_BOARD_B+_FULL (layer F.Cu) (tedit 599D922E)
    (at 155.4607 135.736941)
    (descr "RASPBERRY PI BOARD MODEL B+, FULL OUTLINE WITH POSITION OF BIG CONNECTORS & DRILL HOLES")
    (tags "RASPBERRY PI BOARD MODEL B+, FULL OUTLINE WITH POSITION OF BIG CONNECTORS & DRILL HOLES")
    (attr virtual)
    (fp_text reference PI1 (at 10.4393 -26.586941) (layer F.SilkS) hide)
    (fp_text value RPI-ZERO (at 13.3393 -26.586941) (layer F.SilkS) hide)
    (fp_text user 1 (at 8.5598 -22.88032) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 8.3693 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at 8.3693 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 46 +5V))
    (pad 3 thru_hole circle (at 10.9093 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 62 SDA))
    (pad 4 thru_hole circle (at 10.9093 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 46 +5V))
    (pad 5 thru_hole circle (at 13.4493 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 61 SCL))
    (pad 6 thru_hole circle (at 13.4493 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at 15.9893 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 15.9893 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 18 RXD))
    (pad 9 thru_hole circle (at 18.5293 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole circle (at 18.5293 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 17 TXD))
    (pad 11 thru_hole circle (at 21.0693 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 21.0693 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 23.6093 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 23.6093 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole circle (at 26.1493 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 26.1493 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 28.6893 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 18 thru_hole circle (at 28.6893 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 31.2293 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 31.2293 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole circle (at 33.7693 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at 33.7693 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 36.3093 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at 36.3093 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at 38.8493 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 26 thru_hole circle (at 38.8493 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 27 thru_hole circle (at 41.3893 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 28 thru_hole circle (at 41.3893 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 29 thru_hole circle (at 43.9293 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 30 thru_hole circle (at 43.9293 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 31 thru_hole circle (at 46.4693 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 32 thru_hole circle (at 46.4693 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 33 thru_hole circle (at 49.0093 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 34 thru_hole circle (at 49.0093 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 35 thru_hole circle (at 51.5493 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 36 thru_hole circle (at 51.5493 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 37 thru_hole circle (at 54.0893 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 38 thru_hole circle (at 54.0893 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 63 "Net-(PI1-Pad38)"))
    (pad 39 thru_hole circle (at 56.6293 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 40 thru_hole circle (at 56.6293 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 6 NRST))
    (pad "" np_thru_hole circle (at 3.49758 -3.49758) (size 2.74828 2.74828) (drill 2.74828) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.49758 -26.49982) (size 2.74828 2.74828) (drill 2.74828) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 61.49848 -3.49758) (size 2.74828 2.74828) (drill 2.74828) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 61.49848 -26.49982) (size 2.74828 2.74828) (drill 2.74828) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5A05753E)
    (at 210.42 124.4186 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value I2C (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 VDD))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 SDA))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5A05753B)
    (at 210.42 128 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value DISPLAY (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 +5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 DISP_RXD))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 DISP_TXD))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5A05716D)
    (at 205.6384 114.5032 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at -0.0032 11.1384 270) (layer F.SilkS) hide)
    (fp_text value STLINK (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 VDD))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 SWDIO))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 SWCLK))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module MMDVM:ANT1204 (layer F.Cu) (tedit 5A055CBF)
    (at 158.5 120.75 90)
    (fp_text reference AE1 (at 0 0 90) (layer F.SilkS))
    (fp_text value CERAMIC_ANTENNA (at 0 -1.016 90) (layer F.Fab))
    (pad 1 smd rect (at -5.85 0 90) (size 1.3 4.5) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(AE1-Pad1)"))
    (pad 2 smd rect (at 5.85 0 90) (size 1.3 4.5) (layers F.Cu F.Paste F.Mask))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A056861)
    (at 166 113)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C29 (at -1.75 0) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer F.Cu) (tedit 5A05683B)
    (at 170.5 115.25)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C30 (at 3.4 0 90) (layer F.SilkS))
    (fp_text value 10u/10V (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.375 0) (size 1.95 1.5) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 2 smd rect (at 1.375 0) (size 1.95 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A05688E)
    (at 166 116 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C31 (at 1.75 0 180) (layer F.SilkS))
    (fp_text value 10u (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0402 (layer F.Cu) (tedit 5A0567F4)
    (at 166 114.5)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference L5 (at -1.45 0) (layer F.SilkS))
    (fp_text value 10u (at 0 1.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A05607F)
    (at 166.5 125.75 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C27 (at -0.75 1.5 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C27-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 RF))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A056096)
    (at 164.75 123.6 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C28 (at 0 1 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 RF))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(AE1-Pad1)"))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 5A05690D)
    (at 175.75 127.75)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Symbols:KiCad-Logo_6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 158.8 120.7 270)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo_6mm_SilkScreen (at 0.75 0 270) (layer B.Fab) hide)
  )
  (module Symbols:OSHW-Logo_19x20mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 188 123.3 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_19x20mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Inductors_SMD:L_0402 (layer F.Cu) (tedit 5A9E991E)
    (at 167.15 123.6)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference L1 (at 0 -1.15) (layer F.SilkS))
    (fp_text value 22n (at 0 1.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 RF))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0402 (layer F.Cu) (tedit 5A9E992B)
    (at 170.3 123.6)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference L2 (at -0.35 -1.15) (layer F.SilkS))
    (fp_text value 20n (at 0 1.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0402 (layer F.Cu) (tedit 5ABBDA66)
    (at 172.6 122.35 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference L3 (at -1.6 0 180) (layer F.SilkS))
    (fp_text value 13n (at 0 1.8 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 64 VDD))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0402 (layer F.Cu) (tedit 5ABBDA76)
    (at 172.6 126.1)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference L4 (at 1.6 0) (layer F.SilkS))
    (fp_text value 27n (at 0 1.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducial:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 5A7CB119)
    (at 169.6 112.9)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference "" (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducial:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 5A7CB10B)
    (at 214.1 131.2)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference "" (at 1.3 6.7) (layer F.SilkS) hide)
    (fp_text value Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Inductors_SMD:L_0402 (layer F.Cu) (tedit 5A99B5DE)
    (at 179.1 120.2)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference L6 (at -1.3 0 90) (layer F.SilkS))
    (fp_text value 18n (at 0 1.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(L6-Pad2)"))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(L6-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MMDVM:MMDVM_logo (layer F.Cu) (tedit 0)
    (at 182.7 132.95)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text "14.7456 MHz" (at 169 124.5) (layer B.SilkS))
  (gr_text "12.2880 MHz" (at 169 122) (layer B.SilkS))
  (dimension 30.15 (width 0.3) (layer Dwgs.User)
    (gr_text "30,150 mm" (at 225.1 120.675 270) (layer Dwgs.User))
    (feature1 (pts (xy 217 135.75) (xy 226.45 135.75)))
    (feature2 (pts (xy 217 105.6) (xy 226.45 105.6)))
    (crossbar (pts (xy 223.75 105.6) (xy 223.75 135.75)))
    (arrow1a (pts (xy 223.75 135.75) (xy 223.163579 134.623496)))
    (arrow1b (pts (xy 223.75 135.75) (xy 224.336421 134.623496)))
    (arrow2a (pts (xy 223.75 105.6) (xy 223.163579 106.726504)))
    (arrow2b (pts (xy 223.75 105.6) (xy 224.336421 106.726504)))
  )
  (dimension 65.05 (width 0.3) (layer Dwgs.User)
    (gr_text "65,050 mm" (at 187.975 102.2) (layer Dwgs.User))
    (feature1 (pts (xy 220.5 109) (xy 220.5 100.85)))
    (feature2 (pts (xy 155.45 109) (xy 155.45 100.85)))
    (crossbar (pts (xy 155.45 103.55) (xy 220.5 103.55)))
    (arrow1a (pts (xy 220.5 103.55) (xy 219.373496 104.136421)))
    (arrow1b (pts (xy 220.5 103.55) (xy 219.373496 102.963579)))
    (arrow2a (pts (xy 155.45 103.55) (xy 156.576504 104.136421)))
    (arrow2b (pts (xy 155.45 103.55) (xy 156.576504 102.963579)))
  )
  (target plus (at 169.6 112.9) (size 5) (width 0.15) (layer Edge.Cuts))
  (gr_text NXDN (at 216.35 122.2) (layer F.SilkS))
  (gr_text 3v3 (at 205.6384 116.6876) (layer F.SilkS))
  (gr_text DIO (at 203.0984 116.6876) (layer F.SilkS))
  (gr_text CLK (at 200.5584 116.6876) (layer F.SilkS))
  (gr_text GND (at 198.0184 116.6876) (layer F.SilkS))
  (gr_text STlink (at 195.834 114.4524 90) (layer F.SilkS))
  (gr_text OLED (at 208.25 124.4 90) (layer F.SilkS))
  (gr_text SDA (at 218.0336 126.25) (layer F.SilkS))
  (gr_text SCL (at 215.4936 126.25) (layer F.SilkS))
  (gr_text GND (at 212.9536 126.25) (layer F.SilkS))
  (gr_text 3v3 (at 210.5 126.25) (layer F.SilkS))
  (gr_text GND (at 218.075 129.75) (layer F.SilkS))
  (gr_text TXD (at 215.5 129.75) (layer F.SilkS))
  (gr_text RXD (at 212.975 129.75) (layer F.SilkS))
  (gr_text 5v0 (at 210.425 129.75) (layer F.SilkS))
  (gr_text SVC (at 218.5 113.8) (layer F.SilkS))
  (gr_line (start 158.4 105.6) (end 217.5 105.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 220.5 108.6) (end 220.5 132.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 217.55 135.75) (end 158.3 135.75) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.45 132.9) (end 155.45 108.55) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 217.5 108.6) (end 217.5 105.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 217.55 132.8) (end 220.5 132.9) (angle 88.05851361) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 158.3 132.9) (end 158.3 135.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 158.4 108.55) (end 155.45 108.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "DB9MAT DF2ET\nrev1.6 \n(c) 06/2018" (at 163.45 119.45) (layer F.SilkS))
  (gr_text MMDVM_HS_Hat (at 172.8 112.8) (layer F.SilkS))
  (gr_text Reset (at 210.65 131.35) (layer F.SilkS))
  (gr_text Nextion (at 208.25 128 90) (layer F.SilkS))
  (gr_text YSF (at 215.775 119.85) (layer F.SilkS))
  (gr_text P25 (at 218.4 121) (layer F.SilkS))
  (gr_text DMR (at 218.5 118.7) (layer F.SilkS))
  (gr_text D* (at 215.9 117.45) (layer F.SilkS))
  (gr_text PTT (at 218.4 116.2) (layer F.SilkS))
  (gr_text COS (at 215.775 115.025) (layer F.SilkS))
  (gr_text PWR (at 216 112.7) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.25 105.65) (xy 220.6 105.65) (xy 220.6 135.95) (xy 155.25 135.9)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.25 105.65) (xy 220.6 105.65) (xy 220.6 135.95) (xy 155.25 135.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.2 135.9) (xy 155.2 105.6) (xy 162.6 105.6) (xy 162.6 136) (xy 155.2 136)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.2 135.9) (xy 155.2 105.6) (xy 162.6 105.6) (xy 162.6 136) (xy 155.2 136)
      )
    )
  )
)
