(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 53)
    (tracks 409)
    (zones 0)
    (modules 39)
    (nets 34)
  )
  (page USLetter)
  (title_block
    (title "800 MHz Differential Active Probe")
    (date 2019-10-19)
    (rev 0.1b)
    (company TWMIV)
  )
  (layers
    (0 F.Cu mixed)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu mixed)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.127)
    (user_trace_width 0.25)
    (user_trace_width 0.35)
    (user_trace_width 0.393)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.175)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.127)
    (mod_text_size 0.508 0.508)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.101)
    (aux_axis_origin 0 0)
    (grid_origin 200 100)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C3-Pad2)")
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 "Net-(C5-Pad1)")
  (net 6 "Net-(C6-Pad1)")
  (net 7 VCC)
  (net 8 VSS)
  (net 9 "Net-(R1-Pad1)")
  (net 10 "Net-(R2-Pad1)")
  (net 11 "Net-(R4-Pad1)")
  (net 12 "Net-(R8-Pad1)")
  (net 13 "Net-(R9-Pad1)")
  (net 14 "Net-(R10-Pad1)")
  (net 15 "Net-(R11-Pad2)")
  (net 16 "Net-(R13-Pad1)")
  (net 17 "Net-(U2-Pad7)")
  (net 18 "Net-(U2-Pad9)")
  (net 19 "Net-(U2-Pad11)")
  (net 20 /o-)
  (net 21 /o+)
  (net 22 "Net-(J1-Pad2)")
  (net 23 "Net-(J1-Pad3)")
  (net 24 "Net-(J1-Pad4)")
  (net 25 /o_3)
  (net 26 /o_2)
  (net 27 /o_1)
  (net 28 /vin)
  (net 29 /in+)
  (net 30 /fb1)
  (net 31 /fb2)
  (net 32 /+5v)
  (net 33 /in-)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+5v)
    (add_net /fb1)
    (add_net /fb2)
    (add_net /in+)
    (add_net /in-)
    (add_net /o+)
    (add_net /o-)
    (add_net /vin)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad9)")
    (add_net VCC)
    (add_net VSS)
  )
  (net_class gnd ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class t-line ""
    (clearance 0.2)
    (trace_width 0.349748)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /o_1)
    (add_net /o_2)
    (add_net /o_3)
  )
  (module swiss_pin:conn_01x02_swiss_female_smd (layer F.Cu) (tedit 5DABDE49)
    (at 179 112.5 90)
    (attr smd)
    (fp_text reference J3 (at 3 2.25) (layer F.SilkS))
    (fp_text value "Probe Tip" (at 0 -1.2267 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.27 2.2733 90) (size 0.6 4) (layers F.Cu F.Paste F.Mask)
      (net 33 /in-))
    (pad 2 smd rect (at 1.27 2.2733 90) (size 0.6 4) (layers F.Cu F.Paste F.Mask)
      (net 29 /in+))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (offset (xyz 1.27 0 0.3))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 90))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 188.0296 111.1106)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -0.2796 2.1394) (layer F.SilkS))
    (fp_text value 357 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /fb1))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_CSP:LFCSP-24-1EP_4x4mm_P0.5mm_EP2.5x2.5mm_ThermalVias (layer F.Cu) (tedit 5C33D023)
    (at 189.0837 107.5546 90)
    (descr "LFCSP, 24 Pin (https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/lfcspcp/cp_24_7.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "LFCSP DFN_QFN")
    (attr smd)
    (fp_text reference U2 (at -1.6954 3.1663 180) (layer F.SilkS))
    (fp_text value AD8003 (at 0 3.32 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 25 smd roundrect (at 0 0 90) (size 2.5 2.5) (layers F.Cu F.Mask) (roundrect_rratio 0.1)
      (net 1 GND))
    (pad 25 thru_hole circle (at -1 -1 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 0 -1 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 1 -1 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at -1 0 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 1 0 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at -1 1 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 0 1 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 1 1 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 smd roundrect (at 0 0 90) (size 2.5 2.5) (layers B.Cu) (roundrect_rratio 0.1)
      (net 1 GND))
    (pad "" smd roundrect (at -0.625 -0.625 90) (size 1.08 1.08) (layers F.Paste) (roundrect_rratio 0.231481))
    (pad "" smd roundrect (at -0.625 0.625 90) (size 1.08 1.08) (layers F.Paste) (roundrect_rratio 0.231481))
    (pad "" smd roundrect (at 0.625 -0.625 90) (size 1.08 1.08) (layers F.Paste) (roundrect_rratio 0.231481))
    (pad "" smd roundrect (at 0.625 0.625 90) (size 1.08 1.08) (layers F.Paste) (roundrect_rratio 0.231481))
    (pad 1 smd roundrect (at -1.9375 -1.25 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 VCC))
    (pad 2 smd roundrect (at -1.9375 -0.75 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(R8-Pad1)"))
    (pad 3 smd roundrect (at -1.9375 -0.25 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /fb1))
    (pad 4 smd roundrect (at -1.9375 0.25 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C5-Pad1)"))
    (pad 5 smd roundrect (at -1.9375 0.75 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 VCC))
    (pad 6 smd roundrect (at -1.9375 1.25 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 VSS))
    (pad 7 smd roundrect (at -1.25 1.9375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(U2-Pad7)"))
    (pad 8 smd roundrect (at -0.75 1.9375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /o-))
    (pad 9 smd roundrect (at -0.25 1.9375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(U2-Pad9)"))
    (pad 10 smd roundrect (at 0.25 1.9375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /o+))
    (pad 11 smd roundrect (at 0.75 1.9375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(U2-Pad11)"))
    (pad 12 smd roundrect (at 1.25 1.9375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /o_1))
    (pad 13 smd roundrect (at 1.9375 1.25 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 VSS))
    (pad 14 smd roundrect (at 1.9375 0.75 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 VCC))
    (pad 15 smd roundrect (at 1.9375 0.25 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(R11-Pad2)"))
    (pad 16 smd roundrect (at 1.9375 -0.25 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(R10-Pad1)"))
    (pad 17 smd roundrect (at 1.9375 -0.75 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(R13-Pad1)"))
    (pad 18 smd roundrect (at 1.9375 -1.25 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 VCC))
    (pad 19 smd roundrect (at 1.25 -1.9375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 VCC))
    (pad 20 smd roundrect (at 0.75 -1.9375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(R9-Pad1)"))
    (pad 21 smd roundrect (at 0.25 -1.9375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /fb2))
    (pad 22 smd roundrect (at -0.25 -1.9375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C6-Pad1)"))
    (pad 23 smd roundrect (at -0.75 -1.9375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 VCC))
    (pad 24 smd roundrect (at -1.25 -1.9375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 VSS))
    (model ${KISYS3DMOD}/Package_CSP.3dshapes/LFCSP-24-1EP_4x4mm_P0.5mm_EP2.5x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-24_4x4mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 190.8 120.066 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB1 (at 2.066 -0.05 180) (layer F.SilkS))
    (fp_text value Ferrite_Bead (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /vin))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /+5v))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:SMA_Samtec_SMA-J-P-H-ST-EM1_EdgeMount (layer F.Cu) (tedit 5BA382C0)
    (at 197.8914 106.299)
    (descr http://suddendocs.samtec.com/prints/sma-j-p-x-st-em1-mkt.pdf)
    (tags SMA)
    (attr smd)
    (fp_text reference J2 (at -0.1414 -4.799 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 5 5.9) (layer F.Fab) hide)
    (fp_text user %R (at 4.79 0 270) (layer F.Fab) hide)
    (fp_text user "PCB Edge" (at 2.6 0 90) (layer Dwgs.User) hide)
    (pad 2 smd rect (at 0 2.825 90) (size 1.35 4.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -2.825 90) (size 1.35 4.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 2.825 90) (size 1.35 4.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -2.825 90) (size 1.35 4.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.2 0 90) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /o_3))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Samtec_SMA-J-P-H-ST-EM1_EdgeMount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/SMA-J-P-H-ST-EM1.STP--3DModel-STEP-66336.STEP
      (offset (xyz 4 0 0.55))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 90))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 186.2533 122.4304 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -0.0967 -0.9196) (layer F.SilkS))
    (fp_text value 10K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(R1-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /vin))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 182.2147 123.3194 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -0.0306 -1.1147 180) (layer F.SilkS))
    (fp_text value 1.4Meg (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 VCC))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 183.3577 123.3194 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -0.9923 180) (layer F.SilkS))
    (fp_text value 499K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 184.7547 117.2234)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -1.4047 -0.1234) (layer F.SilkS))
    (fp_text value 499K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(R4-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 184.2467 115.6994 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0.3006 1.0467 180) (layer F.SilkS))
    (fp_text value 1.37Meg (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(R4-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 VSS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 190.0616 111.1106 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -0.6884 -0.8894) (layer F.SilkS))
    (fp_text value 100k (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 185.5277 108.5706 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -0.4294 -1.17 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C6-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 185.5277 106.5386 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at -0.2886 1.0277 180) (layer F.SilkS))
    (fp_text value 357 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(R9-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /fb2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 188.4487 102.4746 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 1.1746 -0.0487 180) (layer F.SilkS))
    (fp_text value 3k (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /o-))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 189.7187 102.4746 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at -1.1746 -0.2813 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(R11-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /o+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 190.0997 103.9986)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0.6503 -1.2486 90) (layer F.SilkS))
    (fp_text value 357 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(R11-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 188.0677 103.9986)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at -0.5677 -1.2486 90) (layer F.SilkS))
    (fp_text value 357 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(R10-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(R13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 192.9 106.3)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 0 1.3) (layer F.SilkS))
    (fp_text value 49.9 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /o_2))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /o_1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SON:WSON-12-1EP_3x2mm_P0.5mm_EP1x2.65_ThermalVias (layer F.Cu) (tedit 5A65F4F1)
    (at 185.7707 119.7634 180)
    (descr "WSON-12 http://www.ti.com/lit/ds/symlink/lm27762.pdf")
    (tags WSON-12)
    (attr smd)
    (fp_text reference U1 (at 2.4207 1.9134) (layer F.SilkS))
    (fp_text value LM27762 (at 0 2.921) (layer F.Fab))
    (fp_text user %R (at 0 -0.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 -1.25 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at -0.95 -0.75 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R2-Pad1)"))
    (pad 3 smd rect (at -0.95 -0.25 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /vin))
    (pad 4 smd rect (at -0.95 0.25 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -0.95 0.75 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 6 smd rect (at -0.95 1.25 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 VSS))
    (pad 7 smd rect (at 0.95 1.25 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R4-Pad1)"))
    (pad 8 smd rect (at 0.95 0.75 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /vin))
    (pad 9 smd rect (at 0.95 0.25 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C3-Pad2)"))
    (pad 10 smd rect (at 0.95 -0.25 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 11 smd rect (at 0.95 -0.75 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 12 smd rect (at 0.95 -1.25 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /vin))
    (pad 13 thru_hole circle (at 0 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 13 thru_hole circle (at 0 -1 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 13 thru_hole circle (at 0 1 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 13 smd rect (at 0 0 180) (size 1 2.65) (layers B.Cu)
      (net 1 GND))
    (pad 13 smd rect (at 0 0 180) (size 1 2.65) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad "" smd rect (at 0 -0.5 180) (size 0.95 0.8) (layers F.Paste))
    (pad "" smd rect (at 0 0.5 180) (size 0.95 0.8) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/WSON-12-1EP_3x2mm_P0.5mm_EP1x2.65.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Package_SON.3dshapes/Texas_R-PWSON-N12_EP0.4x2mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 188.3107 120.5254 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -1.3246 0.0393 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /vin))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 189.579 112.6346 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0.1154 -1.17 180) (layer F.SilkS))
    (fp_text value 2.2p (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /in-))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 184.0037 108.0626 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 0.8126) (layer F.SilkS))
    (fp_text value 2.2p (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /in+))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 186.5056 111.6186 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -0.3814 -1.0056 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 VCC))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 185.0197 105.0146)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 -1.0146) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 183.3577 121.2874 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0.8126 -1.2423 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 VCC))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 186.774 117.2234)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0.076 -1.8734) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 VSS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 192.6143 110.6788 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at -0.0712 1.3857 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 VSS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 185.0197 110.0946)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at -0.2697 0.9054) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 VSS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 186.5437 103.4906 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -1.2406 0.2937 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 VCC))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 191.95 103.55 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0 -1.3 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 VSS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 195.072 106.299 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at -0.028 -1.301) (layer F.SilkS))
    (fp_text value 3p (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /o_2))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /o_3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 189.3648 120.5254 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 1.4254 -0.0148 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /vin))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 183.3577 119.2554 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -0.0946 -1.0077 180) (layer F.SilkS))
    (fp_text value 1u (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 182.2147 121.2874 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0.0626 1.1147 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 186.774 116.1566)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at -0.174 -1.5566) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 VSS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_Micro-B_Amphenol_10103594-0001LF_Horizontal (layer F.Cu) (tedit 5A1DC0BD)
    (at 197.1675 119.9642 90)
    (descr "Micro USB Type B 10103594-0001LF, http://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10103594.pdf")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference J1 (at 4.7142 0.8325 180) (layer F.SilkS))
    (fp_text value USB_B_Micro (at -0.025 4.435 90) (layer F.Fab) hide)
    (fp_text user "PCB edge" (at -0.025 2.235 90) (layer Dwgs.User) hide)
    (fp_text user %R (at -0.025 -0.015 90) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.725 0.185 90) (size 1.35 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.755 0.185 90) (size 1.35 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.975 -0.565 90) (size 1.825 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.975 -0.565 90) (size 1.825 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.875 -1.865 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.875 -1.885 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.325 -1.765 180) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 32 /+5v))
    (pad 2 smd rect (at -0.675 -1.765 180) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at -0.025 -1.765 180) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at 0.625 -1.765 180) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 1.275 -1.765 180) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -2.445 -1.885 180) (size 1.5 1.1) (drill oval 1.05 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.395 -1.885 180) (size 1.5 1.1) (drill oval 1.05 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -2.755 1.115 180) (size 1.7 1.35) (drill oval 1.2 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.705 1.115 180) (size 1.7 1.35) (drill oval 1.2 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -0.985 1.385 180) (size 2.5 1.43) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.935 1.385 180) (size 2.5 1.43) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Amphenol_10103594-0001LF_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/10103594-0001LF--3DModel-STEP-56544.STEP
      (offset (xyz 0 0.2 -0.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 193 120.2 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J5 (at 0 4.95) (layer F.SilkS))
    (fp_text value VIN (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /+5v))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 188.0296 112.2536 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 0.0296 -1.7464) (layer F.SilkS))
    (fp_text value 10k (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /fb1))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /fb2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 188.8 117.8 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -0.9 -1.5 180) (layer F.SilkS))
    (fp_text value 10u (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 4 (at 181.9 101.6) (layer B.Cu))
  (gr_text 3 (at 181.4 101.6) (layer In2.Cu))
  (gr_text 2 (at 180.9 101.6) (layer In1.Cu))
  (gr_text 1 (at 180.4 101.6) (layer F.Cu))
  (gr_text + (at 192.2 121.6) (layer F.SilkS))
  (gr_text V0.1b (at 192.25 115.25) (layer B.SilkS))
  (gr_text "TWMIV\n2019" (at 196.5 113.5) (layer B.SilkS))
  (dimension 11.2 (width 0.15) (layer Dwgs.User)
    (gr_text "11.200 mm" (at 172.8 119.4 270) (layer Dwgs.User))
    (feature1 (pts (xy 179 125) (xy 173.513579 125)))
    (feature2 (pts (xy 179 113.8) (xy 173.513579 113.8)))
    (crossbar (pts (xy 174.1 113.8) (xy 174.1 125)))
    (arrow1a (pts (xy 174.1 125) (xy 173.513579 123.873496)))
    (arrow1b (pts (xy 174.1 125) (xy 174.686421 123.873496)))
    (arrow2a (pts (xy 174.1 113.8) (xy 173.513579 114.926504)))
    (arrow2b (pts (xy 174.1 113.8) (xy 174.686421 114.926504)))
  )
  (dimension 12.5 (width 0.15) (layer Dwgs.User)
    (gr_text "12.500 mm" (at 172.8 106.25 90) (layer Dwgs.User))
    (feature1 (pts (xy 179 100) (xy 173.513579 100)))
    (feature2 (pts (xy 179 112.5) (xy 173.513579 112.5)))
    (crossbar (pts (xy 174.1 112.5) (xy 174.1 100)))
    (arrow1a (pts (xy 174.1 100) (xy 174.686421 101.126504)))
    (arrow1b (pts (xy 174.1 100) (xy 173.513579 101.126504)))
    (arrow2a (pts (xy 174.1 112.5) (xy 174.686421 111.373496)))
    (arrow2b (pts (xy 174.1 112.5) (xy 173.513579 111.373496)))
  )
  (dimension 2 (width 0.15) (layer Dwgs.User)
    (gr_text "2.000 mm" (at 189 130.7) (layer Dwgs.User))
    (feature1 (pts (xy 190 125) (xy 190 129.986421)))
    (feature2 (pts (xy 188 125) (xy 188 129.986421)))
    (crossbar (pts (xy 188 129.4) (xy 190 129.4)))
    (arrow1a (pts (xy 190 129.4) (xy 188.873496 129.986421)))
    (arrow1b (pts (xy 190 129.4) (xy 188.873496 128.813579)))
    (arrow2a (pts (xy 188 129.4) (xy 189.126504 129.986421)))
    (arrow2b (pts (xy 188 129.4) (xy 189.126504 128.813579)))
  )
  (dimension 10 (width 0.15) (layer Dwgs.User)
    (gr_text "10.000 mm" (at 195 128.1) (layer Dwgs.User))
    (feature1 (pts (xy 200 125) (xy 200 127.386421)))
    (feature2 (pts (xy 190 125) (xy 190 127.386421)))
    (crossbar (pts (xy 190 126.8) (xy 200 126.8)))
    (arrow1a (pts (xy 200 126.8) (xy 198.873496 127.386421)))
    (arrow1b (pts (xy 200 126.8) (xy 198.873496 126.213579)))
    (arrow2a (pts (xy 190 126.8) (xy 191.126504 127.386421)))
    (arrow2b (pts (xy 190 126.8) (xy 191.126504 126.213579)))
  )
  (dimension 2 (width 0.15) (layer Dwgs.User)
    (gr_text "2.000 mm" (at 192 97.9) (layer Dwgs.User))
    (feature1 (pts (xy 193 100) (xy 193 98.613579)))
    (feature2 (pts (xy 191 100) (xy 191 98.613579)))
    (crossbar (pts (xy 191 99.2) (xy 193 99.2)))
    (arrow1a (pts (xy 193 99.2) (xy 191.873496 99.786421)))
    (arrow1b (pts (xy 193 99.2) (xy 191.873496 98.613579)))
    (arrow2a (pts (xy 191 99.2) (xy 192.126504 99.786421)))
    (arrow2b (pts (xy 191 99.2) (xy 192.126504 98.613579)))
  )
  (dimension 7 (width 0.15) (layer Dwgs.User)
    (gr_text "7.000 mm" (at 196.5 95.4) (layer Dwgs.User))
    (feature1 (pts (xy 193 100) (xy 193 96.113579)))
    (feature2 (pts (xy 200 100) (xy 200 96.113579)))
    (crossbar (pts (xy 200 96.7) (xy 193 96.7)))
    (arrow1a (pts (xy 193 96.7) (xy 194.126504 96.113579)))
    (arrow1b (pts (xy 193 96.7) (xy 194.126504 97.286421)))
    (arrow2a (pts (xy 200 96.7) (xy 198.873496 96.113579)))
    (arrow2b (pts (xy 200 96.7) (xy 198.873496 97.286421)))
  )
  (dimension 25 (width 0.15) (layer Dwgs.User)
    (gr_text "25.000 mm" (at 213.9 112.5 90) (layer Dwgs.User))
    (feature1 (pts (xy 200 100) (xy 213.186421 100)))
    (feature2 (pts (xy 200 125) (xy 213.186421 125)))
    (crossbar (pts (xy 212.6 125) (xy 212.6 100)))
    (arrow1a (pts (xy 212.6 100) (xy 213.186421 101.126504)))
    (arrow1b (pts (xy 212.6 100) (xy 212.013579 101.126504)))
    (arrow2a (pts (xy 212.6 125) (xy 213.186421 123.873496)))
    (arrow2b (pts (xy 212.6 125) (xy 212.013579 123.873496)))
  )
  (dimension 21 (width 0.15) (layer Dwgs.User)
    (gr_text "21.000 mm" (at 189.5 135.1) (layer Dwgs.User))
    (feature1 (pts (xy 200 125) (xy 200 134.386421)))
    (feature2 (pts (xy 179 125) (xy 179 134.386421)))
    (crossbar (pts (xy 179 133.8) (xy 200 133.8)))
    (arrow1a (pts (xy 200 133.8) (xy 198.873496 134.386421)))
    (arrow1b (pts (xy 200 133.8) (xy 198.873496 133.213579)))
    (arrow2a (pts (xy 179 133.8) (xy 180.126504 134.386421)))
    (arrow2b (pts (xy 179 133.8) (xy 180.126504 133.213579)))
  )
  (gr_line (start 179 125) (end 180 125) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 179 115) (end 179 125) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 179 100) (end 180 100) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 179 106) (end 179 100) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 179 110) (end 179 106) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 181 100) (end 180 100) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 181 125) (end 180 125) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 179 115) (end 179 110) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 191 100) (end 181 100) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 188 125) (end 181 125) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 195 100) (end 200 100) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 190 125) (end 192 125) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 191 100) (end 191 100) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 193 100) (end 191 100) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 200 125) (end 192 125) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 200 100) (end 200 125) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200 125) (xy 200 100) (xy 179 100) (xy 179 125)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu In1.Cu In2.Cu B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186 107) (xy 187.7 107) (xy 187.7 108.1) (xy 186.1 108.1) (xy 186.1 108.6)
        (xy 183.9 108.6) (xy 183.9 113.4) (xy 189 113.4) (xy 189 111) (xy 189.1 111)
        (xy 189.1 109) (xy 189.6 109) (xy 189.6 110.6) (xy 190 110.6) (xy 190 114)
        (xy 183.5 114) (xy 183.5 114.75) (xy 179 114.75) (xy 179 110.5) (xy 183.2 110.5)
        (xy 183.2 108.7) (xy 182.9 108.7) (xy 182.9 107.4) (xy 185 107.4) (xy 185 106.6)
        (xy 186 106.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 190.5 108) (xy 190.5 108.5) (xy 192.3 108.5) (xy 192.3 107.1) (xy 190.5 107.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu In1.Cu In2.Cu B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 189.05 106.15) (xy 188.1 106.15) (xy 188.1 105) (xy 187.7 104.55) (xy 187.2 104.55)
        (xy 187.2 103.55) (xy 189 103.55) (xy 189.05 103.55)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200 125) (xy 200 100) (xy 179 100) (xy 179 125)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 190.35 107.15) (xy 194.1 107.15) (xy 196.6 107.15) (xy 200.05 107.15) (xy 200 105.45)
        (xy 190.35 105.45)
      )
    )
  )
  (zone (net 7) (net_name VCC) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200 125) (xy 200 100) (xy 179 100) (xy 179 125)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.175))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200 125) (xy 200 100) (xy 179 100) (xy 179 125)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu In1.Cu In2.Cu B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.1 101.15) (xy 182.15 101.15) (xy 182.15 102) (xy 180.1 102)
      )
    )
  )
)
