(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 13)
    (no_connects 0)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 21)
    (tracks 39)
    (zones 0)
    (modules 3)
    (nets 14)
  )
  (page USLetter)
  (title_block
    (title "RJ45 Magjack Breakout")
    (date 2018-04-24)
    (rev 1.0)
    (company "Patrick Pelletier")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1524)
    (trace_clearance 0.2)
    (zone_clearance 0.3048)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEF77F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J2-PadR3)")
  (net 8 "Net-(J2-PadR5)")
  (net 9 "Net-(J2-PadR6)")
  (net 10 "Net-(J2-PadR7)")
  (net 11 GND)
  (net 12 "Net-(J2-PadL1)")
  (net 13 "Net-(J2-PadL2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J2-PadL1)")
    (add_net "Net-(J2-PadL2)")
    (add_net "Net-(J2-PadR6)")
    (add_net "Net-(J2-PadR7)")
  )
  (net_class Skinny ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J2-PadR3)")
    (add_net "Net-(J2-PadR5)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5ADFDC51)
    (at 132.08 77.47)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x06 (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myLibrary:RJ45_Amphenol_RJMG1BD3B8K1ANR (layer F.Cu) (tedit 5ADFDC66)
    (at 133.985 97.155)
    (descr "1 Port RJ45 Magjack Connector Through Hole 10/100 Base-T, AutoMDIX, https://www.amphenolcanada.com/ProductSearch/Drawings/AC/RJMG1BD3B8K1ANR.PDF")
    (tags "RJ45 Magjack")
    (fp_text reference J2 (at 4.445 -5.49) (layer F.SilkS) hide)
    (fp_text value RJ45_Amphenol_RJMG1BD3B8K1ANR (at 4.445 18.23) (layer F.Fab))
    (fp_text user %R (at 4.445 6.37) (layer F.Fab))
    (pad R1 thru_hole rect (at 0 0) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad R2 thru_hole circle (at 1.27 -2.54) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad R3 thru_hole circle (at 2.54 0) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-PadR3)"))
    (pad R4 thru_hole circle (at 3.81 -2.54) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad R5 thru_hole circle (at 5.08 0) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-PadR5)"))
    (pad R6 thru_hole circle (at 6.35 -2.54) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-PadR6)"))
    (pad R7 thru_hole circle (at 7.62 0) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-PadR7)"))
    (pad R8 thru_hole circle (at 8.89 -2.54) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad L1 thru_hole circle (at 10.77 9.72) (size 1.89 1.89) (drill 0.89) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-PadL1)"))
    (pad L2 thru_hole circle (at 8.23 11.24) (size 1.89 1.89) (drill 0.89) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-PadL2)"))
    (pad L3 thru_hole circle (at 0.66 9.72) (size 1.89 1.89) (drill 0.89) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad L4 thru_hole circle (at -1.88 11.24) (size 1.89 1.89) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 13 thru_hole circle (at -3.33 3.29) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 13 thru_hole circle (at 12.22 3.29) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad "" np_thru_hole circle (at -1.27 6.34) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 10.16 6.34) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_RJ.3dshapes/RJ45_Amphenol_RJMG1BD3B8K1ANR.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5ADFDC60)
    (at 144.78 77.47)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x06 (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-PadR3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-PadR5)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-PadR6)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-PadL1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-PadL2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "RJ45\nMagjack\nBreakout\n2018-04-24\nPatrick\nPelletier" (at 138.43 83.82) (layer B.SilkS))
  (gr_text Y_K (at 142.875 90.17) (layer F.SilkS))
  (gr_text Y_A (at 142.875 87.63) (layer F.SilkS))
  (gr_text GND (at 142.875 85.09) (layer F.SilkS))
  (gr_text RD- (at 142.875 82.55) (layer F.SilkS))
  (gr_text RCT (at 142.875 80.01) (layer F.SilkS))
  (gr_text RD+ (at 142.875 77.47) (layer F.SilkS))
  (gr_text G_K (at 133.985 90.17) (layer F.SilkS))
  (gr_text G_A (at 133.985 87.63) (layer F.SilkS))
  (gr_text SHLD (at 133.985 85.09) (layer F.SilkS))
  (gr_text TD- (at 133.985 82.55) (layer F.SilkS))
  (gr_text TCT (at 133.985 80.01) (layer F.SilkS))
  (gr_text TD+ (at 133.985 77.47) (layer F.SilkS))
  (gr_line (start 128.905 92.075) (end 128.905 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.175 92.075) (end 128.905 92.075) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.175 75.565) (end 130.175 92.075) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.685 75.565) (end 130.175 75.565) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.685 92.075) (end 146.685 75.565) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.955 92.075) (end 146.685 92.075) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.955 110.49) (end 147.955 92.075) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.905 110.49) (end 147.955 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name "Net-(J1-Pad4)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.685 92.075) (xy 147.955 92.075) (xy 147.955 110.49) (xy 128.905 110.49) (xy 128.905 92.075)
        (xy 130.175 92.075) (xy 130.175 75.565) (xy 146.685 75.565)
      )
    )
  )
  (zone (net 11) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.685 92.075) (xy 147.955 92.075) (xy 147.955 110.49) (xy 128.905 110.49) (xy 128.905 92.075)
        (xy 130.175 92.075) (xy 130.175 75.565) (xy 146.685 75.565)
      )
    )
  )
)
