(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 15)
    (no_connects 1)
    (area 95.824999 88.274999 133.425001 135.225001)
    (thickness 1.6)
    (drawings 26)
    (tracks 19)
    (zones 0)
    (modules 2)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 RED)
  (net 3 R_AUD)
  (net 4 SYNC)
  (net 5 GREEN)
  (net 6 L_AUD)
  (net 7 BLUE)
  (net 8 "Net-(SCART1-Pad16)")
  (net 9 "Net-(SCART1-Pad14)")
  (net 10 "Net-(SCART1-Pad8)")
  (net 11 "Net-(SCART1-Pad10)")
  (net 12 "Net-(SCART1-Pad12)")
  (net 13 "Net-(SCART1-Pad1)")
  (net 14 "Net-(SCART1-Pad3)")
  (net 15 "Net-(SCART1-Pad19)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net BLUE)
    (add_net GND)
    (add_net GREEN)
    (add_net L_AUD)
    (add_net "Net-(SCART1-Pad1)")
    (add_net "Net-(SCART1-Pad10)")
    (add_net "Net-(SCART1-Pad12)")
    (add_net "Net-(SCART1-Pad14)")
    (add_net "Net-(SCART1-Pad16)")
    (add_net "Net-(SCART1-Pad19)")
    (add_net "Net-(SCART1-Pad3)")
    (add_net "Net-(SCART1-Pad8)")
    (add_net RED)
    (add_net R_AUD)
    (add_net SYNC)
  )
  (module SCARTConnectors:3x2_RCA (layer F.Cu) (tedit 5B0A1A4D)
    (at 133.35 111.76 90)
    (fp_text reference RCA1 (at -11.43 -8.89 90) (layer F.SilkS))
    (fp_text value 3x2_RCA (at 10.16 -7.62 90) (layer F.Fab))
    (pad 9 thru_hole circle (at 17.75 -5.25 90) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 3.75 -5.25 90) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at -10.25 -5.25 90) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 17.75 -12.5 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 RED))
    (pad 5 thru_hole circle (at 10.25 -12.5 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 R_AUD))
    (pad 1 thru_hole circle (at -17.75 -12.5 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 SYNC))
    (pad 2 thru_hole circle (at -10.25 -12.5 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GREEN))
    (pad 3 thru_hole circle (at -3.75 -12.5 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 L_AUD))
    (pad 4 thru_hole circle (at 3.75 -12.5 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 BLUE))
  )
  (module SCARTConnectors:SCART_F (layer F.Cu) (tedit 5B0A1858)
    (at 104.14 111.76 270)
    (fp_text reference SCART1 (at 0 6 270) (layer F.SilkS))
    (fp_text value SCART-F (at 0 -6.25 270) (layer F.Fab))
    (pad 20 thru_hole circle (at -17.155 -2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 SYNC))
    (pad 18 thru_hole circle (at -13.345 -2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole circle (at -9.535 -2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(SCART1-Pad16)"))
    (pad 14 thru_hole circle (at -5.725 -2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 9 "Net-(SCART1-Pad14)"))
    (pad 2 thru_hole circle (at 17.135 -2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 R_AUD))
    (pad 4 thru_hole circle (at 13.325 -2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 9.515 -2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 L_AUD))
    (pad 8 thru_hole circle (at 5.705 -2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 "Net-(SCART1-Pad8)"))
    (pad 10 thru_hole circle (at 1.895 -2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(SCART1-Pad10)"))
    (pad 12 thru_hole circle (at -1.915 -2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 "Net-(SCART1-Pad12)"))
    (pad 1 thru_hole circle (at 19.05 2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 13 "Net-(SCART1-Pad1)"))
    (pad 3 thru_hole circle (at 15.24 2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 "Net-(SCART1-Pad3)"))
    (pad 5 thru_hole circle (at 11.43 2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at 7.62 2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 BLUE))
    (pad 9 thru_hole circle (at 3.81 2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole circle (at -19.05 2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole circle (at -15.24 2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 15 "Net-(SCART1-Pad19)"))
    (pad 17 thru_hole circle (at -11.43 2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole circle (at -7.62 2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 RED))
    (pad 13 thru_hole circle (at -3.81 2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole circle (at 0 2.54 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GREEN))
  )
  (gr_line (start 101.75 88.35) (end 95.9 88.35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.75 90.35) (end 101.75 88.35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.35 92.15) (end 133.35 90.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.9 135.15) (end 95.9 88.35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.75 135.15) (end 95.9 135.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.55 90.35) (end 101.75 90.35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.55 88.35) (end 106.55 90.35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.85 90.75) (end 123.1 90.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.8 90.75) (end 118.85 90.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.4 88.35) (end 118.8 90.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.55 88.35) (end 116.4 88.35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.1 90.75) (end 133.35 90.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.1 92.45) (end 126.1 90.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.1 92.45) (end 123.1 90.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.1 92.45) (end 123.1 92.45) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.35 132.8) (end 133.35 92.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.1 132.8) (end 133.35 132.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.1 131.05) (end 126.1 132.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.1 131.05) (end 126.1 131.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.1 132.8) (end 123.1 131.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.5 132.8) (end 123.1 132.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.4 135.15) (end 118.5 132.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.55 135.15) (end 116.4 135.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.55 133.15) (end 106.55 135.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.75 133.15) (end 106.55 133.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.75 135.15) (end 101.75 133.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.62 140.97) (xy 93.98 140.97) (xy 93.98 82.55) (xy 134.62 82.55)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.62 140.97) (xy 93.98 140.97) (xy 93.98 82.55) (xy 134.62 82.55)
      )
    )
  )
)
