<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<text>SPI</text>
<text>A0</text>
<text>A2</text>
<text>A4</text>
<text>UART</text>
<wire x1="20.32" y1="0" x2="0" y2="0" width="0.2032" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="10.16" width="0.2032" layer="20"/>
<wire x1="20.32" y1="0" x2="20.32" y2="10.16" width="0.2032" layer="20"/>
<wire x1="20.32" y1="10.16" x2="0" y2="10.16" width="0.2032" layer="20"/>
<text>dcity.org</text>
<text>RFTB1 (A)</text>
</plain>
<libraries>
<library name="0">
<packages>
<package name="SMA-EDGE">
<description>&lt;b&gt;SMA Antenna Connector&lt;/b&gt;&lt;p&gt;
This is a footprint for an edge mount RF antenna. Works pretty well with SMA type connectors but may also work with other edge mount RF connectors. Keep in mind, these edge mount connectors assume you are using a 0.062" PCB thickness.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J$1" library="0" package="SMA-EDGE" value="SMA_EDGE"/>
<element name="J$2" library="0" package="SMA-EDGE" value="SMA_EDGE"/>
</elements>
<signals>
<signal name="GND">
<contactref element="J$1" pad="GND@0"/>
<contactref element="J$1" pad="GND@1"/>
<contactref element="J$1" pad="GND@2"/>
<contactref element="J$1" pad="GND@3"/>
<contactref element="J$2" pad="GND@3"/>
<contactref element="J$2" pad="GND@2"/>
<contactref element="J$2" pad="GND@1"/>
<contactref element="J$2" pad="GND@0"/>
</signal>
<signal name="IN">
<contactref element="J$1" pad="SIG"/>
</signal>
<signal name="OUT">
<contactref element="J$2" pad="SIG"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
