(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad2)")
  (net 2 "gnd")
  (net 3 "resistorout")
  (footprint "Package_DIP:DIP-8_W8.89mm_SMDSocket_LongPads" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 111.76 119.38)
    (descr "8-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads")
    (attr smd)
    (fp_text reference "REF**" (at 0 -6.14) (layer "F.SilkS"))
    (fp_text value "DIP-8_W8.89mm_SMDSocket_LongPads" (at 0 6.14) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -4.445 -3.81) (size 3.1 1.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "2" smd rect (at -4.445 -1.27) (size 3.1 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "resistorout"))
    (pad "3" smd rect (at -4.445 1.27) (size 3.1 1.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "4" smd rect (at -4.445 3.81) (size 3.1 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "gnd"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W8.89mm_SMDSocket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:PHOENIX_1803277" (layer "F.Cu")
    (tedit 64359783)
    (at 81.28 119.38 -90)
    (property "MANUFACTURER" "Phoenix Contact")
    (property "Sheetfile" "AeronetSolarCableAdapter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P1" (at -1.520835 -2.196195 90) (layer "F.SilkS"))
    (fp_text value "1803277" (at 4.83471 9.04384 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at -1.905 0 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "gnd") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.905 0 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad2)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 87.63 121.424145)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "AeronetSolarCableAdapter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "R_US" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "resistorout") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 76.2 111.76) (end 116.84 127) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_text "Arsenio's Adapter\nNo Pain Mode" (at 93.98 114.3) (layer "F.SilkS"))
  (zone (net 2) (net_name "gnd") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.84 129.54)
        (xy 76.2 129.54)
        (xy 76.2 109.22)
        (xy 116.84 109.22)
      )
    )
  )
)
