(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 95)
    (no_connects 0)
    (area 100.024999 47.534523 180.387584 87.6525)
    (thickness 1.6)
    (drawings 27)
    (tracks 455)
    (zones 0)
    (modules 41)
    (nets 37)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 +3V3)
  (net 4 IR_IN)
  (net 5 TEMP_READ)
  (net 6 LED_DR)
  (net 7 "Net-(C5-Pad2)")
  (net 8 LED_DR_5)
  (net 9 "Net-(P4-Pad2)")
  (net 10 "Net-(P4-Pad4)")
  (net 11 "Net-(P4-Pad6)")
  (net 12 "Net-(P4-Pad8)")
  (net 13 RXD_UA_1)
  (net 14 TXD_UA_1)
  (net 15 "Net-(P6-Pad1)")
  (net 16 "Net-(P6-Pad2)")
  (net 17 "Net-(P6-Pad3)")
  (net 18 "Net-(P6-Pad4)")
  (net 19 "Net-(P6-Pad5)")
  (net 20 "Net-(P7-Pad1)")
  (net 21 "Net-(P7-Pad2)")
  (net 22 "Net-(P7-Pad3)")
  (net 23 "Net-(P7-Pad4)")
  (net 24 TEMT)
  (net 25 "Net-(R6-Pad1)")
  (net 26 "Net-(R7-Pad2)")
  (net 27 "Net-(R8-Pad1)")
  (net 28 "Net-(R9-Pad1)")
  (net 29 "Net-(R10-Pad2)")
  (net 30 "Net-(R11-Pad2)")
  (net 31 "Net-(R12-Pad2)")
  (net 32 "Net-(U3-Pad2)")
  (net 33 USBDM_1_N)
  (net 34 USBDP_1_P)
  (net 35 "Net-(R13-Pad1)")
  (net 36 "Net-(R14-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net IR_IN)
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P4-Pad6)")
    (add_net "Net-(P4-Pad8)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(P6-Pad3)")
    (add_net "Net-(P6-Pad4)")
    (add_net "Net-(P6-Pad5)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(P7-Pad2)")
    (add_net "Net-(P7-Pad3)")
    (add_net "Net-(P7-Pad4)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(U3-Pad2)")
    (add_net RXD_UA_1)
    (add_net TEMP_READ)
    (add_net TEMT)
    (add_net TXD_UA_1)
    (add_net USBDM_1_N)
    (add_net USBDP_1_P)
  )
  (net_class 3v ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net LED_DR)
  )
  (net_class 5v ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net LED_DR_5)
  )
  (net_class GND ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 156.054 75.4564)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 3.0135 0.0451) (layer F.SilkS))
    (fp_text value C (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 156.054 59.9564)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 3.1405 0.0511) (layer F.SilkS))
    (fp_text value C (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyKiCadLibs:USB_Micro-B-OshPark (layer F.Cu) (tedit 57FEB7F7)
    (at 172 67.5 90)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference P1 (at -5.4615 0.593 90) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 4.8 90) (layer F.Fab))
    (pad 1 smd rect (at -1.3009 -1.56254 180) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at -0.6509 -1.56254 180) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 USBDM_1_N))
    (pad 3 smd rect (at -0.0009 -1.56254 180) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 USBDP_1_P))
    (pad 4 smd rect (at 0.6491 -1.56254 180) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.2991 -1.56254 180) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -2.5009 -1.56254 180) (size 1.25 1.25) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole circle (at 2.4991 -1.56254 180) (size 1.25 1.25) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole circle (at -3.5009 1.13746 180) (size 1.55 1.55) (drill 1.15) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole circle (at 3.4991 1.13746 180) (size 1.55 1.55) (drill 1.15) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 0)
    (at 146 55 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0.0545 -2.9075 270) (layer F.SilkS))
    (fp_text value TL1838_PINHEADER (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 IR_IN))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 147 60.7518 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.25 180) (layer F.SilkS))
    (fp_text value "Q_NPN_BEC (MMBT2222ALT1G, 1459098 on E14)" (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 6 LED_DR))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 8 LED_DR_5))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 143 60.75 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.25 180) (layer F.SilkS))
    (fp_text value "Q_NPN_BEC (MMBT2222ALT1G, 1459098 on E14)" (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 6 LED_DR))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 8 LED_DR_5))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 146 73.4 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.435 0.05 90) (layer F.SilkS))
    (fp_text value 25 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P4-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 143.25 73.4 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -3.435 0.133 90) (layer F.SilkS))
    (fp_text value 25 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P4-Pad6)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 134.15 66.5)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.8355 0.175) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 TEMP_READ))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ESP8266:ESP-12E (layer F.Cu) (tedit 559F8D21)
    (at 109 74.5 90)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U1 (at 0.078 16.4125 90) (layer F.SilkS))
    (fp_text value ESP-12E (at 8 1 90) (layer F.Fab))
    (fp_text user "No Copper" (at 6.892 -5.4 90) (layer F.CrtYd))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(R8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 24 TEMT))
    (pad 3 thru_hole oval (at 0 4 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(R9-Pad1)"))
    (pad 4 thru_hole oval (at 0 6 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P6-Pad5)"))
    (pad 5 thru_hole oval (at 0 8 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P6-Pad4)"))
    (pad 6 thru_hole oval (at 0 10 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 5 TEMP_READ))
    (pad 7 thru_hole oval (at 0 12 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P6-Pad3)"))
    (pad 8 thru_hole oval (at 0 14 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 9 smd oval (at 1.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(P7-Pad4)"))
    (pad 10 smd oval (at 3.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(P7-Pad3)"))
    (pad 11 smd oval (at 5.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(P6-Pad1)"))
    (pad 12 smd oval (at 7.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(P6-Pad2)"))
    (pad 13 smd oval (at 9.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(P7-Pad2)"))
    (pad 14 smd oval (at 11.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P7-Pad1)"))
    (pad 15 thru_hole oval (at 14 14 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 16 thru_hole oval (at 14 12 90) (size 2.5 1.1) (drill 0.65 (offset 0.6 0)) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(R10-Pad2)"))
    (pad 17 thru_hole oval (at 14 10 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(R11-Pad2)"))
    (pad 18 thru_hole oval (at 14 8 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(R12-Pad2)"))
    (pad 19 thru_hole oval (at 14 6 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 4 IR_IN))
    (pad 20 thru_hole oval (at 14 4 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 6 LED_DR))
    (pad 21 thru_hole oval (at 14 2 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(R13-Pad1)"))
    (pad 22 thru_hole oval (at 14 0 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(R14-Pad1)"))
    (model ${ESPLIB}/ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0.04 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 54E9291B)
    (at 156.054 67.9553 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at 2.1935 -1.4502 180) (layer F.SilkS))
    (fp_text value AP1117 (at 0 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 0 -1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 54F24281)
    (at 134.96 55)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference P3 (at 1.7555 2.658) (layer F.SilkS))
    (fp_text value DS18B20_PINHEADER_TO92 (at 0 3) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 5 TEMP_READ))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole oval (at 0 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 139 60.75 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.25 180) (layer F.SilkS))
    (fp_text value "Q_NPN_BEC (MMBT2222ALT1G, 1459098 on E14)" (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 6 LED_DR))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 8 LED_DR_5))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 151 60.7518 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 -2.25 180) (layer F.SilkS))
    (fp_text value "Q_NPN_BEC (MMBT2222ALT1G, 1459098 on E14)" (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 6 LED_DR))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 8 LED_DR_5))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 148.5 73.4 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -3.435 0.0265 90) (layer F.SilkS))
    (fp_text value 25 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(P4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 140.75 73.4 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -3.4985 0.2835 90) (layer F.SilkS))
    (fp_text value 25 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(P4-Pad8)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 163.25 61.5 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -3.5645 -0.095 180) (layer F.SilkS))
    (fp_text value C (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 0)
    (at 148.5 65.5 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 1.3655 -2.5665 270) (layer F.SilkS))
    (fp_text value CONN_02X04 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 LED_DR_5))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P4-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 LED_DR_5))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P4-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 LED_DR_5))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P4-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 LED_DR_5))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P4-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 131.5 55 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at -2.1045 3.2935 360) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 RXD_UA_1))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 TXD_UA_1))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 54EA0684)
    (at 132.66 80 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 0.0735 -2.722 270) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P6-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P6-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P6-Pad5)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 129 63.42)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0.032 -2.3965) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(P7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P7-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P7-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(P7-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 0)
    (at 120.5 55 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at -2.3585 0.8025 360) (layer F.SilkS))
    (fp_text value TEMP6000 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 TEMT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 162.25 73.4 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 3.4985 -0.056 270) (layer F.SilkS))
    (fp_text value 27 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 34 USBDP_1_P))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 164.531 73.3703 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at -3.4647 -0.066 90) (layer F.SilkS))
    (fp_text value 27 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 USBDM_1_N))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 134.15 64)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at -0.3555 -4.31) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 134.15 69)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 3.772 0.0245) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R9-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 134.15 74 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 4.102 -0.295 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 134.15 61.5 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at -3.899 -3.0795 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R11-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 134.15 71.5 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at -4.026 0.3165 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R12-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-16_3.9x4.9mm_Pitch0.635mm (layer F.Cu) (tedit 54130A77)
    (at 163.5 67.4125)
    (descr "SSOP16: plastic shrink small outline package; 16 leads; body width 3.9 mm; lead pitch 0.635; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot519-1_po.pdf)")
    (tags "SSOP 0.635")
    (attr smd)
    (fp_text reference U3 (at -0.305 -0.166) (layer F.SilkS))
    (fp_text value FT230XS (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.6 -2.2225) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 TXD_UA_1))
    (pad 2 smd rect (at -2.6 -1.5875) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U3-Pad2)"))
    (pad 3 smd rect (at -2.6 -0.9525) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (pad 4 smd rect (at -2.6 -0.3175) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 RXD_UA_1))
    (pad 5 smd rect (at -2.6 0.3175) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.6 0.9525) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U3-Pad2)"))
    (pad 7 smd rect (at -2.6 1.5875) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -2.6 2.2225) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R6-Pad1)"))
    (pad 9 smd rect (at 2.6 2.2225) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R7-Pad2)"))
    (pad 10 smd rect (at 2.6 1.5875) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (pad 11 smd rect (at 2.6 0.9525) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (pad 12 smd rect (at 2.6 0.3175) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 13 smd rect (at 2.6 -0.3175) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 2.6 -0.9525) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 2.6 -1.5875) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 2.6 -2.2225) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask))
    (model Housings_SSOP.3dshapes/SSOP-16_3.9x4.9mm_Pitch0.635mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_Reflow (layer F.Cu) (tedit 555EF748)
    (at 156.094 72.4564)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow")
    (tags "Tantal Capacitor Size-B EIA-3528 Reflow")
    (attr smd)
    (fp_text reference C1 (at -3.5035 0.0606 90) (layer F.SilkS))
    (fp_text value CP (at 0 2.7) (layer F.Fab))
    (pad 2 smd rect (at 1.46 0) (size 1.8 2.23) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.46 0) (size 1.8 2.23) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_Reflow (layer F.Cu) (tedit 555EF748)
    (at 156.014 62.9564)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow")
    (tags "Tantal Capacitor Size-B EIA-3528 Reflow")
    (attr smd)
    (fp_text reference C4 (at 3.8155 0.0991) (layer F.SilkS))
    (fp_text value CP (at 0 2.7) (layer F.Fab))
    (pad 2 smd rect (at 1.46 0) (size 1.8 2.23) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.46 0) (size 1.8 2.23) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 55DB43C0)
    (at 152.3 80)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW2 (at 0.0365 0.2005) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2.7 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R12-Pad2)"))
    (pad 1 smd rect (at -2.7 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 55DB43C0)
    (at 143.8 80)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW1 (at 0.1545 0.0735) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2.7 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.7 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R8-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C)
    (at 162.5 80 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P9 (at 0.137 -2.6635 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 155.876 57.404)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 4.144 -0.1905) (layer F.SilkS))
    (fp_text value 470 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R13-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 TXD_UA_1))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 155.876 55.118)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 4.144 0.127) (layer F.SilkS))
    (fp_text value 470 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R14-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 RXD_UA_1))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 58C4A91C)
    (at 109.728 54.61)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF04 (at 0.254 -5.334) (layer F.SilkS))
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 58C4A918)
    (at 109.728 80.264)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF03 (at -0.0635 5.207) (layer F.SilkS))
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 58C4A912)
    (at 171.704 80.264)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF02 (at -0.3175 6.4135) (layer F.SilkS))
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 58C4A90A)
    (at 171.704 54.864)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF01 (at 0.1905 -4.445) (layer F.SilkS))
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (gr_text D16 (at 122.428 82.1055) (layer F.SilkS))
  (gr_text D14 (at 125.0315 82.1055) (layer F.SilkS))
  (gr_text D13 (at 127.5715 82.1055) (layer F.SilkS))
  (gr_text D9 (at 132.6515 82.1055) (layer F.SilkS))
  (gr_text D10 (at 130.175 82.1055) (layer F.SilkS))
  (gr_text "IR OUT x 4" (at 144.7165 70.104) (layer F.SilkS))
  (gr_text SPI (at 127.0635 66.7385 90) (layer F.SilkS))
  (gr_text GPIO (at 127.5715 77.7875) (layer F.SilkS))
  (gr_text GND (at 143.51 57.2135 360) (layer F.SilkS))
  (gr_text +3.3 (at 147.066 57.277) (layer F.SilkS))
  (gr_text GND (at 131.5085 57.9755 90) (layer F.SilkS))
  (gr_text LIGHT (at 115.8875 52.8955) (layer F.SilkS))
  (gr_text GND (at 117.983 57.277) (layer F.SilkS))
  (gr_text +3.3 (at 121.9835 57.404) (layer F.SilkS))
  (gr_text TX (at 129.032 57.404 90) (layer F.SilkS))
  (gr_text RX (at 126.365 57.404 90) (layer F.SilkS))
  (gr_text TEMP (at 136.271 52.959) (layer F.SilkS))
  (gr_text "IR IN" (at 141.732 52.8955) (layer F.SilkS))
  (gr_text GND (at 159.8295 82.1055) (layer F.SilkS))
  (gr_text +5 (at 162.687 82.2325) (layer F.SilkS))
  (gr_text PROG (at 152.2095 82.1055) (layer F.SilkS))
  (gr_text RESET (at 143.637 82.042) (layer F.SilkS))
  (gr_text "IRRemote - me@pjr.cc\nhttps://github.com/takigama\n" (at 151.765 70.8025 30) (layer B.SilkS))
  (gr_line (start 175 83.5) (end 106.5 83.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175 51.5) (end 175 83.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.5 51.5) (end 175 51.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.5 83.5) (end 106.5 51.5) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.426 51.435) (xy 106.426 52.07) (xy 175.0695 52.07) (xy 175.0695 51.435)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.0695 51.435) (xy 106.426 51.435) (xy 106.426 52.07) (xy 175.0695 52.07)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.0695 83.566) (xy 175.0695 82.931) (xy 106.426 82.931) (xy 106.426 83.566)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.0695 83.566) (xy 175.0695 82.931) (xy 106.426 82.931) (xy 106.426 83.566)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.0695 51.435) (xy 174.4345 51.435) (xy 174.4345 83.566) (xy 175.0695 83.566)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.0695 51.435) (xy 174.4345 51.435) (xy 174.4345 83.566) (xy 175.0695 83.566)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.426 51.435) (xy 106.426 83.566) (xy 107.061 83.566) (xy 107.061 51.435)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.426 51.435) (xy 106.426 83.566) (xy 107.061 83.566) (xy 107.061 51.435)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.426 51.435) (xy 106.426 83.566) (xy 175.0695 83.566) (xy 175.0695 51.435)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.0695 83.566) (xy 138.43 83.566) (xy 138.43 73.025) (xy 153.035 73.025) (xy 153.035 67.945)
        (xy 159.9565 67.945) (xy 159.9565 64.643) (xy 175.0695 64.643)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.2395 83.566) (xy 138.2395 72.8345) (xy 152.8445 72.8345) (xy 152.8445 67.7545) (xy 156.21 67.7545)
        (xy 156.21 51.435) (xy 112.395 51.435) (xy 112.395 83.566)
      )
    )
  )
)
