(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 8)
    (no_connects 0)
    (area 15.79954 14.890693 41.116335 35.417563)
    (thickness 1.6)
    (drawings 4)
    (tracks 13)
    (zones 0)
    (modules 2)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.2 1.2)
    (pad_drill 0.7)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_00000000)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J101-Pad1)")
  (net 2 "Net-(J101-Pad2)")
  (net 3 "Net-(J101-Pad3)")
  (net 4 "Net-(J101-Pad4)")
  (net 5 "Net-(J101-Pad5)")
  (net 6 "Net-(J101-Pad6)")
  (net 7 "Net-(J101-Pad7)")
  (net 8 "Net-(J101-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J101-Pad1)")
    (add_net "Net-(J101-Pad2)")
    (add_net "Net-(J101-Pad3)")
    (add_net "Net-(J101-Pad4)")
    (add_net "Net-(J101-Pad5)")
    (add_net "Net-(J101-Pad6)")
    (add_net "Net-(J101-Pad7)")
    (add_net "Net-(J101-Pad8)")
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5B5548D0)
    (at 25.273 18.288)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference J102 (at 3.81 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_02x04_Counter_Clockwise (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(J101-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(J101-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(J101-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(J101-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(J101-Pad3)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(J101-Pad7)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(J101-Pad4)"))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(J101-Pad8)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-5-8_PD5.08 (layer F.Cu) (tedit 5B5548BC)
    (at 27.305 20.32 315)
    (descr TO-5-8_PD5.08)
    (tags TO-5-8_PD5.08)
    (fp_text reference J101 (at 5.028943 -7.36381 315) (layer F.SilkS) hide)
    (fp_text value Conn_02x04_Counter_Clockwise (at 2.54 5.82 315) (layer F.Fab))
    (fp_text user %R (at 2.54 -5.82 315) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 315) (size 1.6 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(J101-Pad1)"))
    (pad 2 thru_hole oval (at 0.743949 1.796051 315) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(J101-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 2.54 315) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(J101-Pad3)"))
    (pad 4 thru_hole oval (at 4.336051 1.796051 315) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(J101-Pad4)"))
    (pad 5 thru_hole oval (at 5.08 0 315) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(J101-Pad5)"))
    (pad 6 thru_hole oval (at 4.336051 -1.796051 315) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(J101-Pad6)"))
    (pad 7 thru_hole oval (at 2.54 -2.54 315) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(J101-Pad7)"))
    (pad 8 thru_hole oval (at 0.743949 -1.796051 315) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(J101-Pad8)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-5-8_PD5.08.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 24.384 26.797) (end 24.384 17.399) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 33.782 26.797) (end 24.384 26.797) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 33.782 17.399) (end 33.782 26.797) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 24.384 17.399) (end 33.782 17.399) (angle 90) (layer Edge.Cuts) (width 0.15))
)
