<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="-0.0254" x2="49.4284" y2="-0.0254" width="0.1524" layer="20"/>
<wire x1="49.4284" y1="-0.0254" x2="49.4284" y2="41.8746" width="0.1524" layer="20"/>
<wire x1="49.4284" y1="41.8746" x2="0" y2="41.8746" width="0.1524" layer="20"/>
<wire x1="0" y1="41.8746" x2="0" y2="-0.0254" width="0.1524" layer="20"/>
<text>RV-Project.Com
Remote Controlled 
Switch</text>
<text>Use BUD CU18425 Enclosure</text>
<text>Active</text>
<text>RCS-5A Rev C</text>
<text>5/21/2022</text>
<text>Trigger</text>
<text>++Trigger--</text>
<text>GND</text>
<text>12V</text>
<text>--OUT ++</text>
<text>IN</text>
<text>Common
GND</text>
<text>Power</text>
<hole x="5.08" y="5.08" drill="2.54"/>
<hole x="44.958" y="5.08" drill="2.54"/>
<hole x="5.08" y="37.0332" drill="2.54"/>
<hole x="44.45" y="37.0332" drill="2.54"/>
<text>Trig Sw</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>Aux--</text>
<text>Aux++</text>
<text>5V</text>
<text>3.3V~12V</text>
<text>Made in the USA</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>VCC</text>
<text>OUT</text>
<text>TRG</text>
<text>GND</text>
<text>RST</text>
<text>M1</text>
<text>M2</text>
<text>M3</text>
<text>Squatchy
Engineering</text>
<text>STOMP of
approval.</text>
<text>5V Option</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="RADIAL_ELECTROLYTIC_100MIL(5MM)">
<description>Generic Electrolytic Capacitor.&lt;br&gt;Pitch:0.1&lt;br&gt;
Dia: 0.2"Dia (5.08mm)</description>
</package>
<package name="1206-CAP">
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="1206-RES">
</package>
<package name="SOD-123">
<description>Suitable for 4148
&lt;br&gt;Pad Size:  0.55"x0.8"</description>
</package>
<package name="6PIN_OPTO">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOD-323">
<description>Pad Size: 0.22"x0.8"</description>
</package>
<package name="DIL06">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="GODZILLA_LARGE">
</package>
<package name="G5V">
</package>
<package name="TO-92-AMMO">
</package>
</packages>
</library>
<library name="a-lib_Connectors">
<description>Thru-Hole Connectors (Connectors, Terminals)</description>
<packages>
<package name="MO1-16AWG-SMALL">
</package>
<package name="MO1-24AWG-SMALL">
</package>
<package name="MO1-20AWG-SMALL">
</package>
</packages>
</library>
<library name="a-lib_SMD">
<description>All SMD Devices; Actives, Passives, Connectors</description>
<packages>
<package name="SMD-JUMPER_2">
<description>Pad Size: 0.12"x0.06"&lt;br&gt;Resist remoted between pads for ease of solder bridge.</description>
</package>
</packages>
</library>
<library name="a-lib_Actives">
<description>Thru-Hole Actives (Transistors, Diodes, MPUs)</description>
<packages>
<package name="IPAK_VERTICAL(TO251)">
</package>
</packages>
</library>
<library name="a-lib_Asthetics">
<description>Miscellaneous Items (Hardware, Power Points, Logos, etc)</description>
<packages>
<package name="RVPROJECT_NEWLOGO_SMALL">
</package>
<package name="ART_CHEROKEE_MEDIUM">
</package>
<package name="BIGFOOT_SMALL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C5" library="a-lib" package="RADIAL_ELECTROLYTIC_100MIL(5MM)" value="10UF">
<attribute name="MARKING" value="106"/>
<attribute name="NAME"/>
<attribute name="VOLTAGE" value="25v"/>
</element>
<element name="C7" library="a-lib" package="1206-CAP" value="0.01uF">
<attribute name="NAME"/>
</element>
<element name="C1" library="a-lib" package="1206-CAP" value=".01uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="a-lib" package="1206-CAP" value="0.33uF">
<attribute name="NAME"/>
</element>
<element name="U1" library="a-lib" package="DIP08" value="TINY85-20-DIP">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-09445"/>
</element>
<element name="R10" library="a-lib" package="1206-RES" value="220">
<attribute name="NAME"/>
</element>
<element name="OK1" library="a-lib" package="6PIN_OPTO" value="4N35">
<attribute name="NAME"/>
</element>
<element name="R8" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
</element>
<element name="R5" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
</element>
<element name="R1" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
</element>
<element name="D3" library="a-lib" package="SOD-123" value="TVS-SSOD123">
<attribute name="NAME"/>
</element>
<element name="D2" library="a-lib" package="SOD-323" value="250mA/100V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="R9" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
</element>
<element name="S1" library="a-lib" package="DIL06" value="DIPSWITCH-3">
<attribute name="NAME"/>
</element>
<element name="R2" library="a-lib" package="1206-RES" value="10K">
<attribute name="NAME"/>
</element>
<element name="R3" library="a-lib" package="1206-RES" value="10K">
<attribute name="NAME"/>
</element>
<element name="R4" library="a-lib" package="1206-RES" value="10K">
<attribute name="NAME"/>
</element>
<element name="U$2" library="a-lib" package="GODZILLA_LARGE" value=""/>
<element name="TB9" library="a-lib_Connectors" package="MO1-16AWG-SMALL" value=""/>
<element name="TB10" library="a-lib_Connectors" package="MO1-16AWG-SMALL" value=""/>
<element name="TB15" library="a-lib_Connectors" package="MO1-16AWG-SMALL" value=""/>
<element name="TB16" library="a-lib_Connectors" package="MO1-16AWG-SMALL" value=""/>
<element name="J1" library="a-lib_SMD" package="SMD-JUMPER_2" value="M2JUMPER1"/>
<element name="R6" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
</element>
<element name="U3" library="a-lib_Actives" package="IPAK_VERTICAL(TO251)" value="">
<attribute name="NAME"/>
</element>
<element name="TB2" library="a-lib_Connectors" package="MO1-24AWG-SMALL" value=""/>
<element name="TB1" library="a-lib_Connectors" package="MO1-24AWG-SMALL" value=""/>
<element name="TB13" library="a-lib_Connectors" package="MO1-24AWG-SMALL" value=""/>
<element name="TB14" library="a-lib_Connectors" package="MO1-24AWG-SMALL" value=""/>
<element name="TB3" library="a-lib_Connectors" package="MO1-24AWG-SMALL" value=""/>
<element name="TB4" library="a-lib_Connectors" package="MO1-24AWG-SMALL" value=""/>
<element name="TB6" library="a-lib_Connectors" package="MO1-24AWG-SMALL" value=""/>
<element name="TB7" library="a-lib_Connectors" package="MO1-24AWG-SMALL" value=""/>
<element name="R7" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
</element>
<element name="TB12" library="a-lib_Connectors" package="MO1-16AWG-SMALL" value=""/>
<element name="TB11" library="a-lib_Connectors" package="MO1-16AWG-SMALL" value=""/>
<element name="RY1" library="a-lib" package="G5V" value="G5V5V">
<attribute name="ALTPARTNO" value="G5V-1-1"/>
<attribute name="COIL" value="30mA"/>
<attribute name="CONTACT" value="1Amp"/>
<attribute name="INPUT" value="5V"/>
<attribute name="PARTNO" value="G5V-1-2"/>
</element>
<element name="Q1" library="a-lib" package="TO-92-AMMO" value="2N2222">
<attribute name="NAME"/>
<attribute name="VALUE" value="2N2222"/>
</element>
<element name="D1" library="a-lib" package="SOD-323" value="250mA/100V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="U$1" library="a-lib_Asthetics" package="RVPROJECT_NEWLOGO_SMALL" value=""/>
<element name="U$3" library="a-lib_Asthetics" package="ART_CHEROKEE_MEDIUM" value=""/>
<element name="U$4" library="a-lib_Asthetics" package="BIGFOOT_SMALL" value=""/>
<element name="TB8" library="a-lib_Connectors" package="MO1-20AWG-SMALL" value=""/>
<element name="TB5" library="a-lib_Connectors" package="MO1-20AWG-SMALL" value=""/>
<element name="U2" library="a-lib_Actives" package="IPAK_VERTICAL(TO251)" value="">
<attribute name="NAME"/>
</element>
<element name="C2" library="a-lib" package="1206-CAP" value="0.33uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="a-lib" package="RADIAL_ELECTROLYTIC_100MIL(5MM)" value="10UF">
<attribute name="MARKING" value="106"/>
<attribute name="NAME"/>
<attribute name="VOLTAGE" value="25v"/>
</element>
<element name="C6" library="a-lib" package="1206-CAP" value="0.01uF">
<attribute name="NAME"/>
</element>
<element name="J2" library="a-lib_SMD" package="SMD-JUMPER_2" value="M2JUMPER1"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="OK1" pad="4"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="TB10" pad="P$1"/>
<contactref element="J1" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="U3" pad="G"/>
<contactref element="Q1" pad="1"/>
<contactref element="TB14" pad="P$1"/>
<contactref element="TB16" pad="P$1"/>
<contactref element="TB8" pad="P$1"/>
<contactref element="U2" pad="G"/>
<contactref element="C6" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="12V">
<contactref element="TB9" pad="P$1"/>
<contactref element="TB1" pad="P$1"/>
<contactref element="TB3" pad="P$1"/>
<contactref element="C5" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="U3" pad="I"/>
<contactref element="TB5" pad="P$1"/>
<contactref element="C2" pad="2"/>
<contactref element="U2" pad="I"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$14">
</signal>
<signal name="N$15">
</signal>
<signal name="N$13">
<contactref element="U1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R8" pad="1"/>
<contactref element="OK1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="TB2" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="R9" pad="1"/>
<contactref element="TB6" pad="P$1"/>
</signal>
<signal name="N$16">
<contactref element="R5" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="OK1" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="5"/>
<contactref element="R4" pad="1"/>
<contactref element="S1" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="R3" pad="1"/>
<contactref element="S1" pad="5"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="7"/>
<contactref element="R2" pad="1"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="R6" pad="2"/>
<contactref element="TB4" pad="P$1"/>
</signal>
<signal name="N$20">
<contactref element="R7" pad="1"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="RY1" pad="NO"/>
<contactref element="R10" pad="2"/>
<contactref element="TB15" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="TB13" pad="P$1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="C6" pad="1"/>
<contactref element="U2" pad="O"/>
<contactref element="RY1" pad="COM1"/>
<contactref element="RY1" pad="COM2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="TB12" pad="P$1"/>
<contactref element="OK1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="TB7" pad="P$1"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$17">
<contactref element="TB11" pad="P$1"/>
<contactref element="D2" pad="A"/>
<contactref element="D3" pad="C"/>
</signal>
<signal name="N$21">
<contactref element="Q1" pad="3"/>
<contactref element="RY1" pad="9"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="RY1" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="C7" pad="1"/>
<contactref element="U3" pad="O"/>
<contactref element="D1" pad="C"/>
<contactref element="J2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
