(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 62)
    (no_connects 0)
    (area 76.933667 111.721 121.948334 170.905001)
    (thickness 1.6)
    (drawings 5)
    (tracks 199)
    (zones 0)
    (modules 14)
    (nets 46)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.3302)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.1778)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 86.36 121.92)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 +5V)
  (net 5 +3V3)
  (net 6 "Net-(P1-Pad5)")
  (net 7 D+)
  (net 8 D-)
  (net 9 D2+)
  (net 10 D2-)
  (net 11 "Net-(P2-Pad5)")
  (net 12 "Net-(P3-Pad2)")
  (net 13 "Net-(P3-Pad3)")
  (net 14 "Net-(P3-Pad4)")
  (net 15 "Net-(P3-Pad5)")
  (net 16 "Net-(P3-Pad6)")
  (net 17 "Net-(P3-Pad7)")
  (net 18 "Net-(P3-Pad8)")
  (net 19 "Net-(P3-Pad9)")
  (net 20 "Net-(P3-Pad10)")
  (net 21 "Net-(P3-Pad11)")
  (net 22 "Net-(P3-Pad12)")
  (net 23 "Net-(P3-Pad13)")
  (net 24 "Net-(P3-Pad14)")
  (net 25 "Net-(P3-Pad15)")
  (net 26 "Net-(P3-Pad16)")
  (net 27 RxD)
  (net 28 TxD)
  (net 29 "Net-(P5-Pad7)")
  (net 30 "Net-(P5-Pad8)")
  (net 31 "Net-(P5-Pad9)")
  (net 32 "Net-(P5-Pad10)")
  (net 33 "Net-(P5-Pad11)")
  (net 34 "Net-(P5-Pad12)")
  (net 35 "Net-(P5-Pad13)")
  (net 36 "Net-(P5-Pad14)")
  (net 37 "Net-(P5-Pad15)")
  (net 38 "Net-(P5-Pad16)")
  (net 39 "Net-(U1-Pad14)")
  (net 40 "Net-(U1-Pad13)")
  (net 41 "Net-(U1-Pad12)")
  (net 42 "Net-(U1-Pad11)")
  (net 43 "Net-(U1-Pad10)")
  (net 44 "Net-(U1-Pad9)")
  (net 45 "Net-(U1-Pad15)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net D+)
    (add_net D-)
    (add_net D2+)
    (add_net D2-)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P3-Pad10)")
    (add_net "Net-(P3-Pad11)")
    (add_net "Net-(P3-Pad12)")
    (add_net "Net-(P3-Pad13)")
    (add_net "Net-(P3-Pad14)")
    (add_net "Net-(P3-Pad15)")
    (add_net "Net-(P3-Pad16)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P3-Pad6)")
    (add_net "Net-(P3-Pad7)")
    (add_net "Net-(P3-Pad8)")
    (add_net "Net-(P3-Pad9)")
    (add_net "Net-(P5-Pad10)")
    (add_net "Net-(P5-Pad11)")
    (add_net "Net-(P5-Pad12)")
    (add_net "Net-(P5-Pad13)")
    (add_net "Net-(P5-Pad14)")
    (add_net "Net-(P5-Pad15)")
    (add_net "Net-(P5-Pad16)")
    (add_net "Net-(P5-Pad7)")
    (add_net "Net-(P5-Pad8)")
    (add_net "Net-(P5-Pad9)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad9)")
    (add_net RxD)
    (add_net TxD)
  )
  (module SMD_Packages:SO-16-N (layer F.Cu) (tedit 0)
    (at 104.14 142.24 270)
    (descr "Module CMS SOJ 16 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at 0.127 -1.27 270) (layer F.SilkS))
    (fp_text value CH340G (at 0 1.27 270) (layer F.Fab))
    (pad 16 smd rect (at -4.445 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 14 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U1-Pad14)"))
    (pad 13 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U1-Pad13)"))
    (pad 12 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U1-Pad12)"))
    (pad 11 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U1-Pad11)"))
    (pad 10 smd rect (at 3.175 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U1-Pad10)"))
    (pad 9 smd rect (at 4.445 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U1-Pad9)"))
    (pad 8 smd rect (at 4.445 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 7 smd rect (at 3.175 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 6 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 D-))
    (pad 5 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 D+))
    (pad 4 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 3 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 28 TxD))
    (pad 2 smd rect (at -3.175 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 27 RxD))
    (pad 1 smd rect (at -4.445 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd rect (at -3.175 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U1-Pad15)"))
    (model SMD_Packages.3dshapes/SO-16-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 91.44 142.24 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 22pF (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 91.44 149.86 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 22pF (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 93.98 124.46)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 104.14 129.54 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 101.6 129.54 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:USB_A (layer F.Cu) (tedit 5543E289)
    (at 96.52 157.48)
    (descr "USB A connector")
    (tags "USB USB_A")
    (fp_text reference P2 (at 0 -2.35) (layer F.SilkS))
    (fp_text value USB_B (at 3.84 7.44) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.11 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 4.57 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 D2+))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 D2-))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 5 thru_hole circle (at 10.16 2.67 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 11 "Net-(P2-Pad5)"))
    (pad 5 thru_hole circle (at -3.56 2.67 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 11 "Net-(P2-Pad5)"))
    (model Connectors.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x16_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 82.042 119.38)
    (descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.54mm single row")
    (fp_text reference P3 (at 0 -2.39) (layer F.SilkS))
    (fp_text value CONN_01X16 (at 0 40.49) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(P3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(P3-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(P3-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(P3-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(P3-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(P3-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(P3-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(P3-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(P3-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(P3-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(P3-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(P3-Pad15)"))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(P3-Pad16)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16_Pitch2.54mm.wrl
      (at (xyz 0 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x16_Pitch2.00mm (layer F.Cu) (tedit 5862ED56)
    (at 87.122 121.92)
    (descr "Through hole straight pin header, 1x16, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.00mm single row")
    (fp_text reference P4 (at 0 -2.12) (layer F.SilkS))
    (fp_text value CONN_01X16 (at 0 32.12) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(P3-Pad3)"))
    (pad 4 thru_hole oval (at 0 6) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(P3-Pad4)"))
    (pad 5 thru_hole oval (at 0 8) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(P3-Pad5)"))
    (pad 6 thru_hole oval (at 0 10) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(P3-Pad6)"))
    (pad 7 thru_hole oval (at 0 12) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad7)"))
    (pad 8 thru_hole oval (at 0 14) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(P3-Pad8)"))
    (pad 9 thru_hole oval (at 0 16) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(P3-Pad9)"))
    (pad 10 thru_hole oval (at 0 18) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(P3-Pad10)"))
    (pad 11 thru_hole oval (at 0 20) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(P3-Pad11)"))
    (pad 12 thru_hole oval (at 0 22) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(P3-Pad12)"))
    (pad 13 thru_hole oval (at 0 24) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(P3-Pad13)"))
    (pad 14 thru_hole oval (at 0 26) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(P3-Pad14)"))
    (pad 15 thru_hole oval (at 0 28) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(P3-Pad15)"))
    (pad 16 thru_hole oval (at 0 30) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(P3-Pad16)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x16_Pitch2.00mm (layer F.Cu) (tedit 5862ED56)
    (at 111.76 121.92)
    (descr "Through hole straight pin header, 1x16, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.00mm single row")
    (fp_text reference P5 (at 0 -2.12) (layer F.SilkS))
    (fp_text value CONN_01X16 (at 0 32.12) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 3 thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 D2+))
    (pad 4 thru_hole oval (at 0 6) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 D2-))
    (pad 5 thru_hole oval (at 0 8) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 RxD))
    (pad 6 thru_hole oval (at 0 10) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 TxD))
    (pad 7 thru_hole oval (at 0 12) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(P5-Pad7)"))
    (pad 8 thru_hole oval (at 0 14) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(P5-Pad8)"))
    (pad 9 thru_hole oval (at 0 16) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(P5-Pad9)"))
    (pad 10 thru_hole oval (at 0 18) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(P5-Pad10)"))
    (pad 11 thru_hole oval (at 0 20) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(P5-Pad11)"))
    (pad 12 thru_hole oval (at 0 22) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(P5-Pad12)"))
    (pad 13 thru_hole oval (at 0 24) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(P5-Pad13)"))
    (pad 14 thru_hole oval (at 0 26) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(P5-Pad14)"))
    (pad 15 thru_hole oval (at 0 28) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(P5-Pad15)"))
    (pad 16 thru_hole oval (at 0 30) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(P5-Pad16)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x16_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 116.84 119.38)
    (descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.54mm single row")
    (fp_text reference P6 (at 0 -2.39) (layer F.SilkS))
    (fp_text value CONN_01X16 (at 0 40.49) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 D2+))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 D2-))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 RxD))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 TxD))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(P5-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(P5-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(P5-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(P5-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(P5-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(P5-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(P5-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(P5-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(P5-Pad15)"))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(P5-Pad16)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16_Pitch2.54mm.wrl
      (at (xyz 0 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Crystals:Crystal_SMD_5032-2pin_5.0x3.2mm (layer F.Cu) (tedit 5873B462)
    (at 96.52 144.78 270)
    (descr "SMD Crystal SERIES SMD2520/2 http://www.icbase.com/File/PDF/HKC/HKC00061008.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 0 -2.8 270) (layer F.SilkS))
    (fp_text value 12MHz (at 0 2.8 270) (layer F.Fab))
    (pad 1 smd rect (at -1.85 0 270) (size 2 2.4) (layers F.Cu F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.85 0 270) (size 2 2.4) (layers F.Cu F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Crystals.3dshapes/Crystal_SMD_5032-2pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 583F3B4E)
    (at 93.98 132.08 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 0 -4.5 180) (layer F.SilkS))
    (fp_text value AP1117 (at 0 4.5 180) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connect:USB_Micro-B (layer F.Cu) (tedit 5543E447)
    (at 99.568 117.856 180)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference P1 (at 0 -3.24 180) (layer F.SilkS))
    (fp_text value USB_B (at 0 5.01 180) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.35 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at -0.65 -1.35 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 D-))
    (pad 3 smd rect (at 0 -1.35 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 D+))
    (pad 4 smd rect (at 0.65 -1.35 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.3 -1.35 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at -2.5 -1.35 270) (size 0.95 1.25) (drill oval 0.55 0.85) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.5 -1.35 270) (size 0.95 1.25) (drill oval 0.55 0.85) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at -3.5 1.35 270) (size 1.55 1) (drill oval 1.15 0.5) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.5 1.35 270) (size 1.55 1) (drill oval 1.15 0.5) (layers *.Cu *.Mask))
  )
  (gr_text "Omega 2 Breakout - Rev 1" (at 100.076 163.068) (layer B.SilkS))
  (gr_line (start 119.38 113.284) (end 119.38 165.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.756 165.1) (end 79.756 113.284) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.38 165.1) (end 79.756 165.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.756 113.284) (end 119.38 113.284) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.872 164.592) (xy 80.264 164.592) (xy 80.264 113.792) (xy 118.872 113.792) (xy 118.872 164.592)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.872 113.792) (xy 80.01 113.792) (xy 80.01 164.846) (xy 119.126 164.846) (xy 119.126 113.792)
        (xy 118.618 113.792)
      )
    )
  )
)
