(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (title_block
    (title "Quad ESL-63 Clamp Board")
    (rev "1")
    (company "SDS Labs")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "VCC")
  (net 3 "Net-(R4-Pad1)")
  (net 4 "Net-(U1-DIS)")
  (net 5 "Net-(P5-P1)")
  (net 6 "Net-(P9-P1)")
  (net 7 "Net-(P8-P1)")
  (net 8 "Net-(P2-P1)")
  (net 9 "Net-(P1-P1)")
  (net 10 "Net-(Ant1-P1)")
  (net 11 "Net-(P10-P1)")
  (net 12 "Net-(P4-P1)")
  (net 13 "Net-(Q1-C)")
  (net 14 "Net-(U1-Q)")
  (net 15 "unconnected-(U1-CV-Pad5)")
  (net 16 "Net-(IN1-P1)")
  (footprint "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm" (layer "F.Cu")
    (at 97.719277 110.5916 180)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 2.5 -6.25) (layer "F.SilkS"))
    (fp_text value "CP" (at 2.5 6.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W3.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "F.Cu")
    (at 118.665 116.84 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*3.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 3.5mm Capacitor")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at 2.5 -3) (layer "F.SilkS"))
    (fp_text value "C" (at 2.5 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(U1-DIS)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W3.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (at 105.41 111.76 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D2" (at 9.525 0) (layer "F.SilkS"))
    (fp_text value "D" (at 5.81 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 -90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(Ant1-P1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Axial_L6.6mm_D2.7mm_P10.16mm_Horizontal_Vishay_IM-2" (layer "F.Cu")
    (at 102.235 109.22 -90)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=6.6*2.7mm^2, Vishay, IM-2, http://www.vishay.com/docs/34030/im.pdf")
    (tags "Inductor Axial series Axial Horizontal pin pitch 10.16mm  length 6.6mm diameter 2.7mm Vishay IM-2")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L1" (at 12.065 0) (layer "F.SilkS"))
    (fp_text value "L_Small" (at 5.08 2.47 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(Ant1-P1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L6.6mm_D2.7mm_P10.16mm_Horizontal_Vishay_IM-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm" (layer "F.Cu")
    (at 92.0115 90.424)
    (descr "Soldered wire connection, for a single 1.5 mm² wire, reinforced insulation, conductor diameter 1.7mm, outer diameter 3.9mm, size source Multi-Contact FLEXI-xV 1.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 1.5sqmm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P1" (at 0 -3.15) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 3.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.9 3.9) (drill 2.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.064103)
      (net 9 "Net-(P1-P1)") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm" (layer "F.Cu")
    (at 99.06 90.678)
    (descr "Soldered wire connection, for a single 1.5 mm² wire, reinforced insulation, conductor diameter 1.7mm, outer diameter 3.9mm, size source Multi-Contact FLEXI-xV 1.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 1.5sqmm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P2" (at 0 -3.15) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 3.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.9 3.9) (drill 2.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.064103)
      (net 8 "Net-(P2-P1)") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm" (layer "F.Cu")
    (at 106.172 90.678)
    (descr "Soldered wire connection, for a single 1.5 mm² wire, reinforced insulation, conductor diameter 1.7mm, outer diameter 3.9mm, size source Multi-Contact FLEXI-xV 1.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 1.5sqmm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P3" (at 0 -3.15) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 3.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.9 3.9) (drill 2.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.064103)
      (net 2 "VCC") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm" (layer "F.Cu")
    (at 113.284 90.678)
    (descr "Soldered wire connection, for a single 1.5 mm² wire, reinforced insulation, conductor diameter 1.7mm, outer diameter 3.9mm, size source Multi-Contact FLEXI-xV 1.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 1.5sqmm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P4" (at 0 -3.15) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 3.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.9 3.9) (drill 2.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.064103)
      (net 12 "Net-(P4-P1)") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm" (layer "F.Cu")
    (at 123.444 90.678)
    (descr "Soldered wire connection, for a single 1.5 mm² wire, reinforced insulation, conductor diameter 1.7mm, outer diameter 3.9mm, size source Multi-Contact FLEXI-xV 1.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 1.5sqmm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P5" (at 0 -3.15) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 3.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.9 3.9) (drill 2.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.064103)
      (net 5 "Net-(P5-P1)") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm" (layer "F.Cu")
    (at 131.445 127.635)
    (descr "Soldered wire connection, for a single 1.5 mm² wire, reinforced insulation, conductor diameter 1.7mm, outer diameter 3.9mm, size source Multi-Contact FLEXI-xV 1.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 1.5sqmm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "IN1" (at 0 -3.15) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 3.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.9 3.9) (drill 2.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.064103)
      (net 16 "Net-(IN1-P1)") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm" (layer "F.Cu")
    (at 131.064 90.678)
    (descr "Soldered wire connection, for a single 1.5 mm² wire, reinforced insulation, conductor diameter 1.7mm, outer diameter 3.9mm, size source Multi-Contact FLEXI-xV 1.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 1.5sqmm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P6" (at 0 -3.15) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 3.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.9 3.9) (drill 2.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.064103)
      (net 1 "GND") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm" (layer "F.Cu")
    (at 141.605 90.805)
    (descr "Soldered wire connection, for a single 1.5 mm² wire, reinforced insulation, conductor diameter 1.7mm, outer diameter 3.9mm, size source Multi-Contact FLEXI-xV 1.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 1.5sqmm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P7" (at 0 -3.15) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 3.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.9 3.9) (drill 2.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.064103)
      (net 1 "GND") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm" (layer "F.Cu")
    (at 150.495 90.805)
    (descr "Soldered wire connection, for a single 1.5 mm² wire, reinforced insulation, conductor diameter 1.7mm, outer diameter 3.9mm, size source Multi-Contact FLEXI-xV 1.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 1.5sqmm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P8" (at 0 -3.15) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 3.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.9 3.9) (drill 2.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.064103)
      (net 7 "Net-(P8-P1)") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm" (layer "F.Cu")
    (at 159.385 90.805)
    (descr "Soldered wire connection, for a single 1.5 mm² wire, reinforced insulation, conductor diameter 1.7mm, outer diameter 3.9mm, size source Multi-Contact FLEXI-xV 1.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 1.5sqmm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P9" (at 0 -3.15) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 3.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.9 3.9) (drill 2.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.064103)
      (net 6 "Net-(P9-P1)") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm" (layer "F.Cu")
    (at 168.148 90.678)
    (descr "Soldered wire connection, for a single 1.5 mm² wire, reinforced insulation, conductor diameter 1.7mm, outer diameter 3.9mm, size source Multi-Contact FLEXI-xV 1.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 1.5sqmm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P10" (at 0 -3.15) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 3.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.9 3.9) (drill 2.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.064103)
      (net 11 "Net-(P10-P1)") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm" (layer "F.Cu")
    (at 104.775 105.41)
    (descr "Soldered wire connection, for a single 1.5 mm² wire, reinforced insulation, conductor diameter 1.7mm, outer diameter 3.9mm, size source Multi-Contact FLEXI-xV 1.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 1.5sqmm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "Ant1" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 3.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.9 3.9) (drill 2.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.064103)
      (net 10 "Net-(Ant1-P1)") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (at 104.775 97.79 -90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (attr through_hole)
    (fp_text reference "Q1" (at 1.27 -3.56 -90) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 1.27 2.79 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 270) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(Ant1-P1)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.54 0 270) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(Q1-C)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 111.252 97.028)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 12.573 -1.143) (layer "F.SilkS"))
    (fp_text value "R" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(P4-P1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 121.412 100.584 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at -2.413 1.524 180) (layer "F.SilkS"))
    (fp_text value "R" (at 5.08 2.37 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(Q1-C)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 123.825 104.14 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at 12.065 0) (layer "F.SilkS"))
    (fp_text value "R" (at 5.08 2.37 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(U1-DIS)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 108.585 119.38 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R4" (at -1.905 0 180) (layer "F.SilkS"))
    (fp_text value "R" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(R4-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(U1-Q)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm_Socket" (layer "F.Cu")
    (at 112.395 104.775)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 8.89 10.16) (layer "F.SilkS"))
    (fp_text value "LM555N" (at 3.81 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 4.445) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(Q1-C)") (pinfunction "TR") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(U1-Q)") (pinfunction "Q") (pintype "output"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "R") (pintype "input"))
    (pad "5" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "unconnected-(U1-CV-Pad5)") (pinfunction "CV") (pintype "input"))
    (pad "6" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(U1-DIS)") (pinfunction "THR") (pintype "input"))
    (pad "7" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(U1-DIS)") (pinfunction "DIS") (pintype "input"))
    (pad "8" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_Power_L25.0mm_W9.0mm_P30.48mm" (layer "F.Cu")
    (at 168.275 120.015 180)
    (descr "Resistor, Axial_Power series, Box, pin pitch=30.48mm, 7W, length*width*height=25*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
    (tags "Resistor Axial_Power series Box pin pitch 30.48mm 7W length 25mm width 9mm height 9mm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R5" (at 30.48 -3.175) (layer "F.SilkS"))
    (fp_text value "R" (at 15.24 5.62) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 15.24 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(P8-P1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 30.48 0 180) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L25.0mm_W9.0mm_P30.48mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_Power_L25.0mm_W9.0mm_P30.48mm" (layer "F.Cu")
    (at 168.275 130.175 180)
    (descr "Resistor, Axial_Power series, Box, pin pitch=30.48mm, 7W, length*width*height=25*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
    (tags "Resistor Axial_Power series Box pin pitch 30.48mm 7W length 25mm width 9mm height 9mm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R6" (at 30.48 -3.81) (layer "F.SilkS"))
    (fp_text value "R" (at 15.24 5.62) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 15.24 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(P8-P1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 30.48 0 180) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L25.0mm_W9.0mm_P30.48mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_Power_L25.0mm_W9.0mm_P30.48mm" (layer "F.Cu")
    (at 168.275 99.695 180)
    (descr "Resistor, Axial_Power series, Box, pin pitch=30.48mm, 7W, length*width*height=25*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
    (tags "Resistor Axial_Power series Box pin pitch 30.48mm 7W length 25mm width 9mm height 9mm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R7" (at 30.48 -3.81) (layer "F.SilkS"))
    (fp_text value "R" (at 15.24 5.62) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 15.24 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(P10-P1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 30.48 0 180) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(P9-P1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L25.0mm_W9.0mm_P30.48mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_Power_L25.0mm_W9.0mm_P30.48mm" (layer "F.Cu")
    (at 168.275 109.855 180)
    (descr "Resistor, Axial_Power series, Box, pin pitch=30.48mm, 7W, length*width*height=25*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
    (tags "Resistor Axial_Power series Box pin pitch 30.48mm 7W length 25mm width 9mm height 9mm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R8" (at 30.48 -3.81) (layer "F.SilkS"))
    (fp_text value "R" (at 15.24 5.62) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 15.24 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(P10-P1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 30.48 0 180) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(P9-P1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L25.0mm_W9.0mm_P30.48mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kicad-SDS-footprints:polyfuse-2.5A" (layer "F.Cu")
    (at 172.085 100.33 -90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "F1" (at -4.445 2.54 -180) (layer "F.SilkS"))
    (fp_text value "FUSE" (at 5.08 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers "*.Cu" "*.SilkS" "*.Mask")
      (net 11 "Net-(P10-P1)") (pintype "input"))
    (pad "2" thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers "*.Cu" "*.SilkS" "*.Mask")
      (net 5 "Net-(P5-P1)") (pintype "input"))
    (model "Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl"
      (offset (xyz 5.079999924 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown" (layer "F.Cu")
    (at 120.355 131.445 90)
    (descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 2.54 -20.58 90) (layer "F.SilkS"))
    (fp_text value "TRIAC" (at 2.54 2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -20.58 90) (layer "F.Fab"))
    (pad "" np_thru_hole oval (at 2.54 -16.66 90) (size 3.5 3.5) (drill 3.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(P10-P1)") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(R4-Pad1)") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L18.0mm_W9.0mm_P15.00mm_FKS3_FKP3" (layer "F.Cu")
    (at 130.81 111.76 90)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*9mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 9mm Capacitor")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C5" (at -3.175 -1.905 180) (layer "F.SilkS"))
    (fp_text value "C" (at 7.5 5.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(P9-P1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 15 0 90) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(P8-P1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W9.0mm_P15.00mm_FKS3_FKP3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "sdsLogos:sdsLabs-medium-fSilk" (layer "F.Cu")
    (at 91.44 127.8128 90)
    (attr through_hole)
    (fp_text reference "G***" (at 0 -3.81 90) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0 -2.54 90) (layer "F.SilkS") hide)
  )
  (footprint "Diode_THT:Diode_Bridge_DIP-4_W7.62mm_P5.08mm" (layer "F.Cu")
    (at 93.218 103.4796 90)
    (descr "4-lead dip package for diode bridges, row spacing 7.62 mm (300 mils), see http://cdn-reichelt.de/documents/datenblatt/A400/HDBL101G_20SERIES-TSC.pdf")
    (tags "DIL DIP PDIP 5.08mm 7.62mm 300mil")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Miniature Glass Passivated Single-Phase Bridge Rectifiers, 280V Vrms, 1.0A If, DIP-4")
    (property "ki_keywords" "rectifier acdc")
    (attr through_hole)
    (fp_text reference "D1" (at 3.8 -2.7 90) (layer "F.SilkS"))
    (fp_text value "DF04M" (at 3.8 7.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.005 1.735 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "-") (pintype "passive"))
    (pad "3" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(P2-P1)") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(P1-P1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/Diode_Bridge_DIP-4_W7.62mm_P5.08mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 98.75 142.85)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "sdsLogos:sdsLabs-large-bSilk" (layer "F.Cu")
    (at 114.4016 142.7988)
    (attr through_hole)
    (fp_text reference "G***" (at 0 -7.62) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0 -5.08) (layer "B.SilkS") hide)
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 163.6 142.9)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_THT:CP_Radial_D18.0mm_P7.50mm" (layer "B.Cu")
    (at 149.345 104.14)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at -4.565 8.255) (layer "B.SilkS"))
    (fp_text value "C" (at 3.75 -10.25) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.15 2.54) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(IN1-P1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.5 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(P5-P1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L24.0mm_W12.8mm_P22.50mm_MKT" (layer "B.Cu")
    (at 164.74 130.175 180)
    (descr "C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*12.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf")
    (tags "C Rect series Radial pin pitch 22.50mm  length 24mm width 12.8mm Capacitor")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C4" (at 26.31 -5.715) (layer "B.SilkS"))
    (fp_text value "C" (at 11.25 -7.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 15.515 -0.635) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(P5-P1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 22.5 0 180) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(IN1-P1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L24.0mm_W12.8mm_P22.50mm_MKT.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_Power_L38.0mm_W9.0mm_P40.64mm" (layer "B.Cu")
    (at 131.445 118.745)
    (descr "Resistor, Axial_Power series, Box, pin pitch=40.64mm, 9W, length*width*height=38*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
    (tags "Resistor Axial_Power series Box pin pitch 40.64mm 9W length 38mm width 9mm height 9mm")
    (property "Sheetfile" "esl63_clamp_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R9" (at -2.54 2.54) (layer "B.SilkS"))
    (fp_text value "R" (at 20.32 -5.62) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(IN1-P1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 40.64 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(P5-P1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L38.0mm_W9.0mm_P40.64mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 88.265 86.36) (end 88.265 148.59)
    (layer "Edge.Cuts"))
  (gr_line (start 173.99 86.36) (end 88.265 86.36)
    (layer "Edge.Cuts"))
  (gr_line (start 88.265 148.59) (end 173.99 148.59)
    (layer "Edge.Cuts"))
  (gr_line (start 173.99 148.59) (end 173.99 86.36)
    (layer "Edge.Cuts"))
  (gr_text "ESL-63 Clamp Board" (at 158.115 144.145) (layer "B.SilkS"))
  (gr_text "ESL-63 Clamp Board" (at 95.25 135.89 90) (layer "F.SilkS"))
)
