(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 71.12 90.17)
    (grid_origin 71.12 90.17)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./")
    )
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(D2-Pad2)")
  (net 4 "Net-(D14-Pad2)")
  (net 5 "Net-(D5-Pad2)")
  (net 6 "Net-(D6-Pad2)")
  (net 7 "Net-(D7-Pad2)")
  (net 8 "Net-(D8-Pad2)")
  (net 9 "Net-(D10-Pad1)")
  (net 10 "Net-(D10-Pad2)")
  (net 11 "Net-(D11-Pad2)")
  (net 12 "Net-(D12-Pad2)")
  (net 13 "Net-(D13-Pad2)")
  (footprint "Connector_Wire:SolderWirePad_1x01_Drill2.5mm" (layer "F.Cu")
    (tedit 62DC8131)
    (at 74.29754 85.09)
    (descr "Wire solder connection")
    (tags "connector")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -5.08) (layer "F.SilkS") hide)
    (fp_text value "SolderWirePad_1x01_Drill2.5mm" (at 0 5.08) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 4 4) (drill 3.25) (layers *.Cu *.Mask))
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_Drill2.5mm" (layer "F.Cu")
    (tedit 62DC812B)
    (at 74.29754 33.02)
    (descr "Wire solder connection")
    (tags "connector")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -5.08) (layer "F.SilkS") hide)
    (fp_text value "SolderWirePad_1x01_Drill2.5mm" (at 0 5.08) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 4 4) (drill 3.25) (layers *.Cu *.Mask))
  )
  (footprint "kicad-SDS-footprints:DO-214ac" (layer "F.Cu")
    (tedit 579426A1)
    (at 81.21904 88.265 180)
    (attr through_hole)
    (fp_text reference "D14" (at 0.0635 1.143 180) (layer "F.SilkS"))
    (fp_text value "ZENER" (at 2.54 1.016 270) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 3.302 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(D13-Pad2)"))
    (pad "2" smd rect locked (at 0 -1.143 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(D14-Pad2)"))
  )
  (footprint "kicad-SDS-footprints:DO-214ac" (layer "F.Cu")
    (tedit 5794269C)
    (at 81.21904 81.915 180)
    (attr through_hole)
    (fp_text reference "D13" (at 0 1.016) (layer "F.SilkS"))
    (fp_text value "ZENER" (at 2.54 1.016 270) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 3.302 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(D12-Pad2)"))
    (pad "2" smd rect locked (at 0 -1.143 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(D13-Pad2)"))
  )
  (footprint "kicad-SDS-footprints:DO-214ac" (layer "F.Cu")
    (tedit 57942696)
    (at 81.21904 75.565 180)
    (attr through_hole)
    (fp_text reference "D12" (at 0 1.0795) (layer "F.SilkS"))
    (fp_text value "ZENER" (at 2.54 1.016 270) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 3.302 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(D11-Pad2)"))
    (pad "2" smd rect locked (at 0 -1.143 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(D12-Pad2)"))
  )
  (footprint "kicad-SDS-footprints:DO-214ac" (layer "F.Cu")
    (tedit 57942691)
    (at 81.21904 69.215 180)
    (attr through_hole)
    (fp_text reference "D11" (at 0 0.9525) (layer "F.SilkS"))
    (fp_text value "ZENER" (at 2.54 1.016 270) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 3.302 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D10-Pad2)"))
    (pad "2" smd rect locked (at 0 -1.143 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(D11-Pad2)"))
  )
  (footprint "Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10" (layer "F.Cu")
    (tedit 5DEDAB0E)
    (at 85.725 41.91 -90)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (attr through_hole)
    (fp_text reference "D2" (at 5.715 0) (layer "F.SilkS"))
    (fp_text value "D" (at 4.37134 -3.55854 -90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect locked (at 0 -0.00254 90) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask "F.SilkS")
      (net 2 "Net-(D1-Pad1)"))
    (pad "2" thru_hole circle locked (at 10.16 -0.00254 90) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask "F.SilkS")
      (net 3 "Net-(D2-Pad2)"))
  )
  (footprint "Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10" (layer "F.Cu")
    (tedit 5DEDAB1B)
    (at 75.50404 65.405 -90)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (attr through_hole)
    (fp_text reference "D3" (at 5.715 0) (layer "F.SilkS"))
    (fp_text value "D" (at 4.37134 -3.55854 -90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect locked (at 0 -0.00254 90) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask "F.SilkS")
      (net 1 "Net-(D1-Pad2)"))
    (pad "2" thru_hole circle locked (at 10.16 -0.00254 90) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask "F.SilkS")
      (net 4 "Net-(D14-Pad2)"))
  )
  (footprint "Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10" (layer "F.Cu")
    (tedit 5DEDAB20)
    (at 85.725 65.405 -90)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (attr through_hole)
    (fp_text reference "D4" (at 5.715 0) (layer "F.SilkS"))
    (fp_text value "D" (at 4.37134 -3.55854 -90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect locked (at 0 -0.00254 90) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask "F.SilkS")
      (net 3 "Net-(D2-Pad2)"))
    (pad "2" thru_hole circle locked (at 10.16 -0.00254 90) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask "F.SilkS")
      (net 4 "Net-(D14-Pad2)"))
  )
  (footprint "Wire_Pads:SolderWirePad_single_1-2mmDrill" (layer "F.Cu")
    (tedit 5DEDAAEB)
    (at 74.86904 58.42)
    (attr through_hole)
    (fp_text reference "P1" (at 2.34696 2.286 180) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at -1.905 3.175) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 3.50012 3.50012) (drill 2) (layers *.Cu *.Mask "F.SilkS")
      (net 1 "Net-(D1-Pad2)"))
  )
  (footprint "Wire_Pads:SolderWirePad_single_1-2mmDrill" (layer "F.Cu")
    (tedit 5DEDAAF3)
    (at 86.36 58.42)
    (attr through_hole)
    (fp_text reference "P2" (at -1.905 2.54 180) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at -1.905 3.175) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 3.50012 3.50012) (drill 2) (layers *.Cu *.Mask "F.SilkS")
      (net 3 "Net-(D2-Pad2)"))
  )
  (footprint "kicad-SDS-footprints:DO-214ac" (layer "F.Cu")
    (tedit 5794266E)
    (at 81.21904 31.115 180)
    (attr through_hole)
    (fp_text reference "D5" (at 0 1.0795) (layer "F.SilkS"))
    (fp_text value "ZENER" (at 2.54 1.016 270) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 3.302 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(D1-Pad1)"))
    (pad "2" smd rect locked (at 0 -1.143 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(D5-Pad2)"))
  )
  (footprint "kicad-SDS-footprints:DO-214ac" (layer "F.Cu")
    (tedit 57942673)
    (at 81.21904 37.465 180)
    (attr through_hole)
    (fp_text reference "D6" (at -0.0635 1.016) (layer "F.SilkS"))
    (fp_text value "ZENER" (at 2.54 1.016 270) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 3.302 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(D5-Pad2)"))
    (pad "2" smd rect locked (at 0 -1.143 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(D6-Pad2)"))
  )
  (footprint "kicad-SDS-footprints:DO-214ac" (layer "F.Cu")
    (tedit 5794267D)
    (at 81.21904 43.815 180)
    (attr through_hole)
    (fp_text reference "D7" (at -0.127 0.9525) (layer "F.SilkS"))
    (fp_text value "ZENER" (at 2.54 1.016 270) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 3.302 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(D6-Pad2)"))
    (pad "2" smd rect locked (at 0 -1.143 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(D7-Pad2)"))
  )
  (footprint "kicad-SDS-footprints:DO-214ac" (layer "F.Cu")
    (tedit 57942681)
    (at 81.21904 50.165 180)
    (attr through_hole)
    (fp_text reference "D8" (at -0.127 0.9525) (layer "F.SilkS"))
    (fp_text value "ZENER" (at 2.54 1.016 270) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 3.302 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(D7-Pad2)"))
    (pad "2" smd rect locked (at 0 -1.143 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D8-Pad2)"))
  )
  (footprint "kicad-SDS-footprints:DO-214ac" (layer "F.Cu")
    (tedit 57942688)
    (at 81.21904 56.515 180)
    (attr through_hole)
    (fp_text reference "D9" (at 0 1.016 180) (layer "F.SilkS"))
    (fp_text value "ZENER" (at 2.54 1.016 270) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 3.302 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D8-Pad2)"))
    (pad "2" smd rect locked (at 0 -1.143 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D10-Pad1)"))
  )
  (footprint "kicad-SDS-footprints:DO-214ac" (layer "F.Cu")
    (tedit 5794268D)
    (at 81.21904 62.865 180)
    (attr through_hole)
    (fp_text reference "D10" (at 0 1.0795) (layer "F.SilkS"))
    (fp_text value "ZENER" (at 2.54 1.016 270) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 3.302 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D10-Pad1)"))
    (pad "2" smd rect locked (at 0 -1.143 180) (size 2.21 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D10-Pad2)"))
  )
  (footprint "Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10" (layer "F.Cu")
    (tedit 5DEDAB16)
    (at 75.50404 41.91 -90)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (attr through_hole)
    (fp_text reference "D1" (at 5.715 0) (layer "F.SilkS"))
    (fp_text value "D" (at 4.37134 -3.55854 -90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect locked (at 0 -0.00254 90) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask "F.SilkS")
      (net 2 "Net-(D1-Pad1)"))
    (pad "2" thru_hole circle locked (at 10.16 -0.00254 90) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask "F.SilkS")
      (net 1 "Net-(D1-Pad2)"))
  )
  (footprint "sdsLogos:sdsLabs-large-bSilk" (layer "F.Cu")
    (tedit 5A94A1E6)
    (at 81.28254 69.85 -90)
    (attr through_hole)
    (fp_text reference "G***" (at 0 -7.62 90) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0 -5.08 90) (layer "B.SilkS") hide)
  )
  (gr_line (start 88.265 26.67) (end 88.265 90.17) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 71.12254 26.67) (end 88.265 26.67) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 88.265 90.17) (end 71.12254 90.17) (layer "Edge.Cuts") (width 0.15))
  (gr_circle (center 74.168 85.09) (end 74.168 83.82) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_line (start 71.12254 26.67) (end 71.12254 90.17) (layer "Edge.Cuts") (width 0.15))
  (gr_circle (center 74.168 33.02) (end 74.168 31.75) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_text "ESL Clamp Board" (at 80.64754 48.895 270) (layer "B.SilkS"))
)
