(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" power)
    (2 "In2.Cu" power)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "prepreg") (color "FR4 natural") (thickness 0.48) (material "FR408-HR") (epsilon_r 3.69) (loss_tangent 0.0091))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "core") (color "FR4 natural") (thickness 0.48) (material "FR408-HR") (epsilon_r 3.69) (loss_tangent 0.0091))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "prepreg") (color "FR4 natural") (thickness 0.48) (material "FR408-HR") (epsilon_r 3.69) (loss_tangent 0.0091))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (grid_origin 39.37 96.012)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(U1-VOUT+)")
  (net 2 "Net-(U1-VOUT-)")
  (net 3 "Net-(U2-VOUT+)")
  (net 4 "Net-(U7-ENBL)")
  (net 5 "Net-(U7-INH)")
  (net 6 "GND")
  (net 7 "VCC3V3")
  (net 8 "VCC5V0")
  (net 9 "Net-(U7-VOH)")
  (net 10 "Net-(C13-Pad2)")
  (net 11 "Net-(U7-VIP)")
  (net 12 "Net-(U7-LOP)")
  (net 13 "Net-(U7-LMD2)")
  (net 14 "Net-(U7-VIN)")
  (net 15 "Net-(U7-LON)")
  (net 16 "Net-(U7-VCM)")
  (net 17 "Net-(U7-VPOS)")
  (net 18 "Net-(U7-CLMP)")
  (net 19 "Net-(C10-Pad2)")
  (net 20 "Net-(U7-VOL)")
  (net 21 "Net-(C11-Pad1)")
  (net 22 "GNDA")
  (net 23 "Net-(C24-Pad1)")
  (net 24 "Net-(U7-GAIN)")
  (net 25 "Net-(U9-VREF)")
  (net 26 "Net-(C27-Pad2)")
  (net 27 "Net-(U9-REFB)")
  (net 28 "Net-(U9-REFT)")
  (net 29 "Net-(U9-VIN+)")
  (net 30 "ADC_CLK")
  (net 31 "Net-(U9-VIN-)")
  (net 32 "VDDA")
  (net 33 "Net-(U6-INH)")
  (net 34 "Net-(U6-BYP)")
  (net 35 "ADC_OR")
  (net 36 "VCC")
  (net 37 "Net-(U8-SS)")
  (net 38 "Net-(J24-Pin_1)")
  (net 39 "Net-(U8-FB)")
  (net 40 "5Vclean")
  (net 41 "Net-(D1-A)")
  (net 42 "Net-(D2-A)")
  (net 43 "Net-(D4-A)")
  (net 44 "Net-(D5-A)")
  (net 45 "Net-(D6-A)")
  (net 46 "VGA_GAIN")
  (net 47 "VGA_HILO")
  (net 48 "GlitchLP")
  (net 49 "Glitch")
  (net 50 "ADC_D0")
  (net 51 "ADC_D1")
  (net 52 "ADC_D2")
  (net 53 "ADC_D3")
  (net 54 "ADC_D4")
  (net 55 "ADC_D9")
  (net 56 "ADC_D8")
  (net 57 "ADC_D7")
  (net 58 "ADC_D6")
  (net 59 "ADC_D5")
  (net 60 "Trigger")
  (net 61 "PWR0")
  (net 62 "PWR1")
  (net 63 "PWR2")
  (net 64 "PWR3")
  (net 65 "PWR4")
  (net 66 "PWR5")
  (net 67 "unconnected-(D7-K-Pad3)")
  (net 68 "Net-(D8-A)")
  (net 69 "Net-(D9-A)")
  (net 70 "/Power/-7V8P")
  (net 71 "/Power/+7V8P")
  (net 72 "Net-(D10-A)")
  (net 73 "/Power/GNDP")
  (net 74 "Net-(D11-K)")
  (net 75 "/Power/3V3P")
  (net 76 "Net-(D12-K)")
  (net 77 "Net-(J2-In)")
  (net 78 "PWR_PG")
  (net 79 "PWR_EN")
  (net 80 "unconnected-(J7-Pin_1-Pad1)")
  (net 81 "/Ardu/A0")
  (net 82 "/Ardu/A1")
  (net 83 "/Ardu/A2")
  (net 84 "CSM3V3Gain0")
  (net 85 "/Ardu/A3")
  (net 86 "CSM3V3Gain1")
  (net 87 "CSM3V3Cur")
  (net 88 "CSM5VCur")
  (net 89 "CSM5VGain0")
  (net 90 "CSM5VGain1")
  (net 91 "unconnected-(J7-Pin_3-Pad3)")
  (net 92 "Net-(J10-In)")
  (net 93 "Net-(J11-Pin_3)")
  (net 94 "Net-(J13-In)")
  (net 95 "Net-(J28-Pin_1)")
  (net 96 "Net-(Q1-G)")
  (net 97 "VU_CK")
  (net 98 "/Ardu/A4")
  (net 99 "CSMVarGain1")
  (net 100 "/Ardu/A5")
  (net 101 "CSMVarGain0")
  (net 102 "CSMVarCur")
  (net 103 "FD2C_CLK")
  (net 104 "FC_RST")
  (net 105 "FC2D_CLK")
  (net 106 "FC_IO")
  (net 107 "FD_VREF")
  (net 108 "FD_TF")
  (net 109 "FC_DIO0")
  (net 110 "FC2D_HS")
  (net 111 "FC_DIO1")
  (net 112 "FD2C_HS")
  (net 113 "FC_DIO2")
  (net 114 "FC_PROG")
  (net 115 "FC_DIO3")
  (net 116 "FC_5V")
  (net 117 "FC_3V3")
  (net 118 "FC_Var")
  (net 119 "Net-(Q2-G)")
  (net 120 "Net-(Q3-D)")
  (net 121 "Net-(U3-ADJ)")
  (net 122 "/Ardu/JA2_P")
  (net 123 "/Ardu/JA2_N")
  (net 124 "Net-(U4-ADJ)")
  (net 125 "Net-(U9-MODE)")
  (net 126 "unconnected-(J17-Pad3)")
  (net 127 "unconnected-(U2-0V-Pad5)")
  (net 128 "unconnected-(U3-NC-Pad5)")
  (net 129 "unconnected-(U3-NC-Pad8)")
  (net 130 "unconnected-(U4-NC-Pad5)")
  (net 131 "unconnected-(U4-NC-Pad8)")
  (net 132 "unconnected-(U5-BYP-Pad4)")
  (net 133 "/Ardu/AR_IO0")
  (net 134 "/Ardu/SDA")
  (net 135 "/Ardu/MISO")
  (net 136 "/Ardu/SCK")
  (net 137 "Net-(D14-A)")
  (net 138 "Net-(D3-K)")
  (net 139 "Net-(D14-K)")
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 92.456 67.183546 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "dutconnect.kicad_sch")
    (property "Sheetname" "dutconnect")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -2.920454 0 90) (layer "F.SilkS"))
    (fp_text value "1R" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Glitch") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "Net-(Q1-G)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "cerg:SMA-JOHNSON-142-0701-801" (layer "F.Cu")
    (at 44.958 8.382)
    (property "Sheetfile" "dutconnect.kicad_sch")
    (property "Sheetname" "dutconnect")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr through_hole)
    (fp_text reference "J14" (at 6.604 0 270) (layer "F.SilkS"))
    (fp_text value "Trigger" (at 0 -3.6 180) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 2.3 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "Trigger") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect (at -4.4 0) (size 2.4 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at -4.4 0) (size 2.4 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 4.4 0) (size 2.4 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 4.4 0) (size 2.4 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KIPRJMOD}/cerg_3d_models/SMA_Board_Edge_Molex_732511150.step"
      (offset (xyz 0 2.54 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
    (model "${KIPRJMOD}/cerg_3d_models/SMA_Board_Edge_Molex_732511150.wrl"
      (offset (xyz 0 2.54 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "cerg:SMA-JOHNSON-142-0701-801" (layer "F.Cu")
    (at 105.41 68.072 -90)
    (property "Sheetfile" "dutconnect.kicad_sch")
    (property "Sheetname" "dutconnect")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr through_hole)
    (fp_text reference "J2" (at -5.842 3.556) (layer "F.SilkS"))
    (fp_text value "Glitch" (at 0 -3.6 90) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 270) (size 2.3 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "Net-(J2-In)") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect (at -4.4 0 270) (size 2.4 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at -4.4 0 270) (size 2.4 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 4.4 0 270) (size 2.4 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 4.4 0 270) (size 2.4 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KIPRJMOD}/cerg_3d_models/SMA_Board_Edge_Molex_732511150.step"
      (offset (xyz 0 2.54 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
    (model "${KIPRJMOD}/cerg_3d_models/SMA_Board_Edge_Molex_732511150.wrl"
      (offset (xyz 0 2.54 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 93.98 67.183546 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "dutconnect.kicad_sch")
    (property "Sheetname" "dutconnect")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 2.920454 0 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "Net-(Q1-G)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 72.156 66.675 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C54" (at -2.159 -0.528 180) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "VCC5V0") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 78.74 90.424 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ardu.kicad_sch")
    (property "Sheetname" "Ardu")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R29" (at 0.0255 -1.27 90) (layer "F.SilkS"))
    (fp_text value "1k69 1%" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "/Ardu/A3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "FC_5V") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "cerg:BarrelJack_CUI_PJ-102AH_Horizontal" (layer "F.Cu")
    (at 50.65 82.562 -90)
    (descr "Thin-pin DC Barrel Jack, https://cdn-shop.adafruit.com/datasheets/21mmdcjackDatasheet.pdf")
    (tags "Power Jack")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "DC Barrel Jack with an internal switch")
    (property "ki_keywords" "DC power barrel jack connector")
    (attr through_hole)
    (fp_text reference "J17" (at 6.096 -0.508) (layer "F.SilkS"))
    (fp_text value "Barrel_Jack_Switch" (at -5.2545 6.122) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.5 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.6 2.6) (drill 1.6) (layers "*.Cu" "*.Mask")
      (net 74 "Net-(D11-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 6 270) (size 2.6 2.6) (drill 1.6) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pintype "passive"))
    (pad "3" thru_hole circle (at 4.7 3 270) (size 2.6 2.6) (drill 1.6) (layers "*.Cu" "*.Mask")
      (net 126 "unconnected-(J17-Pad3)") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-102AH_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/cerg_3d_models/CUI_PJ-102AH.step"
      (offset (xyz 0 -13.6 6))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (at 81.203 60.579 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D9" (at 0 -1.447 90) (layer "F.SilkS"))
    (fp_text value "green" (at 0 1.43 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(D9-A)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 100.838 13.208)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C47" (at 3.048 -1.778) (layer "F.SilkS"))
    (fp_text value "10n" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "VCC5V0") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 100.838 10.16 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C48" (at -3.0225 1.524) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "5Vclean") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2" (layer "F.Cu")
    (at 76.556 52.8445)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "800mA Fixed Low Drop Positive Voltage Regulator, Fixed Output 3.3V, SOT-223")
    (property "ki_keywords" "REGULATOR LDO 3.3V")
    (attr smd)
    (fp_text reference "U12" (at -0.102 -4.3305) (layer "F.SilkS"))
    (fp_text value "LD1117S33TR_SOT223" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -2.3) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd rect (at -3.15 0) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "Net-(D14-A)") (pinfunction "VO") (pintype "power_out"))
    (pad "2" smd rect (at 3.15 0) (size 2 3.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "Net-(D14-A)") (pinfunction "VO") (pintype "power_out"))
    (pad "3" smd rect (at -3.15 2.3) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "VCC") (pinfunction "VI") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (at 91.63 50.2575 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D10" (at -0.0255 1.524 90) (layer "F.SilkS"))
    (fp_text value "green" (at 0 1.43 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(D10-A)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 71.324 54.343 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C57" (at 3.035 0.05 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded" (layer "F.Cu")
    (at 40.64 26.67)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (property "Sheetfile" "dutconnect.kicad_sch")
    (property "Sheetname" "dutconnect")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J22" (at 0 2.794) (layer "F.SilkS"))
    (fp_text value "GND" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:MSOP-8_3x3mm_P0.65mm" (layer "F.Cu")
    (at 76.22 66.675)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (attr smd)
    (fp_text reference "U10" (at 4.806 0.127 90) (layer "F.SilkS"))
    (fp_text value "INA225" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.2 -0.975) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "VCC") (pinfunction "Vin+") (pintype "input"))
    (pad "2" smd rect (at -2.2 -0.325) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -2.2 0.325) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "VCC5V0") (pinfunction "Vs") (pintype "power_in"))
    (pad "4" smd rect (at -2.2 0.975) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "CSM5VCur") (pinfunction "Out") (pintype "passive"))
    (pad "5" smd rect (at 2.2 0.975) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "CSM5VGain0") (pinfunction "GS0") (pintype "input"))
    (pad "6" smd rect (at 2.2 0.325) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "CSM5VGain1") (pinfunction "GS1") (pintype "input"))
    (pad "7" smd rect (at 2.2 -0.325) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "Ref") (pintype "input"))
    (pad "8" smd rect (at 2.2 -0.975) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "FC_5V") (pinfunction "Vin-") (pintype "input"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/MSOP-8_3x3mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (at 68.082 60.452 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D12" (at 0 -1.514 -90) (layer "F.SilkS"))
    (fp_text value "green" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(D12-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "VCC3V3") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 86.55 53.28)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R32" (at -2.476 0 270) (layer "F.SilkS"))
    (fp_text value "0R1" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 137 "Net-(D14-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 117 "FC_3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (at 100.838 11.684)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Inductor with ferrite core")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L5" (at 2.54 -1.778) (layer "F.SilkS"))
    (fp_text value "1k/500mA" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "5Vclean") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "VCC5V0") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 85.27 50.232 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J19" (at 0 5.08 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 0 4.87 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 137 "Net-(D14-A)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 117 "FC_3V3") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 77.47 35.052)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "dutconnect.kicad_sch")
    (property "Sheetname" "dutconnect")
    (property "ki_description" "Jumper, 3-pole, both open")
    (property "ki_keywords" "Jumper SPDT")
    (attr through_hole)
    (fp_text reference "JP2" (at -0.254 7.62) (layer "F.SilkS"))
    (fp_text value "ExtClkSel" (at 0 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 103 "FD2C_CLK") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 94 "Net-(J13-In)") (pinfunction "C") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 105 "FC2D_CLK") (pinfunction "B") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 100.838 8.636 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C49" (at 0 1.524) (layer "F.SilkS"))
    (fp_text value "2u2" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "5Vclean") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 73.66 90.3985 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ardu.kicad_sch")
    (property "Sheetname" "Ardu")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R31" (at 0 -1.27 90) (layer "F.SilkS"))
    (fp_text value "1k69 1%" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "/Ardu/A1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "FC_Var") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "cerg:SMA-JOHNSON-142-0701-801" (layer "F.Cu")
    (at 105.41 17.907 -90)
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr through_hole)
    (fp_text reference "J10" (at 6.731 0) (layer "F.SilkS"))
    (fp_text value "ADCin" (at 0 -3.6 90) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 270) (size 2.3 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "Net-(J10-In)") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect (at -4.4 0 270) (size 2.4 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "GNDA") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at -4.4 0 270) (size 2.4 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "GNDA") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 4.4 0 270) (size 2.4 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "GNDA") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 4.4 0 270) (size 2.4 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "GNDA") (pinfunction "Ext") (pintype "passive"))
    (model "${KIPRJMOD}/cerg_3d_models/SMA_Board_Edge_Molex_732511150.step"
      (offset (xyz 0 2.54 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
    (model "${KIPRJMOD}/cerg_3d_models/SMA_Board_Edge_Molex_732511150.wrl"
      (offset (xyz 0 2.54 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 57.912 17.5515 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C39" (at 3.0225 0 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.86718 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "VCC3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "cerg:QSOP-20_3.9x8.7mm_P0.635mm" (layer "F.Cu")
    (at 91.5797 16.7005 180)
    (descr "20-Lead Plastic Shrink Small Outline Narrow Body (http://www.analog.com/media/en/technical-documentation/data-sheets/ADuM7640_7641_7642_7643.pdf)")
    (tags "QSOP 0.635")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Ultralow Noise VGAs with Preamplifier and Programmable Rin")
    (property "ki_keywords" "Ultralow noise preamplifier")
    (attr smd)
    (fp_text reference "U7" (at -4.4323 -2.8575 90) (layer "F.SilkS"))
    (fp_text value "AD8331" (at -1.524 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.6543 -2.8575 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(U7-LMD2)") (pinfunction "LMD2") (pintype "input"))
    (pad "2" smd rect (at -2.6543 -2.2225 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(U7-INH)") (pinfunction "INH") (pintype "input"))
    (pad "3" smd rect (at -2.6543 -1.5875 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(U7-ENBL)") (pinfunction "VPS") (pintype "power_in"))
    (pad "4" smd rect (at -2.6543 -0.9525 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(U7-LON)") (pinfunction "LON") (pintype "input"))
    (pad "5" smd rect (at -2.6543 -0.3175 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(U7-LOP)") (pinfunction "LOP") (pintype "input"))
    (pad "6" smd rect (at -2.6543 0.3175 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "GNDA") (pinfunction "COML") (pintype "power_in"))
    (pad "7" smd rect (at -2.6543 0.9525 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(U7-VIP)") (pinfunction "VIP") (pintype "input"))
    (pad "8" smd rect (at -2.6543 1.5875 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(U7-VIN)") (pinfunction "VIN") (pintype "input"))
    (pad "9" smd rect (at -2.6543 2.2225 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "GNDA") (pinfunction "MODE") (pintype "input"))
    (pad "10" smd rect (at -2.6543 2.8575 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(U7-GAIN)") (pinfunction "GAIN") (pintype "input"))
    (pad "11" smd rect (at 2.6543 2.8575 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(U7-VCM)") (pinfunction "VCM") (pintype "output"))
    (pad "12" smd rect (at 2.6543 2.2225 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(U7-CLMP)") (pinfunction "CLMP") (pintype "input"))
    (pad "13" smd rect (at 2.6543 1.5875 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "VGA_HILO") (pinfunction "HILO") (pintype "input"))
    (pad "14" smd rect (at 2.6543 0.9525 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(U7-VPOS)") (pinfunction "VPOS") (pintype "power_in"))
    (pad "15" smd rect (at 2.6543 0.3175 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(U7-VOH)") (pinfunction "VOH") (pintype "output"))
    (pad "16" smd rect (at 2.6543 -0.3175 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(U7-VOL)") (pinfunction "VOL") (pintype "output"))
    (pad "17" smd rect (at 2.6543 -0.9525 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "GNDA") (pinfunction "COMM") (pintype "power_in"))
    (pad "18" smd rect (at 2.6543 -1.5875 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(U7-ENBL)") (pinfunction "ENBV") (pintype "input"))
    (pad "19" smd rect (at 2.6543 -2.2225 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(U7-ENBL)") (pinfunction "ENBL") (pintype "input"))
    (pad "20" smd rect (at 2.6543 -2.8575 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "GNDA") (pinfunction "COMM") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/QSOP-20_3.9x8.7mm_P0.635mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/QSOP-24_3.9x8.7mm_P0.635mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/QSOP-24_3.9x8.7mm_P0.635mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 84.984 23.1265 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R12" (at -3.0605 0 90) (layer "F.SilkS"))
    (fp_text value "2k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(U7-GAIN)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C27-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 76.454 15.699855 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R14" (at 3.235355 -16.51 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "VDDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(U9-VIN+)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 93.7005 23.982 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C8" (at 2.2605 0) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(U7-ENBL)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (at 85.471 9.1695 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Inductor with ferrite core")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L3" (at 2.3115 -0.127 90) (layer "F.SilkS"))
    (fp_text value "1k/500mA" (at -1.948 2.959 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(U7-VPOS)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "5Vclean") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 93.218 10.1345 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C17" (at -2.7685 0 90) (layer "F.SilkS"))
    (fp_text value "1nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(U7-VCM)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 74.93 12.600855 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R17" (at 3.184355 -16.51 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(U9-VIN-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 86.508 23.1265 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C26" (at 3.0605 0.106 90) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(U7-GAIN)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 65.786 9.070355 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R18" (at 0.254 1.524) (layer "F.SilkS"))
    (fp_text value "100R" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "ADC_CLK") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 79.59118 15.2145 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R8" (at -2.5655 0 90) (layer "F.SilkS"))
    (fp_text value "33R, 0.5%" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(U9-VIN+)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 73.406 15.699855 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C32" (at -3.235355 16.51 90) (layer "F.SilkS"))
    (fp_text value "100p" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(U9-VIN+)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 84.8105 11.43)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C23" (at -3.0225 1.524) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(U7-VPOS)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 66.8275 21.516355)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C35" (at -3.0225 -0.254) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(U9-REFT)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(U9-REFB)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 83.46 23.1265 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C27" (at -3.0605 0 90) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C27-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 70.358 11.877355 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C40" (at 3.222855 -16.51 90) (layer "F.SilkS"))
    (fp_text value "10n" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "VDDA") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 91.694 10.1345 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C18" (at -2.7685 0 90) (layer "F.SilkS"))
    (fp_text value "100n" (at -2.38 2.299 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(U7-VCM)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 63.7285 23.040355 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C31" (at 2.7685 0) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(U9-REFT)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 71.882 19.712855 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C29" (at -3.0225 1.778 90) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(U9-VREF)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 88.6585 10.16 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C22" (at -2.794 0.0125 90) (layer "F.SilkS"))
    (fp_text value "100n" (at -1.524 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(U7-CLMP)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 84.8105 14.478)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C19" (at -3.0225 0.508) (layer "F.SilkS"))
    (fp_text value "1nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(U7-VPOS)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 83.8455 16.002)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C11" (at 2.7685 0) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(U7-VOH)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 87.1345 10.16 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R10" (at -2.794 0.0125 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(U7-CLMP)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 93.7005 22.458 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C9" (at 2.2605 0) (layer "F.SilkS"))
    (fp_text value "1nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(U7-ENBL)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 73.406 19.712855 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R20" (at -3.0735 1.524 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "Net-(U9-MODE)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 59.436 17.5515 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C41" (at 3.0225 0 90) (layer "F.SilkS"))
    (fp_text value "10n" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "VCC3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 71.882 16.449355 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C36" (at -3.222855 16.51 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "VDDA") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 90.1825 10.16 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C20" (at -2.794 0.0125 90) (layer "F.SilkS"))
    (fp_text value "1nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(U7-CLMP)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 69.8755 23.040355)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C30" (at -0.0255 1.524) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(U9-REFB)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 81.936 23.1265 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R13" (at 3.0605 0.106 90) (layer "F.SilkS"))
    (fp_text value "2k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C27-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "VGA_GAIN") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 70.358 19.712855 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C28" (at -3.0225 2.032 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(U9-VREF)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 84.8105 12.954)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C21" (at -3.0225 1.016) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(U7-VPOS)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 78.08568 14.386355 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R11" (at -3.0735 0 90) (layer "F.SilkS"))
    (fp_text value "33R, 0.5%" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(C24-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(U9-VIN-)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 73.406 12.600855 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C33" (at -3.184355 16.256 90) (layer "F.SilkS"))
    (fp_text value "100p" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(U9-VIN-)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 66.8275 23.040355)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C34" (at -0.0255 1.524) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(U9-REFT)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(U9-REFB)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 74.93 19.712855 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R19" (at -3.0735 1.524 90) (layer "F.SilkS"))
    (fp_text value "2k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "Net-(U9-MODE)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "VDDA") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 70.358 16.449355 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C37" (at -3.222855 16.51 90) (layer "F.SilkS"))
    (fp_text value "10n" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "VDDA") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 71.882 11.877355 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C38" (at 3.222855 -16.51 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "VDDA") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 74.93 15.699855 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R16" (at -3.235355 16.51 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(U9-VIN+)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 89.064 23.114)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "BAV99 High-speed switching diodes, SOT-23")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D7" (at 0.016 2.474) (layer "F.SilkS"))
    (fp_text value "BAV99" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(U7-GAIN)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "GNDA") (pinfunction "A") (pintype "passive"))
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "unconnected-(D7-K-Pad3)") (pinfunction "K") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 83.8455 17.526)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C24" (at 2.7685 0) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(C24-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(U7-VOL)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 63.5 42.926 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R22" (at -3.302 0) (layer "F.SilkS"))
    (fp_text value "22K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "PWR_PG") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "PWR_EN") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 69.546 54.32 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C56" (at 3.012 -0.204 270) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.65 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 81.992 49.113 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C59" (at -3.2235 0 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.65 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 137 "Net-(D14-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 51.1325 62.738)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C61" (at -2.8725 3.048) (layer "F.SilkS"))
    (fp_text value "10uF, 10V" (at 0.078 1.8955) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 87.63 60.452 180)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J20" (at 3.302 0) (layer "F.SilkS"))
    (fp_text value "CSM3V3Cur" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 87 "CSM3V3Cur") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (at 97.79 66.795046 -90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (property "Sheetfile" "dutconnect.kicad_sch")
    (property "Sheetname" "dutconnect")
    (property "ki_description" "Power MOSFET, 30V, 11A")
    (property "ki_keywords" "Power MOSFET")
    (attr smd)
    (fp_text reference "Q1" (at 4.445 0 180) (layer "F.SilkS"))
    (fp_text value "IRF7807Z" (at 0 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "S") (pintype "power_out"))
    (pad "2" smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "S") (pintype "power_out"))
    (pad "3" smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "S") (pintype "power_out"))
    (pad "4" smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "Net-(Q1-G)") (pinfunction "G") (pintype "input"))
    (pad "5" smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "Net-(J2-In)") (pinfunction "D") (pintype "power_in"))
    (pad "6" smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "Net-(J2-In)") (pinfunction "D") (pintype "power_in"))
    (pad "7" smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "Net-(J2-In)") (pinfunction "D") (pintype "power_in"))
    (pad "8" smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "Net-(J2-In)") (pinfunction "D") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 55.0395 60.631786 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "Type" "X5R, X7R, ESR < 1Ohm")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C53" (at 0.1755 -1.852214) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.65 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(J24-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 54.61 82.562 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Jumper, 3-pole, both open")
    (property "ki_keywords" "Jumper SPDT")
    (attr through_hole)
    (fp_text reference "JP3" (at 2.552 2.54 180) (layer "F.SilkS"))
    (fp_text value "Power Ext or int" (at -0.2455 7.488 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 74 "Net-(D11-K)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 36 "VCC") (pinfunction "C") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "VCC5V0") (pinfunction "B") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0402_1005Metric" (layer "F.Cu")
    (at 100.838 20.32)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L1" (at 2.286 0) (layer "F.SilkS"))
    (fp_text value "120nH" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.485 0) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(C10-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.485 0) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "Net-(J10-In)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "cerg:573100D00010G" (layer "F.Cu")
    (at 42.58 56.313786 90)
    (descr "573100D00010G-1")
    (tags "Hardware")
    (property "Description" "AAVID THERMALLOY - 573100D00010G - HEAT SINK TO-252")
    (property "Height" "10.16")
    (property "Manufacturer_Name" "Aavid Thermalloy")
    (property "Manufacturer_Part_Number" "573100D00010G")
    (property "Mouser Part Number" "532-573100D00010G")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=532-573100D00010G")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "AAVID THERMALLOY - 573100D00010G - HEAT SINK TO-252")
    (attr smd)
    (fp_text reference "H1" (at 0 0 90) (layer "F.SilkS"))
    (fp_text value "573100D00010G" (at 0 0 90) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -6.05 0 90) (size 1.4 9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "1") (pintype "unspecified"))
    (pad "2" smd rect (at 0 0 90) (size 8.9 9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "2") (pintype "unspecified"))
    (pad "3" smd rect (at 6.05 0 90) (size 1.4 9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "3") (pintype "unspecified"))
    (model "${KISYS3DMOD}/Heatsink.3dshapes/Heatsink_AAVID_573300D00010G_TO-263.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KISYS3DMOD}/Heatsink.3dshapes/Heatsink_AAVID_573300D00010G_TO-263.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 76.454 12.600855 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R15" (at -3.184355 16.51 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "VDDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(U9-VIN-)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 97.0535 15.748)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C14" (at 0.9905 -2.794) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(U7-VIP)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(U7-LOP)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 97.0535 14.224)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C16" (at 0.9905 -2.286) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(U7-VIN)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(U7-LON)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 98.3235 21.844 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C12" (at 0.0255 -4.064) (layer "F.SilkS"))
    (fp_text value "22pF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(U7-INH)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 98.3235 18.796)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C13" (at -0.0255 4.572) (layer "F.SilkS"))
    (fp_text value "18nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(U7-INH)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C13-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 98.3235 17.272)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R9" (at 0.9905 -1.778 90) (layer "F.SilkS"))
    (fp_text value "274R" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(U7-LON)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C13-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 98.3235 20.32)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C10" (at -0.0255 4.318) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(U7-INH)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:MSOP-8_3x3mm_P0.65mm" (layer "F.Cu")
    (at 86.55 56.582)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (attr smd)
    (fp_text reference "U11" (at 4.382 0 90) (layer "F.SilkS"))
    (fp_text value "INA225" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.2 -0.975) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "Net-(D14-A)") (pinfunction "Vin+") (pintype "input"))
    (pad "2" smd rect (at -2.2 -0.325) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -2.2 0.325) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "VCC5V0") (pinfunction "Vs") (pintype "power_in"))
    (pad "4" smd rect (at -2.2 0.975) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "CSM3V3Cur") (pinfunction "Out") (pintype "passive"))
    (pad "5" smd rect (at 2.2 0.975) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "CSM3V3Gain0") (pinfunction "GS0") (pintype "input"))
    (pad "6" smd rect (at 2.2 0.325) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "CSM3V3Gain1") (pinfunction "GS1") (pintype "input"))
    (pad "7" smd rect (at 2.2 -0.325) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "Ref") (pintype "input"))
    (pad "8" smd rect (at 2.2 -0.975) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "FC_3V3") (pinfunction "Vin-") (pintype "input"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/MSOP-8_3x3mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 74.93 60.452 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J18" (at 0 -3.048 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 0 4.87 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.275) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 36 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 116 "FC_5V") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 77.47 70.612)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J15" (at -3.302 0) (layer "F.SilkS"))
    (fp_text value "CSM5VCur" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 88 "CSM5VCur") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Converter_DCDC:Converter_DCDC_muRata_NMAxxxxSC_THT" (layer "F.Cu")
    (at 64.77 75.692 90)
    (descr "muRata NMAxxxxSC footprint based on SIP7, http://power.murata.com/data/power/ncl/kdc_nma.pdf")
    (tags "muRata NMAxxxxSC DCDC-Converter")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "+/-55mA Isolated 1W Dual output DC/DC Converter Module, 5V Input Voltage, +/-9V Output Voltage, SIP3")
    (property "ki_keywords" "Murata isolated isolation dc-dc converter")
    (attr through_hole)
    (fp_text reference "U1" (at -2.032 -2.794 270) (layer "F.SilkS"))
    (fp_text value "RB-0509D" (at -1 19 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.25 6 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 36 "VCC") (pinfunction "VIN+") (pintype "power_in"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "VIN-") (pintype "power_in"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(U1-VOUT-)") (pinfunction "VOUT-") (pintype "power_out"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 73 "/Power/GNDP") (pinfunction "0V") (pintype "power_out"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(U1-VOUT+)") (pinfunction "VOUT+") (pintype "power_out"))
    (model "${KISYS3DMOD}/Converter_DCDC.3dshapes/Converter_DCDC_muRata_NMAxxxxSC_THT.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 71.12 90.3985 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ardu.kicad_sch")
    (property "Sheetname" "Ardu")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R21" (at 0 -1.27 90) (layer "F.SilkS"))
    (fp_text value "1k69 1%" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "/Ardu/A0") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "CSMVarCur") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "cerg:cerg" (layer "F.Cu")
    (at 52.07 34.417)
    (attr smd)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 76.22 63.5)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R28" (at -2.56 0 -90) (layer "F.SilkS"))
    (fp_text value "0R1" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 36 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 116 "FC_5V") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm" (layer "F.Cu")
    (at 65.588 15.420355 180)
    (descr "TSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot361-1_po.pdf)")
    (tags "SSOP 0.65")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "10-Bit, 65/80/105 MSPS 3V A/D Converter")
    (property "ki_keywords" "A/D Converter")
    (attr smd)
    (fp_text reference "U9" (at -2.738 5.768355) (layer "F.SilkS"))
    (fp_text value "AD9215" (at 0 5.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.85 -4.225 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "ADC_OR") (pinfunction "OR") (pintype "output"))
    (pad "2" smd rect (at -2.85 -3.575 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "Net-(U9-MODE)") (pinfunction "MODE") (pintype "input"))
    (pad "3" smd rect (at -2.85 -2.925 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "GNDA") (pinfunction "SENSE") (pintype "input"))
    (pad "4" smd rect (at -2.85 -2.275 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(U9-VREF)") (pinfunction "VREF") (pintype "input"))
    (pad "5" smd rect (at -2.85 -1.625 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(U9-REFB)") (pinfunction "REFB") (pintype "input"))
    (pad "6" smd rect (at -2.85 -0.975 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(U9-REFT)") (pinfunction "REFT") (pintype "input"))
    (pad "7" smd rect (at -2.85 -0.325 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "VDDA") (pinfunction "AVDD") (pintype "power_in"))
    (pad "8" smd rect (at -2.85 0.325 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "GNDA") (pinfunction "AGND") (pintype "power_in"))
    (pad "9" smd rect (at -2.85 0.975 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(U9-VIN+)") (pinfunction "VIN+") (pintype "input"))
    (pad "10" smd rect (at -2.85 1.625 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(U9-VIN-)") (pinfunction "VIN-") (pintype "input"))
    (pad "11" smd rect (at -2.85 2.275 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "GNDA") (pinfunction "AGND") (pintype "output"))
    (pad "12" smd rect (at -2.85 2.925 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "VDDA") (pinfunction "AVDD") (pintype "power_in"))
    (pad "13" smd rect (at -2.85 3.575 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "ADC_CLK") (pinfunction "CLK") (pintype "input"))
    (pad "14" smd rect (at -2.85 4.225 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "PWDN") (pintype "input"))
    (pad "15" smd rect (at 2.85 4.225 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "16" smd rect (at 2.85 3.575 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "17" smd rect (at 2.85 2.925 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "ADC_D0") (pinfunction "D0") (pintype "output"))
    (pad "18" smd rect (at 2.85 2.275 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "ADC_D1") (pinfunction "D1") (pintype "output"))
    (pad "19" smd rect (at 2.85 1.625 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "ADC_D2") (pinfunction "D2") (pintype "output"))
    (pad "20" smd rect (at 2.85 0.975 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "ADC_D3") (pinfunction "D3") (pintype "output"))
    (pad "21" smd rect (at 2.85 0.325 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "ADC_D4") (pinfunction "D4") (pintype "output"))
    (pad "22" smd rect (at 2.85 -0.325 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "ADC_D5") (pinfunction "D5") (pintype "output"))
    (pad "23" smd rect (at 2.85 -0.975 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "DRGND") (pintype "power_in"))
    (pad "24" smd rect (at 2.85 -1.625 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "VCC3V3") (pinfunction "DRVDD") (pintype "power_in"))
    (pad "25" smd rect (at 2.85 -2.275 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "ADC_D6") (pinfunction "D6") (pintype "output"))
    (pad "26" smd rect (at 2.85 -2.925 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "ADC_D7") (pinfunction "D7") (pintype "output"))
    (pad "27" smd rect (at 2.85 -3.575 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "ADC_D8") (pinfunction "D8") (pintype "output"))
    (pad "28" smd rect (at 2.85 -4.225 180) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "ADC_D9") (pinfunction "D9") (pintype "output"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-28_4.4x9.7mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (at 98.044 10.1345 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Inductor with ferrite core")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L2" (at 2.2605 -0.127 90) (layer "F.SilkS"))
    (fp_text value "1k/500mA" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(U7-ENBL)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "5Vclean") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 96.52 10.1345 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C7" (at -2.2605 0 90) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(U7-ENBL)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 94.996 10.1345 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C25" (at -2.7685 0 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(U7-ENBL)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "cerg:SMA-JOHNSON-142-0701-201" (layer "F.Cu")
    (at 69.85 37.592)
    (property "Sheetfile" "dutconnect.kicad_sch")
    (property "Sheetname" "dutconnect")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr through_hole)
    (fp_text reference "J13" (at 0 4.318) (layer "F.SilkS"))
    (fp_text value "Clock" (at 0 -0.5) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.5748) (layers "*.Cu" "*.Mask")
      (net 94 "Net-(J13-In)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54) (size 2.54 2.54) (drill 1.7018) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54) (size 2.54 2.54) (drill 1.7018) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54) (size 2.54 2.54) (drill 1.7018) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54) (size 2.54 2.54) (drill 1.7018) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KIPRJMOD}/3d models/BELFUSE_1420701201/142-0701-201.stp"
      (offset (xyz 0 0 9.652))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x10_P2.54mm_Horizontal" (layer "F.Cu")
    (at 97.79 32.512)
    (descr "Through hole angled IDC box header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x10 2.54mm double row")
    (property "Sheetfile" "dutconnect.kicad_sch")
    (property "Sheetname" "dutconnect")
    (property "ki_description" "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 1.905 -3.175 180) (layer "F.SilkS"))
    (fp_text value "Target" (at 6.105 29.464) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 8.805 11.43 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 116 "FC_5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 117 "FC_3V3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 103 "FD2C_CLK") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 104 "FC_RST") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 105 "FC2D_CLK") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 106 "FC_IO") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 107 "FD_VREF") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 108 "FD_TF") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 109 "FC_DIO0") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 110 "FC2D_HS") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 111 "FC_DIO1") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 112 "FD2C_HS") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 113 "FC_DIO2") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 114 "FC_PROG") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 115 "FC_DIO3") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 2.54 20.32) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 117 "FC_3V3") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 116 "FC_5V") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x10_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbol:Symbol_Barrel_Polarity" (layer "F.Cu")
    (at 41.823 89.027)
    (descr "Barrel connector polarity indicator")
    (tags "barrel polarity")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2) (layer "F.SilkS") hide)
    (fp_text value "Symbol_Barrel_Polarity" (at 0 2) (layer "F.Fab"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 59.319 66.548 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C63" (at 1.524 -1.407 270) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "VCC5V0") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 62.23 60.452 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J24" (at 0 -3.302 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 0.026 -3.327996 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(J24-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 118 "FC_Var") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 62.23 52.832)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J25" (at 5.08 -1.016 90) (layer "F.SilkS"))
    (fp_text value "V_Var" (at 1.27 4.08) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -2.22) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.74 2.19) (drill 1.19) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.143678)
      (net 118 "FC_Var") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.74 2.19) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 81.28 90.424 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ardu.kicad_sch")
    (property "Sheetname" "Ardu")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R34" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1k69 1%" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "/Ardu/A4") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "CSM3V3Cur") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 83.82 90.424 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ardu.kicad_sch")
    (property "Sheetname" "Ardu")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R36" (at -0.063 -1.524 90) (layer "F.SilkS"))
    (fp_text value "1k69 1%" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "/Ardu/A5") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "FC_3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 63.4445 63.5)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R37" (at -2.6115 0 90) (layer "F.SilkS"))
    (fp_text value "0R1" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 38 "Net-(J24-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 118 "FC_Var") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:MSOP-8_3x3mm_P0.65mm" (layer "F.Cu")
    (at 63.51 66.548)
    (descr "MSOP, 8 Pin (https://www.jedec.org/system/files/docs/mo-187F.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "MSOP SO")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (attr smd)
    (fp_text reference "U13" (at 4.816 0 -90) (layer "F.SilkS"))
    (fp_text value "INA225" (at 0 2.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1125 -0.975) (size 1.625 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(J24-Pin_1)") (pinfunction "Vin+") (pintype "input"))
    (pad "2" smd roundrect (at -2.1125 -0.325) (size 1.625 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -2.1125 0.325) (size 1.625 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "VCC5V0") (pinfunction "Vs") (pintype "power_in"))
    (pad "4" smd roundrect (at -2.1125 0.975) (size 1.625 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "Net-(J28-Pin_1)") (pinfunction "Out") (pintype "passive"))
    (pad "5" smd roundrect (at 2.1125 0.975) (size 1.625 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 101 "CSMVarGain0") (pinfunction "GS0") (pintype "input"))
    (pad "6" smd roundrect (at 2.1125 0.325) (size 1.625 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "CSMVarGain1") (pinfunction "GS1") (pintype "input"))
    (pad "7" smd roundrect (at 2.1125 -0.325) (size 1.625 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pinfunction "Ref") (pintype "input"))
    (pad "8" smd roundrect (at 2.1125 -0.975) (size 1.625 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "FC_Var") (pinfunction "Vin-") (pintype "input"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/MSOP-8_3x3mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (at 94.996 75.7175 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D4" (at 0.0255 1.905 90) (layer "F.SilkS"))
    (fp_text value "green" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "/Power/GNDP") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(D4-A)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (at 94.996 78.994 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D2" (at 0.0255 1.905 270) (layer "F.SilkS"))
    (fp_text value "green" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "/Power/-7V8P") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(D2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (at 94.996 82.2705 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D6" (at 0.0255 1.778 90) (layer "F.SilkS"))
    (fp_text value "green" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "/Power/GNDP") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(D6-A)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x03_P2.54mm_Horizontal" (layer "F.Cu")
    (at 97.79 80.772)
    (descr "Through hole IDC box header, 2x03, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole horizontal IDC box header THT 2x03 2.54mm double row")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J11" (at 2.794 -4.826) (layer "F.SilkS"))
    (fp_text value "PP1" (at 6.215 11.18) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 8.83 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.147059)
      (net 71 "/Power/+7V8P") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 73 "/Power/GNDP") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 93 "Net-(J11-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 75 "/Power/3V3P") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 70 "/Power/-7V8P") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 73 "/Power/GNDP") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x03_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x03_P2.54mm_Horizontal" (layer "F.Cu")
    (at 95.25 85.852 -90)
    (descr "Through hole IDC box header, 2x03, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole horizontal IDC box header THT 2x03 2.54mm double row")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J12" (at 3.302 -4.064 180) (layer "F.SilkS"))
    (fp_text value "PP2" (at 6.215 11.18 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 8.83 2.54) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.147059)
      (net 71 "/Power/+7V8P") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 73 "/Power/GNDP") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 93 "Net-(J11-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 75 "/Power/3V3P") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 70 "/Power/-7V8P") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 73 "/Power/GNDP") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x03_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Converter_DCDC:Converter_DCDC_muRata_NMAxxxxSC_THT" (layer "F.Cu")
    (at 64.77 83.312 90)
    (descr "muRata NMAxxxxSC footprint based on SIP7, http://power.murata.com/data/power/ncl/kdc_nma.pdf")
    (tags "muRata NMAxxxxSC DCDC-Converter")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "200mA Isolated 1W Dual output DC/DC Converter Module, 5V Input Voltage, 5V Output Voltage, SIP7")
    (property "ki_keywords" "Recom isolated isolation dc-dc converter")
    (attr through_hole)
    (fp_text reference "U2" (at -2.032 -2.794 90) (layer "F.SilkS"))
    (fp_text value "REE-0505S" (at -1 19 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.25 6 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 36 "VCC") (pinfunction "VIN+") (pintype "power_in"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "VIN-") (pintype "power_in"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 73 "/Power/GNDP") (pinfunction "0V") (pintype "power_out"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 127 "unconnected-(U2-0V-Pad5)") (pinfunction "0V") (pintype "no_connect"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(U2-VOUT+)") (pinfunction "VOUT+") (pintype "power_out"))
    (model "${KISYS3DMOD}/Converter_DCDC.3dshapes/Converter_DCDC_muRata_NMAxxxxSC_THT.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 79.706 49.06 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C58" (at 1.816 -0.712) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 137 "Net-(D14-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 82.486 56.6075 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C55" (at 0.9815 -2.222) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43 270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "VCC5V0") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 96.012 22.3775 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C15" (at -2.7685 0 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(U7-LMD2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad_TopBottom" (layer "F.Cu")
    (at 80.264 9.652)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "fobosshieldZ2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at -0.254 0) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "B.Cu" "B.Mask"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 39.37 93.472)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J21" (at 3.048 1.778) (layer "F.SilkS"))
    (fp_text value "GND" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 102.87 93.472)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J26" (at 0 2.032) (layer "F.SilkS"))
    (fp_text value "AUX" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 93 "Net-(J11-Pin_3)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 105.41 93.472)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J27" (at 0 2.032) (layer "F.SilkS"))
    (fp_text value "GNDP" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 73 "/Power/GNDP") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 76.2 90.3985 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ardu.kicad_sch")
    (property "Sheetname" "Ardu")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R30" (at 0 -1.27 90) (layer "F.SilkS"))
    (fp_text value "1k69 1%" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/Ardu/A2") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "CSM5VCur") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 57.912 56.590786 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C52" (at 2.309 0 90) (layer "F.SilkS"))
    (fp_text value "220p" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(J24-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(U8-FB)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 49.022 57.050286 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C50" (at -0.0255 -1.524 90) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 50.292 55.828786 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C51" (at 2.309 0.254 90) (layer "F.SilkS"))
    (fp_text value "10n" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(U8-SS)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A" (layer "F.Cu")
    (at 50.466 60.631786)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C62" (at -2.206 3.630214) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.35 0) (size 1.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.185185)
      (net 36 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.35 0) (size 1.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.185185)
      (net 6 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:Texas_VQFN-RGW-20" (layer "F.Cu")
    (at 54.102 56.313786 180)
    (descr "http://www.ti.com/general/docs/lit/getliterature.tsp?baseLiteratureNumber=MPQF122&fileType=pdf")
    (tags "QFN 0.65 VQFN")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "1-A, Fast-Transient, Low-Dropout Voltage Regulator")
    (property "ki_keywords" "LDO, Voltage Regulator")
    (attr smd)
    (fp_text reference "U8" (at 0 4.064 180) (layer "F.SilkS"))
    (fp_text value "TPS7A7100_VQFN20" (at 0 4.04 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect (at -2.4 -1.3 180) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(J24-Pin_1)") (pinfunction "OUT") (pintype "power_out") (zone_connect 2))
    (pad "2" smd rect (at -2.4 -0.65 180) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(J24-Pin_1)") (pinfunction "SNS") (pintype "input"))
    (pad "3" smd rect (at -2.4 0 180) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(U8-FB)") (pinfunction "FB") (pintype "input"))
    (pad "4" smd rect (at -2.4 0.65 180) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "PWR_PG") (pinfunction "PG") (pintype "output"))
    (pad "5" smd rect (at -2.4 1.3 180) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "PWR0") (pinfunction "50mV") (pintype "input"))
    (pad "6" smd rect (at -1.3 2.4 270) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "PWR1") (pinfunction "100mV") (pintype "input"))
    (pad "7" smd rect (at -0.65 2.4 270) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "PWR2") (pinfunction "200mV") (pintype "input"))
    (pad "8" smd rect (at 0 2.4 270) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" smd rect (at 0.65 2.4 270) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "PWR3") (pinfunction "400mV") (pintype "input"))
    (pad "10" smd rect (at 1.3 2.4 270) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "PWR4") (pinfunction "800mV") (pintype "input"))
    (pad "11" smd rect (at 2.4 1.3 180) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "PWR5") (pinfunction "1.6V") (pintype "input"))
    (pad "12" smd rect (at 2.4 0.65 180) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "13" smd rect (at 2.4 0 180) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(U8-SS)") (pinfunction "SS") (pintype "input"))
    (pad "14" smd rect (at 2.4 -0.65 180) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "PWR_EN") (pinfunction "EN") (pintype "input"))
    (pad "15" smd rect (at 2.4 -1.3 180) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "VCC") (pinfunction "IN") (pintype "power_in") (zone_connect 2))
    (pad "16" smd rect (at 1.3 -2.4 270) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "VCC") (pinfunction "IN") (pintype "power_in") (zone_connect 2))
    (pad "17" smd rect (at 0.65 -2.4 270) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "VCC") (pinfunction "IN") (pintype "power_in") (zone_connect 2))
    (pad "18" smd rect (at 0 -2.4 270) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "19" smd rect (at -0.65 -2.4 270) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(J24-Pin_1)") (pinfunction "OUT") (pintype "power_out") (zone_connect 2))
    (pad "20" smd rect (at -1.3 -2.4 270) (size 1 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(J24-Pin_1)") (pinfunction "OUT") (pintype "power_out") (zone_connect 2))
    (pad "21" smd rect (at -0.7875 -0.7875 180) (size 1.575 1.575) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "GND") (pintype "power_in") (solder_paste_margin_ratio -0.2))
    (pad "21" smd rect (at -0.7875 0.7875 180) (size 1.575 1.575) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "GND") (pintype "power_in") (solder_paste_margin_ratio -0.2))
    (pad "21" smd rect (at 0.7875 -0.7875 180) (size 1.575 1.575) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "GND") (pintype "power_in") (solder_paste_margin_ratio -0.2))
    (pad "21" smd rect (at 0.7875 0.7875 180) (size 1.575 1.575) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GND") (pinfunction "GND") (pintype "power_in") (solder_paste_margin_ratio -0.2))
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_VQFN-RGW-20-1EP_5x5mm_Pitch0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-20-1EP_5x5mm_P0.65mm_EP3.35x3.35mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-20-1EP_5x5mm_P0.65mm_EP3.35x3.35mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 49.022 53.836786 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R38" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "PWR_EN") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_901-144_Vertical" (layer "F.Cu")
    (at 54.356 70.612)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr through_hole)
    (fp_text reference "J23" (at 0 -4.75) (layer "F.SilkS"))
    (fp_text value "Power" (at 0 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 102 "CSMVarCur") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 64.77 70.612 -90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J28" (at 0 5.334) (layer "F.SilkS"))
    (fp_text value "CSM5VCur" (at -0.2455 4.942 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 95 "Net-(J28-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 102 "CSMVarCur") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded" (layer "F.Cu")
    (at 44.958 16.764)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (property "Sheetfile" "dutconnect.kicad_sch")
    (property "Sheetname" "dutconnect")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J16" (at 0 2.794) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers "*.Cu" "*.Mask")
      (net 60 "Trigger") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 95.0215 69.241046)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "dutconnect.kicad_sch")
    (property "Sheetname" "dutconnect")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at -0.0255 1.778) (layer "B.SilkS"))
    (fp_text value "1R" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 48 "GlitchLP") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 119 "Net-(Q2-G)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 95.758 66.726546 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "dutconnect.kicad_sch")
    (property "Sheetname" "dutconnect")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0.0255 -1.27 90) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 119 "Net-(Q2-G)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x03_P2.54mm_Vertical" (layer "B.Cu")
    (at 83.82 65.532 180)
    (descr "Through hole straight socket strip, 2x03, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x03 2.54mm double row")
    (property "Sheetfile" "ardu.kicad_sch")
    (property "Sheetname" "Ardu")
    (property "ki_description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J5" (at -5.08 -2.667 180) (layer "B.SilkS"))
    (fp_text value "SPI" (at -1.27 -7.85 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 -2.54 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 135 "/Ardu/MISO") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "VCC3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 136 "/Ardu/SCK") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at -2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 49 "Glitch") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "GlitchLP") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at -2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "B.Cu")
    (at 48.26 93.472 -90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Sheetfile" "ardu.kicad_sch")
    (property "Sheetname" "Ardu")
    (property "ki_description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J7" (at 0 2.33 -90) (layer "B.SilkS"))
    (fp_text value "Power" (at 0 -20.11 -90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -8.89 180) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 80 "unconnected-(J7-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "VCC3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "unconnected-(J7-Pin_3-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "VCC3V3") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "VCC5V0") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 97 "VU_CK") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 78.74 57.1755 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R27" (at -3.0735 0 90) (layer "B.SilkS"))
    (fp_text value "330R" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(D8-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(D9-A)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOT-23_ANK" (layer "B.Cu")
    (at 75.962 57.338 180)
    (descr "SOT-23, Single Diode")
    (tags "SOT-23")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Zener diode")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D8" (at 0.016 2.474) (layer "B.SilkS"))
    (fp_text value "3V9" (at 0 -2.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5) (layer "B.Fab"))
    (pad "" smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "1" smd rect (at 1 0 180) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "VCC") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at -1 0.95 180) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 68 "Net-(D8-A)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "cerg:PinSocket_2x10_P2.54mm_Vertical" (layer "B.Cu")
    (at 95.24177 27.432 90)
    (descr "Through hole straight socket strip, 2x10, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x10 2.54mm double row")
    (property "Sheetfile" "ardu.kicad_sch")
    (property "Sheetname" "Ardu")
    (property "ki_description" "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J8" (at -5.08 0.00823) (layer "B.SilkS"))
    (fp_text value "IOL" (at -1.27 -25.63 270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 -11.43) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "VCC3V3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "VCC5V0") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 104 "FC_RST") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at -2.54 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "VCC5V0") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 106 "FC_IO") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at -2.54 -5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 109 "FC_DIO0") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at -2.54 -7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 108 "FD_TF") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at -2.54 -10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 111 "FC_DIO1") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 103 "FD2C_CLK") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at -2.54 -12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 110 "FC2D_HS") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 113 "FC_DIO2") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at -2.54 -15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 112 "FD2C_HS") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at -2.54 -17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 115 "FC_DIO3") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "VCC3V3") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at -2.54 -20.32 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 105 "FC2D_CLK") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 -22.86 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 114 "FC_PROG") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at -2.54 -22.86 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 98.5775 74.93)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R24" (at 3.0225 0) (layer "B.SilkS"))
    (fp_text value "100R" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(D4-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(D1-A)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "cerg:PinSocket_2x10_P2.54mm_Vertical" (layer "B.Cu")
    (at 69.84177 27.432 90)
    (descr "Through hole straight socket strip, 2x10, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x10 2.54mm double row")
    (property "Sheetfile" "ardu.kicad_sch")
    (property "Sheetname" "Ardu")
    (property "ki_description" "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at -5.08 0.00823) (layer "B.SilkS"))
    (fp_text value "IOH" (at -1.27 -25.63 270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 -11.43) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 47 "VGA_HILO") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 46 "VGA_GAIN") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 35 "ADC_OR") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at -2.54 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 55 "ADC_D9") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at -2.54 -5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 56 "ADC_D8") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 122 "/Ardu/JA2_P") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at -2.54 -7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 123 "/Ardu/JA2_N") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 57 "ADC_D7") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at -2.54 -10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 59 "ADC_D5") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at -2.54 -12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 58 "ADC_D6") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 54 "ADC_D4") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at -2.54 -15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 52 "ADC_D2") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at -2.54 -17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 53 "ADC_D3") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 50 "ADC_D0") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at -2.54 -20.32 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 51 "ADC_D1") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 -22.86 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at -2.54 -22.86 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "ADC_CLK") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (at 98.695 66.701046)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Sheetfile" "dutconnect.kicad_sch")
    (property "Sheetname" "dutconnect")
    (property "ki_description" "N-MOSFET transistor, gate/source/drain")
    (property "ki_keywords" "transistor NMOS N-MOS N-MOSFET")
    (attr smd)
    (fp_text reference "Q2" (at 0 2.5) (layer "B.SilkS"))
    (fp_text value "IRLML2502" (at 0 -2.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "B.Fab"))
    (pad "1" smd rect (at -1 0.95) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 119 "Net-(Q2-G)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "GND") (pinfunction "S") (pintype "passive"))
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 77 "Net-(J2-In)") (pinfunction "D") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 77.5716 18.1609 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C46" (at -0.0253 -1.5748 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "VDDA") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:TSOT-23-5" (layer "B.Cu")
    (at 74.5128 22.7076)
    (descr "5-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_5_05-08-1635.pdf")
    (tags "TSOT-23-5")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "150mA Low Dropout Voltage Regulator, Fixed Output 3.3V, TSOT-23-5")
    (property "ki_keywords" "150mA LDO Regulator Fixed Positive")
    (attr smd)
    (fp_text reference "U6" (at 0.0108 2.5908 180) (layer "B.SilkS"))
    (fp_text value "LP3985IM5-3.0" (at 0 -2.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -1.31 0.95) (size 1.22 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "Net-(U6-INH)") (pinfunction "VIN") (pintype "power_in"))
    (pad "2" smd rect (at -1.31 0) (size 1.22 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -1.31 -0.95) (size 1.22 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "Net-(U6-INH)") (pinfunction "INH") (pintype "input"))
    (pad "4" smd rect (at 1.31 -0.95) (size 1.22 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "Net-(U6-BYP)") (pinfunction "BYP") (pintype "input"))
    (pad "5" smd rect (at 1.31 0.95) (size 1.22 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "VDDA") (pinfunction "VOUT") (pintype "power_out"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TSOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 77.6224 23.9015 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C45" (at 0.0255 1.524 90) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "VDDA") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 70.739 23.9015 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C43" (at 3.0225 0 90) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(U6-INH)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 65.786 23.9015 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C42" (at 3.0225 0 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "VCC3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "B.Cu")
    (at 68.3005 23.114 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Inductor with ferrite core")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L4" (at -0.0255 2.8448) (layer "B.SilkS"))
    (fp_text value "1k/500mA" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(U6-INH)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "VCC3V3") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 98.5775 78.486 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R26" (at -3.0225 0) (layer "B.SilkS"))
    (fp_text value "330R" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 138 "Net-(D3-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(D6-A)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 65.7075 73.152)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C60" (at -3.1265 0.508) (layer "B.SilkS"))
    (fp_text value "10uF, 10V" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 67.1575 57.404)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R35" (at -0.0255 -1.524) (layer "B.SilkS"))
    (fp_text value "470R" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 120 "Net-(Q3-D)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(D12-K)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 75.0571 20.066)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C44" (at 0.0255 -1.524) (layer "B.SilkS"))
    (fp_text value "10n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(U6-BYP)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 79.502 81.8135 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at 2.3115 0 90) (layer "B.SilkS"))
    (fp_text value "240R, 1%" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 71 "/Power/+7V8P") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 121 "Net-(U3-ADJ)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOT-23_ANK" (layer "B.Cu")
    (at 104.836 75.93 -90)
    (descr "SOT-23, Single Diode")
    (tags "SOT-23")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Zener diode")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D1" (at 0.016 -2.352 90) (layer "B.SilkS"))
    (fp_text value "5V1" (at 0 -2.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90) (layer "B.Fab"))
    (pad "" smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "1" smd rect (at 1 0 270) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 71 "/Power/+7V8P") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at -1 0.95 270) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 87.122 87.9931 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at -2.2605 0 180) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "/Power/3V3P") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 73 "/Power/GNDP") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 76.9875 81.026 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at -0.0255 1.524) (layer "B.SilkS"))
    (fp_text value "1K2, 1%" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 121 "Net-(U3-ADJ)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 73 "/Power/GNDP") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A" (layer "B.Cu")
    (at 91.186 81.962 90)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at -0.08 2.032) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.75 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.35 0 90) (size 1.4 1.35) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.185185)
      (net 71 "/Power/+7V8P") (pintype "passive"))
    (pad "2" smd roundrect (at 1.35 0 90) (size 1.4 1.35) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.185185)
      (net 73 "/Power/GNDP") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A" (layer "B.Cu")
    (at 91.186 76.788 90)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at -0.174 2.032) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.75 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.35 0 90) (size 1.4 1.35) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.185185)
      (net 73 "/Power/GNDP") (pintype "passive"))
    (pad "2" smd roundrect (at 1.35 0 90) (size 1.4 1.35) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.185185)
      (net 70 "/Power/-7V8P") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "B.Cu")
    (at 84.168 82.931)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "100mA 35V Adjustable Linear Regulator, SO-8")
    (property "ki_keywords" "Adjustable Voltage Regulator 100mA Positive")
    (attr smd)
    (fp_text reference "U3" (at 4.732 1.651) (layer "B.SilkS"))
    (fp_text value "LM317L_SO8" (at 0 -3.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd rect (at -2.7 1.905) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "Net-(U1-VOUT+)") (pinfunction "VI") (pintype "power_in"))
    (pad "2" smd rect (at -2.7 0.635) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 71 "/Power/+7V8P") (pinfunction "VO") (pintype "power_out"))
    (pad "3" smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 71 "/Power/+7V8P") (pinfunction "VO") (pintype "passive"))
    (pad "4" smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 121 "Net-(U3-ADJ)") (pinfunction "ADJ") (pintype "input"))
    (pad "5" smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "unconnected-(U3-NC-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 71 "/Power/+7V8P") (pinfunction "VO") (pintype "passive"))
    (pad "7" smd rect (at 2.7 0.635) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 71 "/Power/+7V8P") (pinfunction "VO") (pintype "passive"))
    (pad "8" smd rect (at 2.7 1.905) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 129 "unconnected-(U3-NC-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 81.28 87.9931 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at -0.7875 -1.524 90) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.43 270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(U2-VOUT+)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 73 "/Power/GNDP") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "B.Cu")
    (at 84.168 77.089 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "100mA 35V Adjustable Negative Linear Regulator, SO-8")
    (property "ki_keywords" "Adjustable Negative Voltage Regulator 100mA")
    (attr smd)
    (fp_text reference "U4" (at -0.16 3.429 180) (layer "B.SilkS"))
    (fp_text value "LM337L_SO8" (at 0 -3.5 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 70 "/Power/-7V8P") (pinfunction "VO") (pintype "power_out"))
    (pad "2" smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "Net-(U1-VOUT-)") (pinfunction "VI") (pintype "power_in"))
    (pad "3" smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "Net-(U1-VOUT-)") (pinfunction "VI") (pintype "passive"))
    (pad "4" smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 124 "Net-(U4-ADJ)") (pinfunction "ADJ") (pintype "input"))
    (pad "5" smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 130 "unconnected-(U4-NC-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "Net-(U1-VOUT-)") (pinfunction "VI") (pintype "passive"))
    (pad "7" smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "Net-(U1-VOUT-)") (pinfunction "VI") (pintype "passive"))
    (pad "8" smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "unconnected-(U4-NC-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:TSOT-23-5" (layer "B.Cu")
    (at 84.344 87.7646 90)
    (descr "TSOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSOT TO_SOT_SMD")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "150mA Low Dropout Voltage Regulator, Fixed Output 3.3V, TSOT-23-5")
    (property "ki_keywords" "150mA LDO Regulator Fixed Positive")
    (attr smd)
    (fp_text reference "U5" (at -2.794 -0.016) (layer "B.SilkS"))
    (fp_text value "LD59015" (at 0 -2.4 270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(U2-VOUT+)") (pinfunction "VIN") (pintype "power_in"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 73 "/Power/GNDP") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(U2-VOUT+)") (pinfunction "INH") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 132 "unconnected-(U5-BYP-Pad4)") (pinfunction "BYP") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "/Power/3V3P") (pinfunction "VOUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 79.502 85.6235 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at -0.0255 1.524 90) (layer "B.SilkS"))
    (fp_text value "100n, 16V" (at 0.6426 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(U1-VOUT+)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 73 "/Power/GNDP") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 79.502 76.9365 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at -2.5145 0 90) (layer "B.SilkS"))
    (fp_text value "100n, 16V" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 73 "/Power/GNDP") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(U1-VOUT-)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 88.9 79.7815 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 2.5145 0 -90) (layer "B.SilkS"))
    (fp_text value "1K2, 1%" (at 0 -1.43 -90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 124 "Net-(U4-ADJ)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 73 "/Power/GNDP") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 88.9 75.9715 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R23" (at -3.0735 -0.254 -90) (layer "B.SilkS"))
    (fp_text value "240R, 1%" (at 0 -1.43 -90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 70 "/Power/-7V8P") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 124 "Net-(U4-ADJ)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOT-23_ANK" (layer "B.Cu")
    (at 104.836 79.486 -90)
    (descr "SOT-23, Single Diode")
    (tags "SOT-23")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Zener diode")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D5" (at 0.016 -2.352 90) (layer "B.SilkS"))
    (fp_text value "5V1" (at 0 -2.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90) (layer "B.Fab"))
    (pad "" smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "1" smd rect (at 1 0 270) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 73 "/Power/GNDP") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at -1 0.95 270) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "Net-(D5-A)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 90.17 46.7615 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R33" (at 0.0255 -1.524 90) (layer "B.SilkS"))
    (fp_text value "330R" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 139 "Net-(D14-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(D10-A)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOT-23_ANK" (layer "B.Cu")
    (at 47.498 79.248)
    (descr "SOT-23, Single Diode")
    (tags "SOT-23")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Zener diode")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D11" (at -2.81 0 90) (layer "B.SilkS"))
    (fp_text value "5V1" (at 0 -2.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5) (layer "B.Fab"))
    (pad "" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "1" smd rect (at 1 0) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 74 "Net-(D11-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at -1 0.95) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 98.5775 76.708)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R25" (at 3.0225 0) (layer "B.SilkS"))
    (fp_text value "100R" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(D2-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(D5-A)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "B.Cu")
    (at 68.3005 24.638 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "openADC.kicad_sch")
    (property "Sheetname" "openADC")
    (property "ki_description" "Inductor with ferrite core")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L6" (at -0.0255 2.9972) (layer "B.SilkS"))
    (fp_text value "1k/500mA" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "GNDA") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (at 63.77 57.404)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "ki_description" "50V Vds, 0.22A Id, N-Channel MOSFET, SOT-23")
    (property "ki_keywords" "N-Channel MOSFET")
    (attr smd)
    (fp_text reference "Q3" (at 0.016 -2.474) (layer "B.SilkS"))
    (fp_text value "BSS138L" (at 1.258 7.66) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -1 0.95) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 78 "PWR_PG") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "GND") (pinfunction "S") (pintype "passive"))
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 120 "Net-(Q3-D)") (pinfunction "D") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "B.Cu")
    (at 71.12 93.472 -90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "ardu.kicad_sch")
    (property "Sheetname" "Ardu")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 0 2.33 90) (layer "B.SilkS"))
    (fp_text value "Analog" (at 0 -15.03 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -6.35) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 81 "/Ardu/A0") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 82 "/Ardu/A1") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 83 "/Ardu/A2") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 85 "/Ardu/A3") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 98 "/Ardu/A4") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 100 "/Ardu/A5") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical" (layer "B.Cu")
    (at 39.37 45.212 -90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (property "Sheetfile" "ardu.kicad_sch")
    (property "Sheetname" "Ardu")
    (property "ki_description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J9" (at 2.54 0 -180) (layer "B.SilkS"))
    (fp_text value "Digital2" (at 0 -25.19 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -11.43) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 134 "/Ardu/SDA") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "Trigger") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 79 "PWR_EN") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 66 "PWR5") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 65 "PWR4") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "PWR3") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 63 "PWR2") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 62 "PWR1") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 61 "PWR0") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "B.Cu")
    (at 66.04 45.212 -90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Sheetfile" "ardu.kicad_sch")
    (property "Sheetname" "Ardu")
    (property "ki_description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J29" (at 2.54 0 -180) (layer "B.SilkS"))
    (fp_text value "Digital1" (at 0 -20.11 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -8.89) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 78 "PWR_PG") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 99 "CSMVarGain1") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 101 "CSMVarGain0") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 89 "CSM5VGain0") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 90 "CSM5VGain1") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 84 "CSM3V3Gain0") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 86 "CSM3V3Gain1") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 133 "/Ardu/AR_IO0") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323" (layer "B.Cu")
    (at 88.392 46.77 -90)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "75V 0.15A Fast switching Diode, SOD-323")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D14" (at 0 1.85 90) (layer "B.SilkS"))
    (fp_text value "1N4148WS" (at 0.1 -1.9 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.85 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.05 0 270) (size 0.6 0.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 139 "Net-(D14-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.05 0 270) (size 0.6 0.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 137 "Net-(D14-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323" (layer "B.Cu")
    (at 104.14 83.024 -90)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "Power")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "75V 0.15A Fast switching Diode, SOD-323")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D3" (at -0.22 -1.778 90) (layer "B.SilkS"))
    (fp_text value "1N4148WS" (at 0.1 -1.9 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.85 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.05 0 270) (size 0.6 0.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 138 "Net-(D3-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.05 0 270) (size 0.6 0.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "/Power/3V3P") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 36.83 5.842) (end 107.95 5.842)
    (layer "Edge.Cuts"))
  (gr_line (start 107.95 5.842) (end 107.95 96.012)
    (layer "Edge.Cuts"))
  (gr_line (start 107.95 96.012) (end 36.83 96.012)
    (layer "Edge.Cuts"))
  (gr_line (start 36.83 96.012) (end 36.83 5.842)
    (layer "Edge.Cuts"))
  (gr_text "Trigger" (at 44.958 12.7) (layer "F.SilkS"))
  (gr_text "CSM VAR" (at 63.5 73.152) (layer "F.SilkS"))
  (gr_text "Power" (at 57.15 85.598) (layer "F.SilkS"))
  (gr_text "+7.8V" (at 93.726 75.946) (layer "F.SilkS"))
  (gr_text "-7.8V" (at 93.726 78.994) (layer "F.SilkS"))
  (gr_text "+3.3V" (at 90.17 82.296) (layer "F.SilkS"))
  (gr_text "Probe Power" (at 85.344 81.788 90) (layer "F.SilkS"))
  (gr_text "Shunt" (at 63.5 57.912) (layer "F.SilkS"))
  (gr_text "Out" (at 80.518 70.612) (layer "F.SilkS"))
  (gr_text "Clock\n" (at 80.01 37.592) (layer "F.SilkS"))
  (gr_text "Shunt" (at 86.36 47.752) (layer "F.SilkS"))
  (gr_text "Int" (at 59.69 78.867 90) (layer "F.SilkS"))
  (gr_text "+" (at 44.871 89.027) (layer "F.SilkS"))
  (gr_text "1.0" (at 52.07 41.91) (layer "F.SilkS"))
  (gr_text "Out" (at 66.681 86.106) (layer "F.SilkS"))
  (gr_text "3.3V max on I/O lines" (at 95.25 43.942 90) (layer "F.SilkS"))
  (gr_text "C2D" (at 80.01 40.386) (layer "F.SilkS"))
  (gr_text "Mea sure" (at 100.838 20.32 90) (layer "F.SilkS"))
  (gr_text "-" (at 38.775 89.027) (layer "F.SilkS"))
  (gr_text "Ext" (at 54.61 78.867 90) (layer "F.SilkS"))
  (gr_text "FOBOS Shield Z2" (at 52.07 38.862) (layer "F.SilkS"))
  (gr_text "Out" (at 91.186 60.452) (layer "F.SilkS"))
  (gr_text "D2C" (at 80.01 35.052) (layer "F.SilkS"))
  (gr_text "Target" (at 92.71 42.037 90) (layer "F.SilkS"))
  (gr_text "Shunt" (at 76.105 57.912) (layer "F.SilkS"))
  (gr_text "CSM 5V" (at 76.105 73.152) (layer "F.SilkS"))
  (gr_text "VAR GND" (at 63.5 48.387) (layer "F.SilkS"))
  (gr_text "cryptography.gmu.edu" (at 56.515 90.932) (layer "F.SilkS"))
  (gr_text "Glitch\n" (at 101.854 67.971046 90) (layer "F.SilkS"))
  (gr_text "CSM 3V3" (at 88.138 62.992) (layer "F.SilkS"))
  (gr_text "GND" (at 40.64 23.622) (layer "F.SilkS"))
  (gr_text "GND" (at 43.815 93.472) (layer "F.SilkS"))
  (gr_text "Out" (at 68.072 70.612) (layer "F.SilkS"))
  (gr_text "5V" (at 41.823 91.059) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 113.03 27.432) (xy 36.83 27.432))
    (height 5.334)
    (gr_text "3.0000 in" (at 74.93 20.948) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 0) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 113.03 98.552) (xy 113.03 27.432))
    (height 5.08)
    (gr_text "2.8000 in" (at 116.96 62.992 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 0) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (zone (net 36) (net_name "VCC") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.07 57.837786)
        (xy 52.324 58.091786)
        (xy 53.594 58.091786)
        (xy 53.594 59.361786)
        (xy 50.546 59.361786)
        (xy 50.546 60.885786)
        (xy 50.038 61.393786)
        (xy 47.752 61.393786)
        (xy 47.752 57.329786)
        (xy 52.07 57.329786)
      )
    )
  )
  (zone (net 38) (net_name "Net-(J24-Pin_1)") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60.96 57.658)
        (xy 62.23 58.928)
        (xy 62.23 64.008)
        (xy 55.118 64.008)
        (xy 55.118 59.615786)
        (xy 54.61 59.107786)
        (xy 54.61 58.345786)
        (xy 55.88 58.345786)
        (xy 56.134 58.091786)
        (xy 56.134 56.769)
        (xy 58.42 56.769)
        (xy 60.96 56.769)
      )
    )
  )
  (zone (net 137) (net_name "Net-(D14-A)") (layer "F.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 78.74 54.61)
        (xy 85.598 54.61)
        (xy 85.598 52.324)
        (xy 84.074 52.324)
        (xy 82.804 51.054)
        (xy 82.804 49.276)
        (xy 78.74 49.276)
      )
    )
  )
  (zone (net 40) (net_name "5Vclean") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.582 9.906)
        (xy 84.582 7.112)
        (xy 102.362 7.112)
        (xy 102.362 12.446)
        (xy 98.933 12.446)
        (xy 98.933 9.9695)
      )
    )
  )
  (zone (net 73) (net_name "/Power/GNDP") (layers "F.Cu" "In1.Cu" "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.95 96.012)
        (xy 85.09 96.012)
        (xy 85.09 87.757)
        (xy 69.342 87.757)
        (xy 69.342 74.168)
        (xy 107.95 74.168)
      )
    )
  )
  (zone (net 22) (net_name "GNDA") (layer "In1.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 69.977 21.5392)
        (xy 64.77 21.5392)
        (xy 64.77 26.162)
        (xy 69.977 26.162)
      )
    )
  )
  (zone (net 22) (net_name "GNDA") (layers "In1.Cu" "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.95 26.162)
        (xy 69.977 26.162)
        (xy 69.977 21.5392)
        (xy 64.77 21.5392)
        (xy 64.77 5.842)
        (xy 107.95 5.842)
      )
    )
  )
  (zone (net 6) (net_name "GND") (layers "In1.Cu" "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.95 73.66)
        (xy 68.834 73.66)
        (xy 68.834 88.138)
        (xy 84.582 88.138)
        (xy 84.582 96.012)
        (xy 36.83 96.012)
        (xy 36.83 5.842)
        (xy 64.262 5.842)
        (xy 64.262 26.67)
        (xy 107.95 26.67)
      )
    )
  )
  (zone (net 7) (net_name "VCC3V3") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 64.262 21.082)
        (xy 79.375 21.082)
        (xy 79.375 26.162)
        (xy 75.438 26.162)
        (xy 75.438 46.228)
        (xy 36.83 46.228)
        (xy 36.83 5.842)
        (xy 64.262 5.842)
      )
    )
  )
  (zone (net 8) (net_name "VCC5V0") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.95 32.512)
        (xy 88.646 32.512)
        (xy 88.646 60.96)
        (xy 80.01 60.96)
        (xy 78.486 62.484)
        (xy 78.486 65.024)
        (xy 82.296 65.024)
        (xy 82.296 73.66)
        (xy 68.834 73.66)
        (xy 68.834 96.012)
        (xy 36.83 96.012)
        (xy 36.83 90.17)
        (xy 59.182 90.17)
        (xy 59.182 65.024)
        (xy 75.946 65.024)
        (xy 75.946 26.67)
        (xy 80.01 26.67)
        (xy 100.33 26.67)
        (xy 100.33 5.842)
        (xy 107.95 5.842)
      )
    )
  )
  (zone (net 32) (net_name "VDDA") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.375 5.842)
        (xy 79.375 20.447)
        (xy 64.77 20.447)
        (xy 64.77 5.842)
      )
    )
  )
  (zone (net 22) (net_name "GNDA") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.822 26.162)
        (xy 80.01 26.162)
        (xy 80.01 5.842)
        (xy 99.822 5.842)
      )
    )
  )
  (zone (net 117) (net_name "FC_3V3") (layer "In2.Cu") (hatch edge 0.5)
    (priority 4)
    (connect_pads (clearance 0.254))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 101.346 54.61)
        (xy 89.154 54.61)
        (xy 89.154 33.02)
        (xy 101.346 33.02)
      )
    )
  )
  (zone (net 6) (net_name "GND") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.95 73.66)
        (xy 82.804 73.66)
        (xy 82.804 65.024)
        (xy 95.504 65.024)
        (xy 95.504 62.23)
        (xy 107.95 62.23)
      )
    )
  )
  (zone (net 6) (net_name "GND") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.582 96.012)
        (xy 69.342 96.012)
        (xy 69.342 88.138)
        (xy 84.582 88.138)
      )
    )
  )
  (zone (net 116) (net_name "FC_5V") (layer "In2.Cu") (hatch edge 0.5)
    (priority 3)
    (connect_pads (clearance 0.254))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 78.994 62.738)
        (xy 80.264 61.468)
        (xy 89.154 61.468)
        (xy 89.154 55.118)
        (xy 101.854 55.118)
        (xy 101.854 33.02)
        (xy 107.95 33.02)
        (xy 107.95 61.722)
        (xy 94.996 61.722)
        (xy 94.996 64.516)
        (xy 78.994 64.516)
      )
    )
  )
  (zone (net 36) (net_name "VCC") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.83 46.736)
        (xy 71.628 46.736)
        (xy 72.898 46.736)
        (xy 75.438 46.736)
        (xy 75.438 64.516)
        (xy 58.674 64.516)
        (xy 58.674 89.662)
        (xy 36.83 89.662)
      )
    )
  )
)
