<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>+15V</text>
<text>-15V</text>
<wire x1="-25.4" y1="44.45" x2="-25.4" y2="-76.2" width="0" layer="20"/>
<wire x1="-25.4" y1="-76.2" x2="25.4" y2="-76.2" width="0" layer="20"/>
<wire x1="25.4" y1="-76.2" x2="25.4" y2="44.45" width="0" layer="20"/>
<wire x1="25.4" y1="44.45" x2="-25.4" y2="44.45" width="0" layer="20"/>
<text>IN_0</text>
<text>IN_1</text>
<text>IN_2</text>
<text>IN_3</text>
<text>OUT_0</text>
<text>OUT_1</text>
<text>OUT_2</text>
<text>OUT_3</text>
<hole x="21.59" y="29.21" drill="3.175"/>
<hole x="-21.59" y="29.21" drill="3.175"/>
<hole x="-21.59" y="-72.39" drill="3.175"/>
<hole x="21.59" y="-72.39" drill="3.175"/>
<text>git.io/vylRr
v1.0</text>
</plain>
<libraries>
<library name="differential-buffer">
<packages>
<package name="SOIC-8">
</package>
</packages>
</library>
<library name="connector-jqi">
<packages>
<package name="BNC90">
<description>Right angle BNC. AMP_227161.</description>
</package>
</packages>
</library>
<library name="Eurocard-HV-piezo-driver">
<description>Generated from &lt;b&gt;Eurocard-HV-piezo-driver.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs-replace2.ulp</description>
<packages>
<package name="BNC90">
<description>Right angle BNC. AMP_227161.</description>
</package>
<package name="R_0603">
</package>
<package name="C_MLCC_0603">
</package>
<package name="C_MLCC_0805">
</package>
<package name="L_FERRITE_0603">
</package>
</packages>
</library>
<library name="jqi_passives">
<description>Library originally designed by Joshua Bienfang NIST.
Pad's sizes are slightly smaller than Eagle's default producing an artwork that is more compact.

Symbols are also compact, but still fit on a standard .1'' grid. 
Additional passive components (RLC and trimpots) can be added.</description>
<packages>
<package name="R_0603">
</package>
<package name="R_0402">
</package>
<package name="PANASONIC_F">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="JQI_Logo">
<description>Connectors &amp; Components for PTS &amp; PulseBlaster related boards</description>
<packages>
<package name="JQI_LOGO_NEGATIVE-SILKSCREEN">
<description>JQI Logo, Silkscreen background with lettering showing stop mask</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="differential-buffer" package="SOIC-8" value="AD8421">
<attribute name="NAME"/>
</element>
<element name="OUT_CH0" library="connector-jqi" package="BNC90" value="BNC-H">
<attribute name="DIGIKEY" value="A32260-ND"/>
</element>
<element name="IN_CH0" library="Eurocard-HV-piezo-driver" package="BNC90" value="BNC-H">
<attribute name="PARTNO" value="A32260-ND"/>
<attribute name="DIGIKEY" value="12345"/>
</element>
<element name="R2" library="Eurocard-HV-piezo-driver" package="R_0603" value="10k">
<attribute name="PARTNO" value="TNP10.0KAACT-ND"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="Eurocard-HV-piezo-driver" package="C_MLCC_0603" value="100nF">
<attribute name="PARTNO" value="1276-1936-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="C4" library="Eurocard-HV-piezo-driver" package="C_MLCC_0805" value="10uF">
<attribute name="PARTNO" value="445-14417-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="L2" library="Eurocard-HV-piezo-driver" package="L_FERRITE_0603" value="1000k Ferrite">
<attribute name="PARTNO" value="445-1548-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="C1" library="Eurocard-HV-piezo-driver" package="C_MLCC_0603" value="100nF">
<attribute name="PARTNO" value="1276-1936-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="Eurocard-HV-piezo-driver" package="C_MLCC_0805" value="10uF">
<attribute name="PARTNO" value="445-14417-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="L1" library="Eurocard-HV-piezo-driver" package="L_FERRITE_0603" value="1000k Ferrite">
<attribute name="PARTNO" value="445-1548-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="jqi_passives" package="R_0603" value="49.9R">
<attribute name="NAME"/>
</element>
<element name="R3" library="jqi_passives" package="R_0603" value="49.9R">
<attribute name="NAME"/>
</element>
<element name="RG0" library="jqi_passives" package="R_0402" value="">
<attribute name="NAME"/>
</element>
<element name="U2" library="differential-buffer" package="SOIC-8" value="AD8421">
<attribute name="NAME"/>
</element>
<element name="OUT_CH1" library="connector-jqi" package="BNC90" value="BNC-H">
<attribute name="DIGIKEY" value="A32260-ND"/>
</element>
<element name="IN_CH1" library="Eurocard-HV-piezo-driver" package="BNC90" value="BNC-H">
<attribute name="PARTNO" value="A32260-ND"/>
<attribute name="DIGIKEY" value="12345"/>
</element>
<element name="R4" library="Eurocard-HV-piezo-driver" package="R_0603" value="10k">
<attribute name="PARTNO" value="TNP10.0KAACT-ND"/>
<attribute name="NAME"/>
</element>
<element name="C5" library="Eurocard-HV-piezo-driver" package="C_MLCC_0603" value="100nF">
<attribute name="PARTNO" value="1276-1936-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="C6" library="Eurocard-HV-piezo-driver" package="C_MLCC_0805" value="10uF">
<attribute name="PARTNO" value="445-14417-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="L3" library="Eurocard-HV-piezo-driver" package="L_FERRITE_0603" value="1000k Ferrite">
<attribute name="PARTNO" value="445-1548-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="C7" library="Eurocard-HV-piezo-driver" package="C_MLCC_0603" value="100nF">
<attribute name="PARTNO" value="1276-1936-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="C8" library="Eurocard-HV-piezo-driver" package="C_MLCC_0805" value="10uF">
<attribute name="PARTNO" value="445-14417-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="L4" library="Eurocard-HV-piezo-driver" package="L_FERRITE_0603" value="1000k Ferrite">
<attribute name="PARTNO" value="445-1548-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="R5" library="jqi_passives" package="R_0603" value="49.9R">
<attribute name="NAME"/>
</element>
<element name="R6" library="jqi_passives" package="R_0603" value="49.9R">
<attribute name="NAME"/>
</element>
<element name="RG1" library="jqi_passives" package="R_0402" value="">
<attribute name="NAME"/>
</element>
<element name="U3" library="differential-buffer" package="SOIC-8" value="AD8421">
<attribute name="NAME"/>
</element>
<element name="OUT_CH2" library="connector-jqi" package="BNC90" value="BNC-H">
<attribute name="DIGIKEY" value="A32260-ND"/>
</element>
<element name="IN_CH2" library="Eurocard-HV-piezo-driver" package="BNC90" value="BNC-H">
<attribute name="PARTNO" value="A32260-ND"/>
<attribute name="DIGIKEY" value="12345"/>
</element>
<element name="R7" library="Eurocard-HV-piezo-driver" package="R_0603" value="10k">
<attribute name="PARTNO" value="TNP10.0KAACT-ND"/>
<attribute name="NAME"/>
</element>
<element name="C9" library="Eurocard-HV-piezo-driver" package="C_MLCC_0603" value="100nF">
<attribute name="PARTNO" value="1276-1936-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="C10" library="Eurocard-HV-piezo-driver" package="C_MLCC_0805" value="10uF">
<attribute name="PARTNO" value="445-14417-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="L5" library="Eurocard-HV-piezo-driver" package="L_FERRITE_0603" value="1000k Ferrite">
<attribute name="PARTNO" value="445-1548-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="C11" library="Eurocard-HV-piezo-driver" package="C_MLCC_0603" value="100nF">
<attribute name="PARTNO" value="1276-1936-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="C12" library="Eurocard-HV-piezo-driver" package="C_MLCC_0805" value="10uF">
<attribute name="PARTNO" value="445-14417-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="L6" library="Eurocard-HV-piezo-driver" package="L_FERRITE_0603" value="1000k Ferrite">
<attribute name="PARTNO" value="445-1548-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="R8" library="jqi_passives" package="R_0603" value="49.9R">
<attribute name="NAME"/>
</element>
<element name="R9" library="jqi_passives" package="R_0603" value="49.9R">
<attribute name="NAME"/>
</element>
<element name="RG2" library="jqi_passives" package="R_0402" value="">
<attribute name="NAME"/>
</element>
<element name="U4" library="differential-buffer" package="SOIC-8" value="AD8421">
<attribute name="NAME"/>
</element>
<element name="OUT_CH3" library="connector-jqi" package="BNC90" value="BNC-H">
<attribute name="DIGIKEY" value="A32260-ND"/>
</element>
<element name="IN_CH3" library="Eurocard-HV-piezo-driver" package="BNC90" value="BNC-H">
<attribute name="PARTNO" value="A32260-ND"/>
<attribute name="DIGIKEY" value="12345"/>
</element>
<element name="R10" library="Eurocard-HV-piezo-driver" package="R_0603" value="10k">
<attribute name="PARTNO" value="TNP10.0KAACT-ND"/>
<attribute name="NAME"/>
</element>
<element name="C13" library="Eurocard-HV-piezo-driver" package="C_MLCC_0603" value="100nF">
<attribute name="PARTNO" value="1276-1936-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="C14" library="Eurocard-HV-piezo-driver" package="C_MLCC_0805" value="10uF">
<attribute name="PARTNO" value="445-14417-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="L7" library="Eurocard-HV-piezo-driver" package="L_FERRITE_0603" value="1000k Ferrite">
<attribute name="PARTNO" value="445-1548-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="C15" library="Eurocard-HV-piezo-driver" package="C_MLCC_0603" value="100nF">
<attribute name="PARTNO" value="1276-1936-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="C16" library="Eurocard-HV-piezo-driver" package="C_MLCC_0805" value="10uF">
<attribute name="PARTNO" value="445-14417-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="L8" library="Eurocard-HV-piezo-driver" package="L_FERRITE_0603" value="1000k Ferrite">
<attribute name="PARTNO" value="445-1548-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="R11" library="jqi_passives" package="R_0603" value="49.9R">
<attribute name="NAME"/>
</element>
<element name="R12" library="jqi_passives" package="R_0603" value="49.9R">
<attribute name="NAME"/>
</element>
<element name="RG3" library="jqi_passives" package="R_0402" value="">
<attribute name="NAME"/>
</element>
<element name="JP1" library="pinhead" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="jqi_passives" package="PANASONIC_F" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="jqi_passives" package="PANASONIC_F" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="JQI_Logo" package="JQI_LOGO_NEGATIVE-SILKSCREEN" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="OUT_CH0" pad="2"/>
<contactref element="C4" pad="P$2"/>
<contactref element="C3" pad="P$2"/>
<contactref element="C2" pad="P$2"/>
<contactref element="C1" pad="P$2"/>
<contactref element="R1" pad="P$1"/>
<contactref element="U1" pad="6"/>
<contactref element="OUT_CH1" pad="2"/>
<contactref element="C6" pad="P$2"/>
<contactref element="C5" pad="P$2"/>
<contactref element="C8" pad="P$2"/>
<contactref element="C7" pad="P$2"/>
<contactref element="R5" pad="P$1"/>
<contactref element="U2" pad="6"/>
<contactref element="OUT_CH2" pad="2"/>
<contactref element="C10" pad="P$2"/>
<contactref element="C9" pad="P$2"/>
<contactref element="C12" pad="P$2"/>
<contactref element="C11" pad="P$2"/>
<contactref element="R8" pad="P$1"/>
<contactref element="U3" pad="6"/>
<contactref element="OUT_CH3" pad="2"/>
<contactref element="C14" pad="P$2"/>
<contactref element="C13" pad="P$2"/>
<contactref element="C16" pad="P$2"/>
<contactref element="C15" pad="P$2"/>
<contactref element="R11" pad="P$1"/>
<contactref element="U4" pad="6"/>
<contactref element="JP1" pad="2"/>
<contactref element="C17" pad="-"/>
<contactref element="C18" pad="+"/>
</signal>
<signal name="N$56">
<contactref element="IN_CH0" pad="1"/>
<contactref element="R2" pad="P$2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$57">
<contactref element="IN_CH0" pad="2"/>
<contactref element="R2" pad="P$1"/>
<contactref element="U1" pad="1"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$1">
<contactref element="OUT_CH0" pad="1"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="7"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="V-">
<contactref element="L2" pad="P$2"/>
<contactref element="L3" pad="P$2"/>
<contactref element="L5" pad="P$2"/>
<contactref element="L7" pad="P$2"/>
<contactref element="JP1" pad="3"/>
<contactref element="C18" pad="-"/>
</signal>
<signal name="N$63">
<contactref element="C4" pad="P$1"/>
<contactref element="C3" pad="P$1"/>
<contactref element="U1" pad="5"/>
<contactref element="L2" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="C2" pad="P$1"/>
<contactref element="C1" pad="P$1"/>
<contactref element="L1" pad="P$1"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="V+">
<contactref element="L1" pad="P$2"/>
<contactref element="L4" pad="P$2"/>
<contactref element="L6" pad="P$2"/>
<contactref element="L8" pad="P$2"/>
<contactref element="C17" pad="+"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="RG0" pad="P$1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="2"/>
<contactref element="RG0" pad="P$2"/>
</signal>
<signal name="N$6">
<contactref element="IN_CH1" pad="1"/>
<contactref element="R4" pad="P$2"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="IN_CH1" pad="2"/>
<contactref element="R4" pad="P$1"/>
<contactref element="U2" pad="1"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="N$8">
<contactref element="OUT_CH1" pad="1"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="U2" pad="7"/>
<contactref element="R6" pad="P$2"/>
</signal>
<signal name="N$10">
<contactref element="C6" pad="P$1"/>
<contactref element="C5" pad="P$1"/>
<contactref element="U2" pad="5"/>
<contactref element="L3" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="C8" pad="P$1"/>
<contactref element="C7" pad="P$1"/>
<contactref element="L4" pad="P$1"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="N$12">
<contactref element="RG1" pad="P$1"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="U2" pad="2"/>
<contactref element="RG1" pad="P$2"/>
</signal>
<signal name="N$14">
<contactref element="IN_CH2" pad="1"/>
<contactref element="R7" pad="P$2"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="N$15">
<contactref element="IN_CH2" pad="2"/>
<contactref element="R7" pad="P$1"/>
<contactref element="U3" pad="1"/>
<contactref element="R8" pad="P$2"/>
</signal>
<signal name="N$16">
<contactref element="OUT_CH2" pad="1"/>
<contactref element="R9" pad="P$1"/>
</signal>
<signal name="N$17">
<contactref element="U3" pad="7"/>
<contactref element="R9" pad="P$2"/>
</signal>
<signal name="N$18">
<contactref element="C10" pad="P$1"/>
<contactref element="C9" pad="P$1"/>
<contactref element="U3" pad="5"/>
<contactref element="L5" pad="P$1"/>
</signal>
<signal name="N$19">
<contactref element="C12" pad="P$1"/>
<contactref element="C11" pad="P$1"/>
<contactref element="L6" pad="P$1"/>
<contactref element="U3" pad="8"/>
</signal>
<signal name="N$20">
<contactref element="RG2" pad="P$1"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="N$21">
<contactref element="U3" pad="2"/>
<contactref element="RG2" pad="P$2"/>
</signal>
<signal name="N$22">
<contactref element="IN_CH3" pad="1"/>
<contactref element="R10" pad="P$2"/>
<contactref element="U4" pad="4"/>
</signal>
<signal name="N$23">
<contactref element="IN_CH3" pad="2"/>
<contactref element="R10" pad="P$1"/>
<contactref element="U4" pad="1"/>
<contactref element="R11" pad="P$2"/>
</signal>
<signal name="N$24">
<contactref element="OUT_CH3" pad="1"/>
<contactref element="R12" pad="P$1"/>
</signal>
<signal name="N$25">
<contactref element="U4" pad="7"/>
<contactref element="R12" pad="P$2"/>
</signal>
<signal name="N$26">
<contactref element="C14" pad="P$1"/>
<contactref element="C13" pad="P$1"/>
<contactref element="U4" pad="5"/>
<contactref element="L7" pad="P$1"/>
</signal>
<signal name="N$27">
<contactref element="C16" pad="P$1"/>
<contactref element="C15" pad="P$1"/>
<contactref element="L8" pad="P$1"/>
<contactref element="U4" pad="8"/>
</signal>
<signal name="N$28">
<contactref element="RG3" pad="P$1"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="N$29">
<contactref element="U4" pad="2"/>
<contactref element="RG3" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
