<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.1">
<drawing>
<board>
<plain>
<wire x1="0.7747" y1="1.0922" x2="0.7747" y2="33.09111875" width="0" layer="20"/>
<wire x1="0.7747" y1="33.09111875" x2="9.45641875" y2="33.09111875" width="0" layer="20"/>
<wire x1="9.45641875" y1="33.09111875" x2="9.45641875" y2="31.61538125" width="0" layer="20"/>
<wire x1="9.45641875" y1="31.61538125" x2="13.091159375" y2="31.61538125" width="0" layer="20"/>
<wire x1="13.091159375" y1="31.61538125" x2="13.091159375" y2="33.09111875" width="0" layer="20"/>
<wire x1="13.091159375" y1="33.09111875" x2="35.7759" y2="33.09111875" width="0" layer="20"/>
<wire x1="35.7759" y1="33.09111875" x2="35.7759" y2="1.0922" width="0" layer="20"/>
<wire x1="35.7759" y1="1.0922" x2="13.1572" y2="1.0922" width="0" layer="20"/>
<wire x1="13.1572" y1="1.0922" x2="13.1572" y2="2.52221875" width="0" layer="20"/>
<wire x1="13.1572" y1="2.52221875" x2="9.3472" y2="2.52221875" width="0" layer="20"/>
<wire x1="9.3472" y1="2.52221875" x2="9.3472" y2="1.0922" width="0" layer="20"/>
<wire x1="9.3472" y1="1.0922" x2="0.7747" y2="1.0922" width="0" layer="20"/>
<wire x1="31.61791875" y1="19.18208125" x2="31.61791875" y2="20.87371875" width="0.010159375" layer="20"/>
<wire x1="31.61791875" y1="20.87371875" x2="31.623" y2="20.94991875" width="0.010159375" layer="20"/>
<wire x1="31.623" y1="20.94991875" x2="31.6357" y2="21.02611875" width="0.010159375" layer="20"/>
<wire x1="31.6357" y1="21.02611875" x2="31.658559375" y2="21.09978125" width="0.010159375" layer="20"/>
<wire x1="31.658559375" y1="21.09978125" x2="31.69158125" y2="21.168359375" width="0.010159375" layer="20"/>
<wire x1="31.69158125" y1="21.168359375" x2="31.72968125" y2="21.2344" width="0.010159375" layer="20"/>
<wire x1="31.72968125" y1="21.2344" x2="31.777940625" y2="21.295359375" width="0.010159375" layer="20"/>
<wire x1="31.777940625" y1="21.295359375" x2="31.83128125" y2="21.3487" width="0.010159375" layer="20"/>
<wire x1="31.83128125" y1="21.3487" x2="31.892240625" y2="21.396959375" width="0.010159375" layer="20"/>
<wire x1="31.892240625" y1="21.396959375" x2="31.95828125" y2="21.435059375" width="0.010159375" layer="20"/>
<wire x1="31.95828125" y1="21.435059375" x2="32.026859375" y2="21.46808125" width="0.010159375" layer="20"/>
<wire x1="32.026859375" y1="21.46808125" x2="32.10051875" y2="21.490940625" width="0.010159375" layer="20"/>
<wire x1="32.10051875" y1="21.490940625" x2="32.17671875" y2="21.503640625" width="0.010159375" layer="20"/>
<wire x1="32.17671875" y1="21.503640625" x2="32.25291875" y2="21.50871875" width="0.010159375" layer="20"/>
<wire x1="32.25291875" y1="21.50871875" x2="32.32911875" y2="21.503640625" width="0.010159375" layer="20"/>
<wire x1="32.32911875" y1="21.503640625" x2="32.40531875" y2="21.490940625" width="0.010159375" layer="20"/>
<wire x1="32.40531875" y1="21.490940625" x2="32.47898125" y2="21.46808125" width="0.010159375" layer="20"/>
<wire x1="32.47898125" y1="21.46808125" x2="32.547559375" y2="21.435059375" width="0.010159375" layer="20"/>
<wire x1="32.547559375" y1="21.435059375" x2="32.6136" y2="21.396959375" width="0.010159375" layer="20"/>
<wire x1="32.6136" y1="21.396959375" x2="32.674559375" y2="21.3487" width="0.010159375" layer="20"/>
<wire x1="32.674559375" y1="21.3487" x2="32.7279" y2="21.295359375" width="0.010159375" layer="20"/>
<wire x1="32.7279" y1="21.295359375" x2="32.776159375" y2="21.2344" width="0.010159375" layer="20"/>
<wire x1="32.776159375" y1="21.2344" x2="32.814259375" y2="21.168359375" width="0.010159375" layer="20"/>
<wire x1="32.814259375" y1="21.168359375" x2="32.84728125" y2="21.09978125" width="0.010159375" layer="20"/>
<wire x1="32.84728125" y1="21.09978125" x2="32.870140625" y2="21.02611875" width="0.010159375" layer="20"/>
<wire x1="32.870140625" y1="21.02611875" x2="32.882840625" y2="20.94991875" width="0.010159375" layer="20"/>
<wire x1="32.882840625" y1="20.94991875" x2="32.88791875" y2="20.87371875" width="0.010159375" layer="20"/>
<wire x1="32.88791875" y1="20.87371875" x2="32.88791875" y2="19.18208125" width="0.010159375" layer="20"/>
<wire x1="32.88791875" y1="19.18208125" x2="32.882840625" y2="19.10588125" width="0.010159375" layer="20"/>
<wire x1="32.882840625" y1="19.10588125" x2="32.870140625" y2="19.02968125" width="0.010159375" layer="20"/>
<wire x1="32.870140625" y1="19.02968125" x2="32.84728125" y2="18.95601875" width="0.010159375" layer="20"/>
<wire x1="32.84728125" y1="18.95601875" x2="32.814259375" y2="18.887440625" width="0.010159375" layer="20"/>
<wire x1="32.814259375" y1="18.887440625" x2="32.776159375" y2="18.8214" width="0.010159375" layer="20"/>
<wire x1="32.776159375" y1="18.8214" x2="32.7279" y2="18.760440625" width="0.010159375" layer="20"/>
<wire x1="32.7279" y1="18.760440625" x2="32.674559375" y2="18.7071" width="0.010159375" layer="20"/>
<wire x1="32.674559375" y1="18.7071" x2="32.6136" y2="18.658840625" width="0.010159375" layer="20"/>
<wire x1="32.6136" y1="18.658840625" x2="32.547559375" y2="18.620740625" width="0.010159375" layer="20"/>
<wire x1="32.547559375" y1="18.620740625" x2="32.47898125" y2="18.58771875" width="0.010159375" layer="20"/>
<wire x1="32.47898125" y1="18.58771875" x2="32.40531875" y2="18.564859375" width="0.010159375" layer="20"/>
<wire x1="32.40531875" y1="18.564859375" x2="32.32911875" y2="18.552159375" width="0.010159375" layer="20"/>
<wire x1="32.32911875" y1="18.552159375" x2="32.25291875" y2="18.54708125" width="0.010159375" layer="20"/>
<wire x1="32.25291875" y1="18.54708125" x2="32.17671875" y2="18.552159375" width="0.010159375" layer="20"/>
<wire x1="32.17671875" y1="18.552159375" x2="32.10051875" y2="18.564859375" width="0.010159375" layer="20"/>
<wire x1="32.10051875" y1="18.564859375" x2="32.026859375" y2="18.58771875" width="0.010159375" layer="20"/>
<wire x1="32.026859375" y1="18.58771875" x2="31.95828125" y2="18.620740625" width="0.010159375" layer="20"/>
<wire x1="31.95828125" y1="18.620740625" x2="31.892240625" y2="18.658840625" width="0.010159375" layer="20"/>
<wire x1="31.892240625" y1="18.658840625" x2="31.83128125" y2="18.7071" width="0.010159375" layer="20"/>
<wire x1="31.83128125" y1="18.7071" x2="31.777940625" y2="18.760440625" width="0.010159375" layer="20"/>
<wire x1="31.777940625" y1="18.760440625" x2="31.72968125" y2="18.8214" width="0.010159375" layer="20"/>
<wire x1="31.72968125" y1="18.8214" x2="31.69158125" y2="18.887440625" width="0.010159375" layer="20"/>
<wire x1="31.69158125" y1="18.887440625" x2="31.658559375" y2="18.95601875" width="0.010159375" layer="20"/>
<wire x1="31.658559375" y1="18.95601875" x2="31.6357" y2="19.02968125" width="0.010159375" layer="20"/>
<wire x1="31.6357" y1="19.02968125" x2="31.623" y2="19.10588125" width="0.010159375" layer="20"/>
<wire x1="31.623" y1="19.10588125" x2="31.61791875" y2="19.18208125" width="0.010159375" layer="20"/>
<text>All Models:

R7-R9 = 3.6MΩ
C1-C3 = 82nf

Package Size 0805</text>
<text>RGB Bypass For SMS 1/2 and
Genesis/MegaDrive 1/2
RF Kickout Installable
Original Design by ArcadeTV

MD1:
R1-3 = 5.6kΩ
R4-6 = 1.0kΩ

MD2:
R1-3 = 5.6kΩ
R4-6 = 1.0kΩ

SMS1/2:
R1-6 = 4.7kΩ</text>
<text>Genesis/MegaDrive 1 and 2
Master System 1 and 2
RGB Bypass Board</text>
<text>Mobius Strip Technologies v2.0</text>
</plain>
<libraries>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD2,54-5,08">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOIC8">
<description>&lt;b&gt;SOIC-8&lt;/b&gt; CASE 751-07&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC34164-D.PDF&lt;p&gt;
&lt;b&gt;D (R-PDSO-G8)&lt;/b&gt;PLATIC SMALL-OUTLINE PACKAGE&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/tlc27l2.pdf</description>
</package>
</packages>
</library>
<library name="special-drill">
<description>&lt;b&gt;Special drills&lt;/b&gt;&lt;p&gt;
For drills bigger as 0.51602 Inch you must draw a circle in Layer 20 Dimension.&lt;br&gt;
See also HELP HOLE,</description>
<packages>
<package name="PAD_0.1000">
<description>&lt;b&gt;0.1000 Inch&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BI" library="wirepad" package="SMD2,54-5,08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GI" library="wirepad" package="SMD2,54-5,08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RI" library="wirepad" package="SMD2,54-5,08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C#I" library="wirepad" package="SMD2,54-5,08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5V" library="wirepad" package="SMD2,54-5,08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND2" library="wirepad" package="SMD2,54-5,08" value="">
<attribute name="VALUE"/>
</element>
<element name="GND" library="wirepad" package="SMD2,54-5,08" value="">
<attribute name="VALUE"/>
</element>
<element name="CSO" library="wirepad" package="SMD2,54-5,08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RO" library="wirepad" package="SMD2,54-5,08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GO" library="wirepad" package="SMD2,54-5,08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BO" library="wirepad" package="SMD2,54-5,08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="2.2K" library="eagle-ltspice" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="eagle-ltspice" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="eagle-ltspice" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="eagle-ltspice" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="eagle-ltspice" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="eagle-ltspice" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="eagle-ltspice" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="eagle-ltspice" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="eagle-ltspice" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="eagle-ltspice" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="eagle-ltspice" package="C0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="eagle-ltspice" package="C0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="eagle-ltspice" package="C0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="100NF" library="eagle-ltspice" package="C0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="22UF" library="eagle-ltspice" package="C0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="THS7314" library="linear" package="SOIC8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$1" library="special-drill" package="PAD_0.1000" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$1">
<contactref element="2.2K" pad="1"/>
<contactref element="C#I" pad="1"/>
<contactref element="CSO" pad="1"/>
</signal>
<signal name="S$2">
<contactref element="2.2K" pad="2"/>
<contactref element="5V" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="THS7314" pad="4"/>
<contactref element="100NF" pad="1"/>
<contactref element="22UF" pad="1"/>
</signal>
<signal name="S$3">
<contactref element="R1" pad="1"/>
<contactref element="RI" pad="1"/>
</signal>
<signal name="S$4">
<contactref element="R4" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="S$5">
<contactref element="R9" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="THS7314" pad="1"/>
</signal>
<signal name="S$6">
<contactref element="R2" pad="1"/>
<contactref element="GI" pad="1"/>
</signal>
<signal name="S$7">
<contactref element="R5" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="S$8">
<contactref element="R8" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="THS7314" pad="2"/>
</signal>
<signal name="S$9">
<contactref element="R7" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="THS7314" pad="3"/>
</signal>
<signal name="S$10">
<contactref element="R6" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="S$11">
<contactref element="BI" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="S$12">
<contactref element="RO" pad="1"/>
<contactref element="THS7314" pad="8"/>
</signal>
<signal name="S$13">
<contactref element="GO" pad="1"/>
<contactref element="THS7314" pad="7"/>
</signal>
<signal name="S$14">
<contactref element="BO" pad="1"/>
<contactref element="THS7314" pad="6"/>
</signal>
<signal name="GND">
<contactref element="GND2" pad="1"/>
<contactref element="GND" pad="1"/>
<contactref element="THS7314" pad="5"/>
<contactref element="100NF" pad="2"/>
<contactref element="22UF" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="E$1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
