(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)
  (general
    (thickness 1.6)
    (drawings 22)
    (tracks 305)
    (zones 0)
    (modules 6)
    (nets 90)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber2/"))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(IC1-Pad25)")
  (net 4 "Net-(IC1-Pad24)")
  (net 5 "Net-(IC1-Pad23)")
  (net 6 "Net-(IC1-Pad22)")
  (net 7 "Net-(IC1-Pad21)")
  (net 8 "Net-(IC1-Pad20)")
  (net 9 "Net-(IC1-Pad19)")
  (net 10 "Net-(IC1-Pad18)")
  (net 11 "Net-(IC1-Pad17)")
  (net 12 "Net-(IC1-Pad16)")
  (net 13 "Net-(IC1-Pad15)")
  (net 14 "Net-(IC1-Pad13)")
  (net 15 "Net-(IC1-Pad12)")
  (net 16 "Net-(IC1-Pad11)")
  (net 17 "Net-(IC1-Pad10)")
  (net 18 "Net-(IC1-Pad9)")
  (net 19 "Net-(IC1-Pad8)")
  (net 20 "Net-(IC1-Pad7)")
  (net 21 "Net-(IC1-Pad6)")
  (net 22 "Net-(IC1-Pad5)")
  (net 23 "Net-(IC1-Pad26)")
  (net 24 "Net-(IC1-Pad27)")
  (net 25 "Net-(IC1-Pad4)")
  (net 26 "Net-(IC1-Pad3)")
  (net 27 "Net-(IC1-Pad2)")
  (net 28 "Net-(IC1-Pad1)")
  (net 29 "Net-(IC2-Pad74)")
  (net 30 "Net-(IC2-Pad73)")
  (net 31 "Net-(IC2-Pad72)")
  (net 32 "Net-(IC2-Pad71)")
  (net 33 "Net-(IC2-Pad69)")
  (net 34 "Net-(IC2-Pad68)")
  (net 35 "Net-(IC2-Pad67)")
  (net 36 "Net-(IC2-Pad66)")
  (net 37 "Net-(IC2-Pad65)")
  (net 38 "Net-(IC2-Pad64)")
  (net 39 "Net-(IC2-Pad63)")
  (net 40 "Net-(IC2-Pad62)")
  (net 41 "Net-(IC2-Pad61)")
  (net 42 "Net-(IC2-Pad60)")
  (net 43 "Net-(IC2-Pad59)")
  (net 44 "Net-(IC2-Pad58)")
  (net 45 "Net-(IC2-Pad57)")
  (net 46 "Net-(IC2-Pad56)")
  (net 47 "Net-(IC2-Pad55)")
  (net 48 "Net-(IC2-Pad54)")
  (net 49 "Net-(IC2-Pad52)")
  (net 50 "Net-(IC2-Pad50)")
  (net 51 "Net-(IC2-Pad49)")
  (net 52 "Net-(IC2-Pad48)")
  (net 53 "Net-(IC2-Pad47)")
  (net 54 "Net-(IC2-Pad46)")
  (net 55 "Net-(IC2-Pad45)")
  (net 56 "Net-(IC2-Pad44)")
  (net 57 "Net-(IC2-Pad43)")
  (net 58 "Net-(IC2-Pad41)")
  (net 59 "Net-(IC2-Pad40)")
  (net 60 "Net-(IC2-Pad39)")
  (net 61 "Net-(IC2-Pad38)")
  (net 62 "Net-(IC2-Pad37)")
  (net 63 "Net-(IC2-Pad36)")
  (net 64 "Net-(IC2-Pad35)")
  (net 65 "Net-(IC2-Pad33)")
  (net 66 "Net-(IC2-Pad32)")
  (net 67 "Net-(IC2-Pad31)")
  (net 68 "Net-(IC2-Pad30)")
  (net 69 "Net-(IC2-Pad29)")
  (net 70 "Net-(IC2-Pad28)")
  (net 71 "Net-(IC2-Pad27)")
  (net 72 "Net-(IC2-Pad24)")
  (net 73 "Net-(IC2-Pad23)")
  (net 74 "Net-(IC2-Pad22)")
  (net 75 "Net-(IC2-Pad21)")
  (net 76 "Net-(IC2-Pad20)")
  (net 77 "Net-(IC2-Pad19)")
  (net 78 "Net-(IC2-Pad18)")
  (net 79 "Net-(IC2-Pad16)")
  (net 80 "Net-(IC2-Pad75)")
  (net 81 "Net-(IC2-Pad76)")
  (net 82 "Net-(IC2-Pad77)")
  (net 83 "Net-(IC2-Pad78)")
  (net 84 "Net-(IC2-Pad79)")
  (net 85 "Net-(IC2-Pad80)")
  (net 86 "Net-(IC2-Pad81)")
  (net 87 "Net-(IC2-Pad82)")
  (net 88 "Net-(IC2-Pad83)")
  (net 89 "Net-(IC2-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad15)")
    (add_net "Net-(IC1-Pad16)")
    (add_net "Net-(IC1-Pad17)")
    (add_net "Net-(IC1-Pad18)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad21)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad23)")
    (add_net "Net-(IC1-Pad24)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(IC2-Pad16)")
    (add_net "Net-(IC2-Pad18)")
    (add_net "Net-(IC2-Pad19)")
    (add_net "Net-(IC2-Pad20)")
    (add_net "Net-(IC2-Pad21)")
    (add_net "Net-(IC2-Pad22)")
    (add_net "Net-(IC2-Pad23)")
    (add_net "Net-(IC2-Pad24)")
    (add_net "Net-(IC2-Pad27)")
    (add_net "Net-(IC2-Pad28)")
    (add_net "Net-(IC2-Pad29)")
    (add_net "Net-(IC2-Pad30)")
    (add_net "Net-(IC2-Pad31)")
    (add_net "Net-(IC2-Pad32)")
    (add_net "Net-(IC2-Pad33)")
    (add_net "Net-(IC2-Pad35)")
    (add_net "Net-(IC2-Pad36)")
    (add_net "Net-(IC2-Pad37)")
    (add_net "Net-(IC2-Pad38)")
    (add_net "Net-(IC2-Pad39)")
    (add_net "Net-(IC2-Pad40)")
    (add_net "Net-(IC2-Pad41)")
    (add_net "Net-(IC2-Pad43)")
    (add_net "Net-(IC2-Pad44)")
    (add_net "Net-(IC2-Pad45)")
    (add_net "Net-(IC2-Pad46)")
    (add_net "Net-(IC2-Pad47)")
    (add_net "Net-(IC2-Pad48)")
    (add_net "Net-(IC2-Pad49)")
    (add_net "Net-(IC2-Pad50)")
    (add_net "Net-(IC2-Pad52)")
    (add_net "Net-(IC2-Pad54)")
    (add_net "Net-(IC2-Pad55)")
    (add_net "Net-(IC2-Pad56)")
    (add_net "Net-(IC2-Pad57)")
    (add_net "Net-(IC2-Pad58)")
    (add_net "Net-(IC2-Pad59)")
    (add_net "Net-(IC2-Pad60)")
    (add_net "Net-(IC2-Pad61)")
    (add_net "Net-(IC2-Pad62)")
    (add_net "Net-(IC2-Pad63)")
    (add_net "Net-(IC2-Pad64)")
    (add_net "Net-(IC2-Pad65)")
    (add_net "Net-(IC2-Pad66)")
    (add_net "Net-(IC2-Pad67)")
    (add_net "Net-(IC2-Pad68)")
    (add_net "Net-(IC2-Pad69)")
    (add_net "Net-(IC2-Pad71)")
    (add_net "Net-(IC2-Pad72)")
    (add_net "Net-(IC2-Pad73)")
    (add_net "Net-(IC2-Pad74)")
    (add_net "Net-(IC2-Pad75)")
    (add_net "Net-(IC2-Pad76)")
    (add_net "Net-(IC2-Pad77)")
    (add_net "Net-(IC2-Pad78)")
    (add_net "Net-(IC2-Pad79)")
    (add_net "Net-(IC2-Pad8)")
    (add_net "Net-(IC2-Pad80)")
    (add_net "Net-(IC2-Pad81)")
    (add_net "Net-(IC2-Pad82)")
    (add_net "Net-(IC2-Pad83)")
  )
  (module Symbol:OSHW-Logo_5.7x6mm_Copper locked (layer F.Cu) (tedit 0)
    (at 106.2 84.925)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_Copper (at 0.75 0) (layer F.Fab) hide)
  )
  (module Stormy:PLCC-84_SMD-Socket_mirrored (layer B.Cu) (tedit 5F4B0E9F)
    (at 90.47 69.225 180)
    (descr "PLCC, 84 pins, surface mount")
    (tags "plcc smt")
    (autoplace_cost180 1)
    (attr smd)
    (fp_text reference "FAT GARY" (at -6.105 15.55 180) (layer B.SilkS))
    (fp_text value FAT_GARY (at 0 -17.571 180) (layer B.Fab))
    (fp_text user %R (at 0 -0.525 180) (layer B.Fab))
    (pad 1 smd rect (at 0 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.27 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(IC1-Pad13)"))
    (pad 3 smd rect (at 2.54 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(IC1-Pad12)"))
    (pad 4 smd rect (at 3.81 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(IC1-Pad11)"))
    (pad 5 smd rect (at 5.08 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(IC1-Pad10)"))
    (pad 6 smd rect (at 6.35 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(IC1-Pad9)"))
    (pad 7 smd rect (at 7.62 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at 8.89 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 89 "Net-(IC2-Pad8)"))
    (pad 9 smd rect (at 10.16 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(IC1-Pad6)"))
    (pad 10 smd rect (at 11.43 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(IC1-Pad5)"))
    (pad 11 smd rect (at 12.7 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(IC1-Pad4)"))
    (pad 84 smd rect (at -1.27 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 83 smd rect (at -2.54 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 88 "Net-(IC2-Pad83)"))
    (pad 82 smd rect (at -3.81 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 87 "Net-(IC2-Pad82)"))
    (pad 81 smd rect (at -5.08 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 86 "Net-(IC2-Pad81)"))
    (pad 80 smd rect (at -6.35 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 85 "Net-(IC2-Pad80)"))
    (pad 79 smd rect (at -7.62 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 84 "Net-(IC2-Pad79)"))
    (pad 78 smd rect (at -8.89 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 83 "Net-(IC2-Pad78)"))
    (pad 77 smd rect (at -10.16 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(IC2-Pad77)"))
    (pad 76 smd rect (at -11.43 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(IC2-Pad76)"))
    (pad 75 smd rect (at -12.7 13.6875 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 80 "Net-(IC2-Pad75)"))
    (pad 12 smd rect (at 14.2125 12.175 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(IC1-Pad3)"))
    (pad 13 smd rect (at 14.2125 10.905 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(IC1-Pad25)"))
    (pad 14 smd rect (at 14.2125 9.635 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(IC1-Pad24)"))
    (pad 15 smd rect (at 14.2125 8.365 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(IC1-Pad23)"))
    (pad 16 smd rect (at 14.2125 7.095 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 79 "Net-(IC2-Pad16)"))
    (pad 17 smd rect (at 14.2125 5.825 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 18 smd rect (at 14.2125 4.555 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(IC2-Pad18)"))
    (pad 19 smd rect (at 14.2125 3.285 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 77 "Net-(IC2-Pad19)"))
    (pad 20 smd rect (at 14.2125 2.015 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(IC2-Pad20)"))
    (pad 21 smd rect (at 14.2125 0.745 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(IC2-Pad21)"))
    (pad 22 smd rect (at 14.2125 -0.525 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(IC2-Pad22)"))
    (pad 23 smd rect (at 14.2125 -1.795 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(IC2-Pad23)"))
    (pad 24 smd rect (at 14.2125 -3.065 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 72 "Net-(IC2-Pad24)"))
    (pad 25 smd rect (at 14.2125 -4.335 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(IC1-Pad17)"))
    (pad 26 smd rect (at 14.2125 -5.605 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(IC1-Pad16)"))
    (pad 27 smd rect (at 14.2125 -6.875 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(IC2-Pad27)"))
    (pad 28 smd rect (at 14.2125 -8.145 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 70 "Net-(IC2-Pad28)"))
    (pad 29 smd rect (at 14.2125 -9.415 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(IC2-Pad29)"))
    (pad 30 smd rect (at 14.2125 -10.685 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(IC2-Pad30)"))
    (pad 31 smd rect (at 14.2125 -11.955 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(IC2-Pad31)"))
    (pad 32 smd rect (at 14.2125 -13.225 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(IC2-Pad32)"))
    (pad 33 smd rect (at 12.7 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(IC2-Pad33)"))
    (pad 34 smd rect (at 11.43 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 35 smd rect (at 10.16 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(IC2-Pad35)"))
    (pad 36 smd rect (at 8.89 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(IC2-Pad36)"))
    (pad 37 smd rect (at 7.62 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(IC2-Pad37)"))
    (pad 38 smd rect (at 6.35 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(IC2-Pad38)"))
    (pad 39 smd rect (at 5.08 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(IC2-Pad39)"))
    (pad 40 smd rect (at 3.81 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(IC2-Pad40)"))
    (pad 41 smd rect (at 2.54 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(IC2-Pad41)"))
    (pad 42 smd rect (at 1.27 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 43 smd rect (at 0 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(IC2-Pad43)"))
    (pad 44 smd rect (at -1.27 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(IC2-Pad44)"))
    (pad 45 smd rect (at -2.54 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(IC2-Pad45)"))
    (pad 46 smd rect (at -3.81 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(IC2-Pad46)"))
    (pad 47 smd rect (at -5.08 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(IC2-Pad47)"))
    (pad 48 smd rect (at -6.35 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(IC2-Pad48)"))
    (pad 49 smd rect (at -7.62 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(IC2-Pad49)"))
    (pad 50 smd rect (at -8.89 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(IC2-Pad50)"))
    (pad 51 smd rect (at -10.16 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 52 smd rect (at -11.43 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(IC2-Pad52)"))
    (pad 53 smd rect (at -12.7 -14.7375 180) (size 0.7 1.925) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(IC1-Pad18)"))
    (pad 54 smd rect (at -14.2125 -13.225 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(IC2-Pad54)"))
    (pad 55 smd rect (at -14.2125 -11.955 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(IC2-Pad55)"))
    (pad 56 smd rect (at -14.2125 -10.685 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(IC2-Pad56)"))
    (pad 57 smd rect (at -14.2125 -9.415 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(IC2-Pad57)"))
    (pad 58 smd rect (at -14.2125 -8.145 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(IC2-Pad58)"))
    (pad 59 smd rect (at -14.2125 -6.875 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(IC2-Pad59)"))
    (pad 60 smd rect (at -14.2125 -5.605 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(IC2-Pad60)"))
    (pad 61 smd rect (at -14.2125 -4.335 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(IC2-Pad61)"))
    (pad 62 smd rect (at -14.2125 -3.065 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(IC2-Pad62)"))
    (pad 63 smd rect (at -14.2125 -1.795 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(IC2-Pad63)"))
    (pad 64 smd rect (at -14.2125 -0.525 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(IC2-Pad64)"))
    (pad 65 smd rect (at -14.2125 0.745 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(IC2-Pad65)"))
    (pad 66 smd rect (at -14.2125 2.015 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(IC2-Pad66)"))
    (pad 67 smd rect (at -14.2125 3.285 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(IC2-Pad67)"))
    (pad 68 smd rect (at -14.2125 4.555 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(IC2-Pad68)"))
    (pad 69 smd rect (at -14.2125 5.825 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(IC2-Pad69)"))
    (pad 70 smd rect (at -14.2125 7.095 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(IC1-Pad2)"))
    (pad 71 smd rect (at -14.2125 8.365 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(IC2-Pad71)"))
    (pad 72 smd rect (at -14.2125 9.635 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(IC2-Pad72)"))
    (pad 73 smd rect (at -14.2125 10.905 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(IC2-Pad73)"))
    (pad 74 smd rect (at -14.2125 12.175 180) (size 1.925 0.7) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(IC2-Pad74)"))
    (model ${KISYS3DMOD}/Package_LCC.3dshapes/PLCC-84_SMD-Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PLCC:PLCC-28 (layer F.Cu) (tedit 5A02ECC8)
    (at 79.3 58.225)
    (descr "PLCC, 28 pins, surface mount")
    (tags "plcc smt")
    (attr smd)
    (fp_text reference GAL22V10-15 (at 0.025 -2.375) (layer F.SilkS))
    (fp_text value GAL22V10 (at 0 7.285) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 25 smd rect (at 5.3225 -3.81) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad25)"))
    (pad 24 smd rect (at 5.3225 -2.54) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad24)"))
    (pad 23 smd rect (at 5.3225 -1.27) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad23)"))
    (pad 22 smd rect (at 5.3225 0) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad22)"))
    (pad 21 smd rect (at 5.3225 1.27) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad21)"))
    (pad 20 smd rect (at 5.3225 2.54) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad20)"))
    (pad 19 smd rect (at 5.3225 3.81) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad19)"))
    (pad 18 smd rect (at 3.81 5.3225) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad18)"))
    (pad 17 smd rect (at 2.54 5.3225) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(IC1-Pad17)"))
    (pad 16 smd rect (at 1.27 5.3225) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad16)"))
    (pad 15 smd rect (at 0 5.3225) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad15)"))
    (pad 14 smd rect (at -1.27 5.3225) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 13 smd rect (at -2.54 5.3225) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad13)"))
    (pad 12 smd rect (at -3.81 5.3225) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad12)"))
    (pad 11 smd rect (at -5.3225 3.81) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad11)"))
    (pad 10 smd rect (at -5.3225 2.54) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(IC1-Pad10)"))
    (pad 9 smd rect (at -5.3225 1.27) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(IC1-Pad9)"))
    (pad 8 smd rect (at -5.3225 0) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(IC1-Pad8)"))
    (pad 7 smd rect (at -5.3225 -1.27) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(IC1-Pad7)"))
    (pad 6 smd rect (at -5.3225 -2.54) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(IC1-Pad6)"))
    (pad 5 smd rect (at -5.3225 -3.81) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(IC1-Pad5)"))
    (pad 26 smd rect (at 3.81 -5.3225) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC1-Pad26)"))
    (pad 27 smd rect (at 2.54 -5.3225) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(IC1-Pad27)"))
    (pad 28 smd rect (at 1.27 -5.3225) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 4 smd rect (at -3.81 -5.3225) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(IC1-Pad4)"))
    (pad 3 smd rect (at -2.54 -5.3225) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad3)"))
    (pad 2 smd rect (at -1.27 -5.3225) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(IC1-Pad2)"))
    (pad 1 smd rect (at 0 -5.3225) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(IC1-Pad1)"))
    (model ${KISYS3DMOD}/Package_LCC.3dshapes/PLCC-28.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm_NumberLabels (layer F.Cu) (tedit 5A3F6CCC)
    (at 97.375 54.325)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open, labeled with numbers")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 -1.8) (layer F.SilkS))
    (fp_text value SolderJumper_3_Open (at 0 1.9) (layer F.Fab) hide)
    (fp_text user 1 (at -2.6 0) (layer F.SilkS))
    (fp_text user 3 (at 2.6 0) (layer F.SilkS))
    (pad 1 smd rect (at -1.3 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 23 "Net-(IC1-Pad26)"))
    (pad 2 smd rect (at 0 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 30 "Net-(IC2-Pad73)"))
    (pad 3 smd rect (at 1.3 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 24 "Net-(IC1-Pad27)"))
  )
  (module Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm_NumberLabels (layer F.Cu) (tedit 5A3F6CCC)
    (at 89.775 54.325)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open, labeled with numbers")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 -1.8) (layer F.SilkS))
    (fp_text value SolderJumper_3_Open (at 0 1.9) (layer F.Fab) hide)
    (fp_text user 1 (at -2.6 0) (layer F.SilkS))
    (fp_text user 3 (at 2.6 0) (layer F.SilkS))
    (pad 1 smd rect (at -1.3 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 0 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 9 "Net-(IC1-Pad19)"))
    (pad 3 smd rect (at 1.3 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 2 "Net-(C1-Pad1)"))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 73.5 67.025 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text ↑IDE (at 107.1 52.15) (layer F.SilkS))
  (gr_text "A4K ROMY REV 3b\namiga.technology" (at 74.775 79.525 90) (layer F.SilkS))
  (gr_line (start 71.925 51.975) (end 73.475 50.425) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 103.3 57.825) (end 103.5 57.825) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 78.075 82.5) (end 78.075 82.7) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 103.3 82.5) (end 103.5 82.5) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 87.8 66.2) (end 88 66.2) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 88.2 57.825) (end 88.2 57.625) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 78.075 66.6) (end 78.075 66.4) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 72.125 88.125) (end 71.925 88.125) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 109 88.125) (end 109.2 88.125) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 109 50.625) (end 109.2 50.625) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88 66.2) (end 88 57.825) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 78.075 66.4) (end 87.8 66.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 103.3 57.625) (end 88.2 57.625) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 103.5 82.5) (end 103.5 57.825) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 78.075 82.7) (end 103.3 82.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 77.875 66.6) (end 77.875 82.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 72.125 88.325) (end 109 88.325) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 71.925 51.975) (end 71.925 88.125) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 109.2 50.625) (end 109.2 88.125) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 73.475 50.425) (end 109 50.425) (layer Edge.Cuts) (width 0.05))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.2 88.3) (xy 72 88.375) (xy 71.85 50.45) (xy 109.275 50.45)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.25 50.425) (xy 109.25 88.425) (xy 71.875 88.35) (xy 71.875 50.4)
      )
    )
  )
)
