(kicad_pcb (version 20170123) (host pcbnew "(2017-07-18 revision f509ccc7c)-makepkg")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 9)
    (zones 0)
    (modules 3)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.2032)
    (zone_clearance 0.2032)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 /ALS)
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.2032)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /ALS)
    (add_net GND)
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer B.Cu) (tedit 598773E0)
    (at 159.25 91.5 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J1 (at 0 5.1 180) (layer B.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 3.1 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 3 /ALS))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Opto-Devices-xil:TEMT6000 (layer F.Cu) (tedit 5987732A)
    (at 154.5 93.75)
    (fp_text reference Q1 (at 2.1 -1.35 90) (layer F.SilkS))
    (fp_text value TEMT6000 (at -2.066839 -1.691513 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 -2.99974) (size 1.00076 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -0.55118 0.55118) (size 0.8001 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 3 /ALS))
    (pad "" smd rect (at 0.55118 0.55118) (size 0.8001 1.09982) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0.04921259842519685 0))
      (scale (xyz 1.4 1.4 1.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 154.5 97)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /ALS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 8.75 (width 0.3) (layer Margin)
    (gr_text "8.750 mm" (at 156.875 83.65) (layer Margin))
    (feature1 (pts (xy 161.25 87.75) (xy 161.25 82.3)))
    (feature2 (pts (xy 152.5 87.75) (xy 152.5 82.3)))
    (crossbar (pts (xy 152.5 85) (xy 161.25 85)))
    (arrow1a (pts (xy 161.25 85) (xy 160.123496 85.586421)))
    (arrow1b (pts (xy 161.25 85) (xy 160.123496 84.413579)))
    (arrow2a (pts (xy 152.5 85) (xy 153.626504 85.586421)))
    (arrow2b (pts (xy 152.5 85) (xy 153.626504 84.413579)))
  )
  (dimension 9.25 (width 0.3) (layer Margin)
    (gr_text "9.250 mm" (at 167.6 94.125 270) (layer Margin))
    (feature1 (pts (xy 164.25 98.75) (xy 168.95 98.75)))
    (feature2 (pts (xy 164.25 89.5) (xy 168.95 89.5)))
    (crossbar (pts (xy 166.25 89.5) (xy 166.25 98.75)))
    (arrow1a (pts (xy 166.25 98.75) (xy 165.663579 97.623496)))
    (arrow1b (pts (xy 166.25 98.75) (xy 166.836421 97.623496)))
    (arrow2a (pts (xy 166.25 89.5) (xy 165.663579 90.626504)))
    (arrow2b (pts (xy 166.25 89.5) (xy 166.836421 90.626504)))
  )
  (gr_text GND (at 157 95.75 90) (layer B.SilkS))
  (gr_text ALS (at 157 93 90) (layer B.SilkS))
  (gr_text 3.3V (at 157 90 90) (layer B.SilkS))
  (gr_text "TEMT6000\nALS" (at 154.25 90 90) (layer B.SilkS))
  (gr_arc (start 160.25 97.75) (end 160.25 98.75) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 153.5 97.75) (end 152.5 97.75) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 153.5 90.5) (end 153.5 89.5) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 160.25 90.5) (end 161.25 90.5) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.5 89.5) (end 160.25 89.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.5 97.75) (end 152.5 90.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.25 98.75) (end 153.5 98.75) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.25 90.5) (end 161.25 97.75) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.25 89.25) (xy 152.25 99) (xy 161.5 99) (xy 161.5 89.25)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.25 89.25) (xy 152.25 99) (xy 161.5 99) (xy 161.5 89.25)
      )
    )
  )
)
