<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="83.8" y2="0" width="0" layer="20"/>
<wire x1="83.8" y1="0" x2="83.8" y2="86.03" width="0" layer="20"/>
<wire x1="83.8" y1="86.03" x2="0" y2="86.03" width="0" layer="20"/>
<wire x1="0" y1="86.03" x2="0" y2="0" width="0" layer="20"/>
<text>COS</text>
<text>PTT</text>
<text>LOW</text>
<text>MED</text>
<text>HIGH</text>
<text>DCOS</text>
<text>DCOS</text>
<text>LOW</text>
<text>HIGH</text>
<text>MED</text>
<text>TX</text>
<text>RX</text>
<text>PWR</text>
<text>NQSMHS V3</text>
<text>NI2O 04/2014</text>
<text>www.gmskhotspot.com</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="DIL28-3">
</package>
<package name="1X06">
</package>
<package name="USB-B-PTH">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="DIODE-1N4001">
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="1X02">
</package>
<package name="1X03">
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
<package name="HC49US">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
</packages>
</library>
<library name="capacitor-wima">
<packages>
<package name="C2.5-2">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 5 x 2.5 mm, grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="v-reg">
<packages>
<package name="78LXX">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ic-package">
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="linear">
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-subd">
<packages>
<package name="M09HP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pot">
<packages>
<package name="CA6V">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
</packages>
</library>
<library name="cml-micro">
<packages>
<package name="DIL24-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
<package name="TSSOP24">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 24&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode-1">
<packages>
<package name="DO35-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="mini_din">
<packages>
<package name="M_DIN6">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC6" library="SparkFun" package="DIL28-3" value="PIC18F2550"/>
<element name="PICKIT2" library="SparkFun" package="1X06" value="PICKIT2"/>
<element name="J1" library="SparkFun" package="USB-B-PTH" value="USBPTH"/>
<element name="LED1" library="SparkFun" package="LED3MM" value="COS">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun" package="CPOL-RADIAL-10UF-25V" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun" package="HC49US" value="24MHz"/>
<element name="D1" library="SparkFun" package="DIODE-1N4001" value="1N4001"/>
<element name="PWR" library="SparkFun" package="1X03" value="PWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun" package="CPOL-RADIAL-10UF-25V" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="SparkFun" package="LED3MM" value="PWR">
<attribute name="VALUE"/>
</element>
<element name="SERIAL" library="SparkFun" package="1X03" value="SERIAL"/>
<element name="R11" library="resistor" package="0207/2V" value="1K"/>
<element name="R12" library="resistor" package="0207/2V" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="resistor" package="0207/2V" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="resistor" package="0207/2V" value="27K"/>
<element name="R20" library="resistor" package="0207/2V" value="1K"/>
<element name="C10" library="capacitor-wima" package="C2.5-2" value="0.1uF"/>
<element name="C11" library="capacitor-wima" package="C2.5-2" value="0.1uF"/>
<element name="C12" library="capacitor-wima" package="C2.5-2" value="22pF"/>
<element name="C13" library="capacitor-wima" package="C2.5-2" value="22pF"/>
<element name="IC2" library="v-reg" package="78LXX" value="78L05"/>
<element name="JP7" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP8" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP9" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP10" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="PROG" library="SparkFun" package="1X02" value="Program"/>
<element name="R15" library="resistor" package="0207/2V" value="510K"/>
<element name="R17" library="resistor" package="0207/2V" value="100K"/>
<element name="C14" library="capacitor-wima" package="C2.5-2" value="22pF"/>
<element name="R3" library="resistor" package="0207/2V" value="180K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="capacitor-wima" package="C2.5-2" value="330p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="pot" package="CA6V" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun" package="TO-92" value="2N3904">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED8" library="SparkFun" package="LED3MM" value="PTT">
<attribute name="VALUE"/>
</element>
<element name="R18" library="resistor" package="0207/2V" value="4k7"/>
<element name="R19" library="resistor" package="0207/2V" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="con-subd" package="M09HP" value="DB9M"/>
<element name="R5" library="resistor" package="0207/2V" value="510K"/>
<element name="C6" library="SparkFun" package="CPOL-RADIAL-10UF-25V" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="capacitor-wima" package="C2.5-2" value="470pF"/>
<element name="R6" library="resistor" package="0207/2V" value="100K"/>
<element name="R36" library="pot" package="CA6V" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="linear" package="DIL08" value="LM4558N"/>
<element name="R2" library="resistor" package="0207/2V" value="100K"/>
<element name="R7" library="resistor" package="0207/2V" value="75K"/>
<element name="C9" library="SparkFun" package="CPOL-RADIAL-10UF-25V" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="capacitor-wima" package="C2.5-2" value="100pF"/>
<element name="C21" library="SparkFun" package="CPOL-RADIAL-10UF-25V" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="resistor" package="0207/2V" value="10K"/>
<element name="C3" library="capacitor-wima" package="C2.5-2" value="0.22uF"/>
<element name="R9" library="resistor" package="0207/2V" value="10K"/>
<element name="D2" library="diode-1" package="DO35-10" value="1N4148"/>
<element name="R4" library="resistor" package="0207/2V" value="75K"/>
<element name="C20" library="SparkFun" package="CPOL-RADIAL-10UF-25V" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="resistor" package="0207/2V" value=""/>
<element name="R16" library="resistor" package="0207/2V" value="0R"/>
<element name="X1" library="mini_din" package="M_DIN6" value=""/>
<element name="IC1" library="ic-package" package="DIL16" value="MAX8213"/>
<element name="R21" library="resistor" package="0207/2V" value="470R"/>
<element name="R22" library="resistor" package="0207/2V" value="470R"/>
<element name="R24" library="resistor" package="0207/2V" value="27K"/>
<element name="R25" library="resistor" package="0207/2V" value="47K"/>
<element name="LED2" library="SparkFun" package="LED3MM" value="MED">
<attribute name="VALUE"/>
</element>
<element name="LED10" library="SparkFun" package="LED3MM" value="LOW">
<attribute name="VALUE"/>
</element>
<element name="LED11" library="SparkFun" package="LED3MM" value="DCOS">
<attribute name="VALUE"/>
</element>
<element name="LED12" library="SparkFun" package="LED3MM" value="HIGH">
<attribute name="VALUE"/>
</element>
<element name="C7" library="capacitor-wima" package="C2.5-2" value="0.1uF"/>
<element name="C8" library="SparkFun" package="CPOL-RADIAL-10UF-25V" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="resistor" package="0207/2V" value="470R"/>
<element name="R28" library="resistor" package="0207/2V" value="470R"/>
<element name="R31" library="pot" package="CA6V" value="100K"/>
<element name="R34" library="pot" package="CA6V" value="10K"/>
<element name="R33" library="pot" package="CA6V" value="100K"/>
<element name="R32" library="pot" package="CA6V" value="100K"/>
<element name="C16" library="capacitor-wima" package="C2.5-2" value="0.027uF"/>
<element name="C15" library="capacitor-wima" package="C2.5-2" value="0.027uF"/>
<element name="R23" library="resistor" package="0207/2V" value="1M"/>
<element name="C17" library="capacitor-wima" package="C2.5-2" value="0.1uF"/>
<element name="Q3" library="SparkFun" package="HC49US" value="4.9152MHz"/>
<element name="C19" library="capacitor-wima" package="C2.5-2" value="22pF"/>
<element name="C18" library="capacitor-wima" package="C2.5-2" value="22pF"/>
<element name="R29" library="resistor" package="0207/2V" value="1M"/>
<element name="U1A" library="cml-micro" package="TSSOP24" value="CMX589AE2"/>
<element name="U1" library="cml-micro" package="DIL24-6" value="CMX589AP4"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="R12" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="PICKIT2" pad="2"/>
<contactref element="IC6" pad="20"/>
<contactref element="PWR" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="R20" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="IC5" pad="8"/>
<contactref element="IC1" pad="16"/>
<contactref element="IC1" pad="15"/>
<contactref element="R22" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="R27" pad="1"/>
<contactref element="R28" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="U1A" pad="24"/>
<contactref element="C17" pad="2"/>
<contactref element="U1A" pad="4"/>
<contactref element="U1A" pad="3"/>
<contactref element="U1A" pad="15"/>
<contactref element="U1A" pad="17"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="17"/>
<contactref element="U1" pad="15"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="PGC">
<contactref element="PICKIT2" pad="5"/>
<contactref element="IC6" pad="27"/>
</signal>
<signal name="PGD">
<contactref element="PICKIT2" pad="4"/>
<contactref element="IC6" pad="28"/>
</signal>
<signal name="GND">
<contactref element="PICKIT2" pad="3"/>
<contactref element="IC6" pad="19"/>
<contactref element="IC6" pad="8"/>
<contactref element="J1" pad="GND"/>
<contactref element="LED1" pad="K"/>
<contactref element="C1" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="IC2" pad="GND"/>
<contactref element="C5" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="LED3" pad="K"/>
<contactref element="SERIAL" pad="2"/>
<contactref element="PROG" pad="1"/>
<contactref element="LED8" pad="K"/>
<contactref element="Q2" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="D2" pad="A"/>
<contactref element="X2" pad="5"/>
<contactref element="X2" pad="G2"/>
<contactref element="X2" pad="G1"/>
<contactref element="X2" pad="8"/>
<contactref element="C2" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="IC5" pad="4"/>
<contactref element="R1" pad="A"/>
<contactref element="R36" pad="E"/>
<contactref element="R8" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="9"/>
<contactref element="R31" pad="E"/>
<contactref element="R32" pad="E"/>
<contactref element="R33" pad="E"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="R34" pad="A"/>
<contactref element="C19" pad="1"/>
<contactref element="C18" pad="2"/>
<contactref element="U1A" pad="12"/>
<contactref element="C17" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="U1A" pad="8"/>
<contactref element="U1A" pad="18"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="12"/>
<contactref element="X1" pad="SH2"/>
<contactref element="X1" pad="SH1"/>
<contactref element="X1" pad="SH3"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="VPP">
<contactref element="PICKIT2" pad="1"/>
<contactref element="IC6" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="PROG" pad="2"/>
</signal>
<signal name="TX/SN">
<contactref element="IC6" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="PTT">
<contactref element="IC6" pad="3"/>
<contactref element="R18" pad="2"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="USB-">
<contactref element="IC6" pad="15"/>
<contactref element="J1" pad="D-"/>
</signal>
<signal name="USB+">
<contactref element="IC6" pad="16"/>
<contactref element="J1" pad="D+"/>
</signal>
<signal name="N$3">
<contactref element="IC6" pad="23"/>
<contactref element="IC6" pad="26"/>
</signal>
<signal name="RXCLOCK">
<contactref element="IC6" pad="21"/>
<contactref element="U1A" pad="21"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="TXCLOCK">
<contactref element="IC6" pad="22"/>
<contactref element="U1A" pad="22"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="RXDATA">
<contactref element="IC6" pad="24"/>
<contactref element="U1A" pad="20"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="RX-232">
<contactref element="IC6" pad="18"/>
<contactref element="SERIAL" pad="1"/>
</signal>
<signal name="TX-232">
<contactref element="IC6" pad="17"/>
<contactref element="SERIAL" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="IC6" pad="5"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="IC6" pad="6"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="LED1" pad="A"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="TXDATA">
<contactref element="IC6" pad="7"/>
<contactref element="U1A" pad="19"/>
</signal>
<signal name="RXSN">
<contactref element="R14" pad="1"/>
<contactref element="R24" pad="2"/>
<contactref element="U1A" pad="23"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="N$9">
<contactref element="Q1" pad="2"/>
<contactref element="IC6" pad="9"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="IC6" pad="10"/>
<contactref element="Q1" pad="1"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="PLLACQ">
<contactref element="IC6" pad="11"/>
<contactref element="U1A" pad="7"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="RXHOLD">
<contactref element="IC6" pad="13"/>
<contactref element="U1A" pad="5"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="IC6" pad="14"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="+12V">
<contactref element="D1" pad="A"/>
<contactref element="X2" pad="9"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="C"/>
<contactref element="IC2" pad="IN"/>
</signal>
<signal name="N$12">
<contactref element="PWR" pad="1"/>
<contactref element="IC2" pad="OUT"/>
</signal>
<signal name="+5V">
<contactref element="J1" pad="VBUS"/>
<contactref element="PWR" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="LED3" pad="A"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="RXDCACQ">
<contactref element="IC6" pad="12"/>
<contactref element="U1A" pad="6"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="DCOS">
<contactref element="IC6" pad="25"/>
<contactref element="IC1" pad="11"/>
<contactref element="LED11" pad="K"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="RPT">
<contactref element="IC6" pad="4"/>
</signal>
<signal name="RXDATA/SPKR">
<contactref element="R1" pad="E"/>
<contactref element="X2" pad="3"/>
<contactref element="X1" pad="5"/>
</signal>
<signal name="N$23">
<contactref element="C4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="IC5" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="RXSIGIN">
<contactref element="R17" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="U1A" pad="11"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="RCFB">
<contactref element="R17" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="U1A" pad="10"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="VBIAS">
<contactref element="R15" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="U1A" pad="9"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="N$26">
<contactref element="C4" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="IC5" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$40">
<contactref element="R15" pad="1"/>
<contactref element="IC5" pad="3"/>
</signal>
<signal name="TRXPTT">
<contactref element="Q2" pad="3"/>
<contactref element="D2" pad="C"/>
<contactref element="X2" pad="4"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="Q2" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="LED8" pad="A"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="COS/COR/SQL">
<contactref element="X2" pad="2"/>
<contactref element="X1" pad="8"/>
</signal>
<signal name="TXDATA/MIC">
<contactref element="X2" pad="1"/>
<contactref element="C21" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="IC5" pad="7"/>
<contactref element="R36" pad="A"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="TXOUT">
<contactref element="R6" pad="1"/>
<contactref element="U1A" pad="16"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="N$18">
<contactref element="R1" pad="S"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="R7" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="R36" pad="S"/>
<contactref element="C21" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="R5" pad="1"/>
<contactref element="IC5" pad="5"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R6" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="IC5" pad="6"/>
<contactref element="R16" pad="1"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="R10" pad="1"/>
<contactref element="C20" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="6"/>
<contactref element="C7" pad="1"/>
<contactref element="R34" pad="S"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="14"/>
<contactref element="LED12" pad="K"/>
</signal>
<signal name="N$41">
<contactref element="R22" pad="1"/>
<contactref element="LED12" pad="A"/>
</signal>
<signal name="N$44">
<contactref element="IC1" pad="13"/>
<contactref element="LED2" pad="K"/>
</signal>
<signal name="N$45">
<contactref element="R21" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$46">
<contactref element="IC1" pad="12"/>
<contactref element="LED10" pad="K"/>
</signal>
<signal name="N$47">
<contactref element="LED11" pad="A"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="N$48">
<contactref element="R28" pad="2"/>
<contactref element="LED10" pad="A"/>
</signal>
<signal name="N$49">
<contactref element="IC1" pad="2"/>
<contactref element="R31" pad="S"/>
</signal>
<signal name="N$50">
<contactref element="IC1" pad="3"/>
<contactref element="R32" pad="S"/>
</signal>
<signal name="N$51">
<contactref element="IC1" pad="5"/>
<contactref element="R33" pad="S"/>
</signal>
<signal name="N$52">
<contactref element="IC1" pad="4"/>
<contactref element="R34" pad="E"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$53">
<contactref element="R31" pad="A"/>
<contactref element="R24" pad="1"/>
<contactref element="R32" pad="A"/>
<contactref element="C8" pad="1"/>
<contactref element="R33" pad="A"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$1">
<contactref element="R23" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="U1A" pad="13"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="N$21">
<contactref element="R23" pad="2"/>
<contactref element="C16" pad="1"/>
<contactref element="U1A" pad="14"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="N$22">
<contactref element="C18" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="R29" pad="1"/>
<contactref element="U1A" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R29" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="U1A" pad="2"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="U1" pad="22"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
