<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="77.2" y1="49.2" x2="77.2" y2="14.3" width="0.254" layer="20"/>
<wire x1="77.2" y1="14.3" x2="72.2" y2="9.3" width="0.254" layer="20" curve="-90"/>
<wire x1="72.2" y1="9.3" x2="36.8" y2="9.3" width="0.254" layer="20"/>
<wire x1="36.8" y1="9.3" x2="31.8" y2="14.3" width="0.254" layer="20" curve="-90"/>
<wire x1="31.8" y1="14.3" x2="31.8" y2="49.2" width="0.254" layer="20"/>
<wire x1="31.8" y1="49.2" x2="36.8" y2="54.2" width="0.254" layer="20" curve="-90"/>
<wire x1="36.8" y1="54.2" x2="72.2" y2="54.2" width="0.254" layer="20"/>
<text>GND</text>
<text>RES</text>
<text>ANT</text>
<text>ANT</text>
<text>CP</text>
<text>VCC</text>
<text>READ</text>
<text>D0</text>
<text>D1</text>
<text>FORM</text>
<text>TIR</text>
<text>Permafrost Exhibit</text>
<text>GND</text>
<text>RES</text>
<text>ANT</text>
<text>ANT</text>
<text>CP</text>
<text>TIR</text>
<text>FORM</text>
<text>D1</text>
<text>D0</text>
<text>READ</text>
<text>VCC</text>
<text>OMSI 2017</text>
<wire x1="72.2" y1="54.2" x2="77.2" y2="49.2" width="0.254" layer="20" curve="-90"/>
<text>RES</text>
<text>RES</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>VCC</text>
<text>D0</text>
<text>RFID ID-12LA</text>
<text>Shield</text>
<text>Thomas Hudson</text>
<text>OMSI 2017</text>
<text>Permafrost Exhibit</text>
<text>RFID ID-12LA</text>
<text>Shield</text>
<text>Thomas Hudson</text>
<text>LED Flashes</text>
<text>Indicates TX</text>
</plain>
<libraries>
<library name="ID Innovations">
<packages>
<package name="ID_PACKAGE">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
</package>
<package name="1X05">
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="7395-04">
<description>&lt;b&gt;MOLEX 2.54mm KK RA CONNECTOR&lt;/b&gt;
&lt;br&gt;Fixed Orientation</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="eagle_libraries">
<packages>
<package name="STANDOFF-ELECTRICAL">
<description>#8 screw hole, 170mill, 0.30 mask</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="ID Innovations" package="ID_PACKAGE" value="RFID"/>
<element name="JP4" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="J1" library="con-molex" package="7395-04" value="22-05-7048-04">
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.3EZ" value="">
<attribute name="VALUE"/>
</element>
<element name="S1" library="eagle_libraries" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S2" library="eagle_libraries" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S3" library="eagle_libraries" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S4" library="eagle_libraries" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="R2" library="SparkFun-Passives" package="0805" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="ANT1">
<contactref element="U1" pad="3"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="ANT2">
<contactref element="U1" pad="4"/>
<contactref element="JP5" pad="4"/>
</signal>
<signal name="CP">
<contactref element="U1" pad="5"/>
<contactref element="JP5" pad="5"/>
</signal>
<signal name="RES">
<contactref element="U1" pad="2"/>
<contactref element="JP5" pad="2"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="READ">
<contactref element="U1" pad="10"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="D0">
<contactref element="U1" pad="9"/>
<contactref element="JP4" pad="4"/>
<contactref element="R1" pad="P$1"/>
<contactref element="J1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="D1">
<contactref element="U1" pad="8"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="FORM">
<contactref element="U1" pad="7"/>
<contactref element="JP4" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="JP5" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="TIR">
<contactref element="U1" pad="6"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="11"/>
<contactref element="JP4" pad="6"/>
<contactref element="D1" pad="A"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$3">
<contactref element="D1" pad="K"/>
<contactref element="R1" pad="P$2"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
