(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 20)
    (no_connects 0)
    (area 206.934999 115.494999 240.105001 135.965001)
    (thickness 0.1)
    (drawings 15)
    (tracks 72)
    (zones 0)
    (modules 13)
    (nets 22)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.006)
    (trace_clearance 0.006)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.006)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.027)
    (via_drill 0.013)
    (via_min_size 0.027)
    (via_min_drill 0.013)
    (uvia_size 0.03)
    (uvia_drill 0.02)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 176.53 118.11)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /CHROMA)
  (net 2 "Net-(C1-Pad2)")
  (net 3 /LUMA)
  (net 4 "Net-(C2-Pad2)")
  (net 5 /RED)
  (net 6 /GREEN)
  (net 7 /CSYNC)
  (net 8 /BLUE)
  (net 9 /GND)
  (net 10 "Net-(J2-Pad3)")
  (net 11 "Net-(J2-Pad4)")
  (net 12 "Net-(J2-Pad5)")
  (net 13 "Net-(J3-Pad1)")
  (net 14 "Net-(J3-Pad2)")
  (net 15 "Net-(J3-Pad3)")
  (net 16 "Net-(C1-Pad1)")
  (net 17 "Net-(C2-Pad1)")
  (net 18 "Net-(J1-Pad1)")
  (net 19 "Net-(J1-Pad2)")
  (net 20 "Net-(J1-Pad3)")
  (net 21 "Net-(J1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.006)
    (trace_width 0.006)
    (via_dia 0.027)
    (via_drill 0.013)
    (uvia_dia 0.03)
    (uvia_drill 0.02)
    (add_net /BLUE)
    (add_net /CHROMA)
    (add_net /CSYNC)
    (add_net /GND)
    (add_net /GREEN)
    (add_net /LUMA)
    (add_net /RED)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
  )
  (module Socket_Strips:Socket_Strip_Straight_2x06_Pitch2.54mm (layer Top) (tedit 59487F58)
    (at 236.855 119.38)
    (descr "Through hole straight socket strip, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x06 2.54mm double row")
    (fp_text reference J1 (at -1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_02X06 (at -1.27 15.03) (layer F.Fab) hide)
    (fp_text user %R (at -1.27 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at -2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /CHROMA))
    (pad 6 thru_hole oval (at -2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /LUMA))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 8 thru_hole oval (at -2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /BLUE))
    (pad 10 thru_hole oval (at -2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /CSYNC))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /GREEN))
    (pad 12 thru_hole oval (at -2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /RED))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x06_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.00mm (layer Top) (tedit 59487F90)
    (at 209.55 133.35 90)
    (descr "Through hole straight socket strip, 1x06, 2.00mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.00mm single row")
    (fp_text reference J2 (at 0 -2.06 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 12.06 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.06 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C2-Pad1)"))
    (pad 3 thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 8 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 0 10 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /CSYNC))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer Bottom) (tedit 59488002)
    (at 228.6 125.73 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 0 1.85 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.9 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers Bottom B.Paste B.Mask)
      (net 9 /GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers Bottom B.Paste B.Mask)
      (net 14 "Net-(J3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2010_HandSoldering (layer Top) (tedit 5948801D)
    (at 226.06 129.54 180)
    (descr "Resistor SMD 2010, hand soldering")
    (tags "resistor 2010")
    (attr smd)
    (fp_text reference R4 (at 0 -2.25 180) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.35 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -3.15 0 180) (size 2.4 2.5) (layers Top F.Paste F.Mask)
      (net 6 /GREEN))
    (pad 2 smd rect (at 3.15 0 180) (size 2.4 2.5) (layers Top F.Paste F.Mask)
      (net 11 "Net-(J2-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2010.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer Bottom) (tedit 59488356)
    (at 214.63 124.46 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 1.75 270) (layer B.SilkS) hide)
    (fp_text value C (at 0 -2 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers Bottom B.Paste B.Mask)
      (net 16 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers Bottom B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-D_EIA-7343-31_Hand (layer Top) (tedit 5948803A)
    (at 214.63 124.46 90)
    (descr "Tantalum capacitor, Case D, EIA 7343-31, 7.3x4.3x2.8mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C2 (at 0 -3.9 90) (layer F.SilkS) hide)
    (fp_text value CP (at 0 3.9 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -3.775 0 90) (size 3.75 2.7) (layers Top F.Paste F.Mask)
      (net 17 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 3.775 0 90) (size 3.75 2.7) (layers Top F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-D_EIA-7343-31.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03_Pitch2.00mm (layer Top) (tedit 59487F88)
    (at 209.55 127 180)
    (descr "Through hole straight socket strip, 1x03, 2.00mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.00mm single row")
    (fp_text reference J3 (at 0 -2.06 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 6.06 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.06 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J3-Pad3)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2010_HandSoldering (layer Top) (tedit 59487FA7)
    (at 226.06 118.11 180)
    (descr "Resistor SMD 2010, hand soldering")
    (tags "resistor 2010")
    (attr smd)
    (fp_text reference R1 (at 0 -2.25 180) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.35 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -3.15 0 180) (size 2.4 2.5) (layers Top F.Paste F.Mask)
      (net 1 /CHROMA))
    (pad 2 smd rect (at 3.15 0 180) (size 2.4 2.5) (layers Top F.Paste F.Mask)
      (net 16 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2010.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2010_HandSoldering (layer Top) (tedit 59487FC2)
    (at 226.06 121.92 180)
    (descr "Resistor SMD 2010, hand soldering")
    (tags "resistor 2010")
    (attr smd)
    (fp_text reference R2 (at 0 -2.25 180) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.35 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -3.15 0 180) (size 2.4 2.5) (layers Top F.Paste F.Mask)
      (net 3 /LUMA))
    (pad 2 smd rect (at 3.15 0 180) (size 2.4 2.5) (layers Top F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2010.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer Bottom) (tedit 5948802A)
    (at 228.6 121.92 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 1.85 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.9 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers Bottom B.Paste B.Mask)
      (net 9 /GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers Bottom B.Paste B.Mask)
      (net 15 "Net-(J3-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2010_HandSoldering (layer Top) (tedit 59488024)
    (at 226.06 125.73 180)
    (descr "Resistor SMD 2010, hand soldering")
    (tags "resistor 2010")
    (attr smd)
    (fp_text reference R6 (at 0 -2.25 180) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.35 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -3.15 0 180) (size 2.4 2.5) (layers Top F.Paste F.Mask)
      (net 5 /RED))
    (pad 2 smd rect (at 3.15 0 180) (size 2.4 2.5) (layers Top F.Paste F.Mask)
      (net 10 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2010.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer Bottom) (tedit 5948800C)
    (at 228.6 129.54 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0 1.85 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.9 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers Bottom B.Paste B.Mask)
      (net 9 /GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers Bottom B.Paste B.Mask)
      (net 13 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2010_HandSoldering (layer Top) (tedit 59487FEA)
    (at 226.06 133.35 180)
    (descr "Resistor SMD 2010, hand soldering")
    (tags "resistor 2010")
    (attr smd)
    (fp_text reference R8 (at 0 -2.25 180) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.35 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -3.15 0 180) (size 2.4 2.5) (layers Top F.Paste F.Mask)
      (net 8 /BLUE))
    (pad 2 smd rect (at 3.15 0 180) (size 2.4 2.5) (layers Top F.Paste F.Mask)
      (net 12 "Net-(J2-Pad5)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2010.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text V1 (at 209.042 118.618) (layer F.SilkS))
  (gr_text SM-SNES-RGB (at 213.36 116.967) (layer F.SilkS))
  (gr_text GG (at 207.772 122.809 90) (layer F.SilkS))
  (gr_text BG (at 207.772 124.968 90) (layer F.SilkS))
  (gr_text RG (at 207.772 127.127 90) (layer F.SilkS))
  (gr_text CS (at 219.583 131.572) (layer F.SilkS))
  (gr_text B (at 217.551 131.572) (layer F.SilkS))
  (gr_text G (at 215.519 131.572) (layer F.SilkS))
  (gr_text R (at 213.487 131.572) (layer F.SilkS))
  (gr_text Y (at 211.582 131.572) (layer F.SilkS))
  (gr_text C (at 209.423 131.572) (layer F.SilkS))
  (gr_line (start 207.01 135.89) (end 240.03 135.89) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 207.01 115.57) (end 207.01 135.89) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 240.03 115.57) (end 207.01 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 240.03 135.89) (end 240.03 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 9) (net_name /GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 240.03 135.89) (xy 207.01 135.89) (xy 207.01 115.57) (xy 240.03 115.57)
      )
    )
  )
)
