(kicad_pcb (version 20171130) (host pcbnew "(5.1.8-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 31)
    (tracks 224)
    (zones 0)
    (modules 29)
    (nets 61)
  )
  (page USLedger)
  (title_block
    (date 2019-12-29)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.1778)
    (zone_clearance 0.4064)
    (zone_45_only no)
    (trace_min 0.1778)
    (via_size 0.6604)
    (via_drill 0.4064)
    (via_min_size 0.4064)
    (via_min_drill 0.3556)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.07)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.0254)
    (solder_mask_min_width 0.0254)
    (aux_axis_origin 0 0)
    (visible_elements FEFDBF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 MOSI)
  (net 4 MISO)
  (net 5 SCK)
  (net 6 "Net-(JL1-Pad3)")
  (net 7 "Net-(JL1-Pad5)")
  (net 8 "Net-(JL1-Pad6)")
  (net 9 "Net-(JL1-Pad8)")
  (net 10 "Net-(JL1-Pad9)")
  (net 11 "Net-(JL1-Pad10)")
  (net 12 "Net-(JL1-Pad11)")
  (net 13 "Net-(JL1-Pad12)")
  (net 14 "Net-(JL1-Pad13)")
  (net 15 "Net-(JL1-Pad14)")
  (net 16 "Net-(JL1-Pad15)")
  (net 17 "Net-(JL1-Pad16)")
  (net 18 "Net-(JL1-Pad17)")
  (net 19 "Net-(JL1-Pad18)")
  (net 20 "Net-(JL1-Pad19)")
  (net 21 "Net-(JL1-Pad20)")
  (net 22 "Net-(JL1-Pad21)")
  (net 23 "Net-(JL1-Pad22)")
  (net 24 "Net-(JR1-Pad24)")
  (net 25 "Net-(JR1-Pad19)")
  (net 26 "Net-(JR1-Pad18)")
  (net 27 "Net-(JR1-Pad17)")
  (net 28 "Net-(JR1-Pad16)")
  (net 29 "Net-(JR1-Pad15)")
  (net 30 "Net-(JR1-Pad14)")
  (net 31 "Net-(JR1-Pad13)")
  (net 32 "Net-(JR1-Pad12)")
  (net 33 "Net-(JR1-Pad5)")
  (net 34 "Net-(JR1-Pad4)")
  (net 35 "Net-(JR1-Pad3)")
  (net 36 "Net-(JL1-Pad7)")
  (net 37 "Net-(JL1-Pad23)")
  (net 38 "Net-(BAT1-Pad1)")
  (net 39 SD_DETECT)
  (net 40 "Net-(J_MICROSD1-Pad1)")
  (net 41 SD_CS)
  (net 42 MOSISD)
  (net 43 SCKSD)
  (net 44 MISOSD)
  (net 45 "Net-(J_MICROSD1-Pad8)")
  (net 46 "Net-(JL1-Pad24)")
  (net 47 "Net-(JL1-Pad4)")
  (net 48 "Net-(JR1-Pad20)")
  (net 49 SDA)
  (net 50 SCL)
  (net 51 CLOCK_INT)
  (net 52 "Net-(L_SD1-Pad1)")
  (net 53 "Net-(RCLKINT1-Pad2)")
  (net 54 "Net-(U_DS3231-Pad1)")
  (net 55 "Net-(U_DS3231-Pad4)")
  (net 56 "Net-(J_TO_UPS1-Pad1)")
  (net 57 CHRGSTAT3)
  (net 58 JACK)
  (net 59 "Net-(RSCL1-Pad2)")
  (net 60 "Net-(RSDA1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.2032)
    (via_dia 0.6604)
    (via_drill 0.4064)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.25)
    (add_net +3V3)
    (add_net CHRGSTAT3)
    (add_net CLOCK_INT)
    (add_net GND)
    (add_net JACK)
    (add_net MISO)
    (add_net MISOSD)
    (add_net MOSI)
    (add_net MOSISD)
    (add_net "Net-(BAT1-Pad1)")
    (add_net "Net-(JL1-Pad10)")
    (add_net "Net-(JL1-Pad11)")
    (add_net "Net-(JL1-Pad12)")
    (add_net "Net-(JL1-Pad13)")
    (add_net "Net-(JL1-Pad14)")
    (add_net "Net-(JL1-Pad15)")
    (add_net "Net-(JL1-Pad16)")
    (add_net "Net-(JL1-Pad17)")
    (add_net "Net-(JL1-Pad18)")
    (add_net "Net-(JL1-Pad19)")
    (add_net "Net-(JL1-Pad20)")
    (add_net "Net-(JL1-Pad21)")
    (add_net "Net-(JL1-Pad22)")
    (add_net "Net-(JL1-Pad23)")
    (add_net "Net-(JL1-Pad24)")
    (add_net "Net-(JL1-Pad3)")
    (add_net "Net-(JL1-Pad4)")
    (add_net "Net-(JL1-Pad5)")
    (add_net "Net-(JL1-Pad6)")
    (add_net "Net-(JL1-Pad7)")
    (add_net "Net-(JL1-Pad8)")
    (add_net "Net-(JL1-Pad9)")
    (add_net "Net-(JR1-Pad12)")
    (add_net "Net-(JR1-Pad13)")
    (add_net "Net-(JR1-Pad14)")
    (add_net "Net-(JR1-Pad15)")
    (add_net "Net-(JR1-Pad16)")
    (add_net "Net-(JR1-Pad17)")
    (add_net "Net-(JR1-Pad18)")
    (add_net "Net-(JR1-Pad19)")
    (add_net "Net-(JR1-Pad20)")
    (add_net "Net-(JR1-Pad24)")
    (add_net "Net-(JR1-Pad3)")
    (add_net "Net-(JR1-Pad4)")
    (add_net "Net-(JR1-Pad5)")
    (add_net "Net-(J_MICROSD1-Pad1)")
    (add_net "Net-(J_MICROSD1-Pad8)")
    (add_net "Net-(J_TO_UPS1-Pad1)")
    (add_net "Net-(L_SD1-Pad1)")
    (add_net "Net-(RCLKINT1-Pad2)")
    (add_net "Net-(RSCL1-Pad2)")
    (add_net "Net-(RSDA1-Pad2)")
    (add_net "Net-(U_DS3231-Pad1)")
    (add_net "Net-(U_DS3231-Pad4)")
    (add_net SCK)
    (add_net SCKSD)
    (add_net SCL)
    (add_net SDA)
    (add_net SD_CS)
    (add_net SD_DETECT)
  )
  (module datalogger:MicroSD (layer F.Cu) (tedit 6039D150)
    (at 78.5241 11.59002 270)
    (attr smd)
    (fp_text reference J_MICROSD1 (at 17.99082 0.8636 90) (layer F.SilkS))
    (fp_text value Micro_SD_Card_Det (at 6.8707 12.1031 90) (layer F.SilkS) hide)
    (fp_text user SWD (at 6.56082 14.04874 90) (layer F.SilkS))
    (fp_text user SWG (at 12.83462 11.04392) (layer F.SilkS))
    (fp_text user %R (at 7.3729 10.44672 90) (layer F.Fab) hide)
    (pad 10 smd rect (at 6.5532 15.50162 270) (size 1.5 1.524) (layers F.Cu F.Paste F.Mask)
      (net 39 SD_DETECT))
    (pad 9 smd rect (at 13.99032 10.9982 270) (size 1.143 1.4224) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 0.7 1 270) (size 1.4 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 13.6 1 270) (size 1.4 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 13.081 15.38986 270) (size 1.5 1.15) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 4.14528 15.5067 270) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 12.15 3.8 270) (size 0.65 2.2) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J_MICROSD1-Pad8)"))
    (pad 7 smd rect (at 11.05 3.8 270) (size 0.65 2.2) (layers F.Cu F.Paste F.Mask)
      (net 44 MISOSD))
    (pad 6 smd rect (at 9.95 3.8 270) (size 0.65 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 8.85 3.8 270) (size 0.65 2.2) (layers F.Cu F.Paste F.Mask)
      (net 43 SCKSD))
    (pad 4 smd rect (at 7.75 3.8 270) (size 0.65 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 3 smd rect (at 6.65 3.8 270) (size 0.65 2.2) (layers F.Cu F.Paste F.Mask)
      (net 42 MOSISD))
    (pad 2 smd rect (at 5.55 3.8 270) (size 0.65 2.2) (layers F.Cu F.Paste F.Mask)
      (net 41 SD_CS))
    (pad 1 smd rect (at 4.45 3.8 270) (size 0.65 2.2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J_MICROSD1-Pad1)"))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x24_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 12.7 35.56 270)
    (descr "Through hole straight pin header, 1x24, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x24 2.54mm single row")
    (fp_text reference JL1 (at 0 2.33 270) (layer B.SilkS))
    (fp_text value Conn_01x24 (at 0 -60.75 270) (layer B.Fab))
    (fp_text user %R (at 0 -29.21) (layer B.Fab))
    (pad 24 thru_hole oval (at 0 -58.42 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(JL1-Pad24)"))
    (pad 23 thru_hole oval (at 0 -55.88 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(JL1-Pad23)"))
    (pad 22 thru_hole oval (at 0 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(JL1-Pad22)"))
    (pad 21 thru_hole oval (at 0 -50.8 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(JL1-Pad21)"))
    (pad 20 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(JL1-Pad20)"))
    (pad 19 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(JL1-Pad19)"))
    (pad 18 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(JL1-Pad18)"))
    (pad 17 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(JL1-Pad17)"))
    (pad 16 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(JL1-Pad16)"))
    (pad 15 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(JL1-Pad15)"))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(JL1-Pad14)"))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(JL1-Pad13)"))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(JL1-Pad12)"))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(JL1-Pad11)"))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(JL1-Pad10)"))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(JL1-Pad9)"))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(JL1-Pad8)"))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(JL1-Pad7)"))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(JL1-Pad6)"))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(JL1-Pad5)"))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(JL1-Pad4)"))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(JL1-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 JACK))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x24_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x24_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 12.7 2.54 270)
    (descr "Through hole straight pin header, 1x24, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x24 2.54mm single row")
    (fp_text reference JR1 (at 0 2.33 270) (layer B.SilkS))
    (fp_text value Conn_01x24 (at 0 -60.75 270) (layer B.Fab))
    (fp_text user %R (at 0 -29.21) (layer B.Fab))
    (pad 24 thru_hole oval (at 0 -58.42 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(JR1-Pad24)"))
    (pad 23 thru_hole oval (at 0 -55.88 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 MOSI))
    (pad 22 thru_hole oval (at 0 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 SCK))
    (pad 21 thru_hole oval (at 0 -50.8 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 MISO))
    (pad 20 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(JR1-Pad20)"))
    (pad 19 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(JR1-Pad19)"))
    (pad 18 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(JR1-Pad18)"))
    (pad 17 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(JR1-Pad17)"))
    (pad 16 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(JR1-Pad16)"))
    (pad 15 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(JR1-Pad15)"))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(JR1-Pad14)"))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(JR1-Pad13)"))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(JR1-Pad12)"))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 SDA))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 SCL))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 CLOCK_INT))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 SD_CS))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 SD_DETECT))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 CHRGSTAT3))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(JR1-Pad5)"))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(JR1-Pad4)"))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(JR1-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x24_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module datalogger:Battery_CR1220 (layer F.Cu) (tedit 5E1684E0)
    (at 28.79598 19.67738 90)
    (descr "CR1220 battery")
    (tags "battery CR1220 coin cell")
    (attr virtual)
    (fp_text reference BAT1 (at 8.63092 3.17754 180) (layer F.SilkS))
    (fp_text value CR1220_CELL (at -1.6129 0.0762) (layer F.Fab) hide)
    (fp_text user - (at -8.22706 -2.40284 90) (layer F.SilkS))
    (fp_text user + (at 8.49122 -2.63906 90) (layer F.SilkS))
    (pad 3 thru_hole circle (at 4 0 90) (size 1.5748 1.5748) (drill 1.4478) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -3.5 0 90) (size 1.18 1.18) (drill 1.06) (layers *.Cu *.Mask))
    (pad 1 smd rect (at 8.18 0 90) (size 3.66 2.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(BAT1-Pad1)"))
    (pad 2 smd rect (at -8.18 0 90) (size 3.66 2.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Battery.3dshapes/Battery_CR1225.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 39.61892 29.32938 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CCLK1 (at 0 1.44526 90) (layer F.SilkS))
    (fp_text value 1uf (at -0.0508 1.1684 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 50.54092 26.28392 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CMISO1 (at -0.02794 -1.57734 90) (layer F.SilkS))
    (fp_text value 0.1uf (at -0.0508 1.1684 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 56.83504 9.59612 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CMOSI1 (at 0 -1.55194 90) (layer F.SilkS))
    (fp_text value 0.1uf (at -0.0508 1.1684 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 50.88382 18.18894 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CSCK1 (at 0 -1.60782 90) (layer F.SilkS))
    (fp_text value 0.1uf (at -0.0508 1.1684 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder (layer F.Cu) (tedit 5FA84C73)
    (at 66.65976 28.15082 180)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference CSD1 (at -0.0508 -1.524) (layer F.SilkS))
    (fp_text value "10uf TANT" (at 0 1.3716) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.4375 0 180) (size 1.575 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4375 0 180) (size 1.575 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder (layer F.Cu) (tedit 5FA84C73)
    (at 60.4012 16.84782 90)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference CSDET1 (at -0.0508 -1.524 90) (layer F.SilkS))
    (fp_text value "10uf TANT" (at 0 1.3716 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.4375 0 90) (size 1.575 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4375 0 90) (size 1.575 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 39 SD_DETECT))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A02C)
    (at 76.77658 7.8105 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference L_SD1 (at 0 -1.4732 90) (layer F.SilkS))
    (fp_text value Green (at 0 1.27 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 52 "Net-(L_SD1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 42.17162 29.337 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RCLKINT1 (at -0.0381 1.52146 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.27 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0.2032 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 53 "Net-(RCLKINT1-Pad2)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 40.32758 7.76224 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RSCL1 (at 0.0508 1.43764 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.27 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0.2032 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 59 "Net-(RSCL1-Pad2)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 43.77182 7.7724 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RSDA1 (at 0.0127 -1.44272 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.27 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0.2032 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 60 "Net-(RSDA1-Pad2)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 60.79236 28.067 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RSDCS1 (at 0 -1.3716) (layer F.SilkS))
    (fp_text value 10K (at 0 1.27) (layer F.Fab) hide)
    (fp_text user %R (at 0 0.2032) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 41 SD_CS))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 72.85736 28.1051)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RSDD1 (at 0 1.56464) (layer F.SilkS))
    (fp_text value 10K (at 0 1.27) (layer F.Fab) hide)
    (fp_text user %R (at 0 0.2032) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 45 "Net-(J_MICROSD1-Pad8)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 67.83578 8.4328 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RSDD2 (at 0 -1.3716 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.27 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0.2032 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 40 "Net-(J_MICROSD1-Pad1)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 60.49264 23.3172 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RSDET1 (at -0.08128 1.69164 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.27 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0.2032 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 39 SD_DETECT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 72.08266 8.48614 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RSDLED1 (at 0 -1.3716 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.27 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0.2032 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 41 SD_CS))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 52 "Net-(L_SD1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5FA7A88B)
    (at 42.74566 13.21586 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_CLKINT1 (at 0 1.6764 270) (layer B.SilkS))
    (fp_text value S_CLKINT1 (at 0.0508 -1.6256 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 53 "Net-(RCLKINT1-Pad2)"))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 51 CLOCK_INT))
  )
  (module Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm (layer F.Cu) (tedit 5FA7AF4B)
    (at 43.10888 20.38604 90)
    (descr "SOIC, 16 Pin (JEDEC MS-013AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/rw_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U_DS3231 (at -0.0508 -5.842 90) (layer F.SilkS))
    (fp_text value DS3231M (at -0.0254 5.715 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 16 smd roundrect (at 4.65 -4.445 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 SCL))
    (pad 15 smd roundrect (at 4.65 -3.175 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 SDA))
    (pad 14 smd roundrect (at 4.65 -1.905 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(BAT1-Pad1)"))
    (pad 13 smd roundrect (at 4.65 -0.635 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 12 smd roundrect (at 4.65 0.635 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at 4.65 1.905 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 10 smd roundrect (at 4.65 3.175 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at 4.65 4.445 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 8 smd roundrect (at -4.65 4.445 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 7 smd roundrect (at -4.65 3.175 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at -4.65 1.905 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 5 smd roundrect (at -4.65 0.635 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at -4.65 -0.635 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(U_DS3231-Pad4)"))
    (pad 3 smd roundrect (at -4.65 -1.905 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(RCLKINT1-Pad2)"))
    (pad 2 smd roundrect (at -4.65 -3.175 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -4.65 -4.445 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 "Net-(U_DS3231-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16W_7.5x10.3mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 5FA7A44B)
    (at 54.77764 25.25268 180)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U_MISOG125 (at -0.16764 -2.53492) (layer F.SilkS))
    (fp_text value 74LVC1G125 (at 0 2.1336) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 5 smd rect (at 1.35 -0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 4 smd rect (at 1.35 0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 MISO))
    (pad 3 smd rect (at -1.35 0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.35 0 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 44 MISOSD))
    (pad 1 smd rect (at -1.35 -0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 41 SD_CS))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 5FA7A44B)
    (at 55.2196 17.15008 180)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U_SCKG125 (at -0.00254 -2.65684) (layer F.SilkS))
    (fp_text value 74LVC1G125 (at 0 2.1336) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 5 smd rect (at 1.35 -0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 4 smd rect (at 1.35 0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 43 SCKSD))
    (pad 3 smd rect (at -1.35 0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.35 0 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 SCK))
    (pad 1 smd rect (at -1.35 -0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 41 SD_CS))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 5FA7A44B)
    (at 52.58816 10.66292)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U_MOSIG125 (at -0.02286 2.37998) (layer F.SilkS))
    (fp_text value 74LVC1G125 (at 0 2.1336) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 5 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 4 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 42 MOSISD))
    (pad 3 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 MOSI))
    (pad 1 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 41 SD_CS))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module datalogger:PinHeader_2x03_P2.54mm_Socket (layer F.Cu) (tedit 6025A74A)
    (at 13.30452 11.69416)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J_TO_UPS1 (at 1.69926 -5.8547) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 4.63042 2.30632 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab) hide)
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 SDA))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 SCL))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 CHRGSTAT3))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(J_TO_UPS1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5FC19350)
    (at 13.81252 25.91816 270)
    (descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J_TO_UPS2 (at -2.70256 0.08128 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1.27 4.06908 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 2 90) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 58 JACK))
    (model ${KISYS3DMOD}/TerminalBlock_TE-Connectivity.3dshapes/TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5FA7A88B)
    (at 11.7983 21.62278 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_JK1 (at 0 1.6764 90) (layer B.SilkS))
    (fp_text value S_CLKINT1 (at 0.0508 -1.6256 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 58 JACK))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 56 "Net-(J_TO_UPS1-Pad1)"))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer F.Cu) (tedit 5FA7A88B)
    (at 40.04056 11.7221 270)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_SCL1 (at 0 1.91516 270) (layer F.SilkS))
    (fp_text value S_SCL (at 0.0508 1.6256 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.65 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 59 "Net-(RSCL1-Pad2)"))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 50 SCL))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer F.Cu) (tedit 5FA7A88B)
    (at 44.06392 11.70432 270)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_SDA1 (at -0.03556 -1.8415 270) (layer F.SilkS))
    (fp_text value S_SDA (at 0.0508 1.6256 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.65 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 60 "Net-(RSDA1-Pad2)"))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 49 SDA))
  )
  (gr_text <—Front (at 10.35558 32.31134) (layer F.SilkS))
  (gr_text "CPU  CRG DET CS INT \n21G D02 D07 D06 D12\n51J D40 D44 D43 D42" (at 27.7495 5.84454) (layer F.SilkS))
  (gr_text "MiniDataLogger\nVersion 4b\n1 Mar 2021" (at 36.83762 19.59864) (layer B.SilkS))
  (gr_text JK (at 9.16178 11.74242) (layer F.SilkS))
  (gr_text CRG (at 20.5105 11.5951) (layer F.SilkS))
  (gr_text 12V (at 8.74776 25.14092) (layer F.SilkS))
  (gr_text GND (at 8.78586 29.22016) (layer F.SilkS))
  (gr_text SDA (at 20.58924 16.9418) (layer F.SilkS))
  (gr_text SCL (at 8.79602 16.8529) (layer F.SilkS))
  (gr_text 3V (at 8.9027 14.26464) (layer F.SilkS))
  (gr_text GND (at 20.70862 14.2494) (layer F.SilkS))
  (gr_text JAC (at 15.29588 37.4777) (layer F.SilkS))
  (gr_text CRG (at 25.34158 0.61722) (layer F.SilkS))
  (gr_text CR1220 (at 33.69818 27.91714) (layer F.SilkS))
  (gr_text "Copyright S. Cooper 2021.\nYou may redistribute and modify this documentation under the terms of the CERN OHL v.1.2.\nThis documentation is distributed WITHOUT ANY EXPRESS OR IMPLIED WARRANTY, \nINCLUDING OF MERCHANTABILITY, SATISFACTORY QUALITY AND FITNESS FOR A PARTICULAR PURPOSE.\nPlease see the CERN OHL v.1.2 for applicable conditions. (http://ohwr.org/cernohl)." (at 44.33824 29.25064) (layer B.SilkS))
  (gr_text SDA (at 38.05682 0.60706) (layer F.SilkS))
  (gr_text SCL (at 35.51936 0.60706) (layer F.SilkS))
  (gr_text INT (at 33.12414 0.65532) (layer F.SilkS))
  (gr_text DET (at 27.97048 0.59436) (layer F.SilkS))
  (gr_text 3V (at 15.20698 0.62738) (layer F.SilkS))
  (gr_text GND (at 12.80922 0.65278) (layer F.SilkS))
  (gr_text GND (at 12.78382 37.49294) (layer F.SilkS))
  (gr_text CS (at 30.48508 0.63246) (layer F.SilkS))
  (gr_text MOSI (at 68.76288 0.60198) (layer F.SilkS))
  (gr_text SCK (at 66.0781 0.60198) (layer F.SilkS))
  (gr_text MISO (at 63.3603 0.61722) (layer F.SilkS))
  (gr_line (start 7.62 38.1) (end 7.62 0) (layer Edge.Cuts) (width 0.05))
  (gr_text "MiniDataLogger\nVersion 4b\n1 Mar 2021" (at 22.59584 31.3309) (layer F.SilkS))
  (gr_line (start 78.74 0) (end 78.74 38.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 7.62 0) (end 78.74 0) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 78.74 38.1) (end 7.62 38.1) (layer Edge.Cuts) (width 0.05))
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.824027 32.810977) (xy 91.395777 32.799547) (xy 91.401175 37.17057) (xy 88.81863 37.162315)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.961 20.828) (xy 68.961 26.543) (xy 61.849 26.543) (xy 61.849 14.351) (xy 64.135 14.351)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.994 38.354) (xy 7.366 38.354) (xy 7.366 -0.254) (xy 78.994 -0.254)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.994 38.354) (xy 7.366 38.354) (xy 7.366 -0.254) (xy 78.994 -0.254)
      )
    )
  )
)
