(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 87)
    (no_connects 0)
    (area 136.984999 82.474999 184.35 140.483001)
    (thickness 1.6)
    (drawings 33)
    (tracks 213)
    (zones 0)
    (modules 23)
    (nets 31)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 /TP1)
  (net 4 "Net-(D1-Pad2)")
  (net 5 +BATT)
  (net 6 "Net-(P2-Pad4)")
  (net 7 "Net-(P2-Pad6)")
  (net 8 "Net-(P2-Pad7)")
  (net 9 "Net-(P2-Pad8)")
  (net 10 +5V)
  (net 11 "Net-(P3-Pad1)")
  (net 12 "Net-(P3-Pad2)")
  (net 13 "Net-(P3-Pad5)")
  (net 14 "Net-(P3-Pad6)")
  (net 15 "Net-(P3-Pad7)")
  (net 16 "Net-(P3-Pad8)")
  (net 17 "Net-(P3-Pad9)")
  (net 18 "Net-(P4-Pad1)")
  (net 19 "Net-(P4-Pad2)")
  (net 20 "Net-(P4-Pad3)")
  (net 21 "Net-(P4-Pad4)")
  (net 22 "Net-(P4-Pad5)")
  (net 23 "Net-(P4-Pad6)")
  (net 24 "Net-(P4-Pad7)")
  (net 25 "Net-(P4-Pad8)")
  (net 26 "Net-(P8-Pad1)")
  (net 27 "Net-(SW1-Pad2)")
  (net 28 "Net-(SW1-Pad1)")
  (net 29 P0.3)
  (net 30 P0.2)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net +BATT)
    (add_net /TP1)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P2-Pad7)")
    (add_net "Net-(P2-Pad8)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P3-Pad6)")
    (add_net "Net-(P3-Pad7)")
    (add_net "Net-(P3-Pad8)")
    (add_net "Net-(P3-Pad9)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P4-Pad5)")
    (add_net "Net-(P4-Pad6)")
    (add_net "Net-(P4-Pad7)")
    (add_net "Net-(P4-Pad8)")
    (add_net "Net-(P8-Pad1)")
    (add_net "Net-(SW1-Pad1)")
    (add_net "Net-(SW1-Pad2)")
    (add_net P0.2)
    (add_net P0.3)
  )
  (module Housings_DIP:DIP-20_W7.62mm_LongPads (layer F.Cu) (tedit 5865D9FE)
    (at 162.56 93.98 270)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 3.81 -1.27 540) (layer F.SilkS))
    (fp_text value C8051F330 (at 3.81 10.795 360) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 P0.3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 P0.2))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(P3-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(P3-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(P2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(P2-Pad4)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(P4-Pad8)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(P4-Pad7)"))
    (pad 11 thru_hole oval (at 7.62 22.86 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(P4-Pad6)"))
    (pad 12 thru_hole oval (at 7.62 20.32 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(P4-Pad5)"))
    (pad 13 thru_hole oval (at 7.62 17.78 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(P4-Pad4)"))
    (pad 14 thru_hole oval (at 7.62 15.24 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(P4-Pad3)"))
    (pad 15 thru_hole oval (at 7.62 12.7 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(P4-Pad2)"))
    (pad 16 thru_hole oval (at 7.62 10.16 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(P4-Pad1)"))
    (pad 17 thru_hole oval (at 7.62 7.62 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(P3-Pad8)"))
    (pad 18 thru_hole oval (at 7.62 5.08 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(P3-Pad7)"))
    (pad 19 thru_hole oval (at 7.62 2.54 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(P3-Pad6)"))
    (pad 20 thru_hole oval (at 7.62 0 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(P3-Pad5)"))
    (model Housings_DIP.3dshapes/DIP-20_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:Resistor_Vertical_RM5mm (layer F.Cu) (tedit 5865E169)
    (at 153.035 117.475 270)
    (descr "Resistor, Vertical, RM 5mm, 1/3W,")
    (tags "Resistor, Vertical, RM 5mm, 1/3W,")
    (fp_text reference R1 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 10K (at 0 -1.27 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.49936 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 /TP1))
    (pad 2 thru_hole circle (at 2.5019 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 +3V3))
  )
  (module Crystals:Crystal_HC50-U_Vertical (layer F.Cu) (tedit 5865D043)
    (at 160.02 86.36 180)
    (descr "Crystal, Quarz, HC50/U, vertical, stehend,")
    (tags "Crystal Quarz HC50/U vertical stehend")
    (fp_text reference Y1 (at 0 0 180) (layer F.SilkS))
    (fp_text value Crystal (at 0 -2.54 180) (layer F.Fab))
    (pad 1 thru_hole oval (at -2.44094 0 180) (size 1.99898 2.49936) (drill 1.19888) (layers *.Cu *.Mask)
      (net 29 P0.3))
    (pad 2 thru_hole oval (at 2.44094 0 180) (size 1.99898 2.49936) (drill 1.19888) (layers *.Cu *.Mask)
      (net 30 P0.2))
  )
  (module Capacitors_THT:C_Rect_L7.5_W6.5_P5 (layer F.Cu) (tedit 5865E14D)
    (at 148.59 111.125 270)
    (descr "Film Capacitor Length 7.5mm x Width 6.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C4 (at 3.81 1.905 270) (layer F.SilkS))
    (fp_text value 2.2uf (at 0 1.905 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /TP1))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistors_THT:Resistor_Vertical_RM5mm (layer F.Cu) (tedit 5861753D)
    (at 143.51 86.36)
    (descr "Resistor, Vertical, RM 5mm, 1/3W,")
    (tags "Resistor, Vertical, RM 5mm, 1/3W,")
    (fp_text reference R3 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 2K (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.49936 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 +3V3))
    (pad 2 thru_hole circle (at 2.5019 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(D1-Pad2)"))
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5865DA6D)
    (at 152.4 90.17 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 2.54 1.905 180) (layer F.SilkS))
    (fp_text value 22pf (at -0.635 1.905 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 P0.3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5865DA5B)
    (at 152.4 86.36 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 2.54 1.905 180) (layer F.SilkS))
    (fp_text value 22pf (at -0.635 1.905 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 P0.2))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5865E11D)
    (at 159.385 122.555 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value .1uf (at 2.54 -1.905 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5865DA76)
    (at 146.05 90.17 180)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D1 (at 5.08 -1.27 180) (layer F.SilkS))
    (fp_text value LED (at 5.715 0 180) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5866921A)
    (at 160.02 133.35 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value "" (at 0 7.62 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 +BATT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05 (layer F.Cu) (tedit 586691CF)
    (at 139.7 118.11)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 1.27 -2.54) (layer F.SilkS))
    (fp_text value "" (at 1.27 13.97) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(P2-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /TP1))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(P2-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(P2-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(P2-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x05.wrl
      (at (xyz 0.05 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x10 (layer F.Cu) (tedit 5866920A)
    (at 166.37 86.36)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 17.78 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 P0.2))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 P0.3))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(P3-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(P3-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(P3-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(P3-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x10.wrl
      (at (xyz 0 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x10 (layer F.Cu) (tedit 586691AF)
    (at 166.37 114.3)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 17.78 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(P4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(P4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(P4-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(P4-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(P4-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(P4-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(P4-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(P4-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x10.wrl
      (at (xyz 0 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 586691DD)
    (at 160.02 127 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value "" (at 0 7.62 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 +BATT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 586691FF)
    (at 170.18 86.36)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 13.97 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 586691B7)
    (at 170.18 114.3)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 13.97 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad9)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 586691EE)
    (at 173.99 86.36)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 10.16 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 586691E6)
    (at 173.99 114.3)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P9 (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 10.16 -6.35) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_THT:Resistor_Vertical_RM5mm (layer F.Cu) (tedit 5865D91A)
    (at 144.145 109.855 270)
    (descr "Resistor, Vertical, RM 5mm, 1/3W,")
    (tags "Resistor, Vertical, RM 5mm, 1/3W,")
    (fp_text reference R2 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 1K (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.49936 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(P2-Pad7)"))
    (pad 2 thru_hole circle (at 2.5019 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 /TP1))
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 5866929D)
    (at 172.085 137.16 180)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q1 (at 8.255 0 180) (layer F.SilkS))
    (fp_text value IRF540N (at 0 2.54 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 25 "Net-(P4-Pad8)"))
  )
  (module Capacitors_THT:C_Rect_L7.5_W6.5_P5 (layer F.Cu) (tedit 5865E138)
    (at 148.59 127 90)
    (descr "Film Capacitor Length 7.5mm x Width 6.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C5 (at 0.635 -2.54 270) (layer F.SilkS))
    (fp_text value 47uf (at 4.445 -2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Buttons_Switches_THT:SW_TH_Tactile_Omron_B3F-10xx (layer B.Cu) (tedit 5865E0F1)
    (at 151.13 132.715 180)
    (descr SW_TH_Tactile_Omron_B3F-10xx)
    (tags "Omron B3F-10xx")
    (fp_text reference SW1 (at 3.175 2.54 360) (layer B.SilkS))
    (fp_text value SW_Push_Dual (at 2.95 2.05 180) (layer B.Fab))
    (pad 4 thru_hole circle (at 6 -4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /TP1))
    (pad 3 thru_hole circle (at 0 -4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 6 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(SW1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(SW1-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 586691C3)
    (at 157.48 137.16 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P10 (at 0 -2.39 270) (layer F.SilkS))
    (fp_text value "" (at 0 4.93 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +BATT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "Version 1.0\n01/02/17" (at 156.845 109.22) (layer B.SilkS))
  (gr_text BitBanger (at 152.4 104.775) (layer F.SilkS))
  (gr_line (start 137.16 139.7) (end 137.16 82.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.53 139.7) (end 137.16 139.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.53 82.55) (end 176.53 139.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 82.55) (end 176.53 82.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.53 139.7) (xy 137.16 139.7) (xy 137.16 82.55) (xy 176.53 82.55)
      )
    )
  )
  (zone (net 2) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.53 139.7) (xy 137.16 139.7) (xy 137.16 82.55) (xy 176.53 82.55)
      )
    )
  )
)
