(kicad_pcb (version 4) (host pcbnew 4.0.7+dfsg1-1)
  (general
    (links 0)
    (no_connects 0)
    (area 111.684999 65.184999 191.845001 144.855001)
    (thickness 1.6002)
    (drawings 7)
    (tracks 590)
    (zones 0)
    (modules 72)
    (nets 101)
  )
  (page USLetter)
  (title_block
    (title Blubaru)
  )
  (layers
    (0 Top signal hide)
    (31 Bottom signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (44 Edge.Cuts user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 115.57 82.55)
    (grid_origin 115.57 82.55)
    (visible_elements FFFFE77F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_BIAS")
  (net 4 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_R-")
  (net 5 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_L+")
  (net 6 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_L-")
  (net 7 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_R+")
  (net 8 "/DB-15 interconnects/Modules/Audio switch/BT_L")
  (net 9 "Net-(C10-Pad2)")
  (net 10 "Net-(C11-Pad1)")
  (net 11 "Net-(C13-Pad1)")
  (net 12 "/DB-15 interconnects/Modules/Audio switch/BT_R")
  (net 13 "Net-(C14-Pad2)")
  (net 14 "/DB-15 interconnects/13_IN")
  (net 15 "/DB-15 interconnects/1_IN")
  (net 16 "/DB-15 interconnects/2_IN")
  (net 17 "/DB-15 interconnects/3_IN")
  (net 18 "/DB-15 interconnects/4_IN")
  (net 19 "/DB-15 interconnects/6_IN")
  (net 20 "/DB-15 interconnects/7_IN")
  (net 21 "/DB-15 interconnects/8_IN")
  (net 22 +12V)
  (net 23 "/DB-15 interconnects/10_IN")
  (net 24 "/DB-15 interconnects/11_IN")
  (net 25 "/DB-15 interconnects/12_IN")
  (net 26 "/DB-15 interconnects/6_OUT")
  (net 27 "/DB-15 interconnects/4_OUT")
  (net 28 "/DB-15 interconnects/2_OUT")
  (net 29 "/DB-15 interconnects/Modules/Audio switch/BT_TRG")
  (net 30 "/DB-15 interconnects/Modules/Bluetooth Module/UART_RX")
  (net 31 "/DB-15 interconnects/Modules/Bluetooth Module/UART_TX")
  (net 32 "/DB-15 interconnects/Modules/Bluetooth Module/CMD")
  (net 33 "/DB-15 interconnects/Modules/Bluetooth Module/EVENT")
  (net 34 "/DB-15 interconnects/Modules/Bluetooth Module/VOL+")
  (net 35 "/DB-15 interconnects/Modules/Bluetooth Module/NEXT")
  (net 36 "/DB-15 interconnects/Modules/Bluetooth Module/PLAY")
  (net 37 "/DB-15 interconnects/Modules/Bluetooth Module/PREV")
  (net 38 "/DB-15 interconnects/Modules/Bluetooth Module/VOL-")
  (net 39 "Net-(C6-Pad1)")
  (net 40 "/DB-15 interconnects/Modules/Bluetooth Module/Line Driver/R-")
  (net 41 "/DB-15 interconnects/Modules/Bluetooth Module/Line Driver/R+")
  (net 42 "Net-(C12-Pad2)")
  (net 43 "Net-(C13-Pad2)")
  (net 44 "/DB-15 interconnects/Modules/Bluetooth Module/Line Driver/L+")
  (net 45 "/DB-15 interconnects/Modules/Bluetooth Module/Line Driver/L-")
  (net 46 "Net-(C16-Pad2)")
  (net 47 "Net-(C20-Pad1)")
  (net 48 "Net-(C21-Pad1)")
  (net 49 "Net-(D2-Pad2)")
  (net 50 "Net-(D4-Pad2)")
  (net 51 "Net-(D5-Pad2)")
  (net 52 "Net-(D6-Pad2)")
  (net 53 "/DB-15 interconnects/Modules/Bluetooth Module/9600")
  (net 54 "/DB-15 interconnects/Modules/Bluetooth Module/PWR_EN")
  (net 55 "/DB-15 interconnects/Modules/Microcontroller/LED1")
  (net 56 "/DB-15 interconnects/Modules/Microcontroller/LED2")
  (net 57 "/DB-15 interconnects/Modules/Line In/JACK_SENSE")
  (net 58 "/DB-15 interconnects/Modules/Microcontroller/MOSI")
  (net 59 "/DB-15 interconnects/Modules/Microcontroller/MISO")
  (net 60 "/DB-15 interconnects/Modules/Audio switch/LINE_TRG")
  (net 61 "/DB-15 interconnects/Modules/Microcontroller/SCK")
  (net 62 "Net-(J3-Pad9)")
  (net 63 "/DB-15 interconnects/Modules/Audio switch/LINE_R")
  (net 64 "/DB-15 interconnects/Modules/Audio switch/LINE_L")
  (net 65 "Net-(J3-Pad3)")
  (net 66 "Net-(J7-Pad13)")
  (net 67 "Net-(J7-Pad14)")
  (net 68 "Net-(J7-Pad1)")
  (net 69 "Net-(J7-Pad2)")
  (net 70 GNDA)
  (net 71 "Net-(D1-Pad2)")
  (net 72 "Net-(D7-Pad2)")
  (net 73 +BATT)
  (net 74 "Net-(C9-Pad1)")
  (net 75 "Net-(D3-Pad2)")
  (net 76 "Net-(D6-Pad1)")
  (net 77 "Net-(D7-Pad1)")
  (net 78 "/DB-15 interconnects/Modules/Microcontroller/RESET")
  (net 79 "/DB-15 interconnects/Modules/Microcontroller/BT_RESET")
  (net 80 "Net-(J1-Pad15)")
  (net 81 "Net-(J2-Pad15)")
  (net 82 "Net-(J5-Pad22)")
  (net 83 "Net-(J5-Pad23)")
  (net 84 "Net-(J5-Pad24)")
  (net 85 "Net-(J5-Pad25)")
  (net 86 "Net-(J5-Pad26)")
  (net 87 "Net-(J5-Pad27)")
  (net 88 "Net-(J5-Pad28)")
  (net 89 "Net-(J5-Pad29)")
  (net 90 "Net-(J5-Pad3)")
  (net 91 "Net-(J5-Pad4)")
  (net 92 "Net-(J5-Pad11)")
  (net 93 "Net-(J5-Pad12)")
  (net 94 "Net-(J5-Pad13)")
  (net 95 "Net-(J5-Pad14)")
  (net 96 "Net-(J5-Pad18)")
  (net 97 "Net-(J6-Pad5)")
  (net 98 "Net-(J6-Pad4)")
  (net 99 "Net-(J7-Pad11)")
  (net 100 "Net-(J8-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net "/DB-15 interconnects/10_IN")
    (add_net "/DB-15 interconnects/11_IN")
    (add_net "/DB-15 interconnects/12_IN")
    (add_net "/DB-15 interconnects/13_IN")
    (add_net "/DB-15 interconnects/1_IN")
    (add_net "/DB-15 interconnects/2_IN")
    (add_net "/DB-15 interconnects/2_OUT")
    (add_net "/DB-15 interconnects/3_IN")
    (add_net "/DB-15 interconnects/4_IN")
    (add_net "/DB-15 interconnects/4_OUT")
    (add_net "/DB-15 interconnects/6_IN")
    (add_net "/DB-15 interconnects/6_OUT")
    (add_net "/DB-15 interconnects/7_IN")
    (add_net "/DB-15 interconnects/8_IN")
    (add_net "/DB-15 interconnects/Modules/Audio switch/BT_L")
    (add_net "/DB-15 interconnects/Modules/Audio switch/BT_R")
    (add_net "/DB-15 interconnects/Modules/Audio switch/BT_TRG")
    (add_net "/DB-15 interconnects/Modules/Audio switch/LINE_L")
    (add_net "/DB-15 interconnects/Modules/Audio switch/LINE_R")
    (add_net "/DB-15 interconnects/Modules/Audio switch/LINE_TRG")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/9600")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/CMD")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/EVENT")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/Line Driver/L+")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/Line Driver/L-")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/Line Driver/R+")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/Line Driver/R-")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_BIAS")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_L+")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_L-")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_R+")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_R-")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/NEXT")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/PLAY")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/PREV")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/PWR_EN")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/UART_RX")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/UART_TX")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/VOL+")
    (add_net "/DB-15 interconnects/Modules/Bluetooth Module/VOL-")
    (add_net "/DB-15 interconnects/Modules/Line In/JACK_SENSE")
    (add_net "/DB-15 interconnects/Modules/Microcontroller/BT_RESET")
    (add_net "/DB-15 interconnects/Modules/Microcontroller/LED1")
    (add_net "/DB-15 interconnects/Modules/Microcontroller/LED2")
    (add_net "/DB-15 interconnects/Modules/Microcontroller/MISO")
    (add_net "/DB-15 interconnects/Modules/Microcontroller/MOSI")
    (add_net "/DB-15 interconnects/Modules/Microcontroller/RESET")
    (add_net "/DB-15 interconnects/Modules/Microcontroller/SCK")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J5-Pad11)")
    (add_net "Net-(J5-Pad12)")
    (add_net "Net-(J5-Pad13)")
    (add_net "Net-(J5-Pad14)")
    (add_net "Net-(J5-Pad18)")
    (add_net "Net-(J5-Pad22)")
    (add_net "Net-(J5-Pad23)")
    (add_net "Net-(J5-Pad24)")
    (add_net "Net-(J5-Pad25)")
    (add_net "Net-(J5-Pad26)")
    (add_net "Net-(J5-Pad27)")
    (add_net "Net-(J5-Pad28)")
    (add_net "Net-(J5-Pad29)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J6-Pad4)")
    (add_net "Net-(J6-Pad5)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J7-Pad11)")
    (add_net "Net-(J7-Pad13)")
    (add_net "Net-(J7-Pad14)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J8-Pad5)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.508)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +12V)
    (add_net +BATT)
    (add_net GND)
    (add_net GNDA)
    (add_net VCC)
  )
  (module blubaru:DIP-20_W7.62mm_Socket (layer Top) (tedit 58CC8E2D)
    (at 121.92 116.84 90)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils), Socket")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference IC1 (at 3.81 -2.39 90) (layer F.SilkS))
    (fp_text value ATTINY4313-P (at 3.81 25.25 90) (layer F.Fab))
    (fp_text user %R (at 3.81 11.43 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 "/DB-15 interconnects/Modules/Microcontroller/RESET"))
    (pad 11 thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "/DB-15 interconnects/Modules/Bluetooth Module/PWR_EN"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "/DB-15 interconnects/Modules/Bluetooth Module/UART_TX"))
    (pad 12 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "/DB-15 interconnects/Modules/Line In/JACK_SENSE"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "/DB-15 interconnects/Modules/Bluetooth Module/UART_RX"))
    (pad 13 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "/DB-15 interconnects/Modules/Audio switch/BT_TRG"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(C20-Pad1)"))
    (pad 14 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "/DB-15 interconnects/Modules/Audio switch/LINE_TRG"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(C21-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "/DB-15 interconnects/Modules/Microcontroller/LED2"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "/DB-15 interconnects/Modules/Microcontroller/BT_RESET"))
    (pad 16 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "/DB-15 interconnects/Modules/Microcontroller/LED1"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "/DB-15 interconnects/Modules/Bluetooth Module/EVENT"))
    (pad 17 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "/DB-15 interconnects/Modules/Microcontroller/MOSI"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "/DB-15 interconnects/Modules/Bluetooth Module/CMD"))
    (pad 18 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "/DB-15 interconnects/Modules/Microcontroller/MISO"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "/DB-15 interconnects/Modules/Bluetooth Module/9600"))
    (pad 19 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "/DB-15 interconnects/Modules/Microcontroller/SCK"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model Housings_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:RN52_Breakout (layer Top) (tedit 5A3753DD)
    (at 113.03 118.11 90)
    (descr "RN52 Breakout, https://cdn.sparkfun.com/datasheets/Wireless/Bluetooth/RN-52%20Breakout_v11.pdf")
    (tags "RN52 Breakout")
    (fp_text reference J5 (at 0 0 90) (layer F.SilkS))
    (fp_text value RN52_BREAKOUT (at 0 50.8 90) (layer F.Fab))
    (pad 21 thru_hole oval (at 16.51 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 22 thru_hole oval (at 16.51 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(J5-Pad22)"))
    (pad 23 thru_hole oval (at 16.51 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(J5-Pad23)"))
    (pad 24 thru_hole oval (at 16.51 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(J5-Pad24)"))
    (pad 25 thru_hole oval (at 16.51 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(J5-Pad25)"))
    (pad 26 thru_hole oval (at 16.51 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(J5-Pad26)"))
    (pad 27 thru_hole oval (at 16.51 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(J5-Pad27)"))
    (pad 28 thru_hole oval (at 16.51 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(J5-Pad28)"))
    (pad 29 thru_hole oval (at 16.51 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(J5-Pad29)"))
    (pad 30 thru_hole oval (at 16.51 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(D7-Pad1)"))
    (pad 31 thru_hole oval (at 16.51 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "Net-(D6-Pad1)"))
    (pad 32 thru_hole oval (at 16.51 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_BIAS"))
    (pad 33 thru_hole oval (at 16.51 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_L+"))
    (pad 34 thru_hole oval (at 16.51 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_R+"))
    (pad 35 thru_hole oval (at 16.51 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_L-"))
    (pad 36 thru_hole oval (at 16.51 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_R-"))
    (pad 37 thru_hole oval (at 16.51 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "/DB-15 interconnects/Modules/Bluetooth Module/Line Driver/R-"))
    (pad 38 thru_hole oval (at 16.51 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "/DB-15 interconnects/Modules/Bluetooth Module/Line Driver/L-"))
    (pad 39 thru_hole oval (at 16.51 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "/DB-15 interconnects/Modules/Bluetooth Module/Line Driver/R+"))
    (pad 40 thru_hole circle (at 16.51 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "/DB-15 interconnects/Modules/Bluetooth Module/Line Driver/L+"))
    (pad 1 thru_hole rect (at -16.51 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "/DB-15 interconnects/Modules/Microcontroller/BT_RESET"))
    (pad 2 thru_hole oval (at -16.51 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "/DB-15 interconnects/Modules/Bluetooth Module/EVENT"))
    (pad 3 thru_hole oval (at -16.51 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(J5-Pad3)"))
    (pad 4 thru_hole oval (at -16.51 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(J5-Pad4)"))
    (pad 5 thru_hole oval (at -16.51 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "/DB-15 interconnects/Modules/Bluetooth Module/VOL+"))
    (pad 6 thru_hole oval (at -16.51 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "/DB-15 interconnects/Modules/Bluetooth Module/NEXT"))
    (pad 7 thru_hole oval (at -16.51 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "/DB-15 interconnects/Modules/Bluetooth Module/PLAY"))
    (pad 8 thru_hole oval (at -16.51 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "/DB-15 interconnects/Modules/Bluetooth Module/PREV"))
    (pad 9 thru_hole oval (at -16.51 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "/DB-15 interconnects/Modules/Bluetooth Module/VOL-"))
    (pad 10 thru_hole oval (at -16.51 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "/DB-15 interconnects/Modules/Bluetooth Module/CMD"))
    (pad 11 thru_hole oval (at -16.51 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(J5-Pad11)"))
    (pad 12 thru_hole oval (at -16.51 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 "Net-(J5-Pad12)"))
    (pad 13 thru_hole oval (at -16.51 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 "Net-(J5-Pad13)"))
    (pad 14 thru_hole oval (at -16.51 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(J5-Pad14)"))
    (pad 15 thru_hole oval (at -16.51 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "/DB-15 interconnects/Modules/Bluetooth Module/UART_TX"))
    (pad 16 thru_hole oval (at -16.51 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "/DB-15 interconnects/Modules/Bluetooth Module/UART_RX"))
    (pad 17 thru_hole oval (at -16.51 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "/DB-15 interconnects/Modules/Bluetooth Module/9600"))
    (pad 18 thru_hole oval (at -16.51 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 "Net-(J5-Pad18)"))
    (pad 19 thru_hole oval (at -16.51 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "/DB-15 interconnects/Modules/Bluetooth Module/PWR_EN"))
    (pad 20 thru_hole oval (at -16.51 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x20_Pitch2.54mm.wrl
      (at (xyz -0.65 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x20_Pitch2.54mm.wrl
      (at (xyz 0.65 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module blubaru:C_Disc_D4.0mm_W2.6mm_P2.50mm (layer Top) (tedit 59532FBE)
    (at 152.4 88.9)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=4.0*2.6mm^2, Capacitor, https://www.vishay.com/docs/45171/kseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 4.0mm width 2.6mm Capacitor")
    (fp_text reference C1 (at 4.572 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.36) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz -0.002632 0 0))
      (scale (xyz 1.052632 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:C_Disc_D4.0mm_W2.6mm_P2.50mm (layer Top) (tedit 59532FBE)
    (at 167.64 88.9)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=4.0*2.6mm^2, Capacitor, https://www.vishay.com/docs/45171/kseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 4.0mm width 2.6mm Capacitor")
    (fp_text reference C2 (at 4.572 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.36) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz -0.002632 0 0))
      (scale (xyz 1.052632 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:CP_Radial_D6.3mm_P2.50mm (layer Top) (tedit 5920C257)
    (at 156.21 129.54 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor http://www.nichicon.co.jp/english/products/pdfs/e-usw.pdf")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C3 (at 5.588 0 180) (layer F.SilkS))
    (fp_text value 220uF (at 1.25 4.21 90) (layer F.Fab))
    (fp_text user %R (at 1.1 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:C_Disc_D4.0mm_W2.6mm_P2.50mm (layer Top) (tedit 59532FBE)
    (at 161.29 132.08 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=4.0*2.6mm^2, Capacitor, https://www.vishay.com/docs/45171/kseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 4.0mm width 2.6mm Capacitor")
    (fp_text reference C4 (at 4.318 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.36 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz -0.002632 0 0))
      (scale (xyz 1.052632 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:C_Disc_D5.0mm_W3.2mm_P2.50mm (layer Top) (tedit 59532CCC)
    (at 177.8 118.07)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, https://www.vishay.com/docs/45171/kseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 3.2mm Capacitor")
    (fp_text reference C5 (at 1.25 2.326) (layer F.SilkS))
    (fp_text value 1uF (at 1.25 2.66) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_BIAS"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.28 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:C_Disc_D4.0mm_W2.6mm_P2.50mm (layer Top) (tedit 59532FBE)
    (at 165.1 128.27 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=4.0*2.6mm^2, Capacitor, https://www.vishay.com/docs/45171/kseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 4.0mm width 2.6mm Capacitor")
    (fp_text reference C6 (at 4.064 -0.762 180) (layer F.SilkS))
    (fp_text value 0.047uF (at 1.25 2.36 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_R-"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz -0.002632 0 0))
      (scale (xyz 1.052632 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:C_Disc_D4.0mm_W2.6mm_P2.50mm (layer Top) (tedit 59532FBE)
    (at 166.37 121.92)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=4.0*2.6mm^2, Capacitor, https://www.vishay.com/docs/45171/kseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 4.0mm width 2.6mm Capacitor")
    (fp_text reference C7 (at 1.27 -2.032) (layer F.SilkS))
    (fp_text value 0.047uF (at 1.25 2.36) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_BIAS"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_R+"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz -0.002632 0 0))
      (scale (xyz 1.052632 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:C_Disc_D4.0mm_W2.6mm_P2.50mm (layer Top) (tedit 59532FBE)
    (at 173.99 121.92 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=4.0*2.6mm^2, Capacitor, https://www.vishay.com/docs/45171/kseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 4.0mm width 2.6mm Capacitor")
    (fp_text reference C8 (at 1.27 2.032 180) (layer F.SilkS))
    (fp_text value 0.047uF (at 1.25 2.36 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_BIAS"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_L+"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz -0.002632 0 0))
      (scale (xyz 1.052632 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:C_Disc_D4.0mm_W2.6mm_P2.50mm (layer Top) (tedit 59532FBE)
    (at 175.26 128.27 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=4.0*2.6mm^2, Capacitor, https://www.vishay.com/docs/45171/kseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 4.0mm width 2.6mm Capacitor")
    (fp_text reference C9 (at 4.064 0.762 180) (layer F.SilkS))
    (fp_text value 0.047uF (at 1.25 2.36 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(C9-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_L-"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz -0.002632 0 0))
      (scale (xyz 1.052632 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:CP_Radial_D4.0mm_P1.50mm (layer Top) (tedit 5920C256)
    (at 120.65 96.52)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor http://www.nichicon.co.jp/english/products/pdfs/e-usw.pdf")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference C10 (at -3.048 0) (layer F.SilkS))
    (fp_text value 1uF (at 0.75 3.06) (layer F.Fab))
    (fp_text user %R (at 0.525 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 40 "/DB-15 interconnects/Modules/Bluetooth Module/Line Driver/R-"))
    (pad 2 thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:C_Disc_D5.0mm_W3.2mm_P2.50mm (layer Top) (tedit 59532CCC)
    (at 144.78 96.52)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, https://www.vishay.com/docs/45171/kseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 3.2mm Capacitor")
    (fp_text reference C11 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 1uF (at 1.25 2.66) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.28 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:CP_Radial_D4.0mm_P1.50mm (layer Top) (tedit 5920C256)
    (at 120.65 91.44)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor http://www.nichicon.co.jp/english/products/pdfs/e-usw.pdf")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference C12 (at -3.048 0) (layer F.SilkS))
    (fp_text value 1uF (at 0.75 3.06) (layer F.Fab))
    (fp_text user %R (at 0.525 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 41 "/DB-15 interconnects/Modules/Bluetooth Module/Line Driver/R+"))
    (pad 2 thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 42 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:C_Disc_D5.0mm_W3.2mm_P2.50mm (layer Top) (tedit 59532CCC)
    (at 144.78 88.9)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, https://www.vishay.com/docs/45171/kseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 3.2mm Capacitor")
    (fp_text reference C13 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 1uF (at 1.25 2.66) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C13-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(C13-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.28 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:CP_Radial_D4.0mm_P1.50mm (layer Top) (tedit 5920C256)
    (at 120.65 86.36)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor http://www.nichicon.co.jp/english/products/pdfs/e-usw.pdf")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference C14 (at -3.048 0) (layer F.SilkS))
    (fp_text value 1uF (at 0.75 3.06) (layer F.Fab))
    (fp_text user %R (at 0.525 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 44 "/DB-15 interconnects/Modules/Bluetooth Module/Line Driver/L+"))
    (pad 2 thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 13 "Net-(C14-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:C_Disc_D5.0mm_W3.2mm_P2.50mm (layer Top) (tedit 59532CCC)
    (at 144.78 81.28)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, https://www.vishay.com/docs/45171/kseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 3.2mm Capacitor")
    (fp_text reference C15 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 1uF (at 1.25 2.66) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.28 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:CP_Radial_D4.0mm_P1.50mm (layer Top) (tedit 5920C256)
    (at 120.65 81.28)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor http://www.nichicon.co.jp/english/products/pdfs/e-usw.pdf")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference C16 (at 4.064 -1.778) (layer F.SilkS))
    (fp_text value 1uF (at 0.75 3.06) (layer F.Fab))
    (fp_text user %R (at 0.525 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 45 "/DB-15 interconnects/Modules/Bluetooth Module/Line Driver/L-"))
    (pad 2 thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 46 "Net-(C16-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:CP_Radial_D4.0mm_P1.50mm (layer Top) (tedit 5920C256)
    (at 182.88 95.25 270)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor http://www.nichicon.co.jp/english/products/pdfs/e-usw.pdf")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference C17 (at 3.81 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 0.75 3.06 270) (layer F.Fab))
    (fp_text user %R (at 0.525 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 22 +12V))
    (pad 2 thru_hole circle (at 1.5 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:CP_Radial_D6.3mm_P2.50mm (layer Top) (tedit 5920C257)
    (at 187.96 101.6 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor http://www.nichicon.co.jp/english/products/pdfs/e-usw.pdf")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C18 (at 5.715 0 360) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 4.21 270) (layer F.Fab))
    (fp_text user %R (at 1.1 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:C_Disc_D4.0mm_W2.6mm_P2.50mm (layer Top) (tedit 59532FBE)
    (at 116.84 111.76 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=4.0*2.6mm^2, Capacitor, https://www.vishay.com/docs/45171/kseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 4.0mm width 2.6mm Capacitor")
    (fp_text reference C19 (at 1.25 2.032 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.36 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz -0.002632 0 0))
      (scale (xyz 1.052632 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:C_Disc_D4.0mm_W2.6mm_P2.50mm (layer Top) (tedit 59532FBE)
    (at 123.19 121.92 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=4.0*2.6mm^2, Capacitor, https://www.vishay.com/docs/45171/kseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 4.0mm width 2.6mm Capacitor")
    (fp_text reference C20 (at 1.25 -2.36 180) (layer F.SilkS))
    (fp_text value 22pF (at 1.25 2.36 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz -0.002632 0 0))
      (scale (xyz 1.052632 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:C_Disc_D4.0mm_W2.6mm_P2.50mm (layer Top) (tedit 59532FBE)
    (at 138.43 121.92)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=4.0*2.6mm^2, Capacitor, https://www.vishay.com/docs/45171/kseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 4.0mm width 2.6mm Capacitor")
    (fp_text reference C21 (at 1.27 2.54) (layer F.SilkS))
    (fp_text value 22pF (at 1.25 2.36) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(C21-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz -0.002632 0 0))
      (scale (xyz 1.052632 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:LED_D3.0mm_Horizontal_O1.27mm_Z6.0mm (layer Top) (tedit 5A374A26)
    (at 120.65 139.7)
    (descr "LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins")
    (tags "LED diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.54) (layer F.SilkS))
    (fp_text value "R LED" (at 1.27 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 71 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm_Horizontal_O1.27mm_Z6.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:LED_D3.0mm_Horizontal_O1.27mm_Z6.0mm (layer Top) (tedit 5A374A26)
    (at 125.73 139.7)
    (descr "LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins")
    (tags "LED diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -2.54) (layer F.SilkS))
    (fp_text value "B LED" (at 1.27 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 49 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm_Horizontal_O1.27mm_Z6.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:LED_D3.0mm_Horizontal_O1.27mm_Z6.0mm (layer Top) (tedit 5A374A26)
    (at 130.81 139.7)
    (descr "LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins")
    (tags "LED diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -2.54) (layer F.SilkS))
    (fp_text value "Y LED" (at 1.27 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 75 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm_Horizontal_O1.27mm_Z6.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:LED_D3.0mm_Horizontal_O1.27mm_Z6.0mm (layer Top) (tedit 5A374A26)
    (at 135.89 139.7)
    (descr "LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins")
    (tags "LED diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -2.54) (layer F.SilkS))
    (fp_text value "O LED" (at 1.27 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 50 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm_Horizontal_O1.27mm_Z6.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:LED_D3.0mm_Horizontal_O1.27mm_Z6.0mm (layer Top) (tedit 5A374A26)
    (at 140.97 139.7)
    (descr "LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins")
    (tags "LED diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -2.54) (layer F.SilkS))
    (fp_text value "G LED" (at 1.27 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 51 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm_Horizontal_O1.27mm_Z6.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:LED_D3.0mm_Horizontal_O1.27mm_Z6.0mm (layer Top) (tedit 5A374A26)
    (at 146.05 139.7)
    (descr "LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins")
    (tags "LED diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -2.54) (layer F.SilkS))
    (fp_text value "B LED" (at 1.27 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 76 "Net-(D6-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 52 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm_Horizontal_O1.27mm_Z6.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:LED_D3.0mm_Horizontal_O1.27mm_Z6.0mm (layer Top) (tedit 5A374A26)
    (at 151.13 139.7)
    (descr "LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins")
    (tags "LED diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins")
    (fp_text reference D7 (at 1.27 -2.54) (layer F.SilkS))
    (fp_text value "R LED" (at 1.27 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 77 "Net-(D7-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 72 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm_Horizontal_O1.27mm_Z6.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-41_SOD81_P7.62mm_Horizontal (layer Top) (tedit 5921392F)
    (at 181.61 88.9 90)
    (descr "D, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D8 (at 4.064 2.286 90) (layer F.SilkS))
    (fp_text value D (at 3.81 2.41 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 +12V))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 73 +BATT))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:DB15FC (layer Top) (tedit 58CEE08D)
    (at 121.92 76.2)
    (descr http://media.digikey.com/pdf/Data%20Sheets/Assmann%20PDFs/A-Dx%20-xx-A_KG-T4_T2_Dwg.pdf)
    (tags "CONN DB15")
    (fp_text reference J1 (at 9.86 2.54) (layer F.SilkS))
    (fp_text value DB15 (at 9.65 -7.62) (layer F.Fab))
    (pad "" thru_hole circle (at 26.345 -1.42) (size 3.81 3.81) (drill 3.05) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -6.955 -1.42) (size 3.81 3.81) (drill 3.05) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/DB-15 interconnects/1_IN"))
    (pad 2 thru_hole circle (at 2.77 0) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/DB-15 interconnects/2_IN"))
    (pad 3 thru_hole circle (at 5.54 0) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/DB-15 interconnects/3_IN"))
    (pad 4 thru_hole circle (at 8.31 0) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/DB-15 interconnects/4_IN"))
    (pad 5 thru_hole circle (at 11.08 0) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 70 GNDA))
    (pad 6 thru_hole circle (at 13.85 0) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/DB-15 interconnects/6_IN"))
    (pad 7 thru_hole circle (at 16.62 0) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/DB-15 interconnects/7_IN"))
    (pad 8 thru_hole circle (at 19.39 0) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/DB-15 interconnects/8_IN"))
    (pad 9 thru_hole circle (at 1.385 -2.84) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 73 +BATT))
    (pad 10 thru_hole circle (at 4.155 -2.84) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 23 "/DB-15 interconnects/10_IN"))
    (pad 11 thru_hole circle (at 6.925 -2.84) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 24 "/DB-15 interconnects/11_IN"))
    (pad 12 thru_hole circle (at 9.695 -2.84) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/DB-15 interconnects/12_IN"))
    (pad 13 thru_hole circle (at 12.465 -2.84) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/DB-15 interconnects/13_IN"))
    (pad 14 thru_hole circle (at 15.235 -2.84) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole circle (at 18.005 -2.84) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(J1-Pad15)"))
    (model Connectors.3dshapes/DB15FC.wrl
      (at (xyz 0.38 0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:DB15MC (layer Top) (tedit 58CEEE42)
    (at 181.61 76.2)
    (descr http://media.digikey.com/pdf/Data%20Sheets/Assmann%20PDFs/A-Dx%20-xx-A_KG-T4_T2_Dwg.pdf)
    (tags "CONN DB15")
    (fp_text reference J2 (at -9.53 2.54) (layer F.SilkS))
    (fp_text value DB15 (at -9.74 -7.62) (layer F.Fab))
    (pad "" thru_hole circle (at 6.955 -1.42) (size 3.81 3.81) (drill 3.05) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -26.345 -1.42) (size 3.81 3.81) (drill 3.05) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -19.39 0) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/DB-15 interconnects/8_IN"))
    (pad 7 thru_hole circle (at -16.62 0) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/DB-15 interconnects/7_IN"))
    (pad 6 thru_hole circle (at -13.85 0) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 26 "/DB-15 interconnects/6_OUT"))
    (pad 5 thru_hole circle (at -11.08 0) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 70 GNDA))
    (pad 4 thru_hole circle (at -8.31 0) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 27 "/DB-15 interconnects/4_OUT"))
    (pad 3 thru_hole circle (at -5.54 0) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/DB-15 interconnects/3_IN"))
    (pad 2 thru_hole circle (at -2.77 0) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 28 "/DB-15 interconnects/2_OUT"))
    (pad 1 thru_hole rect (at 0 0) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/DB-15 interconnects/1_IN"))
    (pad 15 thru_hole circle (at -18.005 -2.84) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(J2-Pad15)"))
    (pad 14 thru_hole circle (at -15.235 -2.84) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole circle (at -12.465 -2.84) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/DB-15 interconnects/13_IN"))
    (pad 12 thru_hole circle (at -9.695 -2.84) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/DB-15 interconnects/12_IN"))
    (pad 11 thru_hole circle (at -6.925 -2.84) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 24 "/DB-15 interconnects/11_IN"))
    (pad 10 thru_hole circle (at -4.155 -2.84) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 23 "/DB-15 interconnects/10_IN"))
    (pad 9 thru_hole circle (at -1.385 -2.84) (size 1.52 1.52) (drill 1) (layers *.Cu *.Mask)
      (net 73 +BATT))
    (model Connectors.3dshapes/DB15MC.wrl
      (at (xyz -0.38 0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:TS5A22364-Q1 (layer Top) (tedit 59337BBB)
    (at 152.4 88.9 90)
    (descr "TS5A22364-Q1, http://www.proto-advantage.com/store/datasheets/PA0027.pdf")
    (tags "MSOP-10 to DIP-10 SMT Adapter")
    (fp_text reference J3 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value TS5A22364-Q1 (at 0 12.7 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 3.81 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 3.81 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "/DB-15 interconnects/Modules/Audio switch/LINE_TRG"))
    (pad 8 thru_hole oval (at 3.81 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/DB-15 interconnects/Modules/Audio switch/BT_R"))
    (pad 9 thru_hole oval (at 3.81 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(J3-Pad9)"))
    (pad 10 thru_hole circle (at 3.81 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "/DB-15 interconnects/Modules/Audio switch/LINE_R"))
    (pad 1 thru_hole rect (at -3.81 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at -3.81 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "/DB-15 interconnects/Modules/Audio switch/LINE_L"))
    (pad 3 thru_hole oval (at -3.81 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at -3.81 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/DB-15 interconnects/Modules/Audio switch/BT_L"))
    (pad 5 thru_hole oval (at -3.81 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "/DB-15 interconnects/Modules/Audio switch/LINE_TRG"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz -0.15 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0.15 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module blubaru:TS5A22364-Q1 (layer Top) (tedit 59337BBB)
    (at 167.64 88.9 90)
    (descr "TS5A22364-Q1, http://www.proto-advantage.com/store/datasheets/PA0027.pdf")
    (tags "MSOP-10 to DIP-10 SMT Adapter")
    (fp_text reference J4 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value TS5A22364-Q1 (at 0 12.7 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 3.81 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 3.81 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "/DB-15 interconnects/Modules/Audio switch/BT_TRG"))
    (pad 8 thru_hole oval (at 3.81 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/DB-15 interconnects/2_IN"))
    (pad 9 thru_hole oval (at 3.81 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "/DB-15 interconnects/2_OUT"))
    (pad 10 thru_hole circle (at 3.81 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(J3-Pad9)"))
    (pad 1 thru_hole rect (at -3.81 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at -3.81 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(J3-Pad3)"))
    (pad 3 thru_hole oval (at -3.81 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "/DB-15 interconnects/4_OUT"))
    (pad 4 thru_hole oval (at -3.81 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/DB-15 interconnects/4_IN"))
    (pad 5 thru_hole oval (at -3.81 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "/DB-15 interconnects/Modules/Audio switch/BT_TRG"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz -0.15 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0.15 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module blubaru:sj1-353xng (layer Top) (tedit 597814B2)
    (at 170.18 143.51 90)
    (descr http://www.cui.com/product/resource/sj1-353xng.pdf)
    (tags "sj1-353xng audio jack")
    (fp_text reference J6 (at 12.065 -5.334 180) (layer F.SilkS))
    (fp_text value JACK_TRS_5PINS (at 5.4 2.5 90) (layer F.Fab))
    (pad 5 thru_hole rect (at 6.1 0 135) (size 2.4 2.4) (drill 1.9) (layers *.Cu *.Mask)
      (net 97 "Net-(J6-Pad5)"))
    (pad 4 thru_hole oval (at 11.6 0 90) (size 2.4 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 98 "Net-(J6-Pad4)"))
    (pad 3 thru_hole rect (at 7.9 -2 135) (size 2.4 2.4) (drill 1.9) (layers *.Cu *.Mask)
      (net 39 "Net-(C6-Pad1)"))
    (pad 2 thru_hole oval (at 2.4 -2 90) (size 2.4 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 74 "Net-(C9-Pad1)"))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.4 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/packages3d/sj1-3535ng.wrl
      (at (xyz 0.147 0.005 0.175))
      (scale (xyz 3.56 3.56 3.56))
      (rotate (xyz 180 0 180))
    )
  )
  (module blubaru:DRV632 (layer Top) (tedit 59337ACE)
    (at 132.08 88.9 90)
    (descr http://www.proto-advantage.com/store/datasheets/PA0033.pdf)
    (tags "DRV632 TSSOP-14 to DIP-14 SMT Adapter (0.65 mm pitch) ")
    (fp_text reference J7 (at -0.254 -0.635 90) (layer F.SilkS))
    (fp_text value DRV632 (at 0 17.78 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 3.81 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(C13-Pad1)"))
    (pad 9 thru_hole oval (at 3.81 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 10 thru_hole oval (at 3.81 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 3.81 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 "Net-(J7-Pad11)"))
    (pad 12 thru_hole oval (at 3.81 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/DB-15 interconnects/Modules/Audio switch/BT_R"))
    (pad 13 thru_hole oval (at 3.81 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(J7-Pad13)"))
    (pad 14 thru_hole circle (at 3.81 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(J7-Pad14)"))
    (pad 1 thru_hole rect (at -3.81 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(J7-Pad1)"))
    (pad 2 thru_hole oval (at -3.81 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(J7-Pad2)"))
    (pad 3 thru_hole oval (at -3.81 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/DB-15 interconnects/Modules/Audio switch/BT_L"))
    (pad 4 thru_hole oval (at -3.81 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at -3.81 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 6 thru_hole oval (at -3.81 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad 7 thru_hole oval (at -3.81 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(C13-Pad2)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz -0.15 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0.15 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module blubaru:sj1-353xng (layer Top) (tedit 597814B2)
    (at 179.07 143.51 90)
    (descr http://www.cui.com/product/resource/sj1-353xng.pdf)
    (tags "sj1-353xng audio jack")
    (fp_text reference J8 (at 12.065 5.08 180) (layer F.SilkS))
    (fp_text value JACK_TRS_5PINS (at 5.4 2.5 90) (layer F.Fab))
    (pad 5 thru_hole rect (at 6.1 0 135) (size 2.4 2.4) (drill 1.9) (layers *.Cu *.Mask)
      (net 100 "Net-(J8-Pad5)"))
    (pad 4 thru_hole oval (at 11.6 0 90) (size 2.4 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 57 "/DB-15 interconnects/Modules/Line In/JACK_SENSE"))
    (pad 3 thru_hole rect (at 7.9 -2 135) (size 2.4 2.4) (drill 1.9) (layers *.Cu *.Mask)
      (net 63 "/DB-15 interconnects/Modules/Audio switch/LINE_R"))
    (pad 2 thru_hole oval (at 2.4 -2 90) (size 2.4 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 64 "/DB-15 interconnects/Modules/Audio switch/LINE_L"))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.4 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 70 GNDA))
    (model ${KIPRJMOD}/packages3d/sj1-3535ng.wrl
      (at (xyz 0.147 0.005 0.175))
      (scale (xyz 3.56 3.56 3.56))
      (rotate (xyz 180 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer Top) (tedit 59650532)
    (at 133.35 130.81 270)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference P1 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 15.03 270) (layer F.Fab))
    (fp_text user %R (at 0 6.35 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "/DB-15 interconnects/Modules/Bluetooth Module/VOL-"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "/DB-15 interconnects/Modules/Bluetooth Module/PREV"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "/DB-15 interconnects/Modules/Bluetooth Module/PLAY"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "/DB-15 interconnects/Modules/Bluetooth Module/NEXT"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "/DB-15 interconnects/Modules/Bluetooth Module/VOL+"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer Top) (tedit 59650532)
    (at 172.72 113.03 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference P2 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "/DB-15 interconnects/Modules/Microcontroller/MISO"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "/DB-15 interconnects/Modules/Microcontroller/SCK"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "/DB-15 interconnects/Modules/Microcontroller/MOSI"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "/DB-15 interconnects/Modules/Microcontroller/RESET"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 151.892 117.094 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 330 (at 2.54 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 52 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 154.686 117.094 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 750 (at 2.54 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 72 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 168.91 129.54 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value 2k2 (at 2.54 1.86 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 39 "Net-(C6-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_BIAS"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 171.45 124.46 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 2k2 (at 2.54 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "/DB-15 interconnects/Modules/Bluetooth Module/Microphone/MIC_BIAS"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 74 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 132.08 96.52)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at 2.54 0) (layer F.SilkS))
    (fp_text value 8.2k (at 2.54 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 69 "Net-(J7-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "/DB-15 interconnects/Modules/Audio switch/BT_L"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 124.46 95.25)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R6 (at 2.54 0) (layer F.SilkS))
    (fp_text value 11k (at 2.54 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 69 "Net-(J7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 124.46 92.71)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R7 (at 2.54 0) (layer F.SilkS))
    (fp_text value 11k (at 2.54 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 42 "Net-(C12-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 68 "Net-(J7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 124.46 90.17)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R8 (at 2.54 0) (layer F.SilkS))
    (fp_text value 8.2k (at 2.54 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 70 GNDA))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 68 "Net-(J7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 124.46 87.63)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R9 (at 2.54 0) (layer F.SilkS))
    (fp_text value 8.2k (at 2.54 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 70 GNDA))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 67 "Net-(J7-Pad14)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 124.46 85.09)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R10 (at 2.54 0) (layer F.SilkS))
    (fp_text value 11k (at 2.54 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(C14-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 67 "Net-(J7-Pad14)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 124.46 82.55)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R11 (at 2.54 0) (layer F.SilkS))
    (fp_text value 11k (at 2.54 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 46 "Net-(C16-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 66 "Net-(J7-Pad13)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 132.08 81.28)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R12 (at 2.54 0) (layer F.SilkS))
    (fp_text value 8.2k (at 2.54 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 66 "Net-(J7-Pad13)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "/DB-15 interconnects/Modules/Audio switch/BT_R"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 179.07 128.27 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R13 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value 100k (at 2.54 1.86 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 63 "/DB-15 interconnects/Modules/Audio switch/LINE_R"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 181.61 128.27 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R14 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value 100k (at 2.54 1.86 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 64 "/DB-15 interconnects/Modules/Audio switch/LINE_L"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 184.15 128.27 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R15 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value 1M (at 2.54 1.86 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 57 "/DB-15 interconnects/Modules/Line In/JACK_SENSE"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 113.792 127 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R16 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value 750 (at 2.54 1.86 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 71 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 116.332 127 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R17 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value 330 (at 2.54 1.86 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 49 "Net-(D2-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 29 "/DB-15 interconnects/Modules/Audio switch/BT_TRG"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 113.792 105.156)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R18 (at 2.54 0) (layer F.SilkS))
    (fp_text value 750 (at 2.54 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 75 "Net-(D3-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 56 "/DB-15 interconnects/Modules/Microcontroller/LED2"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 113.792 107.696)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R19 (at 2.54 0) (layer F.SilkS))
    (fp_text value 750 (at 2.54 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 50 "Net-(D4-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 55 "/DB-15 interconnects/Modules/Microcontroller/LED1"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer Top) (tedit 5874F706)
    (at 144.018 131.572 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R20 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 330 (at 2.54 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 51 "Net-(D5-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 60 "/DB-15 interconnects/Modules/Audio switch/LINE_TRG"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module blubaru:SW_Tactile_SPST_Angled_PTS645Vx58-2LFS (layer Top) (tedit 5A35CFB0)
    (at 162.56 142.24 180)
    (descr "tactile switch SPST right angle, PTS645VL58-2 LFS")
    (tags "tactile switch SPST angled PTS645VL58-2 LFS C&K Button")
    (fp_text reference SW1 (at 2.25 1.68 180) (layer F.SilkS))
    (fp_text value SW_Push (at 2.25 5.38988 180) (layer F.Fab))
    (fp_text user %R (at 2.25 1.68 180) (layer F.Fab))
    (pad "" thru_hole circle (at 5.75 2.55 180) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 4.5 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 78 "/DB-15 interconnects/Modules/Microcontroller/RESET"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at -1.25 2.55 180) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_Tactile_SPST_Angled_PTS645Vx58-2LFS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer Top) (tedit 58CC8E33)
    (at 170.18 104.14 90)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 -2.39 90) (layer F.SilkS))
    (fp_text value DG419 (at 3.81 10.01 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "/DB-15 interconnects/6_OUT"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "/DB-15 interconnects/6_IN"))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "/DB-15 interconnects/Modules/Audio switch/BT_TRG"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 +12V))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 +12V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Vertical (layer Top) (tedit 58CE52AD)
    (at 187.96 90.17 270)
    (descr "TO-220, Vertical, RM 2.54mm")
    (tags "TO-220 Vertical RM 2.54mm")
    (fp_text reference U2 (at 1.27 3.175 270) (layer F.SilkS))
    (fp_text value LD1117V33 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 22 +12V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-4H_Vertical (layer Top) (tedit 58CD2E9C)
    (at 128.37 121.92)
    (descr "Crystal THT HC-49-4H http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49-4H")
    (fp_text reference Y1 (at 2.44 3.556) (layer F.SilkS))
    (fp_text value 11.0592MHz (at 2.44 3.525) (layer F.Fab))
    (fp_text user %R (at 2.44 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 4.88 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_HC49-4H_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer Top) (tedit 5A8507E0)
    (at 187.96 82.55)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer Top) (tedit 5A8507ED)
    (at 115.57 82.55)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer Top) (tedit 5A8507FF)
    (at 115.57 140.97)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer Top) (tedit 5A85080A)
    (at 187.96 140.97)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Symbols:OSHW-Logo_11.4x12mm_SilkScreen (layer Bottom) (tedit 0)
    (at 185.166 111.76 270)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_11.4x12mm_SilkScreen (at 0.75 0 270) (layer B.Fab) hide)
  )
  (module Symbols:ESD-Logo_6.6x6mm_SilkScreen (layer Bottom) (tedit 0)
    (at 123.317 112.649 180)
    (descr "Electrostatic discharge Logo")
    (tags "Logo ESD")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value ESD-Logo_6.6x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Symbols:Symbol_KiCAD-Logo_CopperAndSilkScreenTop (layer Bottom) (tedit 0)
    (at 152.908 106.68 180)
    (descr "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (tags "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (fp_text reference REF** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "KiCAD Logo" (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Symbols:WEEE-Logo_4.2x6mm_SilkScreen (layer Bottom) (tedit 0)
    (at 186.69 133.35 270)
    (descr "Waste Electrical and Electronic Equipment Directive")
    (tags "Logo WEEE")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value WEEE-Logo_4.2x6mm_SilkScreen (at 0.75 0 270) (layer B.Fab) hide)
  )
  (gr_text CD (at 130.81 69.85) (layer B.SilkS))
  (gr_text Stereo (at 172.085 69.85) (layer B.SilkS))
  (gr_text "Blubaru 1.0\ngithub.com/jbebel/blubaru" (at 188.722 122.682 90) (layer F.SilkS))
  (gr_line (start 111.76 144.78) (end 191.77 144.78) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.76 65.26) (end 191.77 65.26) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.77 65.26) (end 191.77 144.78) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.76 65.26) (end 111.76 144.78) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.77 64.77) (xy 191.77 144.78) (xy 111.76 144.78) (xy 111.76 64.77)
      )
    )
  )
)
