(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/~{DRIVE_SELECT}")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "GND")
  (net 4 "/DATA_RATE_1")
  (net 5 "+5V")
  (net 6 "/DRIVE1_STATUS1")
  (net 7 "+12V")
  (net 8 "/~{FF_O_INDEX}")
  (net 9 "/DRIVE0_STATUS0")
  (net 10 "/~{SECURITY_COMMAND}")
  (net 11 "/~{FF_I_MO}")
  (net 12 "/MEDIA1_STATUS3")
  (net 13 "/~{DIRECTION_IN}")
  (net 14 "/~{FF_I_STEP}")
  (net 15 "/~{FF_I_WD}")
  (net 16 "/~{FF_I_WG}")
  (net 17 "/~{FF_O_TZ}")
  (net 18 "/MEDIA0_STATUS2")
  (net 19 "/~{FF_O_WP}")
  (net 20 "/~{FF_O_RD}")
  (net 21 "/~{FF_I_SS}")
  (net 22 "/DATA_RATE_0")
  (net 23 "/~{DISKETTE_CHANGE}")
  (net 24 "/~{FF_O_DENSITY}")
  (net 25 "/~{FF_I_DS1}")
  (footprint "Connector_IDC:IDC-Header_2x17_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 5EAC9A08)
    (at 114.3 114.3 180)
    (descr "Through hole IDC box header, 2x17, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole horizontal IDC box header THT 2x17 2.54mm double row")
    (property "Sheetfile" "PSFF2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -0.762 -6.604) (layer "F.SilkS"))
    (fp_text value "PS2_SIDE" (at -2.794 20.32 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 8.83 20.32 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 3 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/DATA_RATE_1") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "+5V") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/DRIVE1_STATUS1") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "+12V") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/~{FF_O_INDEX}") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/DRIVE0_STATUS0") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/~{DRIVE_SELECT}") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/~{SECURITY_COMMAND}") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole circle (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole circle (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/~{FF_I_MO}") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole circle (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/MEDIA1_STATUS3") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole circle (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/~{DIRECTION_IN}") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole circle (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole circle (at 2.54 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/~{FF_I_STEP}") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole circle (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole circle (at 2.54 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/~{FF_I_WD}") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole circle (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole circle (at 2.54 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/~{FF_I_WG}") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole circle (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole circle (at 2.54 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/~{FF_O_TZ}") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole circle (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/MEDIA0_STATUS2") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole circle (at 2.54 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/~{FF_O_WP}") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole circle (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole circle (at 2.54 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/~{FF_O_RD}") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole circle (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole circle (at 2.54 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/~{FF_I_SS}") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" thru_hole circle (at 0 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/DATA_RATE_0") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole circle (at 2.54 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "/~{DISKETTE_CHANGE}") (pinfunction "Pin_34") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x17_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_DIP_SPSTx02_Piano_10.8x6.64mm_W7.62mm_P2.54mm" (layer "F.Cu")
    (tedit 5A4E1404)
    (at 121.92 127 90)
    (descr "2x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x6.64mm")
    (tags "DIP Switch SPST Piano 7.62mm 300mil")
    (property "Sheetfile" "PSFF2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW2" (at 3.81 -3.11 90) (layer "F.SilkS") hide)
    (fp_text value "MEDIA_TYPE" (at 3.81 -3.302 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "/MEDIA0_STATUS2") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "/MEDIA1_STATUS3") (pintype "passive"))
    (pad "3" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx02_Piano_10.8x6.64mm_W7.62mm_P2.54mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 131.445 70.612 -90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "PSFF2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "DATA_RATE" (at -2.54 2.8575 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/~{SECURITY_COMMAND}") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/DATA_RATE_0") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/DATA_RATE_1") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 134.874 115.316 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PSFF2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 1.524 180) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.65) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 6 "/DRIVE1_STATUS1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 5 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_DIP_SPSTx02_Piano_10.8x6.64mm_W7.62mm_P2.54mm" (layer "F.Cu")
    (tedit 5A4E1404)
    (at 132.08 127 90)
    (descr "2x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x6.64mm")
    (tags "DIP Switch SPST Piano 7.62mm 300mil")
    (property "Sheetfile" "PSFF2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at 3.81 -3.11 90) (layer "F.SilkS") hide)
    (fp_text value "DRIVE_TYPE" (at 3.81 5.65 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "/DRIVE0_STATUS0") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "/DRIVE1_STATUS1") (pintype "passive"))
    (pad "3" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx02_Piano_10.8x6.64mm_W7.62mm_P2.54mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 128.27 107.696 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "PSFF2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at -1.778 0 180) (layer "F.SilkS"))
    (fp_text value "1N914" (at 3.81 2.12 90) (layer "F.Fab") hide)
    (fp_text user "K" (at 0 -1.8 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 4.11 0 90) (layer "F.Fab") hide)
    (fp_text user "K" (at 0 -1.8 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "/~{DRIVE_SELECT}") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 125.222 115.316 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PSFF2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0 1.524 180) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.65) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 12 "/MEDIA1_STATUS3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 5 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 121.666 115.316 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PSFF2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 1.524 180) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.65) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 18 "/MEDIA0_STATUS2") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 5 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 131.318 115.316 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PSFF2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 1.524 180) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.65) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 9 "/DRIVE0_STATUS0") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 5 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 141.605 64.77 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "PSFF2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "POWER" (at -2.54 6.604 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "+12V") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x17_P2.54mm_Horizontal" (layer "B.Cu")
    (tedit 5EAC9A08)
    (at 141.6225 114.3)
    (descr "Through hole IDC box header, 2x17, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole horizontal IDC box header THT 2x17 2.54mm double row")
    (property "Sheetfile" "PSFF2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 6.215 6.1) (layer "B.SilkS"))
    (fp_text value "FF_SIDE" (at -2.5575 -20.32 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 8.83 -20.32 90) (layer "B.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 3 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "/~{FF_O_DENSITY}") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 2.54 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/~{FF_O_INDEX}") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 2.54 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/~{DRIVE_SELECT}") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle (at 2.54 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/~{FF_I_DS1}") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle (at 2.54 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole circle (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole circle (at 2.54 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/~{FF_I_MO}") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole circle (at 0 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole circle (at 2.54 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/~{DIRECTION_IN}") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole circle (at 0 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole circle (at 2.54 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/~{FF_I_STEP}") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole circle (at 0 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole circle (at 2.54 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/~{FF_I_WD}") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole circle (at 0 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole circle (at 2.54 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/~{FF_I_WG}") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole circle (at 0 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole circle (at 2.54 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/~{FF_O_TZ}") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole circle (at 0 -33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole circle (at 2.54 -33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/~{FF_O_WP}") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole circle (at 0 -35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole circle (at 2.54 -35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/~{FF_O_RD}") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole circle (at 0 -38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole circle (at 2.54 -38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/~{FF_I_SS}") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" thru_hole circle (at 0 -40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole circle (at 2.54 -40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "/~{DISKETTE_CHANGE}") (pinfunction "Pin_34") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x17_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 109.22 129.032) (end 147.32 54.356) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "+5V (red)" (at 139.446 64.77) (layer "F.SilkS"))
  (gr_text "DR0" (at 128.905 72.644 90) (layer "F.SilkS"))
  (gr_text "MEDIA\n 0 0  Reserved\n 0 1  4MB (2.88MB)\n 1 0  2MB (1.44MB)\n 1 1  1MB (720KB)\n\nDRIVE\n 0 0  3.5{dblquote}, 1.44MB\n 0 1  3.5{dblquote}, 2.88MB\n 1 0  5.25{dblquote}, 1.2MB\n 1 1  Reserved" (at 121.412 96.012) (layer "F.SilkS"))
  (gr_text "PS2FF Media Sense Adapter\nJune Tate-Gans\njune@theonelab.com\nCC-BY-SA\nBoard Rev A\nSchematic Rev A" (at 110.998 60.833) (layer "F.SilkS"))
  (gr_text "DR1" (at 126.365 72.644 90) (layer "F.SilkS"))
  (gr_text "SECURE_COMMAND" (at 131.572 72.644 90) (layer "F.SilkS"))
  (zone (net 3) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.32 129.032)
        (xy 109.22 129.032)
        (xy 109.22 54.356)
        (xy 147.32 54.356)
      )
    )
  )
)
