(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 117)
    (no_connects 0)
    (area 96.1526 74.9126 141.1584 106.5668)
    (thickness 1.6)
    (drawings 16)
    (tracks 451)
    (zones 0)
    (modules 45)
    (nets 43)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 1.016 0.508)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.75 0.75)
    (mod_text_width 0.12)
    (pad_size 2.7 2.7)
    (pad_drill 2.7)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 /LED_B)
  (net 4 /LED_R)
  (net 5 /LED_G)
  (net 6 +BATT)
  (net 7 /RESET)
  (net 8 /TSC_SAMPLING)
  (net 9 /BATT_2)
  (net 10 /THERM_SENSE)
  (net 11 /THERM_SW)
  (net 12 /TSC_IN)
  (net 13 /SWDIO)
  (net 14 /SWCLK)
  (net 15 "Net-(R1-Pad2)")
  (net 16 "Net-(R4-Pad1)")
  (net 17 /LED_DBG)
  (net 18 /MCO)
  (net 19 "Net-(BT1-Pad1)")
  (net 20 "Net-(BT2-Pad1)")
  (net 21 "Net-(D2-Pad2)")
  (net 22 "Net-(C10-Pad1)")
  (net 23 "Net-(Q1-Pad3)")
  (net 24 "Net-(Q2-Pad3)")
  (net 25 "Net-(Q3-Pad3)")
  (net 26 /LED_R_CONN)
  (net 27 /LED_G_CONN)
  (net 28 /LED_B_CONN)
  (net 29 /UART_TX)
  (net 30 /UART_RX)
  (net 31 "Net-(U2-Pad3)")
  (net 32 "Net-(U2-Pad10)")
  (net 33 "Net-(U2-Pad11)")
  (net 34 "Net-(U2-Pad12)")
  (net 35 "Net-(U2-Pad13)")
  (net 36 "Net-(U2-Pad14)")
  (net 37 "Net-(U2-Pad21)")
  (net 38 "Net-(U2-Pad22)")
  (net 39 "Net-(U2-Pad26)")
  (net 40 "Net-(U2-Pad27)")
  (net 41 "Net-(U2-Pad28)")
  (net 42 +3.3VA)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3.3VA)
    (add_net /BATT_2)
    (add_net /LED_B)
    (add_net /LED_B_CONN)
    (add_net /LED_DBG)
    (add_net /LED_G)
    (add_net /LED_G_CONN)
    (add_net /LED_R)
    (add_net /LED_R_CONN)
    (add_net /MCO)
    (add_net /RESET)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /THERM_SENSE)
    (add_net /THERM_SW)
    (add_net /TSC_IN)
    (add_net /TSC_SAMPLING)
    (add_net /UART_RX)
    (add_net /UART_TX)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(BT2-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q2-Pad3)")
    (add_net "Net-(Q3-Pad3)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad3)")
  )
  (net_class Minimum ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.508)
    (via_dia 1.016)
    (via_drill 0.508)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3V3)
    (add_net +BATT)
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 58B35D39)
    (at 113.0554 103.1494)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P3 (at -0.0508 1.8288) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.39) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer B.Cu) (tedit 58B21526)
    (at 134.62 77.724 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P4 (at 2.1336 0 180) (layer B.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -10.01 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /SWCLK))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /SWDIO))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /RESET))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer B.Cu) (tedit 58B21512)
    (at 131.7244 85.344)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P5 (at -2.6924 -2.4384) (layer B.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 -4.93) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /UART_TX))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /UART_RX))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer B.Cu) (tedit 58B2148D)
    (at 134.6708 103.1748 180)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P6 (at 1.9812 0 180) (layer B.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -2.39 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module components:Keystone_3020_2x2016-CoinCell locked (layer B.Cu) (tedit 58B21456)
    (at 118.8212 89.662 180)
    (descr http://www.keyelco.com/product-pdf.cfm?p=14028)
    (tags "Keystone type 1058 coin cell retainer")
    (attr smd)
    (fp_text reference BT1 (at 0 -7.62 180) (layer B.SilkS))
    (fp_text value CR2016x2 (at 0 9.398 180) (layer B.Fab))
    (pad 1 smd rect (at -14.465 0 180) (size 5.08 5.08) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(BT1-Pad1)"))
    (pad 3 smd rect (at 14.465 0 180) (size 5.08 5.08) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0 0 180) (size 5 5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5883B1A6)
    (at 121.1072 95.758 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 0.254 2.6924 180) (layer F.SilkS))
    (fp_text value TLV70033DDC (at 0 2.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 +BATT))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 +BATT))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module components:R_0603_0805 (layer F.Cu) (tedit 58ABAEA1)
    (at 122.5804 79.1464 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at -2.6416 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 1 0) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /LED_DBG))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module components:R_0603_0805 (layer F.Cu) (tedit 58ABAEA1)
    (at 113.03 81.8388)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0.0508 -1.524) (layer F.SilkS))
    (fp_text value 130R (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /TSC_IN))
    (pad 2 smd rect (at 1 0 180) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_DIN965_Pad locked (layer F.Cu) (tedit 58ABB9DA)
    (at 109 79)
    (descr "Mounting Hole 2.7mm, M2.5, DIN965")
    (tags "mounting hole 2.7mm m2.5 din965")
    (fp_text reference REF** (at 0 -3.35) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_DIN965_Pad (at 0 3.35) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.7 4.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_DIN965_Pad locked (layer F.Cu) (tedit 58ABB98F)
    (at 129 102)
    (descr "Mounting Hole 2.7mm, M2.5, DIN965")
    (tags "mounting hole 2.7mm m2.5 din965")
    (fp_text reference REF** (at 0 -3.35) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_DIN965_Pad (at 0 3.35) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.7 4.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_DIN965_Pad locked (layer F.Cu) (tedit 58ABB9E9)
    (at 129 79)
    (descr "Mounting Hole 2.7mm, M2.5, DIN965")
    (tags "mounting hole 2.7mm m2.5 din965")
    (fp_text reference REF** (at 0 -3.35) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_DIN965_Pad (at 0 3.35) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.7 4.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 122.5296 77.3684)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 2.6924 0.0508) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58B21BCE)
    (at 112.522 86.614 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L1 (at -0.9652 -1.0414 360) (layer F.SilkS))
    (fp_text value Bead (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 128.27 88.2396)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference W1 (at 0 -1.5748) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 18 /MCO))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5883B105)
    (at 124.8664 98.1804 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D1 (at -2.3528 0.9144 180) (layer F.SilkS))
    (fp_text value D_Schottky_x2_KCom_AAK (at 0 2.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(BT2-Pad1)"))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 +BATT))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module components:R_0603_0805 (layer F.Cu) (tedit 58ABAEA1)
    (at 108.1024 86.0552 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 2.286 -0.0508 360) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module components:R_0603_0805 (layer F.Cu) (tedit 58B215A8)
    (at 107.7468 95.9612 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 2.0828 0.0508 270) (layer F.SilkS))
    (fp_text value 80R6 (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(Q3-Pad3)"))
    (pad 2 smd rect (at 1 0) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 /LED_G_CONN))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module components:R_0603_0805 (layer F.Cu) (tedit 58B215AD)
    (at 107.7468 97.8408 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 2.032 0 270) (layer F.SilkS))
    (fp_text value 80R6 (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(Q2-Pad3)"))
    (pad 2 smd rect (at 1 0) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 /LED_B_CONN))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module components:R_0603_0805 (layer F.Cu) (tedit 58B215A3)
    (at 107.7595 94.0816 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 2.0955 0.1016 270) (layer F.SilkS))
    (fp_text value 130R (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at 1 0) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /LED_R_CONN))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module components:R_0603_0805 (layer F.Cu) (tedit 58ABAEA1)
    (at 105.8164 88.9508 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 2.286 -0.0508 360) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /THERM_SW))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /THERM_SENSE))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module components:R_0603_0805 (layer F.Cu) (tedit 58ABAEA1)
    (at 121.9708 102.4382 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 1.1684 1.3208 450) (layer F.SilkS))
    (fp_text value 1M (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /BATT_2))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module components:R_0603_0805 (layer F.Cu) (tedit 58ABAEA1)
    (at 123.8758 102.4382 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0.9906 -1.524 450) (layer F.SilkS))
    (fp_text value 1M (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 +BATT))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /BATT_2))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module components:C_0603_0805 (layer F.Cu) (tedit 58ABAE4C)
    (at 103.9368 88.9508 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C6 (at 2.2352 0 360) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.925 0 270) (size 1.15 1.1) (layers F.Cu F.Paste F.Mask)
      (net 10 /THERM_SENSE))
    (pad 2 smd rect (at 0.925 0 90) (size 1.15 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module components:C_0603_0805 (layer F.Cu) (tedit 58ABAE4C)
    (at 116.8908 78.9432 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C4 (at 1.2192 -1.7272 180) (layer F.SilkS))
    (fp_text value 0.47u (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.925 0 90) (size 1.15 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 /TSC_SAMPLING))
    (pad 2 smd rect (at 0.925 0 270) (size 1.15 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_DIN965_Pad locked (layer F.Cu) (tedit 58ABB997)
    (at 109 102)
    (descr "Mounting Hole 2.7mm, M2.5, DIN965")
    (tags "mounting hole 2.7mm m2.5 din965")
    (fp_text reference REF** (at 0 -3.35) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_DIN965_Pad (at 0 3.35) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.7 4.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5883B105)
    (at 110.744 92.5068 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -2.6416 -0.2032 180) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 /LED_R))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(Q1-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5883B105)
    (at 112.4044 99.0854 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -2.5052 0.9652 180) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 /LED_B))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(Q2-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5883B105)
    (at 111.395 95.7936 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at -2.6002 -0.066 180) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 /LED_G))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(Q3-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5883B1A6)
    (at 127.762 94.1832 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at 2.4892 0.254 360) (layer F.SilkS))
    (fp_text value NCV551SN50T1G (at 0 2.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(BT1-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C10-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S2B-PH-K_02x2.00mm_Angled (layer B.Cu) (tedit 58A42BED)
    (at 133.096 94.996 270)
    (descr "JST PH series connector, S2B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference BT2 (at 4.7752 0.3556 360) (layer B.SilkS))
    (fp_text value LiIon (at 1 -7.25 270) (layer B.Fab))
    (fp_text user %R (at 1 -2.5 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 20 "Net-(BT2-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Connectors_JST.3dshapes/JST_PH_S2B-PH-K_02x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S4B-PH-K_04x2.00mm_Angled (layer B.Cu) (tedit 58A42BED)
    (at 104.14 101.06 90)
    (descr "JST PH series connector, S4B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference P1 (at 7.4356 -1.7018 360) (layer B.SilkS))
    (fp_text value CONN_01X03 (at 3 -7.25 90) (layer B.Fab))
    (fp_text user %R (at 3 -2.5 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 28 /LED_B_CONN))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 27 /LED_G_CONN))
    (pad 3 thru_hole oval (at 4 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 26 /LED_R_CONN))
    (pad 4 thru_hole oval (at 6 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 +BATT))
    (model Connectors_JST.3dshapes/JST_PH_S4B-PH-K_04x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module components:LQFP-32_7x7mm_Pitch0.8mm_QFN-32-1EP_5x5mm_Pitch0.5mm-Combo locked (layer F.Cu) (tedit 58B10B72)
    (at 118.98 87.63)
    (descr "UH Package; 32-Lead Plastic QFN (5mm x 5mm); (see Linear Technology QFN_32_05-08-1693.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U2 (at -4.68 -4.0894) (layer F.SilkS))
    (fp_text value STM32L052KxTx (at 0 6) (layer F.Fab))
    (pad 1 smd rect (at -2.4 -1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at -2.4 -1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /THERM_SW))
    (pad 3 smd rect (at -2.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -2.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /RESET))
    (pad 5 smd rect (at -2.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (pad 6 smd rect (at -2.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /LED_R))
    (pad 7 smd rect (at -2.4 1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /LED_G))
    (pad 8 smd rect (at -2.4 1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /LED_B))
    (pad 9 smd rect (at -1.75 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /THERM_SENSE))
    (pad 10 smd rect (at -1.25 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U2-Pad10)"))
    (pad 11 smd rect (at -0.75 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at -0.25 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U2-Pad12)"))
    (pad 13 smd rect (at 0.25 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U2-Pad13)"))
    (pad 14 smd rect (at 0.75 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U2-Pad14)"))
    (pad 15 smd rect (at 1.25 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /BATT_2))
    (pad 16 smd rect (at 1.75 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at 2.4 1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 18 smd rect (at 2.4 1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /MCO))
    (pad 19 smd rect (at 2.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /UART_TX))
    (pad 20 smd rect (at 2.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 /UART_RX))
    (pad 21 smd rect (at 2.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U2-Pad21)"))
    (pad 22 smd rect (at 2.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U2-Pad22)"))
    (pad 23 smd rect (at 2.4 -1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 /SWDIO))
    (pad 24 smd rect (at 2.4 -1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 /SWCLK))
    (pad 25 smd rect (at 1.75 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 /LED_DBG))
    (pad 26 smd rect (at 1.25 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U2-Pad26)"))
    (pad 27 smd rect (at 0.75 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U2-Pad27)"))
    (pad 28 smd rect (at 0.25 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U2-Pad28)"))
    (pad 29 smd rect (at -0.25 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 /TSC_SAMPLING))
    (pad 30 smd rect (at -0.75 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad2)"))
    (pad 31 smd rect (at -1.25 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R4-Pad1)"))
    (pad 32 smd rect (at -1.75 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 33 smd rect (at 0.8625 0.8625) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at 0.8625 -0.8625) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 0.8625) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 -0.8625) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 1 smd rect (at -4.25 -2.8) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at -4.25 -2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /THERM_SW))
    (pad 3 smd rect (at -4.25 -1.2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -4.25 -0.4) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /RESET))
    (pad 5 smd rect (at -4.25 0.4) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (pad 6 smd rect (at -4.25 1.2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /LED_R))
    (pad 7 smd rect (at -4.25 2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /LED_G))
    (pad 8 smd rect (at -4.25 2.8) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /LED_B))
    (pad 9 smd rect (at -2.8 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /THERM_SENSE))
    (pad 10 smd rect (at -2 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U2-Pad10)"))
    (pad 11 smd rect (at -1.2 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at -0.4 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U2-Pad12)"))
    (pad 13 smd rect (at 0.4 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U2-Pad13)"))
    (pad 14 smd rect (at 1.2 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U2-Pad14)"))
    (pad 15 smd rect (at 2 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /BATT_2))
    (pad 16 smd rect (at 2.8 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at 4.25 2.8) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 18 smd rect (at 4.25 2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /MCO))
    (pad 19 smd rect (at 4.25 1.2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /UART_TX))
    (pad 20 smd rect (at 4.25 0.4) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 /UART_RX))
    (pad 21 smd rect (at 4.25 -0.4) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U2-Pad21)"))
    (pad 22 smd rect (at 4.25 -1.2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U2-Pad22)"))
    (pad 23 smd rect (at 4.25 -2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /SWDIO))
    (pad 24 smd rect (at 4.25 -2.8) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /SWCLK))
    (pad 25 smd rect (at 2.8 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /LED_DBG))
    (pad 26 smd rect (at 2 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U2-Pad26)"))
    (pad 27 smd rect (at 1.2 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U2-Pad27)"))
    (pad 28 smd rect (at 0.4 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U2-Pad28)"))
    (pad 29 smd rect (at -0.4 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /TSC_SAMPLING))
    (pad 30 smd rect (at -1.2 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad2)"))
    (pad 31 smd rect (at -2 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R4-Pad1)"))
    (pad 32 smd rect (at -2.8 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Housings_QFP.3dshapes/LQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 124.3584 92.0496)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -0.0508 1.2192) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 116.6368 95.1484 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -0.508 1.4478 360) (layer F.SilkS))
    (fp_text value 1u (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 111.6972 88.5952 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at -0.0882 -1.1938 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 115.7224 101.4984 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C11 (at 2.6924 0.1016 360) (layer F.SilkS))
    (fp_text value 10u (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 111.8228 84.6328 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 0.0628 1.1684 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 121.6914 99.06)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.0574 -0.508 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 +BATT))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 118.4148 95.2246 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -1.7526 -0.0254 360) (layer F.SilkS))
    (fp_text value 1u (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 127.9144 90.932 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 0.7112 1.2192 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 130.1496 94.5388 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 0.0254 1.2192 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S4B-PH-K_04x2.00mm_Angled (layer B.Cu) (tedit 58A42BED)
    (at 104.14 84.55 90)
    (descr "JST PH series connector, S4B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference P2 (at 7.4356 -1.5494 180) (layer B.SilkS))
    (fp_text value CONN_01X02 (at 3 -7.25 90) (layer B.Fab))
    (fp_text user %R (at 3 -2.5 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 /THERM_SENSE))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 /THERM_SW))
    (pad 3 thru_hole oval (at 4 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 6 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 /TSC_IN))
    (model Connectors_JST.3dshapes/JST_PH_S4B-PH-K_04x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58B21A09)
    (at 111.0488 86.5632 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -0.0508 -1.1176 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 /RESET))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58B34EDD)
    (at 133.0706 90.1192)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C2 (at 0 -2.0828) (layer F.SilkS))
    (fp_text value 100u (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.25) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58B34EC7)
    (at 118.6688 101.473 270)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C14 (at 0.1016 -0.1524 360) (layer F.SilkS))
    (fp_text value 100u (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +BATT))
    (pad 2 smd rect (at 1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text +3V3 (at 113.2332 101.8286) (layer B.SilkS))
  (gr_text +3V3 (at 113.0554 101.7778) (layer F.SilkS))
  (gr_text GND (at 134.6708 101.727) (layer F.SilkS))
  (gr_text "+BATT\nLED_R\nLED_G\nLED_B" (at 105.918 97.3328) (layer B.SilkS))
  (gr_text "TOUCH\nGND\nTH_SW\nTH_SNS" (at 105.664 83.058) (layer B.SilkS))
  (gr_text "CLK\nDIO\nRST\nGND" (at 132.6388 79.5528) (layer B.SilkS))
  (gr_text RX (at 129.9464 82.9056) (layer B.SilkS))
  (gr_text TX (at 129.9464 85.2424) (layer B.SilkS))
  (gr_text +BATT (at 130.7592 95.1992) (layer B.SilkS))
  (gr_text GND (at 130.7592 97.0788) (layer B.SilkS))
  (gr_text GND (at 134.6962 101.727) (layer B.SilkS))
  (gr_text "Faucet LED v2.0\nNick Graumann" (at 119.126 79.248) (layer B.SilkS))
  (gr_line (start 136.144 76.2) (end 101.6 76.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.144 104.648) (end 136.144 76.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.6 104.648) (end 136.144 104.648) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.6 76.2) (end 101.6 104.648) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.0752 85.9028) (xy 117.0305 85.9028) (xy 117.012737 84.390132) (xy 101.6 84.3915) (xy 101.6 104.660068)
        (xy 136.144 104.660068) (xy 136.144 76.212068) (xy 119.0752 76.2)
      )
    )
  )
)
