<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.1">
<drawing>
<board>
<plain>
<hole x="54" y="50" drill="3.4"/>
<hole x="71" y="45" drill="3.4"/>
<wire x1="50.25" y1="34" x2="70" y2="34" width="0.3048" layer="20"/>
<wire x1="70" y1="34" x2="70" y2="40" width="0.3048" layer="20"/>
<wire x1="50.25" y1="34" x2="50.25" y2="54.5" width="0.3048" layer="20"/>
<wire x1="50.25" y1="54.5" x2="74" y2="54.5" width="0.3048" layer="20"/>
<wire x1="74" y1="54.5" x2="74" y2="43" width="0.3048" layer="20"/>
<wire x1="74" y1="43" x2="71" y2="40" width="0.3048" layer="20"/>
<wire x1="71" y1="40" x2="70" y2="40" width="0.3048" layer="20"/>
<text>GND</text>
<text>Vin</text>
<text>Vout</text>
</plain>
<libraries>
<library name="ODboardbak">
<packages>
<package name="1206">
</package>
<package name="1206POL">
</package>
<package name="CONN_06">
<description>Single-row, 6-pin Pin Header (Male) Straight, 2.54 mm (0.10 in) col pitch, 5.84 mm mating length, 15.00 X 2.50 X 8.38 mm body
&lt;p&gt;Single-row (1X6), 6-pin Pin Header (Male) Straight package with 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 5.84 mm mating length with overall size 15.00 X 2.50 X 8.38 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
<package name="SM-42TX105">
</package>
<package name="FD11A">
</package>
<package name="OPA380">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C4" library="ODboardbak" package="1206" value="5/12pF">
<attribute name="VALUE"/>
</element>
<element name="C5" library="ODboardbak" package="1206" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="C6" library="ODboardbak" package="1206" value="1uF">
<attribute name="VALUE"/>
</element>
<element name="C7" library="ODboardbak" package="1206POL" value="10uF">
<attribute name="VALUE"/>
</element>
<element name="J1" library="ODboardbak" package="CONN_06" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="ODboardbak" package="SM-42TX105" value="SM-42TX105"/>
<element name="U$2" library="ODboardbak" package="FD11A" value="FD11A"/>
<element name="U1" library="ODboardbak" package="OPA380" value="OPA380"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U1" pad="P$2"/>
<contactref element="U$1" pad="A"/>
<contactref element="C4" pad="P$2"/>
<contactref element="U$2" pad="P$2"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="P$4"/>
<contactref element="U1" pad="P$3"/>
<contactref element="C7" pad="-"/>
<contactref element="C5" pad="P$2"/>
<contactref element="C6" pad="P$2"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="VOUT">
<contactref element="U1" pad="P$6"/>
<contactref element="U$1" pad="WIPER"/>
<contactref element="C4" pad="P$3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="V+">
<contactref element="U1" pad="P$7"/>
<contactref element="C5" pad="P$3"/>
<contactref element="C6" pad="P$3"/>
<contactref element="C7" pad="+"/>
<contactref element="J1" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
