(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 191)
    (no_connects 1)
    (area 74.208857 54.8166 272.041714 194.39)
    (thickness 1.6)
    (drawings 43)
    (tracks 584)
    (zones 0)
    (modules 125)
    (nets 104)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.1778)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 2)
    (pad_drill 0)
    (pad_to_mask_clearance 0.1)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(BT1-Pad1)")
  (net 2 /VBat)
  (net 3 GND)
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C6-Pad1)")
  (net 8 /PV_ADC)
  (net 9 "Net-(C9-Pad1)")
  (net 10 "Net-(C10-Pad1)")
  (net 11 "Net-(C11-Pad1)")
  (net 12 "Net-(C12-Pad1)")
  (net 13 "Net-(C12-Pad2)")
  (net 14 /Epaper_adapter_sheet/VGH)
  (net 15 +3V3)
  (net 16 /Epaper_adapter_sheet/PRVGL)
  (net 17 /Epaper_adapter_sheet/VGL)
  (net 18 /Epaper_adapter_sheet/VDD)
  (net 19 /Epaper_adapter_sheet/VSH)
  (net 20 /Epaper_adapter_sheet/VGH2)
  (net 21 /Epaper_adapter_sheet/VSL)
  (net 22 /Epaper_adapter_sheet/VCOM)
  (net 23 "Net-(D1-Pad2)")
  (net 24 "Net-(J3-Pad1)")
  (net 25 "Net-(J4-Pad1)")
  (net 26 "Net-(J5-Pad2)")
  (net 27 "Net-(J6-Pad2)")
  (net 28 "Net-(J7-Pad2)")
  (net 29 "Net-(J8-Pad2)")
  (net 30 "Net-(J9-Pad1)")
  (net 31 "Net-(J11-Pad1)")
  (net 32 /PROG1)
  (net 33 "Net-(J12-Pad2)")
  (net 34 "Net-(J13-Pad1)")
  (net 35 /PROG3)
  (net 36 "Net-(J15-Pad1)")
  (net 37 /SCL)
  (net 38 /MOSI)
  (net 39 "Net-(J17-Pad2)")
  (net 40 /SDA)
  (net 41 /Epaper_adapter_sheet/GDR)
  (net 42 /Epaper_adapter_sheet/RESE)
  (net 43 /Epaper_adapter_sheet/BUSY)
  (net 44 /Epaper_adapter_sheet/RESET)
  (net 45 /Epaper_adapter_sheet/D/C)
  (net 46 /Epaper_adapter_sheet/CS)
  (net 47 /Epaper_adapter_sheet/SCK)
  (net 48 /Epaper_adapter_sheet/VPP)
  (net 49 /PWRGD)
  (net 50 "Net-(R2-Pad2)")
  (net 51 "Net-(SC1-Pad2)")
  (net 52 "Net-(SC2-Pad2)")
  (net 53 "Net-(SC3-Pad2)")
  (net 54 "Net-(SC5-Pad2)")
  (net 55 "Net-(TH1-Pad1)")
  (net 56 /PGOOD)
  (net 57 /STATUS2)
  (net 58 /LBO)
  (net 59 /~SHDN)
  (net 60 "Net-(TP11-Pad1)")
  (net 61 "Net-(TP12-Pad1)")
  (net 62 "Net-(J16-Pad1)")
  (net 63 "Net-(J18-Pad1)")
  (net 64 "Net-(C8-Pad2)")
  (net 65 "Net-(J19-Pad1)")
  (net 66 "Net-(J19-Pad2)")
  (net 67 "Net-(J19-Pad3)")
  (net 68 "Net-(J19-Pad4)")
  (net 69 "Net-(J19-Pad5)")
  (net 70 "Net-(J19-Pad6)")
  (net 71 /Epaper_adapter_sheet/TSCL)
  (net 72 /Epaper_adapter_sheet/TSDA)
  (net 73 "Net-(J19-Pad30)")
  (net 74 "Net-(J19-Pad31)")
  (net 75 "Net-(J19-Pad32)")
  (net 76 "Net-(J19-Pad33)")
  (net 77 "Net-(J19-Pad34)")
  (net 78 "Net-(TP7-Pad1)")
  (net 79 "Net-(TP8-Pad1)")
  (net 80 "Net-(TP34-Pad1)")
  (net 81 "Net-(TP35-Pad1)")
  (net 82 "Net-(TP36-Pad1)")
  (net 83 "Net-(Q2-Pad1)")
  (net 84 "Net-(TP38-Pad1)")
  (net 85 "Net-(TP39-Pad1)")
  (net 86 "Net-(TP40-Pad1)")
  (net 87 "Net-(TP41-Pad1)")
  (net 88 "Net-(TP42-Pad1)")
  (net 89 "Net-(TP43-Pad1)")
  (net 90 "Net-(TP44-Pad1)")
  (net 91 "Net-(TP45-Pad1)")
  (net 92 "Net-(TP46-Pad1)")
  (net 93 "Net-(U2-Pad1)")
  (net 94 "Net-(U2-Pad5)")
  (net 95 "Net-(U2-Pad8)")
  (net 96 "Net-(U2-Pad10)")
  (net 97 "Net-(U2-Pad12)")
  (net 98 "Net-(U4-Pad5)")
  (net 99 "Net-(U4-Pad6)")
  (net 100 "Net-(U4-Pad7)")
  (net 101 "Net-(U5-PadVin)")
  (net 102 "Net-(U5-PadAGND)")
  (net 103 VCC)
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.254)
    (add_net /Epaper_adapter_sheet/BUSY)
    (add_net /Epaper_adapter_sheet/CS)
    (add_net /Epaper_adapter_sheet/D/C)
    (add_net /Epaper_adapter_sheet/GDR)
    (add_net /Epaper_adapter_sheet/PRVGL)
    (add_net /Epaper_adapter_sheet/RESE)
    (add_net /Epaper_adapter_sheet/RESET)
    (add_net /Epaper_adapter_sheet/SCK)
    (add_net /Epaper_adapter_sheet/TSCL)
    (add_net /Epaper_adapter_sheet/TSDA)
    (add_net /Epaper_adapter_sheet/VCOM)
    (add_net /Epaper_adapter_sheet/VDD)
    (add_net /Epaper_adapter_sheet/VGH)
    (add_net /Epaper_adapter_sheet/VGH2)
    (add_net /Epaper_adapter_sheet/VGL)
    (add_net /Epaper_adapter_sheet/VPP)
    (add_net /Epaper_adapter_sheet/VSH)
    (add_net /Epaper_adapter_sheet/VSL)
    (add_net /LBO)
    (add_net /MOSI)
    (add_net /PGOOD)
    (add_net /PROG1)
    (add_net /PROG3)
    (add_net /PV_ADC)
    (add_net /PWRGD)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /STATUS2)
    (add_net /~SHDN)
    (add_net GND)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J12-Pad2)")
    (add_net "Net-(J13-Pad1)")
    (add_net "Net-(J15-Pad1)")
    (add_net "Net-(J16-Pad1)")
    (add_net "Net-(J17-Pad2)")
    (add_net "Net-(J18-Pad1)")
    (add_net "Net-(J19-Pad1)")
    (add_net "Net-(J19-Pad2)")
    (add_net "Net-(J19-Pad3)")
    (add_net "Net-(J19-Pad30)")
    (add_net "Net-(J19-Pad31)")
    (add_net "Net-(J19-Pad32)")
    (add_net "Net-(J19-Pad33)")
    (add_net "Net-(J19-Pad34)")
    (add_net "Net-(J19-Pad4)")
    (add_net "Net-(J19-Pad5)")
    (add_net "Net-(J19-Pad6)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J8-Pad2)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(TH1-Pad1)")
    (add_net "Net-(TP11-Pad1)")
    (add_net "Net-(TP12-Pad1)")
    (add_net "Net-(TP34-Pad1)")
    (add_net "Net-(TP35-Pad1)")
    (add_net "Net-(TP36-Pad1)")
    (add_net "Net-(TP38-Pad1)")
    (add_net "Net-(TP39-Pad1)")
    (add_net "Net-(TP40-Pad1)")
    (add_net "Net-(TP41-Pad1)")
    (add_net "Net-(TP42-Pad1)")
    (add_net "Net-(TP43-Pad1)")
    (add_net "Net-(TP44-Pad1)")
    (add_net "Net-(TP45-Pad1)")
    (add_net "Net-(TP46-Pad1)")
    (add_net "Net-(TP7-Pad1)")
    (add_net "Net-(TP8-Pad1)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U4-Pad6)")
    (add_net "Net-(U4-Pad7)")
    (add_net "Net-(U5-PadAGND)")
    (add_net "Net-(U5-PadVin)")
  )
  (net_class PWR ""
    (clearance 0.1778)
    (trace_width 0.508)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.254)
    (add_net +3V3)
    (add_net /VBat)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(SC1-Pad2)")
    (add_net "Net-(SC2-Pad2)")
    (add_net "Net-(SC3-Pad2)")
    (add_net "Net-(SC5-Pad2)")
    (add_net VCC)
  )
  (module CustomFootprints:MSOP-12_3x4mm_Pitch0.65mm_Handsolder (layer F.Cu) (tedit 5A317D2D)
    (at 144.018 74.93)
    (descr "MS Package; 12-Lead Plastic MSOP; (see Linear Technology 05081668_A_MS12.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at -2.032 -3.05) (layer F.SilkS))
    (fp_text value LT3011 (at -3.6576 1.3208 90) (layer F.SilkS))
    (pad 1 smd rect (at -2.232 -1.625) (size 1.652 0.42) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(U2-Pad1)"))
    (pad 2 smd rect (at -2.232 -0.975) (size 1.652 0.42) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at -2.232 -0.325) (size 1.652 0.42) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R2-Pad2)"))
    (pad 4 smd rect (at -2.232 0.325) (size 1.652 0.42) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 5 smd rect (at -2.232 0.975) (size 1.652 0.42) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(U2-Pad5)"))
    (pad 6 smd rect (at -2.232 1.625) (size 1.652 0.42) (layers F.Cu F.Paste F.Mask)
      (net 49 /PWRGD))
    (pad 7 smd rect (at 2.232 1.625) (size 1.652 0.42) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 8 smd rect (at 2.232 0.975) (size 1.652 0.42) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(U2-Pad8)"))
    (pad 9 smd rect (at 2.232 0.325) (size 1.652 0.42) (layers F.Cu F.Paste F.Mask)
      (net 59 /~SHDN))
    (pad 10 smd rect (at 2.232 -0.325) (size 1.652 0.42) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(U2-Pad10)"))
    (pad 11 smd rect (at 2.232 -0.975) (size 1.652 0.42) (layers F.Cu F.Paste F.Mask)
      (net 2 /VBat))
    (pad 12 smd rect (at 2.232 -1.625) (size 1.652 0.42) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(U2-Pad12)"))
    (model Housings_SSOP.3dshapes/MSOP-12_3x4mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A1F250C)
    (at 201.803 126.2126)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer Cmts.User) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A1F250C)
    (at 147.2692 125.9078)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer Cmts.User) hide)
    (pad 1 np_thru_hole circle (at 0.1016 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A1F250C)
    (at 83.7438 126.0348)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer Cmts.User) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A1F250C)
    (at 201.7522 59.9694)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer Cmts.User) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A1F250C)
    (at 147.3454 59.9694)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer Cmts.User) hide)
    (pad 1 np_thru_hole circle (at 0.0254 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5A273EA4)
    (at 137.0076 81.1022 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 2.4892 1.778 270) (layer F.SilkS))
    (fp_text value 1uF (at -1.651 1.778 270) (layer F.SilkS))
    (fp_text user %R (at 2.5146 1.7526 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /VBat))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5A273DE9)
    (at 147.6502 70.4342)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at -2.3876 -1.778) (layer F.SilkS))
    (fp_text value 4.7uF (at 1.397 -1.7526) (layer F.SilkS))
    (fp_text user %R (at -2.3622 -1.8034) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5A273F03)
    (at 115.0874 62.4078 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C3 (at -2.6162 2.413 360) (layer F.SilkS))
    (fp_text value 100uF (at -2.6162 -2.7432 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5A273ED4)
    (at 130.81 72.4728 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C4 (at 2.9906 -3.6068 270) (layer F.SilkS))
    (fp_text value 10uF (at -0.7178 -3.6322 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5A273DD9)
    (at 149.6822 78.5876 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at -4.0132 0.0508 360) (layer F.SilkS))
    (fp_text value 1nF (at -2.159 1.8542 270) (layer F.SilkS))
    (fp_text user %R (at -4.0132 0.1016 360) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5A273DF3)
    (at 149.1742 94.4626 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at 1.7526 1.8034 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -2.4384 1.8034 270) (layer F.SilkS))
    (fp_text user %R (at 1.7526 1.8034 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5A273D76)
    (at 142.8496 93.1672 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C7 (at 3.048 3.6068 270) (layer F.SilkS))
    (fp_text value 10uF (at -0.8128 3.6576 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5A273F5B)
    (at 117.8814 87.5538 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C8 (at 2.4384 -1.8796 180) (layer F.SilkS))
    (fp_text value 10nF (at -1.8288 -1.8288 180) (layer F.SilkS))
    (fp_text user %R (at 2.4638 -1.8796 180) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /PV_ADC))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C8-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5A273CF7)
    (at 156.9466 87.6554)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C9 (at -2.1844 -1.905) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.2606 -1.9304) (layer F.SilkS))
    (fp_text user %R (at -2.159 -1.8542) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5A273EB9)
    (at 148.971 100.6348 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C10 (at 2.5654 1.778 180) (layer F.SilkS))
    (fp_text value 0.1uF (at -2.1336 1.778 180) (layer F.SilkS))
    (fp_text user %R (at 2.54 1.778 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5A273EC7)
    (at 162.3822 106.7054 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C11 (at 3.1496 1.7526 450) (layer F.SilkS))
    (fp_text value 0.22uF (at -2.0574 1.8288 270) (layer F.SilkS))
    (fp_text user %R (at 3.1242 1.7272 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 5A274007)
    (at 186.055 108.6866)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C12 (at 2.2606 -1.9304) (layer B.SilkS))
    (fp_text value 2.2uF (at -2.2352 -2) (layer B.SilkS))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C12-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 5A274392)
    (at 183.007 114.2746 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C13 (at 1.4986 1.8796 90) (layer B.SilkS))
    (fp_text value 1uF (at -2.1082 1.8288 90) (layer B.SilkS))
    (fp_text user %R (at 1.524 1.905 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 14 /Epaper_adapter_sheet/VGH))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 5A274001)
    (at 180.086 99.7204 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C14 (at 0.0254 1.9304 90) (layer B.SilkS))
    (fp_text value 1uF (at 0 -2 90) (layer B.SilkS))
    (fp_text user %R (at 0 1.9304 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 5A274396)
    (at 187.5028 114.3254 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C15 (at 1.905 1.9304 90) (layer B.SilkS))
    (fp_text value 1uF (at -1.9304 1.8796 90) (layer B.SilkS))
    (fp_text user %R (at 1.905 1.9304 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 16 /Epaper_adapter_sheet/PRVGL))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58AA84D1)
    (at 173.5074 126.1872 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C16 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 1uF (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 17 /Epaper_adapter_sheet/VGL))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58AA84D1)
    (at 176.662533 126.1872 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C17 (at -4.1656 0.081733 360) (layer B.SilkS))
    (fp_text value 1uF (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 18 /Epaper_adapter_sheet/VDD))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58AA84D1)
    (at 180.246866 126.1872 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C18 (at -4.064 0.059266 360) (layer B.SilkS))
    (fp_text value 1uF (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 19 /Epaper_adapter_sheet/VSH))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58AA84D1)
    (at 183.616599 126.1872 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C19 (at -4.1656 0.025399 360) (layer B.SilkS))
    (fp_text value 1uF (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 20 /Epaper_adapter_sheet/VGH2))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58AA84D1)
    (at 187.10148 126.1856 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C20 (at -4.1132 -0.04572 360) (layer B.SilkS))
    (fp_text value 1uF (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 21 /Epaper_adapter_sheet/VSL))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58AA84D1)
    (at 190.2714 126.1856 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C21 (at 0.027 -1.8034 270) (layer B.SilkS))
    (fp_text value 1uF (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 22 /Epaper_adapter_sheet/VCOM))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 5A1D9C41)
    (at 105.1868 59.1312 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value Schottky (at 0.1 1.9 180) (layer Cmts.User) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D1-Pad2)"))
    (model Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 5A1D9C4D)
    (at 108.3564 63.2968 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value 6.5V (at 0.1 1.9 270) (layer Cmts.User) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 5A273F18)
    (at 103.9368 64.77 90)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference "J1: VCC" (at 1.016 -2.0574 90) (layer F.SilkS))
    (fp_text value TEST_2P (at 1.27 2 90) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 103 VCC))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 23 "Net-(D1-Pad2)"))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 5A1DB8FE)
    (at 146.6342 66.548)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference J2 (at 1.27 -2) (layer F.SilkS))
    (fp_text value TEST_2P (at 1.27 2) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 +3V3))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 5A1D9C59)
    (at 136.779 71.7804)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference J3 (at 1.2446 1.9812) (layer F.SilkS))
    (fp_text value TEST_2P (at 1.27 2) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 /VBat))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 5A1D9C55)
    (at 128.27 68.834)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference J4 (at -2.255 0.175) (layer F.SilkS))
    (fp_text value TEST_2P (at 1.27 2) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 25 "Net-(J4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 5A1D9C1E)
    (at 110.7694 68.4276)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference J5 (at -2.286 -0.0508) (layer F.SilkS))
    (fp_text value TEST_2P (at 1.27 2) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 26 "Net-(J5-Pad2)"))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 5A1D9C1A)
    (at 110.744 71.0438)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference J6 (at -2.2606 0) (layer F.SilkS))
    (fp_text value TEST_2P (at 1.27 2) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 "Net-(J6-Pad2)"))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 5A1D9C15)
    (at 110.7186 73.6092)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference J7 (at -2.2352 0.0254) (layer F.SilkS))
    (fp_text value TEST_2P (at 1.27 2) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 28 "Net-(J7-Pad2)"))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 5A1D9C10)
    (at 110.7948 76.073)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference J8 (at -2.3114 0.0254) (layer F.SilkS))
    (fp_text value TEST_2P (at 1.27 2) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 29 "Net-(J8-Pad2)"))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 5A27202F)
    (at 107.569 97.0534 270)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference J9 (at 4.9022 -0.0762 270) (layer F.SilkS))
    (fp_text value TEST_2P (at 1.27 2 270) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 30 "Net-(J9-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 5A1DC300)
    (at 140.3604 88.9254)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference J10 (at 1.016 -1.778) (layer F.SilkS))
    (fp_text value TEST_2P (at 1.27 2) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad1)"))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 5A1D9D45)
    (at 132.08 83.058 180)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference J11 (at 5.207 0.0762 180) (layer F.SilkS))
    (fp_text value TEST_2P (at 1.27 2 180) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 31 "Net-(J11-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 32 /PROG1))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 5A1DC303)
    (at 110.0836 80.9244)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference J12 (at -2.7686 0) (layer F.SilkS))
    (fp_text value TEST_2P (at 1.27 2) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 103 VCC))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 "Net-(J12-Pad2)"))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 5A1D9D49)
    (at 132.08 86.36 180)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference J13 (at 5.1562 0.127 180) (layer F.SilkS))
    (fp_text value TEST_2P (at 1.27 2 180) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 34 "Net-(J13-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 35 /PROG3))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 5A1DC310)
    (at 158.8262 100.584)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference J14 (at -2.921 0.0762) (layer F.SilkS))
    (fp_text value TEST_2P (at 1.27 2) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "Net-(C11-Pad1)"))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 5A273E22)
    (at 135.382 99.314)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference 3V3 (at 5.2832 -0.0254) (layer F.SilkS))
    (fp_text value TEST_2P (at 1.27 2) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 36 "Net-(J15-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 +3V3))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 5A1DB7CA)
    (at 135.382 112.014)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference J16 (at -1.6002 -2.2098 90) (layer F.SilkS))
    (fp_text value TEST_2P (at 1.27 2) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 62 "Net-(J16-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 37 /SCL))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 5A1DBC5B)
    (at 110.0836 114.48415)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference J17 (at -2.794 2.60985 90) (layer F.SilkS))
    (fp_text value TEST_2P (at 1.27 2) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 38 /MOSI))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 39 "Net-(J17-Pad2)"))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 5A1DB7CD)
    (at 135.382 114.554)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference J18 (at -1.4478 2.1336 90) (layer F.SilkS))
    (fp_text value TEST_2P (at 1.27 2) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 63 "Net-(J18-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 40 /SDA))
  )
  (module CustomFootprints:FPC_34 (layer F.Cu) (tedit 5A2740B8)
    (at 182.1434 119.8626)
    (fp_text reference J19 (at 0 1.95) (layer F.SilkS))
    (fp_text value Z5263CT-ND (at -0.0254 3.6068) (layer F.SilkS))
    (pad 1 smd rect (at -8.25 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(J19-Pad1)"))
    (pad 2 smd rect (at -7.75 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(J19-Pad2)"))
    (pad 3 smd rect (at -7.25 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(J19-Pad3)"))
    (pad 4 smd rect (at -6.75 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(J19-Pad4)"))
    (pad 5 smd rect (at -6.25 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(J19-Pad5)"))
    (pad 6 smd rect (at -5.75 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(J19-Pad6)"))
    (pad 7 smd rect (at -5.25 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 41 /Epaper_adapter_sheet/GDR))
    (pad 8 smd rect (at -4.75 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 42 /Epaper_adapter_sheet/RESE))
    (pad 9 smd rect (at -4.25 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /Epaper_adapter_sheet/VGL))
    (pad 10 smd rect (at -3.75 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /Epaper_adapter_sheet/VGH))
    (pad 11 smd rect (at -3.25 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 71 /Epaper_adapter_sheet/TSCL))
    (pad 12 smd rect (at -2.75 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 72 /Epaper_adapter_sheet/TSDA))
    (pad 13 smd rect (at -2.25 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 14 smd rect (at -1.75 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 43 /Epaper_adapter_sheet/BUSY))
    (pad 15 smd rect (at -1.25 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 44 /Epaper_adapter_sheet/RESET))
    (pad 16 smd rect (at -0.75 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 45 /Epaper_adapter_sheet/D/C))
    (pad 17 smd rect (at -0.25 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 46 /Epaper_adapter_sheet/CS))
    (pad 18 smd rect (at 0.25 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 47 /Epaper_adapter_sheet/SCK))
    (pad 19 smd rect (at 0.75 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 /MOSI))
    (pad 20 smd rect (at 1.25 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 21 smd rect (at 1.75 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 22 smd rect (at 2.25 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 23 smd rect (at 2.75 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /Epaper_adapter_sheet/VDD))
    (pad 24 smd rect (at 3.25 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 48 /Epaper_adapter_sheet/VPP))
    (pad 25 smd rect (at 3.75 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /Epaper_adapter_sheet/VSH))
    (pad 26 smd rect (at 4.25 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /Epaper_adapter_sheet/VGH2))
    (pad 27 smd rect (at 4.75 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /Epaper_adapter_sheet/VSL))
    (pad 28 smd rect (at 5.25 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /Epaper_adapter_sheet/PRVGL))
    (pad 29 smd rect (at 5.75 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /Epaper_adapter_sheet/VCOM))
    (pad 30 smd rect (at 6.25 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(J19-Pad30)"))
    (pad 31 smd rect (at 6.75 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(J19-Pad31)"))
    (pad 32 smd rect (at 7.25 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(J19-Pad32)"))
    (pad 33 smd rect (at 7.75 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(J19-Pad33)"))
    (pad 34 smd rect (at 8.25 0) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(J19-Pad34)"))
    (pad 0 smd rect (at -10.25 3.3) (size 3 2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 0 smd rect (at 10.25 3.3) (size 3 2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module Inductors_SMD:L_Coilcraft_XAL5030 (layer B.Cu) (tedit 58886050)
    (at 178.3842 107.8992 180)
    (descr L_Coilcraft_XAL5030)
    (tags "L Coilcraft XAL5030")
    (attr smd)
    (fp_text reference L1 (at 0 3.81 180) (layer B.SilkS))
    (fp_text value 47uH (at 0 -4.572 180) (layer B.Fab))
    (pad 1 smd rect (at -1.655 0 180) (size 1.2 4.7) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V3))
    (pad 2 smd rect (at 1.655 0 180) (size 1.2 4.7) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C12-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5883B105)
    (at 175.4726 114.4168)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 2.5) (layer B.SilkS))
    (fp_text value AO3418 (at 0 -2.5) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 41 /Epaper_adapter_sheet/GDR))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C12-Pad1)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 42 /Epaper_adapter_sheet/RESE))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A273DBD)
    (at 143.8402 80.5942)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -1.4732 -1.8542) (layer F.SilkS))
    (fp_text value 1M (at 1.2446 -1.905) (layer F.SilkS))
    (fp_text user %R (at -1.4986 -1.8796) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /VBat))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 49 /PWRGD))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A273C71)
    (at 154.1272 71.8312 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value "332k 1%" (at 0 1.9 270) (layer F.SilkS))
    (fp_text user %R (at 0 -1.85 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A273C74)
    (at 154.1272 79.5274 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value "200k 1%" (at 0 1.9 270) (layer F.SilkS))
    (fp_text user %R (at 0 -1.85 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A273DB1)
    (at 130.785819 79.9084)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at -2.261819 -1.85) (layer F.SilkS))
    (fp_text value 2k (at 1.497381 -1.8542) (layer F.SilkS))
    (fp_text user %R (at -2.261819 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J11-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A273E76)
    (at 143.51 114.554 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 2.286 -1.8288 180) (layer F.SilkS))
    (fp_text value 4.7k (at -2.2352 -1.905 180) (layer F.SilkS))
    (fp_text user %R (at 2.3114 -1.8034 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 40 /SDA))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A273E7D)
    (at 143.51 112.014 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 2.1336 1.905 180) (layer F.SilkS))
    (fp_text value 4.7k (at -1.9558 1.905 180) (layer F.SilkS))
    (fp_text user %R (at 2.1082 1.8796 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 37 /SCL))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A273F39)
    (at 117.8814 80.9752)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at -2.6416 -1.778) (layer F.SilkS))
    (fp_text value 10k (at 1.8288 -1.8034) (layer F.SilkS))
    (fp_text user %R (at -2.7178 -1.778) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J12-Pad2)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 /PV_ADC))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A273D8C)
    (at 130.785819 89.408 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 1.753819 -1.8796 180) (layer F.SilkS))
    (fp_text value 100k (at -2.132381 -1.8796 180) (layer F.SilkS))
    (fp_text user %R (at 1.753819 -1.8542 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J13-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A273F5F)
    (at 117.8814 84.582 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at -4.4196 1.3208 180) (layer F.SilkS))
    (fp_text value 10.3k (at -5.5372 -0.2032 180) (layer F.SilkS))
    (fp_text user %R (at -4.3942 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 /PV_ADC))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 5A274012)
    (at 170.7134 114.4524 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at 0 1.85 90) (layer B.SilkS))
    (fp_text value "2.2R 1%" (at 0 -1.9 90) (layer B.SilkS))
    (fp_text user %R (at 0 1.85 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 42 /Epaper_adapter_sheet/RESE))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CustomFootprints:MONO_SOLAR_CELL_22MMx7MM_KXOB22-04X3F (layer F.Cu) (tedit 5A1D9C74)
    (at 104.5384 74.7216 180)
    (fp_text reference SC1 (at 10.5076 8.6308 180) (layer F.SilkS))
    (fp_text value Solar_Cell (at 11.5 8.5 180) (layer Cmts.User) hide)
    (pad 1 smd rect (at 0.5 3.5 180) (size 3 7) (layers F.Cu F.Paste F.Mask)
      (net 103 VCC))
    (pad 2 smd rect (at 21.5 3.5 180) (size 3 7) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(SC1-Pad2)"))
  )
  (module CustomFootprints:MONO_SOLAR_CELL_22MMx7MM_KXOB22-04X3F (layer F.Cu) (tedit 5A1D9C78)
    (at 82.5384 76.29664)
    (fp_text reference SC2 (at 11.4924 -0.75704) (layer F.SilkS))
    (fp_text value Solar_Cell (at 11.5 8.5) (layer Cmts.User) hide)
    (pad 1 smd rect (at 0.5 3.5) (size 3 7) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(SC1-Pad2)"))
    (pad 2 smd rect (at 21.5 3.5) (size 3 7) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(SC2-Pad2)"))
  )
  (module CustomFootprints:MONO_SOLAR_CELL_22MMx7MM_KXOB22-04X3F (layer F.Cu) (tedit 5A1D9C7B)
    (at 104.5384 91.9682 180)
    (fp_text reference SC3 (at 10.5076 7.7418 180) (layer F.SilkS))
    (fp_text value Solar_Cell (at 11.5 8.5 180) (layer Cmts.User) hide)
    (pad 1 smd rect (at 0.5 3.5 180) (size 3 7) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(SC2-Pad2)"))
    (pad 2 smd rect (at 21.5 3.5 180) (size 3 7) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(SC3-Pad2)"))
  )
  (module CustomFootprints:MONO_SOLAR_CELL_22MMx7MM_KXOB22-04X3F (layer F.Cu) (tedit 5A1D9C88)
    (at 82.5384 93.64992)
    (fp_text reference SC4 (at 11.4924 -0.86372) (layer F.SilkS))
    (fp_text value Solar_Cell (at 11.5 8.5) (layer Cmts.User) hide)
    (pad 1 smd rect (at 0.5 3.5) (size 3 7) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(SC3-Pad2)"))
    (pad 2 smd rect (at 21.5 3.5) (size 3 7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J9-Pad1)"))
  )
  (module CustomFootprints:MONO_SOLAR_CELL_22MMx7MM_KXOB22-04X3F (layer F.Cu) (tedit 5A1D9C8B)
    (at 104.5384 109.2402 180)
    (fp_text reference SC5 (at 10.5076 -0.7672 180) (layer F.SilkS))
    (fp_text value Solar_Cell (at 11.5 8.5 180) (layer Cmts.User) hide)
    (pad 1 smd rect (at 0.5 3.5 180) (size 3 7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J9-Pad1)"))
    (pad 2 smd rect (at 21.5 3.5 180) (size 3 7) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(SC5-Pad2)"))
  )
  (module CustomFootprints:MONO_SOLAR_CELL_22MMx7MM_KXOB22-04X3F (layer F.Cu) (tedit 5A1D9C8F)
    (at 82.5384 111.0032)
    (fp_text reference SC6 (at 11.4924 8.5038) (layer F.SilkS))
    (fp_text value Solar_Cell (at 11.5 8.5) (layer Cmts.User) hide)
    (pad 1 smd rect (at 0.5 3.5) (size 3 7) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(SC5-Pad2)"))
    (pad 2 smd rect (at 21.5 3.5) (size 3 7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5A1D9C63)
    (at 128.27 66.294)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference TH1 (at 1.27 -1.86) (layer F.SilkS))
    (fp_text value "Thermistor_NTC 10k" (at 1.27 1.86) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 55 "Net-(TH1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module CustomFootprints:LGA-8_3x5mm_Pitch1.25mm_handsolder (layer F.Cu) (tedit 5A273D12)
    (at 156.769 93.883)
    (descr LGA-8-handsolder)
    (tags "lga land grid array")
    (attr smd)
    (fp_text reference U3 (at 0 -3.65) (layer F.SilkS))
    (fp_text value MPL3115A2 (at 0 3.65) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -1.575 1.875) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 1 smd rect (at -1.575 -1.875) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at -1.575 -0.625) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (pad 3 smd rect (at -1.575 0.625) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 8 smd rect (at 1.5875 -1.8669) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 /SCL))
    (pad 7 smd rect (at 1.575 -0.625) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 /SDA))
    (pad 6 smd rect (at 1.575 0.625) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(TP11-Pad1)"))
    (pad 5 smd rect (at 1.575 1.875) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(TP12-Pad1)"))
    (model ${KISYS3DMOD}/Housings_LGA.3dshapes/LGA-8_3x5mm_Pitch1.25mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer B.Cu) (tedit 58645DC7)
    (at 179.2986 114.5032 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at 1.4478 2.0066 90) (layer B.SilkS))
    (fp_text value MBR0530 (at 0 -2.1 90) (layer B.Fab))
    (fp_text user %R (at 0 2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 14 /Epaper_adapter_sheet/VGH))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer B.Cu) (tedit 58645DC7)
    (at 192.6844 114.681 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D4 (at 0.0762 -2.159 270) (layer B.SilkS))
    (fp_text value MBR0530 (at 0 -2.1 270) (layer B.Fab))
    (fp_text user %R (at 0 2 270) (layer B.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C12-Pad2)"))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 16 /Epaper_adapter_sheet/PRVGL))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer B.Cu) (tedit 58645DC7)
    (at 192.6844 107.823 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D5 (at -0.1524 -2.2098 270) (layer B.SilkS))
    (fp_text value MBR0530 (at 0 -2.1 270) (layer B.Fab))
    (fp_text user %R (at 0 2 270) (layer B.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S2B-PH-SM4-TB_02x2.00mm_Angled (layer F.Cu) (tedit 5A1DBBDA)
    (at 136.7818 62.9618 180)
    (descr "JST PH series connector, S2B-PH-SM4-TB, side entry type, surface mount, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (attr smd)
    (fp_text reference BT1 (at 0 -5.625 180) (layer Cmts.User) hide)
    (fp_text value Battery_Cell (at 0 5.375 180) (layer F.Fab))
    (fp_text user %R (at 0 1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -2.875 180) (size 1 3.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at 1 -2.875 180) (size 1 3.5) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad "" smd rect (at -3.35 2.875 180) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.35 2.875 180) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S2B-PH-SM4-TB_02x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CustomFootprints:Teensy_Header_Straight_2x14_Pitch2.54mm (layer F.Cu) (tedit 5A273F81)
    (at 116.078 94.234)
    (descr "Through hole straight pin header, 2x14, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x14 2.54mm double row")
    (fp_text reference U5 (at 0 -2.54) (layer F.SilkS))
    (fp_text value Teensy3.2 (at 5.5626 -2.5654) (layer F.SilkS))
    (pad GND thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad Vin thru_hole oval (at 15.24 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 "Net-(U5-PadVin)"))
    (pad 0 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(TP38-Pad1)"))
    (pad AGND thru_hole oval (at 15.24 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 "Net-(U5-PadAGND)"))
    (pad 1 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(TP39-Pad1)"))
    (pad 3V3 thru_hole oval (at 15.24 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J15-Pad1)"))
    (pad 2 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(TP7-Pad1)"))
    (pad 23 thru_hole oval (at 15.24 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(TP40-Pad1)"))
    (pad 3 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(TP8-Pad1)"))
    (pad 22 thru_hole oval (at 15.24 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /PV_ADC))
    (pad 4 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(TP34-Pad1)"))
    (pad 21 thru_hole oval (at 15.24 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(TP35-Pad1)"))
    (pad 5 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(TP41-Pad1)"))
    (pad 20 thru_hole oval (at 15.24 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(TP36-Pad1)"))
    (pad 6 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(TP42-Pad1)"))
    (pad 19 thru_hole oval (at 15.24 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(J16-Pad1)"))
    (pad 7 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J17-Pad2)"))
    (pad 18 thru_hole oval (at 15.24 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(J18-Pad1)"))
    (pad 8 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(TP43-Pad1)"))
    (pad 17 thru_hole oval (at 15.24 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /Epaper_adapter_sheet/CS))
    (pad 9 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(TP44-Pad1)"))
    (pad 16 thru_hole oval (at 15.24 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /Epaper_adapter_sheet/D/C))
    (pad 10 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(TP45-Pad1)"))
    (pad 15 thru_hole oval (at 15.24 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /Epaper_adapter_sheet/RESET))
    (pad 11 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 /PGOOD))
    (pad 14 thru_hole oval (at 15.24 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /Epaper_adapter_sheet/BUSY))
    (pad 12 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(TP46-Pad1)"))
    (pad 13 thru_hole oval (at 15.24 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /Epaper_adapter_sheet/SCK))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x14_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A2743F3)
    (at 116.6114 72.2884)
    (fp_text reference PGOOD (at 0.0762 3.0734 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 /PGOOD))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A2743FE)
    (at 120.5484 77.2668)
    (fp_text reference STATUS2 (at 0 -1.6256) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 /STATUS2))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A273C07)
    (at 123.825 77.2668)
    (fp_text reference LBO (at 0.1016 1.7018) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 /LBO))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A273C84)
    (at 145.288 83.6422)
    (fp_text reference PWRGD (at -3.6576 0.1778) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /PWRGD))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A1DB761)
    (at 158.242 77.47)
    (fp_text reference TP5 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(R2-Pad2)"))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A273C90)
    (at 148.336 83.6168)
    (fp_text reference ~SHDN (at 1.4224 1.9558) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 /~SHDN))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A2726A5)
    (at 142.24 117.856)
    (fp_text reference SDA (at 0.7112 1.7272) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /SDA))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A2726B0)
    (at 145.6944 117.856)
    (fp_text reference SCL (at 0.5842 1.7526) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /SCL))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A1DC31C)
    (at 162.56 93.98)
    (fp_text reference TP11 (at -0.0254 -1.8288) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(TP11-Pad1)"))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A1DC319)
    (at 162.56 97.028)
    (fp_text reference TP12 (at 0.0254 1.7272) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(TP12-Pad1)"))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A2726F4)
    (at 136.144 104.394)
    (fp_text reference A8 (at 2.076486 0.0254) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /PV_ADC))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A27236C)
    (at 111.3536 124.72035)
    (fp_text reference 11 (at -2.25419 -0.00635) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 /PGOOD))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A271CC3)
    (at 202.9206 80.8482)
    (fp_text reference GDR (at 0 -2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /Epaper_adapter_sheet/GDR))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A271CC8)
    (at 202.9206 84.542745)
    (fp_text reference RESE (at 0 -2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /Epaper_adapter_sheet/RESE))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A271CCF)
    (at 202.9206 88.23729)
    (fp_text reference 3V3 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 +3V3))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A271CD5)
    (at 202.9206 91.931835)
    (fp_text reference VGH (at 0 -2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /Epaper_adapter_sheet/VGH))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A271CDB)
    (at 202.9206 95.62638)
    (fp_text reference PRVGL (at 0 -2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Epaper_adapter_sheet/PRVGL))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A27269C)
    (at 136.144 117.348)
    (fp_text reference CS (at 2.147914 0.0762) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /Epaper_adapter_sheet/CS))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A272695)
    (at 136.144 119.888)
    (fp_text reference D/C (at 2.695533 0.0254) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /Epaper_adapter_sheet/D/C))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A27265D)
    (at 136.144 122.428)
    (fp_text reference RESET (at 3.433629 0.0762) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /Epaper_adapter_sheet/RESET))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A272651)
    (at 136.144 124.968)
    (fp_text reference BUSY (at 3.100295 -0.0508) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /Epaper_adapter_sheet/BUSY))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A271CF2)
    (at 202.9206 99.320925)
    (fp_text reference VPP (at 0 -2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /Epaper_adapter_sheet/VPP))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A272644)
    (at 136.144 127.508)
    (fp_text reference SCK (at 2.647914 0.0508) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /Epaper_adapter_sheet/SCK))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A27233C)
    (at 107.188 114.554)
    (fp_text reference MOSI (at 0.127 -2.8448 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /MOSI))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A271FB0)
    (at 96.774 124.6632)
    (fp_text reference GND (at 0 -2) (layer F.SilkS))
    (fp_text value GND (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A271CF9)
    (at 202.9206 103.01547)
    (fp_text reference VGL (at 0 -2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /Epaper_adapter_sheet/VGL))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A271D01)
    (at 202.9206 106.710015)
    (fp_text reference VDD (at 0 -2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /Epaper_adapter_sheet/VDD))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A271D0C)
    (at 202.9206 110.40456)
    (fp_text reference VSH (at 0 -2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /Epaper_adapter_sheet/VSH))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A271D12)
    (at 202.9206 114.099105)
    (fp_text reference VGH2 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /Epaper_adapter_sheet/VGH2))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A271D17)
    (at 202.9206 117.79365)
    (fp_text reference VSL (at 0 -2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /Epaper_adapter_sheet/VSL))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A271D1C)
    (at 202.9206 121.488195)
    (fp_text reference VCOM (at 0 -2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /Epaper_adapter_sheet/VCOM))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A272314)
    (at 111.3536 101.6889)
    (fp_text reference 2 (at -1.778 -0.0381) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(TP7-Pad1)"))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A27231D)
    (at 111.3536 104.24795)
    (fp_text reference 3 (at -1.778 0.09525) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(TP8-Pad1)"))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A272327)
    (at 111.3536 106.807)
    (fp_text reference 4 (at -1.778 -0.0254) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(TP34-Pad1)"))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A2726E9)
    (at 136.144 106.934)
    (fp_text reference A7 (at 2.076486 0.0762) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(TP35-Pad1)"))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A2726E1)
    (at 136.144 109.474)
    (fp_text reference A6 (at 2.076486 0) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(TP36-Pad1)"))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A1DBBA6)
    (at 112.4966 89.8398)
    (fp_text reference TP37 (at -1.905 0.254 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(Q2-Pad1)"))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A272013)
    (at 111.3536 96.5708)
    (fp_text reference 0 (at -1.778 -0.0508) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(TP38-Pad1)"))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A272019)
    (at 111.3536 99.12985)
    (fp_text reference 1 (at -1.778 -0.09525) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(TP39-Pad1)"))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A2726FC)
    (at 136.144 101.854)
    (fp_text reference A9 (at 2.076486 0.1778) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(TP40-Pad1)"))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A272330)
    (at 111.3536 109.36605)
    (fp_text reference 5 (at -1.778 0.15875) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(TP41-Pad1)"))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A272344)
    (at 111.3536 111.9251)
    (fp_text reference 6 (at -1.778 0.2159) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(TP42-Pad1)"))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A272382)
    (at 111.3536 117.0432)
    (fp_text reference 8 (at -1.778 -0.0508) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(TP43-Pad1)"))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A27237C)
    (at 111.3536 119.60225)
    (fp_text reference 9 (at -1.778 -0.04445) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(TP44-Pad1)"))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A272374)
    (at 111.3536 122.1613)
    (fp_text reference 10 (at -2.25419 -0.0127) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(TP45-Pad1)"))
  )
  (module CustomFootprints:TestPointHole (layer F.Cu) (tedit 5A272362)
    (at 111.3536 127.2794)
    (fp_text reference 12 (at -2.25419 -0.0508) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer Cmts.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(TP46-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A273F70)
    (at 111.4298 85.5218 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 3.2004 0.0762 180) (layer F.SilkS))
    (fp_text value AO3418 (at 0 2.5 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C8-Pad2)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A1F250C)
    (at 83.8454 59.9694)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer Cmts.User) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module KNEK-TEK_logo:KNEK-TEK_logo_11mm (layer F.Cu) (tedit 0)
    (at 157.2006 119.3292)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Symbols:OSHW-Logo_7.5x8mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 103.0224 124.4346)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_7.5x8mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module CustomFootprints:SO-8_5.3x6.2mm_Pitch1.27mm_Handsolder (layer F.Cu) (tedit 5A306DB6)
    (at 154.686 106.7054)
    (descr "8-Lead Plastic Small Outline, 5.3x6.2mm Body (http://www.ti.com.cn/cn/lit/ds/symlink/tl7705a.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 0 -4.13) (layer F.SilkS))
    (fp_text value HIH6130-I2C (at 0 4.13) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.7 -1.905) (size 2.258 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at -3.7 -0.635) (size 2.258 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -3.7 0.635) (size 2.258 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 /SCL))
    (pad 4 smd rect (at -3.7 1.905) (size 2.258 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 /SDA))
    (pad 5 smd rect (at 3.7 1.905) (size 2.258 0.55) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(U4-Pad5)"))
    (pad 6 smd rect (at 3.7 0.635) (size 2.258 0.55) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(U4-Pad6)"))
    (pad 7 smd rect (at 3.7 -0.635) (size 2.258 0.55) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(U4-Pad7)"))
    (pad 8 smd rect (at 3.7 -1.905) (size 2.258 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SO-8_5.3x6.2mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CustomFootprints:QFN-20-1EP_4x4mm_Pitch0.5mm_Handsolder (layer F.Cu) (tedit 5A317A4D)
    (at 121.031 69.4182)
    (descr "20-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -3.33) (layer F.SilkS))
    (fp_text value MCP73871 (at 0 3.33) (layer F.SilkS))
    (pad 1 smd rect (at -2.092 -1) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at -2.092 -0.5) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 3 smd rect (at -2.092 0) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J5-Pad2)"))
    (pad 4 smd rect (at -2.092 0.5) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J6-Pad2)"))
    (pad 5 smd rect (at -2.092 1) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(TH1-Pad1)"))
    (pad 6 smd rect (at -1 2.092 90) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 56 /PGOOD))
    (pad 7 smd rect (at -0.5 2.092 90) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 57 /STATUS2))
    (pad 8 smd rect (at 0 2.092 90) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 58 /LBO))
    (pad 9 smd rect (at 0.5 2.092 90) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J7-Pad2)"))
    (pad 10 smd rect (at 1 2.092 90) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 11 smd rect (at 2.092 1) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 12 smd rect (at 2.092 0.5) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 35 /PROG3))
    (pad 13 smd rect (at 2.092 0) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 /PROG1))
    (pad 14 smd rect (at 2.092 -0.5) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J4-Pad1)"))
    (pad 15 smd rect (at 2.092 -1) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J4-Pad1)"))
    (pad 16 smd rect (at 1 -2.092 90) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J4-Pad1)"))
    (pad 17 smd rect (at 0.5 -2.092 90) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J8-Pad2)"))
    (pad 18 smd rect (at 0 -2.092 90) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 19 smd rect (at -0.5 -2.092 90) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 20 smd rect (at -1 -2.092 90) (size 0.984 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J3-Pad1)"))
    (pad 21 smd rect (at 0.625 0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.2))
    (pad 21 smd rect (at 0.625 -0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.2))
    (pad 21 smd rect (at -0.625 0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.2))
    (pad 21 smd rect (at -0.625 -0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text + (at 86.8426 114.4778) (layer F.SilkS))
  (gr_text + (at 100.5332 105.5116) (layer F.SilkS))
  (gr_text + (at 86.868 97.2312) (layer F.SilkS))
  (gr_text + (at 99.8728 88.3412) (layer F.SilkS))
  (gr_text + (at 86.9188 79.756) (layer F.SilkS))
  (gr_text + (at 100.7364 70.993) (layer F.SilkS))
  (dimension 74.1934 (width 0.3) (layer Dwgs.User)
    (gr_text "2.9210 in" (at 210.7984 93.1037 90) (layer Dwgs.User))
    (feature1 (pts (xy 205.74 56.007) (xy 212.1484 56.007)))
    (feature2 (pts (xy 205.74 130.2004) (xy 212.1484 130.2004)))
    (crossbar (pts (xy 209.4484 130.2004) (xy 209.4484 56.007)))
    (arrow1a (pts (xy 209.4484 56.007) (xy 210.034821 57.133504)))
    (arrow1b (pts (xy 209.4484 56.007) (xy 208.861979 57.133504)))
    (arrow2a (pts (xy 209.4484 130.2004) (xy 210.034821 129.073896)))
    (arrow2b (pts (xy 209.4484 130.2004) (xy 208.861979 129.073896)))
  )
  (dimension 125.857208 (width 0.3) (layer Dwgs.User)
    (gr_text "4.9550 in" (at 142.802912 134.839731 359.8959311) (layer Dwgs.User))
    (feature1 (pts (xy 205.74 130.2258) (xy 205.72896 136.304029)))
    (feature2 (pts (xy 79.883 129.9972) (xy 79.87196 136.075429)))
    (crossbar (pts (xy 79.876864 133.375433) (xy 205.733864 133.604033)))
    (arrow1a (pts (xy 205.733864 133.604033) (xy 204.606297 134.188407)))
    (arrow1b (pts (xy 205.733864 133.604033) (xy 204.608427 133.015567)))
    (arrow2a (pts (xy 79.876864 133.375433) (xy 81.002301 133.963899)))
    (arrow2b (pts (xy 79.876864 133.375433) (xy 81.004431 132.791059)))
  )
  (gr_text GND-> (at 194.8434 128.4732) (layer B.SilkS))
  (gr_text "K'NEK-TEK Solar Powered Home Monitor v1.0\nDesign files available at: \nhttps://github.com/Erik-k/SolarClapboard\nDecember 2017" (at 170.5102 59.69) (layer F.SilkS))
  (gr_text "Short J9 for 4 panels. \nOpen for 6." (at 107.7214 90.9574 90) (layer F.SilkS))
  (gr_line (start 79.883 130.175) (end 79.883 56.007) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 205.6892 130.2258) (end 79.883 130.175) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 205.74 56.007) (end 205.74 130.2258) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.883 56.007) (end 205.74 56.007) (layer Edge.Cuts) (width 0.15))
  (gr_text E-Paper (at 182.3466 65.5828) (layer F.SilkS))
  (gr_text "Autumn 2017" (at 222.758 193.04) (layer Dwgs.User))
  (gr_text "SPHM Development Board" (at 202.184 189.484) (layer Dwgs.User))
  (gr_text 1.0 (at 270.256 193.04) (layer Dwgs.User))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.772 56.9976) (xy 80.6958 129.413) (xy 205.0034 129.4384) (xy 204.978 56.6674)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.6958 129.413) (xy 80.772 56.9976) (xy 204.978 56.6674) (xy 205.0034 129.4384)
      )
    )
  )
)
