(kicad_pcb (version 20171130) (host pcbnew 5.1.7-a382d34a8~88~ubuntu16.04.1)
  (general
    (thickness 1.6)
    (drawings 34)
    (tracks 210)
    (zones 0)
    (modules 11)
    (nets 27)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFDFF7F)
    (pcbplotparams
      (layerselection 0x010f8_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 Vcc)
  (net 3 AFilt)
  (net 4 SWDio)
  (net 5 SWClk)
  (net 6 P1.0)
  (net 7 AlarmIRQ)
  (net 8 SDA)
  (net 9 SCL)
  (net 10 P1.4)
  (net 11 P1.5)
  (net 12 P1.6)
  (net 13 P1.7)
  (net 14 P3.2)
  (net 15 P3.1)
  (net 16 P3.0)
  (net 17 P2.7)
  (net 18 P2.6)
  (net 19 P2.5)
  (net 20 P2.4)
  (net 21 P2.3)
  (net 22 P2.2)
  (net 23 P2.1)
  (net 24 P2.0)
  (net 25 Xtal2)
  (net 26 Xtal1)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net AFilt)
    (add_net AlarmIRQ)
    (add_net GND)
    (add_net P1.0)
    (add_net P1.4)
    (add_net P1.5)
    (add_net P1.6)
    (add_net P1.7)
    (add_net P2.0)
    (add_net P2.1)
    (add_net P2.2)
    (add_net P2.3)
    (add_net P2.4)
    (add_net P2.5)
    (add_net P2.6)
    (add_net P2.7)
    (add_net P3.0)
    (add_net P3.1)
    (add_net P3.2)
    (add_net SCL)
    (add_net SDA)
    (add_net SWClk)
    (add_net SWDio)
    (add_net Xtal1)
    (add_net Xtal2)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Vcc)
  )
  (module Crystal:Crystal_SMD_3215-2Pin_3.2x1.5mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 101.5 60.1 180)
    (descr "SMD Crystal FC-135 https://support.epson.biz/td/api/doc_check.php?dl=brief_FC-135R_en.pdf")
    (tags "SMD SMT Crystal")
    (attr smd)
    (fp_text reference Y1 (at -1.6 -2) (layer F.SilkS) hide)
    (fp_text value 32.768kHz (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at -1.25 0 180) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 26 Xtal1))
    (pad 1 smd rect (at 1.25 0 180) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 25 Xtal2))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3215-2Pin_3.2x1.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm_ThermalVias (layer F.Cu) (tedit 5DC5F6A3)
    (at 101.5 49.45)
    (descr "QFN, 24 Pin (http://www.alfarzpp.lv/eng/sc/AS3330.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U4 (at 0 -3.32) (layer F.SilkS) hide)
    (fp_text value Msp430fr2433 (at 0 3.32) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd roundrect (at 0.675 0.675) (size 1.17 1.17) (layers F.Paste) (roundrect_rratio 0.213674358974359))
    (pad "" smd roundrect (at 0.675 -0.675) (size 1.17 1.17) (layers F.Paste) (roundrect_rratio 0.213674358974359))
    (pad "" smd roundrect (at -0.675 0.675) (size 1.17 1.17) (layers F.Paste) (roundrect_rratio 0.213674358974359))
    (pad "" smd roundrect (at -0.675 -0.675) (size 1.17 1.17) (layers F.Paste) (roundrect_rratio 0.213674358974359))
    (pad 25 smd rect (at 0 0) (size 2.7 2.7) (layers B.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 1.1 1.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 0 1.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at -1.1 1.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 1.1 0) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at -1.1 0) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 1.1 -1.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 0 -1.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at -1.1 -1.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 smd rect (at 0 0) (size 2.7 2.7) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 24 smd roundrect (at -1.25 -1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Vcc))
    (pad 23 smd roundrect (at -0.75 -1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 22 smd roundrect (at -0.25 -1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 P2.1))
    (pad 21 smd roundrect (at 0.25 -1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 P2.0))
    (pad 20 smd roundrect (at 0.75 -1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 P3.2))
    (pad 19 smd roundrect (at 1.25 -1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 P2.7))
    (pad 18 smd roundrect (at 1.9625 -1.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 17 smd roundrect (at 1.9625 -0.75) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 P2.6))
    (pad 16 smd roundrect (at 1.9625 -0.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 P2.5))
    (pad 15 smd roundrect (at 1.9625 0.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 P2.4))
    (pad 14 smd roundrect (at 1.9625 0.75) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 P3.1))
    (pad 13 smd roundrect (at 1.9625 1.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 P2.3))
    (pad 12 smd roundrect (at 1.25 1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 P3.0))
    (pad 11 smd roundrect (at 0.75 1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 P2.2))
    (pad 10 smd roundrect (at 0.25 1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 SCL))
    (pad 9 smd roundrect (at -0.25 1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 SDA))
    (pad 8 smd roundrect (at -0.75 1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 AlarmIRQ))
    (pad 7 smd roundrect (at -1.25 1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 P1.0))
    (pad 6 smd roundrect (at -1.9625 1.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 P1.7))
    (pad 5 smd roundrect (at -1.9625 0.75) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 P1.6))
    (pad 4 smd roundrect (at -1.9625 0.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 P1.5))
    (pad 3 smd roundrect (at -1.9625 -0.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 P1.4))
    (pad 2 smd roundrect (at -1.9625 -0.75) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 SWClk))
    (pad 1 smd roundrect (at -1.9625 -1.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 SWDio))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.75x1.75mm (layer F.Cu) (tedit 5DC5F6A3)
    (at 101 56 180)
    (descr "QFN, 16 Pin (https://www.onsemi.com/pub/Collateral/NCN4555-D.PDF), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U1 (at 0 -2.8) (layer F.SilkS) hide)
    (fp_text value AB0805 (at 0 2.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd roundrect (at 0.44 0.44 180) (size 0.71 0.71) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.44 -0.44 180) (size 0.71 0.71) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.44 0.44 180) (size 0.71 0.71) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.44 -0.44 180) (size 0.71 0.71) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 17 smd rect (at 0 0 180) (size 1.75 1.75) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 16 smd roundrect (at -0.75 -1.4625 180) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 Xtal1))
    (pad 15 smd roundrect (at -0.25 -1.4625 180) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 Xtal2))
    (pad 14 smd roundrect (at 0.25 -1.4625 180) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 AFilt))
    (pad 13 smd roundrect (at 0.75 -1.4625 180) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Vcc))
    (pad 12 smd roundrect (at 1.4625 -0.75 180) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 11 smd roundrect (at 1.4625 -0.25 180) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 AlarmIRQ))
    (pad 10 smd roundrect (at 1.4625 0.25 180) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at 1.4625 0.75 180) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 8 smd roundrect (at 0.75 1.4625 180) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at 0.25 1.4625 180) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 SCL))
    (pad 6 smd roundrect (at -0.25 1.4625 180) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 SDA))
    (pad 5 smd roundrect (at -0.75 1.4625 180) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at -1.4625 0.75 180) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -1.4625 0.25 180) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -1.4625 -0.25 180) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4625 -0.75 180) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_P0.5mm_EP1.75x1.75mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 97.7 57.9 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference Cby1 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Vcc))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 100 44 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference Cby2 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Vcc))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 98 44 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference Cby3 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Vcc))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 98.4 61 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference Cf1 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 47pF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 AFilt))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootprints:TC2030-CTX-NL (layer F.Cu) (tedit 59C7D319)
    (at 101 39 270)
    (descr "Tag Connect small footprint SWD connector ( No Leg version )")
    (solder_paste_ratio -0.5)
    (clearance 0.2)
    (attr virtual)
    (fp_text reference CON1 (at 0 4.064 90) (layer F.SilkS) hide)
    (fp_text value TC2030-CTX-NL (at 0 4.572 90) (layer F.SilkS))
    (pad 1 smd circle (at -0.635 -1.27 270) (size 0.787 0.787) (layers F.Cu F.Mask)
      (net 2 Vcc))
    (pad 2 smd circle (at 0.635 -1.27 270) (size 0.787 0.787) (layers F.Cu F.Mask)
      (net 4 SWDio))
    (pad 3 smd circle (at -0.635 0 270) (size 0.787 0.787) (layers F.Cu F.Mask))
    (pad 4 smd circle (at 0.635 0 270) (size 0.787 0.787) (layers F.Cu F.Mask)
      (net 5 SWClk))
    (pad 5 smd circle (at -0.635 1.27 270) (size 0.787 0.787) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd circle (at 0.635 1.27 270) (size 0.787 0.787) (layers F.Cu F.Mask))
    (pad "" np_thru_hole circle (at 0 -2.54 270) (size 0.991 0.991) (drill 0.991) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.016 2.54 270) (size 0.991 0.991) (drill 0.991) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 1.016 2.54 270) (size 0.991 0.991) (drill 0.991) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x12_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 93 38)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x12 (at 0 30.27) (layer F.Fab))
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 Vcc))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 P1.0))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 AlarmIRQ))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 SDA))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 SCL))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 P1.4))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 P1.5))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 P1.6))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 P1.7))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x12_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 109.1 66 180)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J2 (at 3.1 0) (layer F.SilkS) hide)
    (fp_text value Conn_01x12 (at 0 30.27) (layer F.Fab))
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 P3.2))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 P3.1))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 P3.0))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 P2.7))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 P2.6))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 P2.5))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 P2.4))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 P2.3))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 P2.2))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 P2.1))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 P2.0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 98 65 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 Vcc))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 Vcc))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 Vcc))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 1.5 (at 95.6 55.9) (layer F.SilkS))
  (gr_text 1.6 (at 95.6 58.2) (layer F.SilkS))
  (gr_text 2.1 (at 106.5 63.4) (layer F.SilkS))
  (gr_text 2.2 (at 106.5 61) (layer F.SilkS))
  (gr_text 2.3 (at 106.5 58.4) (layer F.SilkS))
  (gr_text 3.1 (at 106.6 43.2) (layer F.SilkS))
  (gr_text 2.5 (at 106.5 53.4) (layer F.SilkS))
  (gr_text 2.6 (at 106.4 50.9) (layer F.SilkS))
  (gr_text 2.4 (at 106.7 55.9) (layer F.SilkS))
  (gr_text "MSP430FR2433Breakout\nw AB0805 RTC" (at 96.3 46.1 90) (layer B.SilkS))
  (gr_text 10uF (at 102.7 42.9) (layer F.SilkS))
  (gr_text 0.1uF (at 102.9 44.4) (layer F.SilkS))
  (gr_text 0.1uF (at 97.7 54.8 90) (layer F.SilkS))
  (gr_text 47pF (at 100.3 62.7) (layer F.SilkS))
  (gr_text Vcc (at 100.6 67.2) (layer F.SilkS))
  (gr_text Gnd (at 95.8 66) (layer F.SilkS))
  (gr_text Gnd (at 95.8 63.4) (layer F.SilkS))
  (gr_text 1.7 (at 95.6 60.8) (layer F.SilkS))
  (gr_text 1.4 (at 95.6 53.2) (layer F.SilkS))
  (gr_text SCL (at 95.8 50.8) (layer F.SilkS))
  (gr_text SDA (at 95.8 48.2) (layer F.SilkS))
  (gr_text IRQ (at 95.6 45.4) (layer F.SilkS))
  (gr_text 1.0 (at 95.6 43) (layer F.SilkS))
  (gr_text Gnd (at 95.8 40.6) (layer F.SilkS))
  (gr_text Vcc (at 95.8 38) (layer F.SilkS))
  (gr_text Gnd (at 106.4 38.2) (layer F.SilkS))
  (gr_text 3.2 (at 106.6 40.6) (layer F.SilkS))
  (gr_text 3.0 (at 106.5 45.8) (layer F.SilkS))
  (gr_text 2.7 (at 106.5 48.4) (layer F.SilkS))
  (gr_text 2.0 (at 106.6 66) (layer F.SilkS))
  (gr_line (start 91 68) (end 91 36) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111 68) (end 91 68) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111 36) (end 111 68) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91 36) (end 111 36) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.3) (thermal_bridge_width 0.26))
    (polygon
      (pts
        (xy 113 69) (xy 86 69) (xy 86 35) (xy 113 35)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.26))
    (polygon
      (pts
        (xy 113 69) (xy 86 69) (xy 86 35) (xy 113 35)
      )
    )
  )
)
