<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="15.24" width="0.254" layer="20"/>
<wire x1="0" y1="15.24" x2="22.86" y2="15.24" width="0.254" layer="20"/>
<wire x1="22.86" y1="15.24" x2="22.86" y2="0" width="0.254" layer="20"/>
<wire x1="22.86" y1="0" x2="0" y2="0" width="0.254" layer="20"/>
<text>William Laney 2016</text>
<text>DS1339B Breakout v1</text>
<text>10k</text>
<text>10k</text>
<text>10k</text>
<text>0.1uF</text>
<text>VCC</text>
<text>SDA</text>
<text>SCL</text>
<text>SQW</text>
<text>GND</text>
<text>GND</text>
<text>SQW</text>
<text>SDA</text>
<text>VCC</text>
<text>DS1339B</text>
<text>ABS25</text>
<text>WM Physics</text>
<text>VIMS</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="BATTCON_12MM_CURVED">
</package>
<package name="1X06">
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="0805-NO">
</package>
</packages>
</library>
<library name="sharkdunio">
<packages>
<package name="8U-SOP">
</package>
</packages>
</library>
<library name="abracon">
<packages>
<package name="ABS25">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BAT1" library="SparkFun" package="BATTCON_12MM_CURVED" value="3V"/>
<element name="C4" library="microbuilder" package="0805-NO" value="0.1uF"/>
<element name="JP5" library="SparkFun" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="microbuilder" package="0805-NO" value="10K"/>
<element name="R2" library="microbuilder" package="0805-NO" value="10K"/>
<element name="R3" library="microbuilder" package="0805-NO" value="10K"/>
<element name="U$1" library="sharkdunio" package="8U-SOP" value="DS1339BDS1339B"/>
<element name="Y1" library="abracon" package="ABS25" value="CRYSTAL.ABS25"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="U$1" pad="2"/>
<contactref element="Y1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="3"/>
<contactref element="BAT1" pad="PWR@1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="4"/>
<contactref element="BAT1" pad="GND"/>
<contactref element="JP5" pad="6"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="JP5" pad="1"/>
<contactref element="U$1" pad="8"/>
<contactref element="C4" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="JP5" pad="2"/>
<contactref element="U$1" pad="5"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="JP5" pad="3"/>
<contactref element="U$1" pad="6"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="SQW/INT">
<contactref element="U$1" pad="7"/>
<contactref element="JP5" pad="4"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="Y1" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
