(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 408)
    (zones 0)
    (modules 37)
    (nets 104)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.2)
    (user_trace_width 0.35)
    (user_trace_width 0.5)
    (trace_clearance 0.1)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad16)")
  (net 2 "Net-(U1-Pad17)")
  (net 3 "Net-(U1-Pad9)")
  (net 4 "Net-(J2-Pad1)")
  (net 5 Teensy_UART_5_RX)
  (net 6 Teensy_UART_5_Tx)
  (net 7 GND)
  (net 8 "Net-(R10-Pad1)")
  (net 9 +3V3)
  (net 10 "Net-(U1-Pad18)")
  (net 11 Teensy_GPIO_35)
  (net 12 Teensy_GPIO_36)
  (net 13 Teensy_SCK_0)
  (net 14 Teensy_MISO_0)
  (net 15 Teensy_MOSI_0)
  (net 16 "Net-(U1-Pad5)")
  (net 17 "Net-(U1-Pad4)")
  (net 18 +BATT)
  (net 19 "Net-(U6-Pad7)")
  (net 20 "Net-(U6-Pad8)")
  (net 21 "Net-(U6-Pad15)")
  (net 22 "Net-(U6-Pad16)")
  (net 23 "Net-(U8-Pad2)")
  (net 24 "Net-(U8-Pad3)")
  (net 25 "Net-(U8-Pad4)")
  (net 26 "Net-(U8-Pad5)")
  (net 27 "Net-(J5-Pad1)")
  (net 28 Teensy_CS_Temp)
  (net 29 MUX_Temp_1)
  (net 30 MUX_Temp_2)
  (net 31 Teensy_CS_IMU)
  (net 32 "Net-(D1-Pad1)")
  (net 33 "Net-(D1-Pad2)")
  (net 34 +5V)
  (net 35 Teensy_Iridium_OnOff)
  (net 36 Teensy_UART_2_RX)
  (net 37 Teensy_UART_2_TX)
  (net 38 Teensy_UART_RTS)
  (net 39 Teensy_UART_CTS)
  (net 40 Teensy_UART_DTR)
  (net 41 "Net-(D3-Pad2)")
  (net 42 "Net-(D2-Pad2)")
  (net 43 "Net-(R3-Pad2)")
  (net 44 "Net-(D2-Pad1)")
  (net 45 "Net-(D3-Pad1)")
  (net 46 "Net-(R11-Pad1)")
  (net 47 IMU_SCL)
  (net 48 IMU_SDA)
  (net 49 "Net-(U2-Pad4)")
  (net 50 "Net-(U2-Pad5)")
  (net 51 "Net-(U2-Pad9)")
  (net 52 "Net-(U2-Pad16)")
  (net 53 "Net-(U2-Pad17)")
  (net 54 "Net-(U2-Pad18)")
  (net 55 "Net-(U3-Pad5)")
  (net 56 "Net-(C3-Pad1)")
  (net 57 "Net-(C6-Pad1)")
  (net 58 "Net-(C7-Pad1)")
  (net 59 "Net-(J3-Pad9)")
  (net 60 "Net-(J3-Pad10)")
  (net 61 "Net-(J3-Pad11)")
  (net 62 "Net-(J3-Pad12)")
  (net 63 "Net-(J3-Pad13)")
  (net 64 "Net-(J3-Pad16)")
  (net 65 "Net-(J3-Pad17)")
  (net 66 "Net-(J4-Pad2)")
  (net 67 "Net-(J4-Pad1)")
  (net 68 "Net-(J5-Pad2)")
  (net 69 "Net-(L1-Pad1)")
  (net 70 "Net-(R1-Pad1)")
  (net 71 "Net-(R2-Pad1)")
  (net 72 "Net-(R4-Pad2)")
  (net 73 "Net-(U1-Pad13)")
  (net 74 "Net-(U1-Pad15)")
  (net 75 "Net-(U2-Pad19)")
  (net 76 "Net-(U2-Pad20)")
  (net 77 "Net-(U2-Pad21)")
  (net 78 "Net-(U2-Pad22)")
  (net 79 "Net-(U2-Pad23)")
  (net 80 "Net-(U2-Pad24)")
  (net 81 "Net-(U2-Pad25)")
  (net 82 "Net-(U2-Pad26)")
  (net 83 "Net-(U2-Pad27)")
  (net 84 "Net-(U2-Pad28)")
  (net 85 "Net-(U2-Pad29)")
  (net 86 "Net-(U2-Pad36)")
  (net 87 "Net-(U2-Pad37)")
  (net 88 "Net-(U2-Pad10)")
  (net 89 "Net-(U2-Pad8)")
  (net 90 "Net-(U2-Pad7)")
  (net 91 "Net-(U2-Pad6)")
  (net 92 "Net-(U2-Pad3)")
  (net 93 "Net-(U2-Pad2)")
  (net 94 "Net-(U2-Pad38)")
  (net 95 "Net-(U2-Pad41)")
  (net 96 "Net-(U2-Pad48)")
  (net 97 "Net-(U2-Pad52)")
  (net 98 "Net-(U2-Pad54)")
  (net 99 "Net-(U2-Pad55)")
  (net 100 "Net-(U2-Pad56)")
  (net 101 "Net-(U2-Pad57)")
  (net 102 "Net-(U5-Pad5)")
  (net 103 +5VD)
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net +5VD)
    (add_net +BATT)
    (add_net GND)
    (add_net IMU_SCL)
    (add_net IMU_SDA)
    (add_net MUX_Temp_1)
    (add_net MUX_Temp_2)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(J3-Pad11)")
    (add_net "Net-(J3-Pad12)")
    (add_net "Net-(J3-Pad13)")
    (add_net "Net-(J3-Pad16)")
    (add_net "Net-(J3-Pad17)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad36)")
    (add_net "Net-(U2-Pad37)")
    (add_net "Net-(U2-Pad38)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad41)")
    (add_net "Net-(U2-Pad48)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad52)")
    (add_net "Net-(U2-Pad54)")
    (add_net "Net-(U2-Pad55)")
    (add_net "Net-(U2-Pad56)")
    (add_net "Net-(U2-Pad57)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U5-Pad5)")
    (add_net "Net-(U6-Pad15)")
    (add_net "Net-(U6-Pad16)")
    (add_net "Net-(U6-Pad7)")
    (add_net "Net-(U6-Pad8)")
    (add_net "Net-(U8-Pad2)")
    (add_net "Net-(U8-Pad3)")
    (add_net "Net-(U8-Pad4)")
    (add_net "Net-(U8-Pad5)")
    (add_net Teensy_CS_IMU)
    (add_net Teensy_CS_Temp)
    (add_net Teensy_GPIO_35)
    (add_net Teensy_GPIO_36)
    (add_net Teensy_Iridium_OnOff)
    (add_net Teensy_MISO_0)
    (add_net Teensy_MOSI_0)
    (add_net Teensy_SCK_0)
    (add_net Teensy_UART_2_RX)
    (add_net Teensy_UART_2_TX)
    (add_net Teensy_UART_5_RX)
    (add_net Teensy_UART_5_Tx)
    (add_net Teensy_UART_CTS)
    (add_net Teensy_UART_DTR)
    (add_net Teensy_UART_RTS)
  )
  (module SS4-10-3:Irid_9603 (layer F.Cu) (tedit 5FBD22F4)
    (at 117.348 101.6)
    (fp_text reference J3 (at -0.425695 3.841385 270) (layer F.SilkS))
    (fp_text value SS4-10-3.00-L-D-K-TR (at 3.81 -5.08 180) (layer F.Fab))
    (pad 1 smd rect (at -1.8 2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 34 +5V))
    (pad 2 smd rect (at -1.8 -2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 34 +5V))
    (pad 3 smd rect (at -1.4 2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 4 smd rect (at -1.4 -2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 5 smd rect (at -1 2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 35 Teensy_Iridium_OnOff))
    (pad 6 smd rect (at -1 -2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 37 Teensy_UART_2_TX))
    (pad 7 smd rect (at -0.6 2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 36 Teensy_UART_2_RX))
    (pad 8 smd rect (at -0.6 -2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 9 smd rect (at -0.2 2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(J3-Pad9)"))
    (pad 10 smd rect (at -0.2 -2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(J3-Pad10)"))
    (pad 11 smd rect (at 0.2 2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(J3-Pad11)"))
    (pad 12 smd rect (at 0.2 -2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(J3-Pad12)"))
    (pad 13 smd rect (at 0.6 2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(J3-Pad13)"))
    (pad 14 smd rect (at 0.6 -2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 40 Teensy_UART_DTR))
    (pad 15 smd rect (at 1 2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 16 smd rect (at 1 -2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(J3-Pad16)"))
    (pad 17 smd rect (at 1.4 2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(J3-Pad17)"))
    (pad 18 smd rect (at 1.4 -2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 19 smd rect (at 1.8 2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D3-Pad2)"))
    (pad 20 smd rect (at 1.8 -2.335 90) (size 0.93 0.23) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D2-Pad2)"))
    (pad 21 thru_hole circle (at 10 -25.8) (size 5.3 5.3) (drill 3.9) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at -15 -25.8) (size 5.3 5.3) (drill 3.9) (layers *.Cu *.Mask))
  )
  (module AD7791BRMZ:AD7791BRMZ (layer F.Cu) (tedit 5F7B665E)
    (at 148.59 76.835)
    (fp_text reference U7 (at 0 -0.635) (layer F.SilkS))
    (fp_text value AD7791BRMZ (at 0.762 2.413) (layer F.SilkS))
    (fp_text user * (at -1.1684 -1.4732) (layer F.SilkS))
    (fp_text user * (at -2.4257 -2.4732) (layer F.SilkS))
    (fp_text user * (at -1.1684 -1.4732) (layer F.Fab))
    (fp_text user * (at -2.4257 -2.4732) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 1.27 -0.635) (layer Cmts.User))
    (pad 10 smd rect (at 2.1717 -1.000001) (size 1.524 0.3302) (layers F.Cu F.Paste F.Mask)
      (net 15 Teensy_MOSI_0))
    (pad 9 smd rect (at 2.1717 -0.499999) (size 1.524 0.3302) (layers F.Cu F.Paste F.Mask)
      (net 14 Teensy_MISO_0))
    (pad 8 smd rect (at 2.1717 0) (size 1.524 0.3302) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (pad 7 smd rect (at 2.1717 0.499999) (size 1.524 0.3302) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 6 smd rect (at 2.1717 1.000001) (size 1.524 0.3302) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 5 smd rect (at -2.1717 1.000001) (size 1.524 0.3302) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(C6-Pad1)"))
    (pad 4 smd rect (at -2.1717 0.499999) (size 1.524 0.3302) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(C6-Pad1)"))
    (pad 3 smd rect (at -2.1717 0) (size 1.524 0.3302) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at -2.1717 -0.499999) (size 1.524 0.3302) (layers F.Cu F.Paste F.Mask)
      (net 28 Teensy_CS_Temp))
    (pad 1 smd rect (at -2.1717 -1.000001) (size 1.524 0.3302) (layers F.Cu F.Paste F.Mask)
      (net 13 Teensy_SCK_0))
  )
  (module ADG1636BRUZ:ADG1636BRUZ (layer F.Cu) (tedit 5F7B66CE)
    (at 146.05 63.5)
    (fp_text reference U6 (at 0.635 0) (layer F.SilkS))
    (fp_text value ADG1636BRUZ (at -4.826 -1.524 90) (layer F.SilkS))
    (fp_text user * (at -1.8669 -2.4765) (layer F.SilkS))
    (fp_text user * (at -3.0734 -3.773601) (layer F.SilkS))
    (fp_text user * (at -1.8669 -2.4765) (layer F.Fab))
    (fp_text user * (at -3.0734 -3.773601) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 16 smd rect (at 2.8194 -2.274999) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U6-Pad16)"))
    (pad 15 smd rect (at 2.8194 -1.624998) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U6-Pad15)"))
    (pad 14 smd rect (at 2.8194 -0.974999) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (pad 13 smd rect (at 2.8194 -0.324998) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (pad 12 smd rect (at 2.8194 0.325001) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J5-Pad1)"))
    (pad 11 smd rect (at 2.8194 0.974999) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R10-Pad1)"))
    (pad 10 smd rect (at 2.8194 1.625001) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(J4-Pad1)"))
    (pad 9 smd rect (at 2.8194 2.274999) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 30 MUX_Temp_2))
    (pad 8 smd rect (at -2.8194 2.274999) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U6-Pad8)"))
    (pad 7 smd rect (at -2.8194 1.624998) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U6-Pad7)"))
    (pad 6 smd rect (at -2.8194 0.974999) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 5 smd rect (at -2.8194 0.324998) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 4 smd rect (at -2.8194 -0.325001) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(J5-Pad2)"))
    (pad 3 smd rect (at -2.8194 -0.974999) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at -2.8194 -1.625001) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(J4-Pad2)"))
    (pad 1 smd rect (at -2.8194 -2.274999) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 29 MUX_Temp_1))
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 151.384 87.884 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100K (at 4.572 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 72 "Net-(R4-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 56 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 107.696 104.14)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 3.556 0) (layer F.SilkS))
    (fp_text value 167 (at 0 -2.032) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 44 "Net-(D2-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 152.4 139.065 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at -3.81 0) (layer F.SilkS))
    (fp_text value 4K7 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 -0.635) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 47 IMU_SCL))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 9 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 136.307 77.47)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at -3.556 -0.042) (layer F.SilkS))
    (fp_text value "10K 0.1%" (at 0 1.82) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 8 "Net-(R10-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 136.307 73.025)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at -4.064 0.085) (layer F.SilkS))
    (fp_text value 10K (at 0 1.82) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 57 "Net-(C6-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 8 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 136.307 69.215)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at -4.227 -0.127) (layer F.SilkS))
    (fp_text value 10K (at 0 1.82) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 46 "Net-(R11-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 58 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module REF200AU:REF200AU (layer F.Cu) (tedit 5F7A1AFE)
    (at 148.59 71.12)
    (fp_text reference U8 (at -0.385 -3.537) (layer F.SilkS))
    (fp_text value REF200AU (at 0.254 -0.508) (layer F.Fab))
    (pad 1 smd rect (at -2.47 -1.905) (size 1.97 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at -2.47 -0.635) (size 1.97 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U8-Pad2)"))
    (pad 3 smd rect (at -2.47 0.635) (size 1.97 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U8-Pad3)"))
    (pad 4 smd rect (at -2.47 1.905) (size 1.97 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U8-Pad4)"))
    (pad 5 smd rect (at 2.47 1.905) (size 1.97 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U8-Pad5)"))
    (pad 6 smd rect (at 2.47 0.635) (size 1.97 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 7 smd rect (at 2.47 -0.635) (size 1.97 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (pad 8 smd rect (at 2.47 -1.905) (size 1.97 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 175.895 90.17 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 47u (at 0 1.82 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 9 +3V3))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 152.908 93.472 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 3.556 0) (layer F.SilkS))
    (fp_text value 100n (at 0 -2.032) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 56 "Net-(C3-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-15_P12.70mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 113.665 114.935 270)
    (descr "Diode, DO-15 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
    (tags "Diode DO-15 series Axial Horizontal pin pitch 12.7mm  length 7.6mm diameter 3.6mm")
    (fp_text reference D1 (at 6.35 -2.92 90) (layer F.SilkS))
    (fp_text value D (at 6.35 2.92 90) (layer F.Fab))
    (fp_text user %R (at 6.35 -0.635 90) (layer F.Fab))
    (fp_text user K (at 0 -2.2 90) (layer F.Fab))
    (fp_text user K (at 0 -2.2 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 32 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 33 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-15_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 114.935 132.932 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 1.472K (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 2.1225 -2.54 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 GND))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 43 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LTST-C190EKT:LTST-C190EKT (layer F.Cu) (tedit 5F7DD4CA)
    (at 101.815 104.013 180)
    (fp_text reference D2 (at 0.215 -1.272349) (layer F.SilkS))
    (fp_text value LTST-C190EKT (at 2.755 1.905) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D2-Pad1)"))
  )
  (module LTST-C190EKT:LTST-C190EKT (layer F.Cu) (tedit 5F7DD4CA)
    (at 101.6 107.696 180)
    (fp_text reference D3 (at 0.508 -1.524) (layer F.SilkS))
    (fp_text value LTST-C190EKT (at 1.908781 1.27252) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D3-Pad2)"))
  )
  (module ul_1206L300SLTHYR_fuse:1206L300SLTHYR (layer F.Cu) (tedit 0)
    (at 121.92 140.97)
    (fp_text reference F1 (at -0.635 -2.54) (layer F.SilkS))
    (fp_text value 1206L300SLTHYR (at 0 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0.8128 -0.635) (layer Cmts.User))
    (fp_text user * (at -2.286 -1.397) (layer F.SilkS))
    (fp_text user * (at -1.016 -0.381) (layer F.Fab))
    (fp_text user * (at -1.016 -0.381) (layer F.Fab))
    (fp_text user * (at -2.286 -1.397) (layer F.SilkS))
    (pad 1 smd rect (at -1.7272 0) (size 0.762 1.6764) (layers F.Cu F.Paste F.Mask)
      (net 103 +5VD))
    (pad 2 smd rect (at 1.7272 0) (size 0.762 1.6764) (layers F.Cu F.Paste F.Mask)
      (net 34 +5V))
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 172.085 90.17 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.82 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 GND))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 9 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 154.94 78.232 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at -3.556 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.82 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 GND))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 9 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 154.432 71.12 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at -3.556 0.381 90) (layer F.SilkS))
    (fp_text value 100n (at 0 -2.032 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 9 +3V3))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 142.24 77.724 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 1u (at -0.508 2.032 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 GND))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 57 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 142.24 71.628 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 0 2.032 90) (layer F.SilkS))
    (fp_text value 1u (at 0 -2.032 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 GND))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 58 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 1760510000:1760490000 (layer F.Cu) (tedit 5F7A1FED)
    (at 104.14 116.84 270)
    (fp_text reference J1 (at 0.63547 -5.08367 90) (layer F.SilkS))
    (fp_text value 1760510000 (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.25 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 2.25 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 33 "Net-(D1-Pad2)"))
  )
  (module uFL_RSP12281101:RSP-122811-01 (layer F.Cu) (tedit 0)
    (at 166.624 84.328)
    (fp_text reference J2 (at 0 0) (layer F.SilkS))
    (fp_text value RSP-122811-01 (at 0 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.9906 1.0414) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at -1.475001 -1.525001 90) (size 2.2098 1.0414) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 3 smd rect (at 1.475001 -1.525001 90) (size 2.2098 1.0414) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
  )
  (module 1760510000:1760490000 (layer F.Cu) (tedit 5F7A1FED)
    (at 129.54 62.992 180)
    (fp_text reference J4 (at 0.63547 -5.08367) (layer F.SilkS))
    (fp_text value 1760510000 (at 0 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 2.25 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 66 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.25 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 67 "Net-(J4-Pad1)"))
  )
  (module 1760510000:1760490000 (layer F.Cu) (tedit 5F7A1FED)
    (at 166.116 75.184 180)
    (fp_text reference J5 (at 0.63547 -5.08367) (layer F.SilkS))
    (fp_text value 1760510000 (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.25 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 27 "Net-(J5-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 2.25 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 68 "Net-(J5-Pad2)"))
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 158.473 86.36)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at 0 -1.17) (layer F.SilkS))
    (fp_text value L (at 2.54 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(L1-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 171.45 100.33 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.82 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 70 "Net-(R1-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 Teensy_UART_5_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 174.625 99.06 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 4.445 0 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.82 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 Teensy_UART_5_Tx))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 71 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 152.4 135.255 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at -3.81 0) (layer F.SilkS))
    (fp_text value 4K7 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 9 +3V3))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 48 IMU_SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 107.696 107.696 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at -4.064 -0.381) (layer F.SilkS))
    (fp_text value 167 (at 0 -2.413) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 GND))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 45 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ul_TESEOLIV3F:TESEO-LIV3F (layer F.Cu) (tedit 0)
    (at 163.195 94.996 180)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value TESEO-LIV3F (at 6.223 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at -5.5372 -5.314401) (layer F.SilkS))
    (fp_text user * (at -4.2672 -4.5974) (layer F.Fab))
    (fp_text user * (at -4.2672 -4.5974) (layer F.Fab))
    (fp_text user * (at -5.5372 -5.314401) (layer F.SilkS))
    (pad 1 smd rect (at -4.92125 -4.400001 180) (size 0.8763 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at -4.92125 -3.300001 180) (size 0.8763 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(R1-Pad1)"))
    (pad 3 smd rect (at -4.92125 -2.200001 180) (size 0.8763 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(R2-Pad1)"))
    (pad 4 smd rect (at -4.92125 -1.1 180) (size 0.8763 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at -4.92125 0 180) (size 0.8763 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -4.92125 1.1 180) (size 0.8763 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 18 +BATT))
    (pad 7 smd rect (at -4.92125 2.200001 180) (size 0.8763 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (pad 8 smd rect (at -4.92125 3.299998 180) (size 0.8763 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (pad 9 smd rect (at -4.92125 4.399999 180) (size 0.8763 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at 4.92125 4.400001 180) (size 0.8763 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 11 smd rect (at 4.92125 3.300001 180) (size 0.8763 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 12 smd rect (at 4.92125 2.200001 180) (size 0.8763 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 13 smd rect (at 4.92125 1.1 180) (size 0.8763 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at 4.92125 0 180) (size 0.8763 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C3-Pad1)"))
    (pad 15 smd rect (at 4.92125 -1.1 180) (size 0.8763 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U1-Pad15)"))
    (pad 16 smd rect (at 4.92125 -2.200001 180) (size 0.8763 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at 4.92125 -3.299998 180) (size 0.8763 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad17)"))
    (pad 18 smd rect (at 4.92125 -4.399999 180) (size 0.8763 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad18)"))
  )
  (module teensy:Teensy35_36 (layer F.Cu) (tedit 5ED51FDE)
    (at 139.065 111.125 90)
    (fp_text reference U2 (at 0 -10.16 90) (layer F.SilkS))
    (fp_text value Teensy3.5 (at 0 10.16 90) (layer F.Fab))
    (fp_text user MK66FX1MBVMD18/ (at 1.27 0 90) (layer F.SilkS))
    (fp_text user MK64FX512VMD12 (at 1.27 1.143 90) (layer F.SilkS))
    (pad 17 thru_hole circle (at 11.43 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 53 "Net-(U2-Pad17)"))
    (pad 18 thru_hole circle (at 13.97 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 54 "Net-(U2-Pad18)"))
    (pad 19 thru_hole circle (at 16.51 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 75 "Net-(U2-Pad19)"))
    (pad 20 thru_hole circle (at 19.05 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 76 "Net-(U2-Pad20)"))
    (pad 16 thru_hole circle (at 8.89 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 52 "Net-(U2-Pad16)"))
    (pad 15 thru_hole circle (at 6.35 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +3V3))
    (pad 14 thru_hole circle (at 3.81 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 Teensy_MISO_0))
    (pad 21 thru_hole circle (at 21.59 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 77 "Net-(U2-Pad21)"))
    (pad 22 thru_hole circle (at 24.13 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 78 "Net-(U2-Pad22)"))
    (pad 23 thru_hole circle (at 26.67 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 79 "Net-(U2-Pad23)"))
    (pad 24 thru_hole circle (at 29.21 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 80 "Net-(U2-Pad24)"))
    (pad 25 thru_hole circle (at 16.51 5.08 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 81 "Net-(U2-Pad25)"))
    (pad 26 thru_hole circle (at 16.51 2.54 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 82 "Net-(U2-Pad26)"))
    (pad 27 thru_hole circle (at 16.51 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 83 "Net-(U2-Pad27)"))
    (pad 28 thru_hole circle (at 16.51 -2.54 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 84 "Net-(U2-Pad28)"))
    (pad 29 thru_hole circle (at 16.51 -5.08 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 85 "Net-(U2-Pad29)"))
    (pad 30 thru_hole circle (at 29.21 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 Teensy_UART_5_Tx))
    (pad 31 thru_hole circle (at 26.67 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 Teensy_UART_5_RX))
    (pad 32 thru_hole circle (at 24.13 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 Teensy_GPIO_35))
    (pad 33 thru_hole circle (at 21.59 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 Teensy_GPIO_36))
    (pad 34 thru_hole circle (at 19.05 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 47 IMU_SCL))
    (pad 35 thru_hole circle (at 16.51 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 48 IMU_SDA))
    (pad 36 thru_hole circle (at 13.97 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 86 "Net-(U2-Pad36)"))
    (pad 37 thru_hole circle (at 11.43 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 87 "Net-(U2-Pad37)"))
    (pad 13 thru_hole circle (at 1.27 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 Teensy_MOSI_0))
    (pad 12 thru_hole circle (at -1.27 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 37 Teensy_UART_2_TX))
    (pad 11 thru_hole circle (at -3.81 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 36 Teensy_UART_2_RX))
    (pad 10 thru_hole circle (at -6.35 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 88 "Net-(U2-Pad10)"))
    (pad 9 thru_hole circle (at -8.89 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 51 "Net-(U2-Pad9)"))
    (pad 8 thru_hole circle (at -11.43 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 89 "Net-(U2-Pad8)"))
    (pad 7 thru_hole circle (at -13.97 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 90 "Net-(U2-Pad7)"))
    (pad 6 thru_hole circle (at -16.51 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 91 "Net-(U2-Pad6)"))
    (pad 5 thru_hole circle (at -19.05 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 50 "Net-(U2-Pad5)"))
    (pad 4 thru_hole circle (at -21.59 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 49 "Net-(U2-Pad4)"))
    (pad 3 thru_hole circle (at -24.13 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 92 "Net-(U2-Pad3)"))
    (pad 2 thru_hole circle (at -26.67 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 93 "Net-(U2-Pad2)"))
    (pad 1 thru_hole rect (at -29.21 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 38 thru_hole circle (at 8.89 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 94 "Net-(U2-Pad38)"))
    (pad 39 thru_hole circle (at 6.35 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 40 thru_hole circle (at 3.81 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 Teensy_SCK_0))
    (pad 41 thru_hole circle (at 1.27 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 95 "Net-(U2-Pad41)"))
    (pad 42 thru_hole circle (at -1.27 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 Teensy_CS_IMU))
    (pad 43 thru_hole circle (at -3.81 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 35 Teensy_Iridium_OnOff))
    (pad 44 thru_hole circle (at -6.35 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 40 Teensy_UART_DTR))
    (pad 45 thru_hole circle (at -8.89 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 39 Teensy_UART_CTS))
    (pad 46 thru_hole circle (at -11.43 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 38 Teensy_UART_RTS))
    (pad 47 thru_hole circle (at -13.97 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 28 Teensy_CS_Temp))
    (pad 48 thru_hole circle (at -16.51 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 96 "Net-(U2-Pad48)"))
    (pad 49 thru_hole circle (at -19.05 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 29 MUX_Temp_1))
    (pad 50 thru_hole circle (at -21.59 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 30 MUX_Temp_2))
    (pad 51 thru_hole circle (at -24.13 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 +3V3))
    (pad 52 thru_hole circle (at -26.67 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 97 "Net-(U2-Pad52)"))
    (pad 53 thru_hole circle (at -29.21 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 +5V))
    (pad 54 thru_hole circle (at -26.67 -5.08 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 98 "Net-(U2-Pad54)"))
    (pad 55 thru_hole circle (at -21.59 -5.08 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 99 "Net-(U2-Pad55)"))
    (pad 56 thru_hole circle (at -19.05 -5.08 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 100 "Net-(U2-Pad56)"))
    (pad 57 thru_hole circle (at -16.51 -5.08 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 101 "Net-(U2-Pad57)"))
    (pad 58 thru_hole circle (at -22.86 4.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 59 thru_hole circle (at -20.32 4.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 60 thru_hole circle (at -17.78 4.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 61 thru_hole circle (at -15.24 4.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 62 thru_hole circle (at -12.7 4.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KICAD_USER_DIR}/teensy.pretty/Teensy_3.6_Assembly.STEP
      (offset (xyz -30.48 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OKX-T5-D12N-C:OKX-T5-D12N-C (layer F.Cu) (tedit 0)
    (at 120.65 134.62 90)
    (fp_text reference U3 (at 10.16 2.286 90) (layer F.SilkS))
    (fp_text value OKX-T_5-D12N-C (at 10.16 2.286 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at -2.54 0 90) (layer F.SilkS))
    (fp_text user * (at -1.27 0 90) (layer F.Fab))
    (fp_text user * (at -1.27 0 90) (layer F.Fab))
    (fp_text user * (at -2.54 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.9558 1.9558) (drill 1.4478) (layers *.Cu *.Mask)
      (net 103 +5VD))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.9558 1.9558) (drill 1.4478) (layers *.Cu *.Mask)
      (net 43 "Net-(R3-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.9558 1.9558) (drill 1.4478) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 4 thru_hole circle (at 17.78 0 90) (size 1.9558 1.9558) (drill 1.4478) (layers *.Cu *.Mask)
      (net 32 "Net-(D1-Pad1)"))
    (pad 5 thru_hole circle (at 20.32 0 90) (size 1.9558 1.9558) (drill 1.4478) (layers *.Cu *.Mask)
      (net 55 "Net-(U3-Pad5)"))
  )
  (module TPS22943:TPS22943DCKR (layer F.Cu) (tedit 5FBCFE93)
    (at 154.432 88.9 270)
    (fp_text reference U4 (at 0.232 -1.9064 90) (layer F.SilkS))
    (fp_text value TPS22943DCKR (at -2.54 -2.032 270) (layer F.Fab))
    (pad 1 smd rect (at -0.96 -0.65 270) (size 1.19 0.4) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at -0.96 0 270) (size 1.19 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 3 smd rect (at -0.96 0.65 270) (size 1.19 0.4) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(R4-Pad2)"))
    (pad 4 smd rect (at 0.96 0.65 270) (size 1.19 0.4) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U1-Pad13)"))
    (pad 5 smd rect (at 0.96 -0.65 270) (size 1.19 0.4) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C3-Pad1)"))
  )
  (module Drifter_Temp_IMU:MinIMU_9_v5 (layer F.Cu) (tedit 5F9B70A6)
    (at 161.29 122.555 90)
    (fp_text reference U5 (at 0 0.5 90) (layer F.SilkS))
    (fp_text value MinIMU_9_v5 (at 0 -0.5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -8.73 2.83 90) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 47 IMU_SCL))
    (pad 2 thru_hole circle (at -8.73 0.29 90) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 48 IMU_SDA))
    (pad 3 thru_hole circle (at -8.73 -2.25 90) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 4 thru_hole circle (at -8.73 -4.79 90) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 34 +5V))
    (pad 5 thru_hole circle (at -8.73 -7.33 90) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 102 "Net-(U5-Pad5)"))
    (pad 6 thru_hole circle (at -6.19 -2.25 90) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 7.8 1.6 90) (size 2.8 2.8) (drill 2.18) (layers *.Cu *.Mask))
  )
  (module BK-5058:BK-5058 (layer F.Cu) (tedit 5FBD067E)
    (at 163.83 107.95 180)
    (fp_text reference BT1 (at -8.325 -4.135) (layer F.SilkS))
    (fp_text value BK-5058 (at -4.515 4.135) (layer F.Fab))
    (pad S+1 thru_hole circle (at -5 1.8 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 +BATT))
    (pad S+2 thru_hole circle (at 5 1.8 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 +BATT))
    (pad - thru_hole circle (at 0 -1.8 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 GND))
  )
  (gr_text --Batt (at 97.028 116.84) (layer F.SilkS))
  (gr_text +Batt (at 98.044 121.92) (layer F.SilkS))
  (gr_text "Dog Ball Drifter\nUSNA Oceanography\nV 4.0" (at 112.268 69.596) (layer F.SilkS))
  (gr_text "Iridium Pwr" (at 97.028 104.14) (layer F.SilkS))
  (gr_text "Sat. Visable" (at 97.028 107.696) (layer F.SilkS))
  (gr_text "Bottom Therm." (at 132.588 57.912) (layer F.SilkS))
  (gr_text "TOP Therm." (at 163.068 69.596) (layer F.SilkS))
  (gr_circle (center 135.255 100.965) (end 180.255 100.965) (layer Edge.Cuts) (width 0.15))
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 201.676 53.848) (xy 202.692 152.4) (xy 71.12 152.908) (xy 70.104 52.832)
      )
    )
  )
  (zone (net 9) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 201.676 54.356) (xy 202.692 151.892) (xy 71.628 152.4) (xy 70.104 53.34)
      )
    )
  )
)
