<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="29.1592" y2="0" width="0" layer="20"/>
<wire x1="29.1592" y1="0" x2="29.1592" y2="39.7764" width="0" layer="20"/>
<wire x1="29.1592" y1="39.7764" x2="0" y2="39.7764" width="0" layer="20"/>
<wire x1="0" y1="39.7764" x2="0" y2="0" width="0" layer="20"/>
<text>LINBUS BEEPER</text>
<text>REV-B</text>
<text>12V</text>
<text>GND</text>
<text>LIN</text>
<text>GND</text>
<text>5V</text>
<text>1</text>
<text>DTR</text>
<text>+</text>
<text>+</text>
<text>RX</text>
<text>TX</text>
<text>CTS</text>
<text>1</text>
<text>LINBUS BEEPER - REV B</text>
<text>ICSP</text>
<text>FEB/2014</text>
</plain>
<libraries>
<library name="beeper">
<packages>
<package name="SO-08">
</package>
<package name="AL60P">
</package>
<package name="1206-LED">
</package>
<package name="1206">
</package>
<package name="RESONATOR-SMD">
</package>
<package name="R0805">
</package>
<package name="C0805">
</package>
<package name="UD-6,3X5,8_NICHICON">
</package>
<package name="A/3216-18R">
</package>
<package name="1X03">
</package>
<package name="1X06">
</package>
<package name="2X03">
</package>
<package name="SOD123FL">
</package>
<package name="SOT23-BEC">
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R5" library="beeper" package="R0805" value="3K3">
<attribute name="NAME"/>
</element>
<element name="R6" library="beeper" package="R0805" value="3K3">
<attribute name="NAME"/>
</element>
<element name="C6" library="beeper" package="C0805" value="220pF">
<attribute name="NAME"/>
</element>
<element name="J1" library="beeper" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="beeper" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C7" library="beeper" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R1" library="beeper" package="R0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R2" library="beeper" package="R0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="J4" library="beeper" package="2X03" value="ICSP">
<attribute name="NAME"/>
</element>
<element name="R3" library="beeper" package="R0805" value="3K3">
<attribute name="NAME"/>
</element>
<element name="T1" library="beeper" package="SOT23-BEC" value="MMBT3904">
<attribute name="NAME"/>
</element>
<element name="R4" library="beeper" package="R0805" value="200R">
<attribute name="NAME"/>
</element>
<element name="R8" library="beeper" package="R0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="U1" library="beeper" package="SO-08" value="ATA6631">
<attribute name="NAME"/>
</element>
<element name="J3" library="beeper" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="beeper" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="beeper" package="SOD123FL" value="MBR0540">
<attribute name="NAME"/>
</element>
<element name="U2" library="beeper" package="TQFP32-08" value="ATMEGA328">
<attribute name="NAME"/>
</element>
<element name="D2" library="beeper" package="SOD123FL" value="MBR0540">
<attribute name="NAME"/>
</element>
<element name="D3" library="beeper" package="SOD123FL" value="MBR0540">
<attribute name="NAME"/>
</element>
<element name="X1" library="beeper" package="RESONATOR-SMD" value="16MHz">
<attribute name="NAME"/>
</element>
<element name="SP1" library="beeper" package="AL60P" value="WT-1205">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="D4" library="beeper" package="SOD123FL" value="MBR0540">
<attribute name="NAME"/>
</element>
<element name="D5" library="beeper" package="1206-LED" value="RED">
<attribute name="NAME"/>
</element>
<element name="D6" library="beeper" package="1206-LED" value="GREEN">
<attribute name="NAME"/>
</element>
<element name="C1" library="beeper" package="UD-6,3X5,8_NICHICON" value="22uF 40V">
<attribute name="NAME"/>
</element>
<element name="C2" library="beeper" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C5" library="beeper" package="A/3216-18R" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="beeper" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="F1" library="beeper" package="1206" value="250ma Slow">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J3" pad="2"/>
<contactref element="J3" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="5"/>
<contactref element="U2" pad="21"/>
<contactref element="J4" pad="6"/>
<contactref element="T1" pad="E"/>
<contactref element="X1" pad="2"/>
<contactref element="D5" pad="C"/>
<contactref element="D6" pad="C"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="-"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="R6" pad="1"/>
<contactref element="D6" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="R5" pad="1"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="RESET">
<contactref element="J4" pad="5"/>
<contactref element="C7" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="U2" pad="29"/>
</signal>
<signal name="LIN_RX">
<contactref element="U1" pad="5"/>
<contactref element="U2" pad="32"/>
</signal>
<signal name="LIN">
<contactref element="U1" pad="4"/>
<contactref element="C6" pad="1"/>
<contactref element="J1" pad="3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="+12V">
<contactref element="U1" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="C1" pad="+"/>
<contactref element="C2" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="DTR">
<contactref element="C7" pad="1"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="+5V">
<contactref element="J4" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="C3" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="18"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="+"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="SER_RX">
<contactref element="R2" pad="1"/>
<contactref element="U2" pad="30"/>
</signal>
<signal name="TXO">
<contactref element="R2" pad="2"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="SER_TX">
<contactref element="R1" pad="1"/>
<contactref element="U2" pad="31"/>
</signal>
<signal name="RXI">
<contactref element="R1" pad="2"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="VBAT">
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="S-5V">
<contactref element="J3" pad="3"/>
<contactref element="D2" pad="A"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="MOSI/LIN_ERROR">
<contactref element="J4" pad="4"/>
<contactref element="U2" pad="15"/>
</signal>
<signal name="MISO/LIN_DATA">
<contactref element="J4" pad="1"/>
<contactref element="U2" pad="16"/>
</signal>
<signal name="SCK">
<contactref element="J4" pad="3"/>
<contactref element="U2" pad="17"/>
</signal>
<signal name="ERROR_LED">
<contactref element="R5" pad="2"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="FRAME_LED">
<contactref element="R6" pad="2"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="N$31">
<contactref element="T1" pad="C"/>
<contactref element="SP1" pad="2"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="BUZZER">
<contactref element="R3" pad="1"/>
<contactref element="U2" pad="9"/>
</signal>
<signal name="N$19">
<contactref element="T1" pad="B"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="R4" pad="1"/>
<contactref element="SP1" pad="1"/>
<contactref element="D4" pad="C"/>
</signal>
<signal name="XTAL1">
<contactref element="U2" pad="7"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="XTAL2">
<contactref element="X1" pad="1"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="F1" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$5">
</signal>
<signal name="N$1">
</signal>
<signal name="GP_DEBUG">
<contactref element="U2" pad="10"/>
</signal>
<signal name="LIN_TICK">
<contactref element="U2" pad="1"/>
</signal>
<signal name="LIN_BREAK">
<contactref element="U2" pad="23"/>
</signal>
<signal name="LIN_ISR">
<contactref element="U2" pad="26"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
