(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 22)
    (no_connects 0)
    (area 101.924999 102.924999 163.075001 137.075001)
    (thickness 1.6)
    (drawings 20)
    (tracks 78)
    (zones 0)
    (modules 13)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.5 1.75)
    (pad_drill 2.25)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/home/harrison/Documents/kicad/transverter control board/gerber files/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(D2-Pad2)")
  (net 4 "Net-(D3-Pad2)")
  (net 5 "Net-(D3-Pad1)")
  (net 6 "Net-(K1-Pad3)")
  (net 7 "Net-(K1-Pad4)")
  (net 8 "Net-(K1-Pad5)")
  (net 9 "Net-(K1-Pad6)")
  (net 10 "Net-(K1-Pad7)")
  (net 11 "Net-(K1-Pad8)")
  (net 12 "Net-(K2-Pad3)")
  (net 13 "Net-(K2-Pad4)")
  (net 14 "Net-(K2-Pad6)")
  (net 15 "Net-(K2-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(K1-Pad3)")
    (add_net "Net-(K1-Pad4)")
    (add_net "Net-(K1-Pad5)")
    (add_net "Net-(K1-Pad6)")
    (add_net "Net-(K1-Pad7)")
    (add_net "Net-(K1-Pad8)")
    (add_net "Net-(K2-Pad3)")
    (add_net "Net-(K2-Pad4)")
    (add_net "Net-(K2-Pad6)")
    (add_net "Net-(K2-Pad7)")
  )
  (module relays:I395PS-Series (layer F.Cu) (tedit 59F7EEB6)
    (at 137 114)
    (fp_text reference K2 (at 0 -3.31) (layer F.SilkS))
    (fp_text value RELAY_I395PS_series (at 0 -4.31) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.75 5) (drill 2.25) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D3-Pad2)"))
    (pad 2 thru_hole oval (at 14 0) (size 2.75 5) (drill 2.25) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
    (pad 3 thru_hole oval (at 2 7.25) (size 5 2.75) (drill 2.25) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(K2-Pad6)"))
    (pad 4 thru_hole oval (at 2 13.25) (size 5 2.75) (drill 2.25) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(K2-Pad4)"))
    (pad 5 thru_hole oval (at 2 18) (size 5 2.75) (drill 2.25) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(K1-Pad7)"))
    (pad 6 thru_hole oval (at 12 7.25) (size 5 2.75) (drill 2.25) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(K2-Pad3)"))
    (pad 7 thru_hole oval (at 12 13.25) (size 5 2.75) (drill 2.25) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(K2-Pad7)"))
    (pad 8 thru_hole oval (at 12 18) (size 5 2.75) (drill 2.25) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(K1-Pad4)"))
    (model "/home/harrison/Documents/kicad/transverter control board/untitled.x3d"
      (at (xyz 0.28 -0.33 0.55))
      (scale (xyz 150 150 150))
      (rotate (xyz 90 0 0))
    )
  )
  (module I395PS-Series (layer F.Cu) (tedit 59F7EE28)
    (at 114 114)
    (fp_text reference K1 (at 0 -3.31) (layer F.SilkS))
    (fp_text value RELAY_I395PS_series (at 0 -4.31) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.75 5) (drill 2.25) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 14 0) (size 2.75 5) (drill 2.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2 7.25) (size 5 2.75) (drill 2.25) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(K1-Pad3)"))
    (pad 4 thru_hole oval (at 2 13.25) (size 5 2.75) (drill 2.25) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(K1-Pad4)"))
    (pad 5 thru_hole oval (at 2 18) (size 5 2.75) (drill 2.25) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(K1-Pad5)"))
    (pad 6 thru_hole oval (at 12 7.25) (size 5 2.75) (drill 2.25) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(K1-Pad6)"))
    (pad 7 thru_hole oval (at 12 13.25) (size 5 2.75) (drill 2.25) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(K1-Pad7)"))
    (pad 8 thru_hole oval (at 12 18) (size 5 2.75) (drill 2.25) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(K1-Pad8)"))
    (model "../../../../../home/harrison/Documents/kicad/transverter control board/untitled.x3d"
      (at (xyz 0.28 -0.33 0.55))
      (scale (xyz 150 150 150))
      (rotate (xyz 90 0 0))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Vertical_KathodeUp (layer F.Cu) (tedit 59F7AB92)
    (at 135 105 180)
    (descr "Diode, DO-41, SOD81, Vertica,l Anode Up,")
    (tags "Diode, DO-41, SOD81, Vertical, Anode Up, 1N4007, SB140,")
    (fp_text reference D4 (at -2 -1 180) (layer F.SilkS))
    (fp_text value D_Small (at 0 -2.7 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Vertical_AnodeUp (layer F.Cu) (tedit 59F7AB8A)
    (at 123 105)
    (descr "Diode, DO-41, SOD81, Vertical, Anode Up,")
    (tags "Diode, DO-41, SOD81, Vertical, Anode Up, 1N4007, SB140,")
    (fp_text reference D1 (at -2.5 1) (layer F.SilkS))
    (fp_text value D_Small (at 0.05 -2) (layer F.Fab))
    (fp_text user A (at 2.794 1.651) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 59F7AB9D)
    (at 158.5 111.5 90)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D2 (at 6 -1.5 360) (layer F.SilkS))
    (fp_text value LED (at 1.524 -3.937 90) (layer F.Fab))
    (fp_text user K (at -1.905 1.905 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Vertical_AnodeUp (layer F.Cu) (tedit 59F7AB85)
    (at 111 105)
    (descr "Diode, DO-41, SOD81, Vertical, Anode Up,")
    (tags "Diode, DO-41, SOD81, Vertical, Anode Up, 1N4007, SB140,")
    (fp_text reference D3 (at -2.5 0) (layer F.SilkS))
    (fp_text value D_Small (at 0.05 -2) (layer F.Fab))
    (fp_text user A (at 2.794 1.651) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D3-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 59F8ABB7)
    (at 107 120)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -2) (layer F.SilkS))
    (fp_text value "IF in" (at 0 5.588) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(K1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(K1-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 59F8AB99)
    (at 158 127.5)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -2) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(K2-Pad7)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(K2-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 59F8ABBB)
    (at 107 113)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at -0.5 -2.5) (layer F.SilkS))
    (fp_text value PTT (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 59F8ABB1)
    (at 107 129.5 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 4.5 180) (layer F.SilkS))
    (fp_text value "HF Ant" (at 0 5.588 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(K1-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(K1-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 59F8ABA2)
    (at 158 120.5)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -2) (layer F.SilkS))
    (fp_text value Transverter (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(K2-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(K2-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 59F7AB94)
    (at 139.5 105)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 13 -0.5) (layer F.SilkS))
    (fp_text value R (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 59F8ABA7)
    (at 158 116)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -2) (layer F.SilkS))
    (fp_text value "Power switch" (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text TRANSVTR (at 161 122.5 90) (layer F.SilkS))
  (gr_text "HF Ant" (at 104 128.5 270) (layer F.SilkS))
  (gr_text +12V (at 161 116.5 90) (layer F.SilkS))
  (gr_text "IF In" (at 161 128.5 90) (layer F.SilkS))
  (gr_text "IF Out" (at 104 121.5 270) (layer F.SilkS))
  (gr_text PTT (at 104 114 270) (layer F.SilkS))
  (gr_text "Rev 1.1\nOctober 2017" (at 121 117) (layer B.SilkS))
  (gr_text "VA2HK Transverter\nControler board" (at 144 118) (layer B.SilkS))
  (gr_circle (center 104.5 105.5) (end 106 105.5) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 160.5 105.5) (end 159 105.5) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 160.5 134.5) (end 162 134.5) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 104.5 134.5) (end 103 134.5) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 104 105) (end 102 105) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 104 135) (end 104 137) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 161 135) (end 163 135) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 161 105) (end 161 103) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104 103) (end 161 103) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102 135) (end 102 105) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161 137) (end 104 137) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163 105) (end 163 135) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163 137) (xy 102 137) (xy 102 103) (xy 163 103) (xy 163 137)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163 137) (xy 102 137) (xy 102 103) (xy 163 103) (xy 163 137)
      )
    )
  )
)
