<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="20.32" y2="0" width="0" layer="20"/>
<wire x1="20.32" y1="0" x2="20.32" y2="44.45" width="0" layer="20"/>
<wire x1="20.32" y1="44.45" x2="0" y2="44.45" width="0" layer="20"/>
<wire x1="0" y1="44.45" x2="0" y2="0" width="0" layer="20"/>
<text>Paua 2</text>
<text>BigNoise</text>
<text>c2014</text>
<text>+IN</text>
<text>+IN</text>
<text>-IN</text>
<text>-IN</text>
<text>+OUT</text>
<text>+OUT</text>
<text>GND</text>
<text>GND</text>
<text>BigNoise</text>
<text>Paua 2</text>
<text>GND</text>
</plain>
<libraries>
<library name="diodes">
<description>&lt;b&gt;Diodes&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Zener 1N47xx (as in protection for the MOSFET in the AMZ MOSFET Booster)
&lt;li&gt;rectifier 1N4001-1N4008 (for polarity reversal protection in power supply sections)
&lt;li&gt;clipping 1N914 (as in a TS808)
&lt;li&gt;LED (light emitting diode, 3mm and 5mm)
&lt;li&gt;mostly gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DO41-2">
<description>&lt;b&gt;DO-41 0.2" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="capacitors-elec">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="080_035">
<description>&lt;b&gt;8mm diameter, 3.5 mm lead spacing&lt;/b&gt;
&lt;p&gt;7mm height/length and more</description>
</package>
<package name="063_025">
<description>&lt;b&gt;6.3mm diameter, 2.5 mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="capacitors-film">
<description>&lt;b&gt;Capacitors, Ceramic&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;very small capacitances: 1 - 1000pF
&lt;/ul&gt;</description>
<packages>
<package name="BOX_SMALL">
</package>
</packages>
</library>
<library name="regulators">
<packages>
<package name="TO220-STANDING">
</package>
</packages>
</library>
<library name="potentiometers">
<packages>
<package name="2262_TRIM">
<description>&lt;b&gt;Potentiometer&lt;/b&gt;&lt;p&gt;
1/4" on-board trim potentiometer</description>
</package>
</packages>
</library>
<library name="resistors">
<description>&lt;b&gt;Resistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;6mm long -- the size of 1/4 watt resistors
&lt;li&gt; all resistor values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="R0207/3">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 6mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 3 holes

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="diodes" package="DO41-2" value="4001"/>
<element name="D2" library="diodes" package="DO41-2" value="4001"/>
<element name="D3" library="diodes" package="DO41-2" value="4001"/>
<element name="D4" library="diodes" package="DO41-2" value="4001"/>
<element name="C1" library="capacitors-elec" package="080_035" value="1000uF 35V"/>
<element name="C2" library="capacitors-film" package="BOX_SMALL" value="0.1uF"/>
<element name="LM317" library="regulators" package="TO220-STANDING" value=""/>
<element name="D5" library="diodes" package="DO41-2" value="4001"/>
<element name="POT1" library="potentiometers" package="2262_TRIM" value="1K"/>
<element name="R1" library="resistors" package="R0207/3" value="1K"/>
<element name="R2" library="resistors" package="R0207/3" value="240R"/>
<element name="C3" library="capacitors-elec" package="063_025" value="10uF"/>
<element name="D6" library="diodes" package="DO41-2" value="4001"/>
<element name="C4" library="capacitors-elec" package="063_025" value="47uF"/>
<element name="C5" library="capacitors-film" package="BOX_SMALL" value="0.1uF"/>
<element name="D7" library="diodes" package="DO41-2" value="5817"/>
<element name="D8" library="diodes" package="DO41-2" value="5817"/>
<element name="C6" library="capacitors-elec" package="080_035" value="470uF 35V"/>
<element name="C7" library="capacitors-elec" package="080_035" value="470uF 35V"/>
<element name="INDUCTOR" library="resistors" package="R0207/3" value=".22mH"/>
</elements>
<signals>
<signal name="ACIN">
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="A"/>
<contactref element="INDUCTOR" pad="1"/>
<contactref element="C7" pad="+"/>
</signal>
<signal name="N$3">
<contactref element="D4" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="LM317" pad="P$3"/>
<contactref element="C1" pad="+"/>
<contactref element="C2" pad="1"/>
<contactref element="D5" pad="C"/>
</signal>
<signal name="GND">
<contactref element="D1" pad="A"/>
<contactref element="D3" pad="A"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="C3" pad="-"/>
<contactref element="C4" pad="-"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="LM317" pad="P$1"/>
<contactref element="POT1" pad="3"/>
</signal>
<signal name="+OUT">
<contactref element="LM317" pad="P$2"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="+"/>
<contactref element="D6" pad="C"/>
<contactref element="R2" pad="2"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="R2" pad="1"/>
<contactref element="POT1" pad="2"/>
<contactref element="D6" pad="A"/>
<contactref element="C3" pad="+"/>
</signal>
<signal name="N$16">
<contactref element="POT1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="D8" pad="C"/>
<contactref element="INDUCTOR" pad="2"/>
<contactref element="C6" pad="+"/>
<contactref element="D7" pad="C"/>
</signal>
<signal name="+IN">
<contactref element="D8" pad="A"/>
</signal>
<signal name="-IN">
<contactref element="D3" pad="C"/>
<contactref element="D4" pad="A"/>
<contactref element="D7" pad="A"/>
<contactref element="C6" pad="-"/>
<contactref element="C7" pad="-"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
