(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 123)
    (no_connects 0)
    (area -0.075001 -95.960001 90.245001 0.075001)
    (thickness 1.6)
    (drawings 16)
    (tracks 440)
    (zones 0)
    (modules 29)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEEF1F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 2)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /tmp/))
  )
  (net 0 "")
  (net 1 /qam_encoder/IQ_CLK)
  (net 2 /qam_encoder/s6)
  (net 3 /qam_encoder/SCK)
  (net 4 GND)
  (net 5 /qam_encoder/MOSI)
  (net 6 /qam_encoder/s5)
  (net 7 +3V3)
  (net 8 "Net-(C4-Pad1)")
  (net 9 +5V)
  (net 10 "/Base band/UART_RX")
  (net 11 "/Base band/UART_TX")
  (net 12 "/Myriad RF-1/IQSEL")
  (net 13 "/Myriad RF-1/IQ0")
  (net 14 "/Base band/BROADBAND")
  (net 15 "/Myriad RF-1/CLK_24M_IN")
  (net 16 "/Myriad RF-1/TXEN")
  (net 17 "/Myriad RF-1/IQ11")
  (net 18 "/Base band/RADIO_~RESET")
  (net 19 "/Base band/SPI_MISO")
  (net 20 "/Base band/SPI_CS")
  (net 21 "/Base band/~RST")
  (net 22 "/Base band/TEST")
  (net 23 "/Base band/TDO")
  (net 24 "/Base band/TDI")
  (net 25 "/Base band/TMS")
  (net 26 "/Base band/TCK")
  (net 27 "Net-(U2-Pad3)")
  (net 28 "Net-(U3-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net "/Base band/BROADBAND")
    (add_net "/Base band/RADIO_~RESET")
    (add_net "/Base band/SPI_CS")
    (add_net "/Base band/SPI_MISO")
    (add_net "/Base band/TCK")
    (add_net "/Base band/TDI")
    (add_net "/Base band/TDO")
    (add_net "/Base band/TEST")
    (add_net "/Base band/TMS")
    (add_net "/Base band/UART_RX")
    (add_net "/Base band/UART_TX")
    (add_net "/Base band/~RST")
    (add_net "/Myriad RF-1/CLK_24M_IN")
    (add_net "/Myriad RF-1/IQ0")
    (add_net "/Myriad RF-1/IQ11")
    (add_net "/Myriad RF-1/IQSEL")
    (add_net "/Myriad RF-1/TXEN")
    (add_net /qam_encoder/IQ_CLK)
    (add_net /qam_encoder/MOSI)
    (add_net /qam_encoder/SCK)
    (add_net /qam_encoder/s5)
    (add_net /qam_encoder/s6)
    (add_net GND)
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U3-Pad3)")
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 85.09 -5.08)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference MK4 (at 0 -4.2) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 82.55 -90.805)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference MK3 (at 0 -4.2) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 5.08 -5.08)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference MK2 (at 0 -4.2) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 8.89 -90.805)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference MK1 (at 0 -4.2) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module SAMTEC_ESQ-126-39-G-D:SAMTEC_ESQ-126-39-G-D (layer F.Cu) (tedit 598B9964)
    (at 13.97 -83.185 90)
    (fp_text reference J7 (at 1.27 -2.286 90) (layer F.SilkS))
    (fp_text value CONN_02X26 (at 1.27 31.75 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 2.54 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 2.54 2.54 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 5.08 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 2.54 5.08 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 0 7.62 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 2.54 7.62 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 0 10.16 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 2.54 10.16 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 0 12.7 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 2.54 12.7 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 0 15.24 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 2.54 15.24 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 0 17.78 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 2.54 17.78 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 0 20.32 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at 2.54 20.32 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 0 22.86 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 2.54 22.86 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at 0 25.4 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at 2.54 25.4 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 0 27.94 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at 2.54 27.94 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at 0 30.48 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 26 thru_hole circle (at 2.54 30.48 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 27 thru_hole circle (at 0 33.02 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 28 thru_hole circle (at 2.54 33.02 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 29 thru_hole circle (at 0 35.56 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 30 thru_hole circle (at 2.54 35.56 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 31 thru_hole circle (at 0 38.1 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 32 thru_hole circle (at 2.54 38.1 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 33 thru_hole circle (at 0 40.64 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 34 thru_hole circle (at 2.54 40.64 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 35 thru_hole circle (at 0 43.18 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 36 thru_hole circle (at 2.54 43.18 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 37 thru_hole circle (at 0 45.72 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 38 thru_hole circle (at 2.54 45.72 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 39 thru_hole circle (at 0 48.26 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 40 thru_hole circle (at 2.54 48.26 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 41 thru_hole circle (at 0 50.8 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 42 thru_hole circle (at 2.54 50.8 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 43 thru_hole circle (at 0 53.34 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 44 thru_hole circle (at 2.54 53.34 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 45 thru_hole circle (at 0 55.88 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 46 thru_hole circle (at 2.54 55.88 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 47 thru_hole circle (at 0 58.42 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 48 thru_hole circle (at 2.54 58.42 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 49 thru_hole circle (at 0 60.96 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 50 thru_hole circle (at 2.54 60.96 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 51 thru_hole circle (at 0 63.5 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 52 thru_hole circle (at 2.54 63.5 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (model SAMTEC_ESQ-126-39-G-D.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SAMTEC_ESQ-126-39-G-D:SAMTEC_ESQ-126-39-G-D (layer F.Cu) (tedit 598B9964)
    (at 13.97 -88.265 90)
    (fp_text reference J6 (at 1.27 -2.286 90) (layer F.SilkS))
    (fp_text value CONN_02X26 (at 1.27 31.75 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 2.54 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 2.54 2.54 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 5.08 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 2.54 5.08 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 0 7.62 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 2.54 7.62 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 0 10.16 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 2.54 10.16 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 0 12.7 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 2.54 12.7 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 0 15.24 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 2.54 15.24 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 0 17.78 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 2.54 17.78 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 0 20.32 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at 2.54 20.32 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 0 22.86 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 2.54 22.86 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at 0 25.4 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at 2.54 25.4 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 0 27.94 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at 2.54 27.94 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at 0 30.48 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 26 thru_hole circle (at 2.54 30.48 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 27 thru_hole circle (at 0 33.02 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 28 thru_hole circle (at 2.54 33.02 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 29 thru_hole circle (at 0 35.56 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 30 thru_hole circle (at 2.54 35.56 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 31 thru_hole circle (at 0 38.1 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 32 thru_hole circle (at 2.54 38.1 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 33 thru_hole circle (at 0 40.64 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 34 thru_hole circle (at 2.54 40.64 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 35 thru_hole circle (at 0 43.18 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 36 thru_hole circle (at 2.54 43.18 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 37 thru_hole circle (at 0 45.72 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 38 thru_hole circle (at 2.54 45.72 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 39 thru_hole circle (at 0 48.26 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 40 thru_hole circle (at 2.54 48.26 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 41 thru_hole circle (at 0 50.8 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 42 thru_hole circle (at 2.54 50.8 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 43 thru_hole circle (at 0 53.34 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 44 thru_hole circle (at 2.54 53.34 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 45 thru_hole circle (at 0 55.88 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 46 thru_hole circle (at 2.54 55.88 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 47 thru_hole circle (at 0 58.42 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 48 thru_hole circle (at 2.54 58.42 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 49 thru_hole circle (at 0 60.96 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 50 thru_hole circle (at 2.54 60.96 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 51 thru_hole circle (at 0 63.5 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (pad 52 thru_hole circle (at 2.54 63.5 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask))
    (model SAMTEC_ESQ-126-39-G-D.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 3M-2514-6002:3M-2514-6002 (layer F.Cu) (tedit 598B8B41)
    (at 15.24 -59.944 180)
    (fp_text reference J5 (at 1.524 21.082 180) (layer F.SilkS))
    (fp_text value JTAG (at 1.27 -5.842 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 "/Base band/TDO"))
    (pad 3 thru_hole circle (at 0 2.54 90) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 24 "/Base band/TDI"))
    (pad 5 thru_hole circle (at 0 5.08 90) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 25 "/Base band/TMS"))
    (pad 7 thru_hole circle (at 0 7.62 90) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 26 "/Base band/TCK"))
    (pad 9 thru_hole circle (at 0 10.16 90) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 11 thru_hole circle (at 0 12.7 90) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 21 "/Base band/~RST"))
    (pad 13 thru_hole circle (at 0 15.24 90) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 2.54 2.54 90) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (pad 6 thru_hole circle (at 2.54 5.08 90) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 2.54 7.62 90) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 22 "/Base band/TEST"))
    (pad 10 thru_hole circle (at 2.54 10.16 90) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 2.54 12.7 90) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 2.54 15.24 90) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask))
    (model 3M-2514-6002.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 29.972 -64.516 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C9 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 2.2n (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Mask)
      (net 21 "/Base band/~RST"))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DA-38:DA-38 (layer B.Cu) (tedit 598B587D)
    (at 23.368 -61.468 90)
    (fp_text reference U4 (at -7.45 0.15 360) (layer B.SilkS))
    (fp_text value MSP430FR5739DA (at -0.05 -0.05 90) (layer B.Fab))
    (pad 38 smd rect (at -5.85 3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 4 GND))
    (pad 37 smd rect (at -5.2 3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 3 /qam_encoder/SCK))
    (pad 36 smd rect (at -4.55 3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 20 "/Base band/SPI_CS"))
    (pad 35 smd rect (at -3.9 3.55 90) (size 0.4 2) (layers B.Cu B.Mask))
    (pad 34 smd rect (at -3.25 3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 7 +3V3))
    (pad 33 smd rect (at -2.6 3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 4 GND))
    (pad 32 smd rect (at -1.95 3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 8 "Net-(C4-Pad1)"))
    (pad 31 smd rect (at -1.3 3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 14 "/Base band/BROADBAND"))
    (pad 30 smd rect (at -0.65 3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 18 "/Base band/RADIO_~RESET"))
    (pad 29 smd rect (at 0 3.55 90) (size 0.4 2) (layers B.Cu B.Mask))
    (pad 28 smd rect (at 0.65 3.55 90) (size 0.4 2) (layers B.Cu B.Mask))
    (pad 27 smd rect (at 1.3 3.55 90) (size 0.4 2) (layers B.Cu B.Mask))
    (pad 26 smd rect (at 1.95 3.55 90) (size 0.4 2) (layers B.Cu B.Mask))
    (pad 25 smd rect (at 2.6 3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 16 "/Myriad RF-1/TXEN"))
    (pad 24 smd rect (at 3.25 3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 10 "/Base band/UART_RX"))
    (pad 23 smd rect (at 3.9 3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 11 "/Base band/UART_TX"))
    (pad 22 smd rect (at 4.55 3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 21 "/Base band/~RST"))
    (pad 21 smd rect (at 5.2 3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 22 "/Base band/TEST"))
    (pad 20 smd rect (at 5.85 3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 19 "/Base band/SPI_MISO"))
    (pad 1 smd rect (at -5.85 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 28 "Net-(U3-Pad3)"))
    (pad 2 smd rect (at -5.2 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 15 "/Myriad RF-1/CLK_24M_IN"))
    (pad 3 smd rect (at -4.55 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 4 GND))
    (pad 4 smd rect (at -3.9 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 7 +3V3))
    (pad 5 smd rect (at -3.25 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask))
    (pad 6 smd rect (at -2.6 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask))
    (pad 7 smd rect (at -1.95 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask))
    (pad 8 smd rect (at -1.3 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask))
    (pad 9 smd rect (at -0.65 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask))
    (pad 10 smd rect (at 0 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask))
    (pad 11 smd rect (at 0.65 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask))
    (pad 12 smd rect (at 1.3 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask))
    (pad 13 smd rect (at 1.95 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask))
    (pad 14 smd rect (at 2.6 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask))
    (pad 15 smd rect (at 3.25 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 23 "/Base band/TDO"))
    (pad 16 smd rect (at 3.9 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 24 "/Base band/TDI"))
    (pad 17 smd rect (at 4.55 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 25 "/Base band/TMS"))
    (pad 18 smd rect (at 5.2 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 26 "/Base band/TCK"))
    (pad 19 smd rect (at 5.85 -3.55 90) (size 0.4 2) (layers B.Cu B.Mask)
      (net 5 /qam_encoder/MOSI))
    (model DA-38.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223-3Lead_TabPin2 (layer F.Cu) (tedit 58CE4E7E)
    (at 14.224 -46.736 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U5 (at 0 -4.5 90) (layer F.SilkS))
    (fp_text value LM1117IMP-3.3 (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 3.15 0 90) (size 2 3.8) (layers F.Cu F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at -3.15 0 90) (size 2 1.5) (layers F.Cu F.Mask)
      (net 7 +3V3))
    (pad 3 smd rect (at -3.15 2.3 90) (size 2 1.5) (layers F.Cu F.Mask)
      (net 9 +5V))
    (pad 1 smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers F.Cu F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-16_4.4x5mm_Pitch0.65mm (layer B.Cu) (tedit 54130A77)
    (at 23.368 -45.72 180)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at 0 3.55 180) (layer B.SilkS))
    (fp_text value SN74LV175APWR (at 0 -3.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -2.95 2.275 180) (size 1.5 0.45) (layers B.Cu B.Mask)
      (net 16 "/Myriad RF-1/TXEN"))
    (pad 2 smd rect (at -2.95 1.625 180) (size 1.5 0.45) (layers B.Cu B.Mask)
      (net 12 "/Myriad RF-1/IQSEL"))
    (pad 3 smd rect (at -2.95 0.975 180) (size 1.5 0.45) (layers B.Cu B.Mask)
      (net 27 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -2.95 0.325 180) (size 1.5 0.45) (layers B.Cu B.Mask)
      (net 27 "Net-(U2-Pad3)"))
    (pad 5 smd rect (at -2.95 -0.325 180) (size 1.5 0.45) (layers B.Cu B.Mask)
      (net 6 /qam_encoder/s5))
    (pad 6 smd rect (at -2.95 -0.975 180) (size 1.5 0.45) (layers B.Cu B.Mask)
      (net 17 "/Myriad RF-1/IQ11"))
    (pad 7 smd rect (at -2.95 -1.625 180) (size 1.5 0.45) (layers B.Cu B.Mask)
      (net 13 "/Myriad RF-1/IQ0"))
    (pad 8 smd rect (at -2.95 -2.275 180) (size 1.5 0.45) (layers B.Cu B.Mask)
      (net 4 GND))
    (pad 9 smd rect (at 2.95 -2.275 180) (size 1.5 0.45) (layers B.Cu B.Mask)
      (net 2 /qam_encoder/s6))
    (pad 10 smd rect (at 2.95 -1.625 180) (size 1.5 0.45) (layers B.Cu B.Mask)
      (net 13 "/Myriad RF-1/IQ0"))
    (pad 11 smd rect (at 2.95 -0.975 180) (size 1.5 0.45) (layers B.Cu B.Mask))
    (pad 12 smd rect (at 2.95 -0.325 180) (size 1.5 0.45) (layers B.Cu B.Mask)
      (net 5 /qam_encoder/MOSI))
    (pad 13 smd rect (at 2.95 0.325 180) (size 1.5 0.45) (layers B.Cu B.Mask)
      (net 5 /qam_encoder/MOSI))
    (pad 14 smd rect (at 2.95 0.975 180) (size 1.5 0.45) (layers B.Cu B.Mask))
    (pad 15 smd rect (at 2.95 1.625 180) (size 1.5 0.45) (layers B.Cu B.Mask))
    (pad 16 smd rect (at 2.95 2.275 180) (size 1.5 0.45) (layers B.Cu B.Mask)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-16_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 8.128 -55.372)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/Base band/UART_RX"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/Base band/TEST"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x06_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 8.128 -59.944 180)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J4 (at 4.385 -2.27 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 4.385 14.97 180) (layer F.Fab))
    (fp_text user %R (at 2.77 6.35 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/Base band/UART_RX"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/Base band/UART_TX"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/Base band/~RST"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KEYSTONE_TP_5000-5004:KEYSTONE_TP_5000-5004 (layer F.Cu) (tedit 598A60A6)
    (at 8.128 -48.26 90)
    (fp_text reference J3 (at 0.05 2.15 90) (layer F.SilkS))
    (fp_text value 5V_RED (at 0 -2.159 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.54 2.54) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model Keystone-5000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KEYSTONE_TP_5000-5004:KEYSTONE_TP_5000-5004 (layer F.Cu) (tedit 598A60A6)
    (at 8.128 -43.688 90)
    (fp_text reference J2 (at 0.05 2.15 90) (layer F.SilkS))
    (fp_text value GND_BLACK (at 0 -2.159 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.54 2.54) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GND))
    (model Keystone-5000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module FX10A-80S:FX10A-80S (layer F.Cu) (tedit 598CFB57)
    (at 23.368 -56.007 90)
    (fp_text reference J1 (at -16.4 0 180) (layer F.SilkS))
    (fp_text value Myriad-RF1 (at 0 0 90) (layer F.Fab))
    (pad 89 smd rect (at -14.95 0 90) (size 1.6 3.1) (layers F.Cu F.Mask))
    (pad 90 smd rect (at 14.95 0 90) (size 1.6 3.1) (layers F.Cu F.Mask))
    (pad "" np_thru_hole circle (at -13.2 0 90) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 13.2 0 90) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -11.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 9 +5V))
    (pad 2 smd rect (at -11.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 9 +5V))
    (pad 3 smd rect (at -11.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 9 +5V))
    (pad 5 smd rect (at -10.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 7 smd rect (at -10.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 9 smd rect (at -9.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 81 smd rect (at -9 -3.05 90) (size 0.7 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 11 smd rect (at -8.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 13 smd rect (at -7.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 15 smd rect (at -7.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 17 smd rect (at -6.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 19 smd rect (at -6.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 12 "/Myriad RF-1/IQSEL"))
    (pad 21 smd rect (at -5.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 23 smd rect (at -5.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 13 "/Myriad RF-1/IQ0"))
    (pad 25 smd rect (at -4.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 13 "/Myriad RF-1/IQ0"))
    (pad 27 smd rect (at -4.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 29 smd rect (at -3.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 13 "/Myriad RF-1/IQ0"))
    (pad 83 smd rect (at -3 -3.05 90) (size 0.7 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 31 smd rect (at -2.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 13 "/Myriad RF-1/IQ0"))
    (pad 33 smd rect (at -1.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 13 "/Myriad RF-1/IQ0"))
    (pad 35 smd rect (at -1.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 13 "/Myriad RF-1/IQ0"))
    (pad 37 smd rect (at -0.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 39 smd rect (at -0.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 41 smd rect (at 0.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 43 smd rect (at 0.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 45 smd rect (at 1.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 47 smd rect (at 1.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 49 smd rect (at 2.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 85 smd rect (at 3 -3.05 90) (size 0.7 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 51 smd rect (at 3.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 53 smd rect (at 4.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 55 smd rect (at 4.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 57 smd rect (at 5.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 59 smd rect (at 5.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 61 smd rect (at 6.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 63 smd rect (at 6.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 65 smd rect (at 7.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 67 smd rect (at 7.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 69 smd rect (at 8.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 14 "/Base band/BROADBAND"))
    (pad 87 smd rect (at 9 -3.05 90) (size 0.7 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 71 smd rect (at 9.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 73 smd rect (at 10.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 75 smd rect (at 10.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 15 "/Myriad RF-1/CLK_24M_IN"))
    (pad 77 smd rect (at 11.25 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 79 smd rect (at 11.75 -3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 16 "/Myriad RF-1/TXEN"))
    (pad 4 smd rect (at -11.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 9 +5V))
    (pad 6 smd rect (at -10.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 8 smd rect (at -10.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 10 smd rect (at -9.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 82 smd rect (at -9 3.05 90) (size 0.7 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 12 smd rect (at -8.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 14 smd rect (at -7.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 16 smd rect (at -7.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 18 smd rect (at -6.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 20 smd rect (at -6.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 22 smd rect (at -5.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 24 smd rect (at -5.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 13 "/Myriad RF-1/IQ0"))
    (pad 26 smd rect (at -4.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 13 "/Myriad RF-1/IQ0"))
    (pad 28 smd rect (at -4.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 30 smd rect (at -3.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 13 "/Myriad RF-1/IQ0"))
    (pad 84 smd rect (at -3 3.05 90) (size 0.7 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 32 smd rect (at -2.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 13 "/Myriad RF-1/IQ0"))
    (pad 34 smd rect (at -1.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 13 "/Myriad RF-1/IQ0"))
    (pad 36 smd rect (at -1.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 17 "/Myriad RF-1/IQ11"))
    (pad 38 smd rect (at -0.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 40 smd rect (at -0.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 42 smd rect (at 0.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 44 smd rect (at 0.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 46 smd rect (at 1.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 48 smd rect (at 1.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 50 smd rect (at 2.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 86 smd rect (at 3 3.05 90) (size 0.7 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 52 smd rect (at 3.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 54 smd rect (at 4.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 56 smd rect (at 4.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 58 smd rect (at 5.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 60 smd rect (at 5.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 1 /qam_encoder/IQ_CLK))
    (pad 62 smd rect (at 6.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 64 smd rect (at 6.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 66 smd rect (at 7.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 18 "/Base band/RADIO_~RESET"))
    (pad 68 smd rect (at 7.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 5 /qam_encoder/MOSI))
    (pad 70 smd rect (at 8.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 19 "/Base band/SPI_MISO"))
    (pad 88 smd rect (at 9 3.05 90) (size 0.7 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 72 smd rect (at 9.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 3 /qam_encoder/SCK))
    (pad 74 smd rect (at 10.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 20 "/Base band/SPI_CS"))
    (pad 76 smd rect (at 10.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 78 smd rect (at 11.25 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask))
    (pad 80 smd rect (at 11.75 3.05 90) (size 0.3 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 91 thru_hole circle (at -19.65 0.5 90) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask))
    (pad 91 thru_hole circle (at 20.35 0.5 90) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask))
    (pad 91 thru_hole circle (at 20.35 38.7 90) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask))
    (pad 91 thru_hole circle (at -19.65 38.7 90) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask))
    (model FX10A-80S8-SV.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model MYRIAD-RF1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module D_SOD_923:D_SOD_923 (layer B.Cu) (tedit 598A5828)
    (at 10.16 -67.564)
    (fp_text reference D1 (at 0 -0.6) (layer B.SilkS))
    (fp_text value ESD9X3.3ST5G (at 0 0.6) (layer B.Fab))
    (pad 1 smd rect (at -0.42 0) (size 0.5 0.4) (layers B.Cu B.Mask)
      (net 10 "/Base band/UART_RX"))
    (pad 2 smd rect (at 0.42 0) (size 0.5 0.4) (layers B.Cu B.Mask)
      (net 4 GND))
    (model D_SOD_923.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SN74LVC74ADBR:SN74LVC74ADBR (layer B.Cu) (tedit 598A6E3E)
    (at 23.368 -51.816 180)
    (descr "SSOP14: plastic shrink small outline package; 14 leads; body width 5.3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot337-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 4.2 360) (layer B.SilkS))
    (fp_text value SN74LVC74ADBR (at 0 -4.2 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -3.45 1.95 180) (size 1.6 0.4) (layers B.Cu B.Mask)
      (net 16 "/Myriad RF-1/TXEN"))
    (pad 2 smd rect (at -3.45 1.3 180) (size 1.6 0.4) (layers B.Cu B.Mask)
      (net 2 /qam_encoder/s6))
    (pad 3 smd rect (at -3.45 0.65 180) (size 1.6 0.4) (layers B.Cu B.Mask)
      (net 3 /qam_encoder/SCK))
    (pad 4 smd rect (at -3.45 0 180) (size 1.6 0.4) (layers B.Cu B.Mask)
      (net 7 +3V3))
    (pad 5 smd rect (at -3.45 -0.65 180) (size 1.6 0.4) (layers B.Cu B.Mask)
      (net 1 /qam_encoder/IQ_CLK))
    (pad 6 smd rect (at -3.45 -1.3 180) (size 1.6 0.4) (layers B.Cu B.Mask)
      (net 2 /qam_encoder/s6))
    (pad 7 smd rect (at -3.45 -1.95 180) (size 1.6 0.4) (layers B.Cu B.Mask)
      (net 4 GND))
    (pad 8 smd rect (at 3.45 -1.95 180) (size 1.6 0.4) (layers B.Cu B.Mask))
    (pad 9 smd rect (at 3.45 -1.3 180) (size 1.6 0.4) (layers B.Cu B.Mask)
      (net 6 /qam_encoder/s5))
    (pad 10 smd rect (at 3.45 -0.65 180) (size 1.6 0.4) (layers B.Cu B.Mask)
      (net 7 +3V3))
    (pad 11 smd rect (at 3.45 0 180) (size 1.6 0.4) (layers B.Cu B.Mask)
      (net 1 /qam_encoder/IQ_CLK))
    (pad 12 smd rect (at 3.45 0.65 180) (size 1.6 0.4) (layers B.Cu B.Mask)
      (net 5 /qam_encoder/MOSI))
    (pad 13 smd rect (at 3.45 1.3 180) (size 1.6 0.4) (layers B.Cu B.Mask)
      (net 16 "/Myriad RF-1/TXEN"))
    (pad 14 smd rect (at 3.45 1.95 180) (size 1.6 0.4) (layers B.Cu B.Mask)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/SSOP-14_5.3x6.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module D_SOD_923:D_SOD_923 (layer B.Cu) (tedit 598A5828)
    (at 10.16 -70.104)
    (fp_text reference D2 (at 0 -0.6) (layer B.SilkS))
    (fp_text value ESD9X3.3ST5G (at 0 0.6) (layer B.Fab))
    (pad 1 smd rect (at -0.42 0) (size 0.5 0.4) (layers B.Cu B.Mask)
      (net 11 "/Base band/UART_TX"))
    (pad 2 smd rect (at 0.42 0) (size 0.5 0.4) (layers B.Cu B.Mask)
      (net 4 GND))
    (model D_SOD_923.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 17.78 -51.816 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 18.288 -45.72 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 17.272 -56.388 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 100n (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 29.972 -59.944 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value .47u (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers B.Cu B.Mask)
      (net 8 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers B.Cu B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 29.972 -55.372 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 4.7u (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 14.224 -41.148 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 1u (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Mask)
      (net 9 +5V))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 14.224 -52.324 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C8 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 29.972 -69.088 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 1.85 270) (layer B.SilkS))
    (fp_text value 47k (at 0 -1.95 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 21 "/Base band/~RST"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module D_SOD_923:D_SOD_923 (layer B.Cu) (tedit 598A5828)
    (at 10.16 -72.644)
    (fp_text reference D3 (at 0 -0.6) (layer B.SilkS))
    (fp_text value ESD9X3.3ST5G (at 0 0.6) (layer B.Fab))
    (pad 1 smd rect (at -0.42 0) (size 0.5 0.4) (layers B.Cu B.Mask)
      (net 21 "/Base band/~RST"))
    (pad 2 smd rect (at 0.42 0) (size 0.5 0.4) (layers B.Cu B.Mask)
      (net 4 GND))
    (model D_SOD_923.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ECS-TXO-2520:ECS-TXO-2520 (layer B.Cu) (tedit 59A06FAC)
    (at 14.224 -56.388)
    (fp_text reference U3 (at 0 -2) (layer B.SilkS))
    (fp_text value ECS-TXO-2520 (at 0 2) (layer B.Fab))
    (pad 4 smd rect (at -0.925 0.725) (size 1.1 1.1) (layers B.Cu B.Mask)
      (net 7 +3V3))
    (pad 3 smd rect (at 0.925 0.725) (size 1.1 1.1) (layers B.Cu B.Mask)
      (net 28 "Net-(U3-Pad3)"))
    (pad 2 smd rect (at 0.925 -0.725) (size 1.1 1.1) (layers B.Cu B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.925 -0.725) (size 1.1 1.1) (layers B.Cu B.Mask))
  )
  (gr_arc (start 90.17 -12.7) (end 90.17 -10.16) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.63 -90.805) (end 87.63 -12.7) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 82.55 -90.805) (end 82.55 -95.885) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 8.89 -90.805) (end 3.81 -90.805) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.09 0) (end 76.581 0) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 73.66 0) (end 73.66 -2.921) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 14.351 0) (end 11.43 0) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 85.09 -5.08) (end 90.17 -5.08) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0 -8.89) (end 0 -5.08) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 0 -12.7) (end 3.81 -12.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 5.08 -5.08) (end 5.08 0) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 14.351 -2.921) (end 73.664894 -2.921) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 3.81 -90.805) (end 3.81 -12.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 82.55 -95.885) (end 8.89 -95.885) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.17 -5.08) (end 90.17 -10.16) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 5.08 0) (end 11.43 0) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 0 -96.52) (xy 91.44 -96.52) (xy 91.44 0) (xy 0 0)
      )
    )
  )
)
