<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="9" x2="0.05" y2="9" width="0" layer="20"/>
<wire x1="0.05" y1="9" x2="9" y2="0.05" width="0" layer="20"/>
<wire x1="9" y1="0.05" x2="32.5" y2="0" width="0" layer="20"/>
<wire x1="32.5" y1="0" x2="39" y2="6.5" width="0" layer="20"/>
<wire x1="39" y1="6.5" x2="39" y2="25.5" width="0" layer="20"/>
<wire x1="39" y1="25.5" x2="34" y2="30.5" width="0" layer="20"/>
<wire x1="34" y1="30.5" x2="5" y2="30.5" width="0" layer="20"/>
<wire x1="5" y1="30.5" x2="0" y2="25.5" width="0" layer="20"/>
<wire x1="0" y1="25.5" x2="0" y2="9" width="0" layer="20"/>
<text>MOSI</text>
<text>SCLK</text>
<text>MISO</text>
<text>GDO2</text>
<text>GDO0</text>
<text>CSN</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>TEST</text>
<text>RST</text>
<text>VCC</text>
<text>T-G</text>
<text>T-V</text>
<text>T-R</text>
<text>T-T</text>
<text>Shoulder Angel v2b
Clemson University
Connor Bolton
06/2016</text>
<text>GND</text>
<text>VCC</text>
<text>RST</text>
<text>TEST</text>
<text>GDO0</text>
<text>CSN</text>
<text>VCC</text>
<text>GND</text>
<text>MOSI</text>
<text>SCLK</text>
<text>MISO</text>
<text>GDO2</text>
<text>T-G</text>
<text>T-V</text>
<text>T-R</text>
<text>T-T</text>
<text>T_3.2</text>
<text>T_3.1</text>
<text>T_3.0</text>
<text>T_2.7</text>
<text>T_2.6</text>
<text>T_6.4</text>
<text>T_VCC</text>
<text>GND</text>
</plain>
<libraries>
<library name="tiny_passives">
<packages>
<package name="0402">
</package>
</packages>
</library>
<library name="msp430">
<packages>
<package name="PZ100">
</package>
</packages>
</library>
<library name="ADG801">
<packages>
<package name="ADG801">
</package>
</packages>
</library>
<library name="ncp583">
<packages>
<package name="SC82-AB_1PRIMARY">
<description>Original name &lt;b&gt;SC82-AB&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="max9938">
<description>&lt;b&gt;1μA, 4-Bump UCSP/SOT23, Precision Current-Sense Amplifier&lt;/b&gt;&lt;br&gt;
&lt;p&gt;The MAX9938 high-side current-sense amplifier offers precision accuracy specifications of VOS less than 500μV (max) and gain error less than 0.5% (max). Quiescent supply current is an ultra-low 1μA. The MAX9938 fits in a tiny, 1mm x 1mm UCSPTM package size or a 5-pin SOT23 package, making the part ideal for applications in notebook computers, cell phones, PDAs, and all battery-operated portable devices where accura- cy, low quiescent current, and small size are critical.&lt;/p&gt;&lt;p&gt;
The MAX9938 features an input common-mode voltage range from 1.6V to 28V. These current-sense amplifiers have a voltage output and are offered in four gain versions: 25V/V (MAX9938T), 50V/V (MAX9938F), 100V/V (MAX9938H), and 200V/V (MAX9938W).&lt;/p&gt;&lt;p&gt;
The four gain selections offer flexibility in the choice of the external current-sense resistor. The very low 500μV (max) input offset voltage allows small 25mV to 50mV full-scale VSENSE voltage for very low voltage drop at full-current measurement.&lt;/p&gt;&lt;p&gt;
The MAX9938 is offered in tiny 4-bump, UCSP (1mm x 1mm x 0.6mm footprint), 5-pin SOT23, and 6-pin μDFN (2mm x 2mm x 0.8mm) packages specified for operation over the -40°C to +85°C extended temperature range.&lt;/p&gt;</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;5-Lead Small Outline Transistor&lt;/b&gt; Package SOT-23&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/346131962AD8067_a.pdf</description>
</package>
</packages>
</library>
<library name="adxl362">
<packages>
<package name="ADXL362">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
<package name="1X08_ROUND">
</package>
</packages>
</library>
<library name="msp430fr5989">
<packages>
<package name="RGC0064B">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C4" library="tiny_passives" package="0402" value="1uF">
<attribute name="MOUSER" value="603-CC402KRX5R6BB105"/>
<attribute name="DIGIKEY" value="311-1439-1-ND"/>
</element>
<element name="C5" library="tiny_passives" package="0402" value="0.1uF">
<attribute name="MOUSER" value="603-CC402KRX7R7BB104"/>
<attribute name="DIGIKEY" value="311-1338-1-ND"/>
</element>
<element name="C6" library="tiny_passives" package="0402" value="0.1uF">
<attribute name="MOUSER" value="603-CC402KRX7R7BB104"/>
<attribute name="DIGIKEY" value="311-1338-1-ND"/>
</element>
<element name="C7" library="tiny_passives" package="0402" value="1uF">
<attribute name="MOUSER" value="603-CC402KRX5R6BB105"/>
<attribute name="DIGIKEY" value="311-1439-1-ND"/>
</element>
<element name="MSP1" library="msp430" package="PZ100" value="MSP430FR6989_PZ100">
<attribute name="MOUSER" value="595-MSP430FR6989IPZ"/>
<attribute name="DIGIKEY" value="296-38379-5-ND"/>
</element>
<element name="R1" library="tiny_passives" package="0402" value="10">
<attribute name="MOUSER" value="603-RT0402BRD0710RL"/>
<attribute name="DIGIKEY" value="YAG3340CT-ND"/>
</element>
<element name="R10" library="tiny_passives" package="0402" value="330">
<attribute name="MOUSER" value="603-RC0402FR-07330RL"/>
</element>
<element name="R11" library="tiny_passives" package="0402" value="330">
<attribute name="MOUSER" value="603-RC0402FR-07330RL"/>
</element>
<element name="R12" library="tiny_passives" package="0402" value="330">
<attribute name="MOUSER" value="603-RC0402FR-07330RL"/>
</element>
<element name="R13" library="tiny_passives" package="0402" value="330">
<attribute name="MOUSER" value="603-RC0402FR-07330RL"/>
</element>
<element name="R14" library="tiny_passives" package="0402" value="330">
<attribute name="MOUSER" value="603-RC0402FR-07330RL"/>
</element>
<element name="R2" library="tiny_passives" package="0402" value="1M">
<attribute name="MOUSER" value="603-RC0402FR-071ML"/>
<attribute name="DIGIKEY" value="311-1.00MLRCT-ND"/>
</element>
<element name="R3" library="tiny_passives" package="0402" value="1M">
<attribute name="MOUSER" value="603-RC0402FR-071ML"/>
<attribute name="DIGIKEY" value="311-1.00MLRCT-ND"/>
</element>
<element name="R7" library="tiny_passives" package="0402" value="330">
<attribute name="MOUSER" value="603-RC0402FR-07330RL"/>
</element>
<element name="R8" library="tiny_passives" package="0402" value="330">
<attribute name="MOUSER" value="603-RC0402FR-07330RL"/>
</element>
<element name="R9" library="tiny_passives" package="0402" value="330">
<attribute name="MOUSER" value="603-RC0402FR-07330RL"/>
</element>
<element name="U$1" library="ADG801" package="ADG801" value="ADG801">
<attribute name="MOUSER" value="584-ADG801BRT-R7"/>
</element>
<element name="U$2" library="ADG801" package="ADG801" value="ADG801">
<attribute name="MOUSER" value="584-ADG801BRT-R7"/>
</element>
<element name="U$3" library="ADG801" package="ADG801" value="ADG801">
<attribute name="MOUSER" value="584-ADG801BRT-R7"/>
</element>
<element name="U$4" library="ADG801" package="ADG801" value="ADG801">
<attribute name="MOUSER" value="584-ADG801BRT-R7"/>
</element>
<element name="U2" library="ncp583" package="SC82-AB_1PRIMARY" value="NCP583">
<attribute name="MOUSER" value="863-NCP583SQ33T1G"/>
<attribute name="DIGIKEY" value="NCP583SQ33T1GOSCT-ND"/>
</element>
<element name="U3" library="max9938" package="SOT23-5" value="MAX9938">
<attribute name="MOUSER" value="700-MAX9938WEUK+T"/>
<attribute name="DIGIKEY" value="MAX9938WEUK+TCT-ND"/>
</element>
<element name="U5" library="adxl362" package="ADXL362" value="ADXL362">
<attribute name="MOUSER" value="584-ADXL362BCCZ-R7"/>
<attribute name="DIGIKEY" value="ADXL362BCCZ-RL7CT-ND"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="msp430fr5989" package="RGC0064B" value="Value">
<attribute name="PARTNUMBER" value="MSP430FR5989IRGCR"/>
<attribute name="REFDES" value="RefDes"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="TYPE" value="TYPE"/>
<attribute name="ROHS" value="Y"/>
<attribute name="COMPTYPE" value="IC"/>
<attribute name="PACKAGEREFERENCE" value="RGC0064B"/>
<attribute name="PIN_COUNT" value="65"/>
<attribute name="MOUNTTYPE" value="SMT"/>
<attribute name="ALTERNATEPARTNUMBER" value="MSP430FR5989IRGCT"/>
<attribute name="MOUSER" value="595-SP430FR5989IRGCR"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
</element>
</elements>
<signals>
<signal name="BATT+">
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U3" pad="1"/>
<contactref element="U3" pad="2"/>
<contactref element="U5" pad="P$12"/>
<contactref element="U5" pad="P$13"/>
<contactref element="U5" pad="P$16"/>
<contactref element="MSP1" pad="76"/>
<contactref element="MSP1" pad="6"/>
<contactref element="MSP1" pad="98"/>
<contactref element="MSP1" pad="57"/>
<contactref element="MSP1" pad="26"/>
<contactref element="MSP1" pad="80"/>
<contactref element="MSP1" pad="86"/>
<contactref element="MSP1" pad="83"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U$2" pad="GND"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$3" pad="GND"/>
<contactref element="U$4" pad="GND"/>
<contactref element="J3" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="U4" pad="56"/>
<contactref element="U4" pad="59"/>
<contactref element="U4" pad="53"/>
<contactref element="U4" pad="17"/>
<contactref element="U4" pad="34"/>
<contactref element="U4" pad="62"/>
<contactref element="U4" pad="49"/>
<contactref element="J4" pad="4"/>
<contactref element="J2" pad="1"/>
<contactref element="U4" pad="65"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="SA_VCC">
<contactref element="U2" pad="3"/>
<contactref element="U3" pad="5"/>
<contactref element="R1" pad="2"/>
<contactref element="U4" pad="52"/>
<contactref element="U4" pad="48"/>
<contactref element="U4" pad="63"/>
<contactref element="U4" pad="35"/>
<contactref element="U4" pad="18"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U3" pad="4"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="U$1" pad="VDD"/>
<contactref element="U$1" pad="D"/>
<contactref element="U$2" pad="VDD"/>
<contactref element="U$3" pad="VDD"/>
<contactref element="U$3" pad="D"/>
<contactref element="U$4" pad="VDD"/>
<contactref element="U$4" pad="D"/>
</signal>
<signal name="SA_CS">
<contactref element="U3" pad="3"/>
<contactref element="U4" pad="46"/>
</signal>
<signal name="SA_VS">
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="U4" pad="47"/>
</signal>
<signal name="T_VCC">
<contactref element="MSP1" pad="75"/>
<contactref element="MSP1" pad="27"/>
<contactref element="MSP1" pad="79"/>
<contactref element="MSP1" pad="99"/>
<contactref element="MSP1" pad="58"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U$3" pad="S"/>
<contactref element="J2" pad="2"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="SA_T_VCC_SEL">
<contactref element="U$3" pad="IN"/>
<contactref element="U4" pad="13"/>
</signal>
<signal name="R_VCC">
<contactref element="U$2" pad="S"/>
<contactref element="U$4" pad="S"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="SA_T_R_VCC_ENA">
<contactref element="U$1" pad="IN"/>
<contactref element="U4" pad="61"/>
<contactref element="MSP1" pad="72"/>
</signal>
<signal name="SA_TEST">
<contactref element="J3" pad="4"/>
<contactref element="U4" pad="19"/>
</signal>
<signal name="SA_RST">
<contactref element="J3" pad="3"/>
<contactref element="U4" pad="20"/>
</signal>
<signal name="SA_BSL_TX">
<contactref element="R7" pad="1"/>
<contactref element="U4" pad="33"/>
</signal>
<signal name="SA_BSL_RX">
<contactref element="R8" pad="1"/>
<contactref element="U4" pad="32"/>
</signal>
<signal name="T_BSL_RX">
<contactref element="MSP1" pad="51"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="T_BSL_TX">
<contactref element="MSP1" pad="50"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="R_SCLK">
<contactref element="R11" pad="1"/>
<contactref element="U4" pad="2"/>
<contactref element="U4" pad="14"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="R_MISO">
<contactref element="R10" pad="1"/>
<contactref element="U4" pad="5"/>
<contactref element="U4" pad="15"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="R_GDO2">
<contactref element="R14" pad="1"/>
<contactref element="U4" pad="8"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="R_MOSI">
<contactref element="R9" pad="1"/>
<contactref element="U4" pad="4"/>
<contactref element="U4" pad="16"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="R_CSN">
<contactref element="R12" pad="1"/>
<contactref element="U4" pad="6"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="R_GDO0">
<contactref element="R13" pad="1"/>
<contactref element="U4" pad="7"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="T_R_VCC_SEL">
<contactref element="U$2" pad="IN"/>
<contactref element="MSP1" pad="70"/>
</signal>
<signal name="A_SCLK">
<contactref element="U5" pad="P$4"/>
<contactref element="MSP1" pad="2"/>
</signal>
<signal name="A_MOSI">
<contactref element="U5" pad="P$6"/>
<contactref element="MSP1" pad="4"/>
</signal>
<signal name="A_MISO">
<contactref element="U5" pad="P$7"/>
<contactref element="MSP1" pad="5"/>
</signal>
<signal name="A_CSN">
<contactref element="U5" pad="P$8"/>
<contactref element="MSP1" pad="87"/>
</signal>
<signal name="A_VCC">
<contactref element="U5" pad="P$1"/>
<contactref element="U5" pad="P$14"/>
<contactref element="MSP1" pad="15"/>
</signal>
<signal name="A_INT1">
<contactref element="U5" pad="P$11"/>
<contactref element="MSP1" pad="14"/>
</signal>
<signal name="A_INT2">
<contactref element="U5" pad="P$9"/>
<contactref element="MSP1" pad="3"/>
</signal>
<signal name="T_R_MOSI">
<contactref element="R9" pad="2"/>
<contactref element="MSP1" pad="96"/>
</signal>
<signal name="T_R_MISO">
<contactref element="R10" pad="2"/>
<contactref element="MSP1" pad="97"/>
</signal>
<signal name="T_R_SCLK">
<contactref element="R11" pad="2"/>
<contactref element="MSP1" pad="92"/>
</signal>
<signal name="T_R_CSN">
<contactref element="R12" pad="2"/>
<contactref element="MSP1" pad="63"/>
</signal>
<signal name="T_R_GDO0">
<contactref element="R13" pad="2"/>
<contactref element="MSP1" pad="64"/>
</signal>
<signal name="T_R_GDO2">
<contactref element="R14" pad="2"/>
<contactref element="MSP1" pad="66"/>
</signal>
<signal name="BSL_RST">
<contactref element="MSP1" pad="29"/>
<contactref element="J2" pad="3"/>
<contactref element="U4" pad="27"/>
</signal>
<signal name="SA_R_VCC_SEL">
<contactref element="U$4" pad="IN"/>
<contactref element="U4" pad="60"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="S"/>
<contactref element="U$2" pad="D"/>
</signal>
<signal name="BSL_TEST">
<contactref element="MSP1" pad="28"/>
<contactref element="J2" pad="4"/>
<contactref element="U4" pad="26"/>
</signal>
<signal name="N$5">
<contactref element="MSP1" pad="100"/>
</signal>
<signal name="N$7">
<contactref element="MSP1" pad="91"/>
</signal>
<signal name="N$16">
<contactref element="MSP1" pad="93"/>
</signal>
<signal name="N$20">
<contactref element="U4" pad="31"/>
</signal>
<signal name="N$2">
</signal>
<signal name="JMP_3.2">
<contactref element="MSP1" pad="25"/>
<contactref element="J7" pad="8"/>
</signal>
<signal name="JMP_2.7">
<contactref element="MSP1" pad="17"/>
<contactref element="J7" pad="5"/>
</signal>
<signal name="JMP_2.6">
<contactref element="MSP1" pad="16"/>
<contactref element="J7" pad="4"/>
</signal>
<signal name="JMP_6.4">
<contactref element="J7" pad="3"/>
<contactref element="MSP1" pad="11"/>
</signal>
<signal name="JMP_3.1">
<contactref element="J7" pad="7"/>
<contactref element="MSP1" pad="24"/>
</signal>
<signal name="JMP_3.0">
<contactref element="J7" pad="6"/>
<contactref element="MSP1" pad="23"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
