(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 96)
    (tracks 63)
    (zones 0)
    (modules 7)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 2 1)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module SamacSys_Parts:agb2 (layer F.Cu) (tedit 0)
    (at 163 109.75)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module SamacSys_Parts:SKSHAAE010 (layer F.Cu) (tedit 0)
    (at 119 90)
    (descr SKSHAAE010)
    (tags Switch)
    (attr smd)
    (fp_text reference S2 (at 0 0) (layer F.SilkS))
    (fp_text value SKSHAAE010 (at 0 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at 1.55 -1.025 90) (size 0.45 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 1.55 1.025 90) (size 0.45 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.55 1.025 90) (size 0.45 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.55 -1.025 90) (size 0.45 0.55) (layers F.Cu F.Paste F.Mask))
  )
  (module SamacSys_Parts:SKSHAAE010 (layer F.Cu) (tedit 0)
    (at 119 81.9)
    (descr SKSHAAE010)
    (tags Switch)
    (attr smd)
    (fp_text reference S3 (at 0 0) (layer F.SilkS))
    (fp_text value SKSHAAE010 (at 0 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at 1.55 -1.025 90) (size 0.45 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 1.55 1.025 90) (size 0.45 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.55 1.025 90) (size 0.45 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.55 -1.025 90) (size 0.45 0.55) (layers F.Cu F.Paste F.Mask))
  )
  (module SamacSys_Parts:SKRR (layer F.Cu) (tedit 0)
    (at 109.2 69.7)
    (descr SKRR)
    (tags Switch)
    (attr smd)
    (fp_text reference S7 (at -0.315 -0.046) (layer F.SilkS))
    (fp_text value SKRR (at -0.315 -0.046) (layer F.SilkS) hide)
    (fp_text user %R (at -0.315 -0.046) (layer F.Fab))
    (pad 4 smd rect (at 3 2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 3 -2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3 2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -3 -2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (model C:\Users\meeps\Downloads\LIBCAD\SamacSys_Parts.3dshapes\SKRRAAE010.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:SKRR (layer F.Cu) (tedit 0)
    (at 117.3 61.8)
    (descr SKRR)
    (tags Switch)
    (attr smd)
    (fp_text reference S4 (at -0.315 -0.046) (layer F.SilkS))
    (fp_text value SKRR (at -0.315 -0.046) (layer F.SilkS) hide)
    (fp_text user %R (at -0.315 -0.046) (layer F.Fab))
    (pad 4 smd rect (at 3 2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 3 -2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3 2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -3 -2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (model C:\Users\meeps\Downloads\LIBCAD\SamacSys_Parts.3dshapes\SKRRAAE010.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:SKRR (layer F.Cu) (tedit 0)
    (at 101 61.8)
    (descr SKRR)
    (tags Switch)
    (attr smd)
    (fp_text reference S5 (at -0.315 -0.046) (layer F.SilkS))
    (fp_text value SKRR (at -0.315 -0.046) (layer F.SilkS) hide)
    (fp_text user %R (at -0.315 -0.046) (layer F.Fab))
    (pad 4 smd rect (at 3 2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 3 -2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3 2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -3 -2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (model C:\Users\meeps\Downloads\LIBCAD\SamacSys_Parts.3dshapes\SKRRAAE010.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:SKRR (layer F.Cu) (tedit 0)
    (at 109.1 53.8)
    (descr SKRR)
    (tags Switch)
    (attr smd)
    (fp_text reference S6 (at -0.315 -0.046) (layer F.SilkS))
    (fp_text value SKRR (at -0.315 -0.046) (layer F.SilkS) hide)
    (fp_text user %R (at -0.315 -0.046) (layer F.Fab))
    (pad 4 smd rect (at 3 2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 3 -2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3 2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -3 -2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (model C:\Users\meeps\Downloads\LIBCAD\SamacSys_Parts.3dshapes\SKRRAAE010.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_circle (center 109.2 61.7) (end 112.7 61.6) (layer Edge.Cuts) (width 0.05))
  (gr_text v3 (at 103.2 66.6) (layer F.SilkS))
  (gr_text meeps (at 117.1 66.2) (layer F.SilkS))
  (gr_text TP7 (at 114.9 70.7) (layer F.SilkS))
  (gr_text TP5 (at 100.4 57.2) (layer F.SilkS))
  (gr_text TP6 (at 123.5 56.4) (layer F.SilkS))
  (gr_text TP4 (at 121 57.5) (layer F.SilkS))
  (gr_text TP3 (at 122.8 66) (layer F.SilkS))
  (gr_text TP2 (at 122.8 76.2) (layer F.SilkS))
  (gr_text GND (at 120.4 86) (layer F.SilkS))
  (gr_arc (start 109.25 61.75) (end 109.75 75.75) (angle -24.58449512) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 108 76.5) (end 109.75 75.75) (angle -110.0422762) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 109.25 61.75) (end 98 69.4) (angle -44.96280077) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 98 69.3) (end 98 69.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 98 67.75) (end 98 69.3) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 113.6 77.1) (end 117 77.5) (angle -62.40125915) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 118.8 74.5) (end 120.2 73.6) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 119.25 81.2) (end 117 77.5) (angle -48.03552821) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 115 84.75) (end 114.994323 80.398931) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 114 86) (end 115 87.25) (angle -102.6803835) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 114.998145 90.006006) (end 115 87.25) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 118.19336 89.946642) (end 114.998145 90.006006) (angle -71.76665945) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124 93) (end 117.25 93) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124 75.5) (end 124 93) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 122.6 74.5) (end 124 75.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 122.6 74) (end 122.6 74.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 123.7 73) (end 122.6 74) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 123.7 66.7) (end 123.7 73) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.4 66) (end 123.7 66.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.4 64.9) (end 124.4 66) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.4 63.8) (end 122.797804 63.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.4 64.9) (end 124.4 63.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 122.8 57.5) (end 122.797804 63.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.5 55.25) (end 120.75 55.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.5 56.25) (end 125.5 55.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.5 57.5) (end 122.8 57.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.5 56.25) (end 125.5 57.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 109.25 61.75) (end 120.75 55.25) (angle -87.53526112) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 103.25 53.25) (end 103.250566 49.981109) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 98 53.25) (end 103.25 53.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 98 55.75) (end 98 53.25) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 108.75 61.75) (end 98 55.75) (angle -58.33522676) (layer Edge.Cuts) (width 0.05))
)
