(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 13)
    (no_connects 0)
    (area 102.286999 98.476999 152.983001 125.297001)
    (thickness 1.6)
    (drawings 17)
    (tracks 41)
    (zones 0)
    (modules 14)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.35)
    (user_trace_width 0.4)
    (user_trace_width 0.45)
    (user_trace_width 0.5)
    (user_trace_width 2)
    (user_trace_width 3)
    (user_trace_width 4)
    (trace_clearance 0.2)
    (zone_clearance 0.4)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 3)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "//vmware-host/Shared Folders/Downloads/RelayDriverV1.1/"))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(D1-Pad1)")
  (net 3 GND)
  (net 4 /signal_in)
  (net 5 "Net-(Q1-Pad1)")
  (net 6 "Net-(P3-Pad1)")
  (net 7 "Net-(P3-Pad2)")
  (net 8 "Net-(P3-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /signal_in)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(Q1-Pad1)")
  )
  (module Connect:1pin (layer F.Cu) (tedit 57462BB7)
    (at 131.064 122.555)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Connect:1pin (layer F.Cu) (tedit 57441487)
    (at 131.191 101.854)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Connect:1pin (layer F.Cu) (tedit 57462BB3)
    (at 106.68 122.428)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Connect:1pin (layer F.Cu) (tedit 57441487)
    (at 106.68 101.6)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 (layer F.Cu) (tedit 57462C85)
    (at 135.128 109.728 270)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference D1 (at 5.588 0 270) (layer F.SilkS))
    (fp_text value D (at 4.37134 -3.55854 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 -0.00254 90) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 -0.00254 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module Connect:bornier2 (layer F.Cu) (tedit 57613F07)
    (at 147.828 105.664 270)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference P1:SIGNAL (at -5.588 1.778 360) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 5.08 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at -2.54 0 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 4 /signal_in))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier2 (layer F.Cu) (tedit 57613F8D)
    (at 147.828 116.84 270)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference "P2:5V POWER" (at 5.715 0.889 360) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 5.08 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at -2.54 0 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Wide_Oval (layer F.Cu) (tedit 57613ED0)
    (at 135.636 104.648)
    (descr "TO-92 leads molded, wide, oval pads, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 0 -2.794) (layer F.SilkS))
    (fp_text value 2N2222 (at 2.54 -4.318) (layer F.SilkS))
    (pad 1 thru_hole oval (at 2.54 -2.54 90) (size 1.99898 1.50114) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole oval (at 0 0 90) (size 1.50114 1.99898) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(D1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.50114 1.99898) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Wide_Oval.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57462C88)
    (at 138.176 114.808 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R1 (at 0.508 0 270) (layer F.SilkS))
    (fp_text value R (at 3.81 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.08 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 /signal_in))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57462C8D)
    (at 141.224 114.808 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R2 (at 0.762 0 270) (layer F.SilkS))
    (fp_text value R (at 0 0.508 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -5.08 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module bench_computer:SONGLE_5V_Relay (layer F.Cu) (tedit 57636793)
    (at 122.936 111.379)
    (fp_text reference U1 (at -2.794 0.381 90) (layer F.SilkS))
    (fp_text value 5V/10A_relay (at -0.508 -2.54) (layer F.SilkS) hide)
    (fp_text user close (at -4.826 6.477 90) (layer F.SilkS))
    (fp_text user open (at -5.08 -5.207 90) (layer F.SilkS))
    (fp_text user common (at 4.445 0.381 90) (layer F.SilkS))
    (fp_text user coil (at 0.5 0.5 90) (layer F.SilkS))
    (fp_text user "5V Relay" (at -8.382 0.508 90) (layer F.SilkS))
    (pad 4 thru_hole circle (at -7 -5.5) (size 3 3) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P3-Pad1)"))
    (pad 5 thru_hole circle (at -7 6.5) (size 3 3) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P3-Pad3)"))
    (pad 2 thru_hole circle (at 5.5 6.5) (size 1.7 1.7) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(D1-Pad2)"))
    (pad 3 thru_hole circle (at 7.5 0.5) (size 3 3) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P3-Pad2)"))
    (pad 1 thru_hole circle (at 5.5 -5.5) (size 1.7 1.7) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module Connect:bornier3 (layer F.Cu) (tedit 576137C7)
    (at 108.077 111.887 270)
    (descr "Bornier d'alimentation 3 pins")
    (tags DEV)
    (fp_text reference P3 (at 0 -5.08 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 5.08 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at -5.08 0 270) (size 3 3) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P3-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 270) (size 3 3) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P3-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P3-Pad3)"))
    (model Connect.3dshapes/bornier3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen (layer B.Cu) (tedit 57440603)
    (at 122.428 111.125 180)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 4.38912 180) (layer B.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 -6.56082 180) (layer B.Fab) hide)
  )
  (module "Kicad Logos:TE_Logo_12mm" (layer F.Cu) (tedit 0)
    (at 118.364 101.219)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text 1N4004 (at 133.223 114.808 90) (layer F.SilkS))
  (gr_text 9.973k (at 141.224 122.936 90) (layer F.SilkS))
  (gr_text 469 (at 138.303 122.174 90) (layer F.SilkS))
  (gr_text "I have changed the size of the holes for the\npower side of the relay and the three-pin\nscrew terminal. Total diameter for pad is\n3mm and diameter of hole is 2.5mm for\nthe screw terminal and 2mm for the relay\nopen, close and common pins. I did this\nto try and match the size of the connected\ntraces." (at 66.294 111.506) (layer Cmts.User))
  (gr_text "Note: I have interchanged pins 1 and 2. \nThe TO-92 footprint has 2 in the base \n(middle) of the transistor. However, to \nmatch the schematic correctly, pin 1 \nshould be the base (middle) and 2 the \ncollector (left pin)." (at 121.92 93.218) (layer Cmts.User))
  (gr_line (start 152.908 98.552) (end 102.362 98.552) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.908 125.222) (end 152.908 98.552) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.362 125.222) (end 152.908 125.222) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.362 98.552) (end 102.362 125.222) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Relay Driver v1.1" (at 118.364 122.428) (layer F.SilkS))
  (gr_text NO (at 103.124 106.172 90) (layer F.SilkS))
  (gr_text NC (at 103.124 116.967 90) (layer F.SilkS))
  (gr_text CO (at 103.124 111.887 90) (layer F.SilkS))
  (gr_text 5V (at 152.273 119.38 90) (layer F.SilkS))
  (gr_text SIGNAL (at 152.273 108.204 90) (layer F.SilkS))
  (gr_text GND (at 152.273 114.3 90) (layer F.SilkS))
  (gr_text GND (at 152.273 103.124 90) (layer F.SilkS))
)
