(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "Exit Poll")
		(date "2024-11-07")
		(rev "0.7")
		(company "PDX Hackerspace")
		(comment 1 "John Romkey")
		(comment 2 "simple PCB connecting TinyS3 to TFT LCD display and LED strip")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/SCL")
	(net 2 "/SDA")
	(net 3 "GND")
	(net 4 "/MO")
	(net 5 "/MI")
	(net 6 "/SCK")
	(net 7 "/TFT_CS")
	(net 8 "/TFT_RST")
	(net 9 "/TFT_DCRS")
	(net 10 "/~{CPU_RST}")
	(net 11 "+3V3")
	(net 12 "/BOOT{slash}IO0")
	(net 13 "/T_IRQ")
	(net 14 "unconnected-(J4-Pin_7-Pad7)")
	(net 15 "unconnected-(J4-Pin_8-Pad8)")
	(net 16 "/BAT")
	(net 17 "/T_CS")
	(net 18 "/IO37")
	(net 19 "Net-(D1-K)")
	(net 20 "Net-(D1-A)")
	(net 21 "/CPU_RX")
	(net 22 "/CPU_TX")
	(net 23 "/IO1")
	(net 24 "/LED_DATA")
	(net 25 "+5V")
	(net 26 "/LED_CLK")
	(net 27 "unconnected-(J3-Pad0)")
	(net 28 "unconnected-(J3-Pad0)_1")
	(footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 24.384 29.972)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "U3"
			(at -3.048 0.032 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at -4.064 2.572 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged*")
		(sheetname "Root")
		(sheetfile "PDX Hackerspace Exit Poll.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(net_tie_pad_groups "1, 2")
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 19 "Net-(D1-K)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "1myFootprints:SPI_TFT_TOUCH"
		(layer "F.Cu")
		(at 66.294 20.066 90)
		(property "Reference" "J1"
			(at -5.08 -38.862 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at -2.54 -41.68 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "1myFootprints:SPI_TFT_TOUCH"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PDX Hackerspace Exit Poll.kicad_sch")
		(attr through_hole exclude_from_bom)
		(fp_text user "LED"
			(at -5.334 -17.526 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "T_IRQ"
			(at -5.334 -2.286 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "T_CLK"
			(at -5.334 -12.446 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "T_CS"
			(at -5.334 -9.906 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "T_DO"
			(at -5.334 -4.826 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "CS"
			(at -5.334 -30.226 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "SDO(MISO)"
			(at -5.334 -14.986 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "SDI(MOSI)"
			(at -5.334 -22.606 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "T_DIN"
			(at -5.334 -7.366 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "GND"
			(at -5.334 -32.766 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "SCK"
			(at -5.334 -20.066 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "Generic SPI TFT display"
			(at -0.254 -11.938 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "DC/RS"
			(at -5.334 -25.146 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "RESET"
			(at -5.334 -27.686 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "VCC"
			(at -5.334 -35.306 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "T_DIN"
			(at -5.08 -7.62 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "T_CS"
			(at -5.08 -10.16 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -5.08 -33.02 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "RESET"
			(at -5.08 -27.94 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "LED"
			(at -5.08 -17.78 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "CS"
			(at -5.08 -30.48 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "DC/RS"
			(at -5.08 -25.4 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "VCC"
			(at -5.08 -35.56 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SCK"
			(at -5.08 -20.32 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SDO(MISO)"
			(at -5.334 -15.24 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "T_DO"
			(at -5.08 -5.08 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "T_CLK"
			(at -5.08 -12.7 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SDI(MOSI)"
			(at -5.08 -22.86 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "T_IRQ"
			(at -5.08 -2.54 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at -2.54 -40.18 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at -2.54 -35.56 90)
			(size 2.5 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "2" thru_hole rect
			(at -2.54 -33.02 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" thru_hole circle
			(at -2.54 -30.48 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/TFT_CS")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -2.54 -27.94 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/TFT_RST")
			(pinfunction "RESET")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at -2.54 -25.4 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/TFT_DCRS")
			(pinfunction "DC/RS")
			(pintype "input")
		)
		(pad "6" thru_hole circle
			(at -2.54 -22.86 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/MO")
			(pinfunction "SDI_(MOSI)")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at -2.54 -20.32 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/SCK")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at -2.54 -17.78 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "+3V3")
			(pinfunction "LED")
			(pintype "input")
		)
		(pad "9" thru_hole circle
			(at -2.54 -15.24 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/MI")
			(pinfunction "SDO_(MISO)")
			(pintype "input")
		)
		(pad "10" thru_hole circle
			(at -2.54 -12.7 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/SCK")
			(pinfunction "T_CLK")
			(pintype "input")
		)
		(pad "11" thru_hole circle
			(at -2.54 -10.16 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/T_CS")
			(pinfunction "T_CS")
			(pintype "input")
		)
		(pad "12" thru_hole circle
			(at -2.54 -7.62 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/MO")
			(pinfunction "T_DIN")
			(pintype "input")
		)
		(pad "13" thru_hole circle
			(at -2.54 -5.08 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/MI")
			(pinfunction "T_DO")
			(pintype "output")
		)
		(pad "14" thru_hole circle
			(at -2.54 -2.54 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/T_IRQ")
			(pinfunction "T_IRQ")
			(pintype "output")
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 24.242 36.862)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at -3.414 -0.032 0)
			(layer "F.SilkS")
		)
		(property "Value" "475"
			(at 0 1.82 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C323067"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PDX Hackerspace Exit Poll.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 25 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 20 "Net-(D1-A)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 27.432 56.4915 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C4355002"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PDX Hackerspace Exit Poll.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/SCL")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "1myFootprints:TinyS3"
		(layer "F.Cu")
		(at 50.038 56.642 180)
		(property "Reference" "U1"
			(at 7.874 19.304 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "1myFootprints:TinyS3"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://unexpectedmaker.com/shop.html#!/TinyPICO/p/577111313/category=154494282"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PDX Hackerspace Exit Poll.kicad_sch")
		(attr through_hole exclude_from_bom)
		(fp_text user "Unexpected Maker TinyS3"
			(at 7.0993 13.208 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SCK"
			(at -10.668 -7.62 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -10.922 9.906 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "IO6"
			(at -10.414 12.446 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "BOOT/IO0"
			(at 20.066 12.954 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "RST"
			(at -10.668 7.366 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "3V3"
			(at 15.748 -5.08 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SS"
			(at -7.62 -5.08 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "IO5"
			(at 15.24 7.62 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "ANT"
			(at 3.302 18.034 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "USB"
			(at 3.81 -14.478 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "RX0"
			(at -10.668 2.286 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SDA"
			(at -10.668 0.254 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "IO7"
			(at -10.414 15.24 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "IO2"
			(at 15.24 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "IO4"
			(at 15.24 5.08 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "5V"
			(at 14.732 -7.62 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "M0"
			(at -9.906 -12.7 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 15.748 -10.16 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "IO21"
			(at 16.256 10.414 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "IO3"
			(at 15.24 2.54 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "MI"
			(at -9.398 -10.414 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "IO1"
			(at 15.24 -2.54 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "VBAT"
			(at 16.256 -12.7 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "TX0"
			(at -10.414 5.08 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SCL"
			(at -10.414 -2.54 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at -3.302 18.542 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at -5.08 -12.7 180)
			(size 2.5 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/T_IRQ")
			(pinfunction "M0/IO35")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole circle
			(at -5.08 -10.16 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/IO37")
			(pinfunction "MI/IO37")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole circle
			(at -5.08 -7.62 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/MO")
			(pinfunction "SCK/IO36")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole circle
			(at -5.08 -5.08 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/T_CS")
			(pinfunction "SS/IO34")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole circle
			(at -5.08 -2.54 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/SCK")
			(pinfunction "SCL/IO9")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole circle
			(at -5.08 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/MI")
			(pinfunction "SDA/IO8")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole circle
			(at -5.08 2.54 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/LED_CLK")
			(pinfunction "IO7")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole circle
			(at -5.08 5.08 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/LED_DATA")
			(pinfunction "IO6")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole circle
			(at -5.08 7.62 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/~{CPU_RST}")
			(pinfunction "RST")
			(pintype "input")
		)
		(pad "10" thru_hole rect
			(at -5.08 10.16 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "11" thru_hole circle
			(at -5.08 12.7 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/CPU_TX")
			(pinfunction "TX/IO43")
			(pintype "input")
		)
		(pad "12" thru_hole circle
			(at -5.08 15.24 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/CPU_RX")
			(pinfunction "RX/IO44")
			(pintype "output")
		)
		(pad "13" thru_hole circle
			(at 10.16 12.7 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/BOOT{slash}IO0")
			(pinfunction "BOOT/IO0")
			(pintype "bidirectional")
		)
		(pad "14" thru_hole circle
			(at 10.16 10.16 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/SDA")
			(pinfunction "IO21")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole circle
			(at 10.16 7.62 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/SCL")
			(pinfunction "IO5")
			(pintype "bidirectional")
		)
		(pad "16" thru_hole circle
			(at 10.16 5.08 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/TFT_DCRS")
			(pinfunction "IO4")
			(pintype "bidirectional")
		)
		(pad "17" thru_hole circle
			(at 10.16 2.54 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/TFT_RST")
			(pinfunction "IO3")
			(pintype "bidirectional")
		)
		(pad "18" thru_hole circle
			(at 10.16 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/TFT_CS")
			(pinfunction "IO2")
			(pintype "bidirectional")
		)
		(pad "19" thru_hole circle
			(at 10.16 -2.54 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/IO1")
			(pinfunction "IO1")
			(pintype "bidirectional")
		)
		(pad "20" thru_hole circle
			(at 10.16 -5.08 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "+3V3")
			(pinfunction "3V3")
			(pintype "power_out")
		)
		(pad "21" thru_hole circle
			(at 10.16 -7.62 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "+5V")
			(pinfunction "5V")
			(pintype "power_out")
		)
		(pad "22" thru_hole circle
			(at 10.16 -10.16 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "23" thru_hole circle
			(at 10.16 -12.7 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/BAT")
			(pinfunction "BAT")
			(pintype "output+no_connect")
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 22.5 22.5)
		(descr "Mounting Hole 2.2mm, no annular, M2")
		(tags "mounting hole 2.2mm no annular m2")
		(property "Reference" "REF**"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.2mm_M2"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "F&B.Cu" "*.Mask")
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x15_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 71.628 63.754 180)
		(descr "Through hole straight socket strip, 1x15, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x15 2.54mm single row")
		(property "Reference" "J4"
			(at 0 -2.77 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x15_Socket"
			(at 0 38.33 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x15_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "PDX Hackerspace Exit Poll.kicad_sch")
		(attr through_hole exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 17.78 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/SDA")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/CPU_TX")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/CPU_RX")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/~{CPU_RST}")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/BOOT{slash}IO0")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(J4-Pin_7-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive+no_connect")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(J4-Pin_8-Pad8)")
			(pinfunction "Pin_8")
			(pintype "passive+no_connect")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/IO37")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/IO1")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "+3V3")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 0 27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "+5V")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 30.48 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 0 33.02 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 35.56 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x15_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 22.86 56.388 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C4355002"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PDX Hackerspace Exit Poll.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/SDA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:CP_Elec_6.3x7.7"
		(layer "F.Cu")
		(at 32.766 34.434 90)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 6.3x7.7mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C1"
			(at 0 -4.35 90)
			(layer "F.SilkS")
		)
		(property "Value" "100µF"
			(at 0 4.35 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:CP_Elec_6.3x7.7"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C72477"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "PDX Hackerspace Exit Poll.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.7 0 90)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.15625)
			(net 25 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.7 0 90)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.15625)
			(net 3 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_6.3x7.7.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 71.5 22.5)
		(descr "Mounting Hole 2.2mm, no annular, M2")
		(tags "mounting hole 2.2mm no annular m2")
		(property "Reference" "REF**"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.2mm_M2"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "F&B.Cu" "*.Mask")
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 22.606 68.834)
		(descr "Mounting Hole 2.2mm, no annular, M2")
		(tags "mounting hole 2.2mm no annular m2")
		(property "Reference" "REF**"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.2mm_M2"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "F&B.Cu" "*.Mask")
		)
	)
	(footprint "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 24.384 33.274)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D1"
			(at -3.556 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.82 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C28310439"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "PDX Hackerspace Exit Poll.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4875 0)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 19 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4875 0)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 20 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 71.5 69.5)
		(descr "Mounting Hole 2.2mm, no annular, M2")
		(tags "mounting hole 2.2mm no annular m2")
		(property "Reference" "REF**"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.2mm_M2"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "F&B.Cu" "*.Mask")
		)
	)
	(footprint "footprint:CONN-SMD_BM04B-SRSS-TB"
		(layer "F.Cu")
		(at 30.226 68.834)
		(descr "CONN-SMD_BM04B-SRSS-TB footprint")
		(tags "CONN-SMD_BM04B-SRSS-TB footprint C160390")
		(property "Reference" "J3"
			(at -4.572 -2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at -0.000127 3.26251 0)
			(layer "F.Fab")
		)
		(property "Footprint" "footprint:CONN-SMD_BM04B-SRSS-TB"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://item.szlcsc.com/171770.html"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C160390"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C160390"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PDX Hackerspace Exit Poll.kicad_sch")
		(attr smd)
		(pad "0" smd rect
			(at -2.799975 -1.26251)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "unconnected-(J3-Pad0)")
			(pinfunction "0")
			(pintype "unspecified+no_connect")
		)
		(pad "0" smd rect
			(at 2.799975 -1.26251)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "unconnected-(J3-Pad0)_1")
			(pinfunction "0")
			(pintype "unspecified+no_connect")
		)
		(pad "1" smd rect
			(at -1.5 1.26251)
			(size 0.6 1.550013)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "GND")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -0.5 1.26251)
			(size 0.6 1.550013)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "+3V3")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 0.5 1.26251)
			(size 0.6 1.550013)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "/SDA")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 1.5 1.26251)
			(size 0.6 1.550013)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "/SCL")
			(pinfunction "4")
			(pintype "unspecified")
		)
		(model "/Users/romkey/Documents/KiCad/easyeda2kicad/footprint/packages3d/CONN-SMD_BM04B-SRSS-TB.step"
			(offset
				(xyz -1.5 0.150012 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_S4B-PH-K_1x04_P2.00mm_Horizontal"
		(layer "F.Cu")
		(at 27.342 42.974 -90)
		(descr "JST PH series connector, S4B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH top entry")
		(property "Reference" "J2"
			(at 3 -2.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_Socket"
			(at 3 7.45 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_JST:JST_PH_S4B-PH-K_1x04_P2.00mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C160235"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "PDX Hackerspace Exit Poll.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3 2.5 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net 3 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2 0 270)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "+5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 4 0 270)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/LED_DATA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 6 0 270)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/LED_CLK")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S4B-PH-K_1x04_P2.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "1myFootprints:OSHW-Logo2_7.3x6mm_SilkScreen"
		(layer "B.Cu")
		(at 35.306 55.626 180)
		(descr "Open Source Hardware Symbol")
		(tags "Logo Symbol OSHW")
		(property "Reference" "REF**"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "OSHW-Logo2_7.3x6mm_SilkScreen"
			(at 0.75 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "1myFootprints:CTRLH Logo"
		(layer "B.Cu")
		(at 26.67 55.88 180)
		(property "Reference" "REF**"
			(at 4.173109 2.895837 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "CTRLH Logo"
			(at 4.173109 1.395837 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only)
	)
	(footprint "Symbol:KiCad-Logo2_5mm_SilkScreen"
		(layer "B.Cu")
		(at 47.498 55.372 180)
		(descr "KiCad Logo")
		(tags "Logo KiCad")
		(property "Reference" "REF**"
			(at 0 5.08 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "KiCad-Logo2_5mm_SilkScreen"
			(at 0 -5.08 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Symbol:KiCad-Logo2_5mm_SilkScreen"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 47.244 45.466 180)
		(property "Reference" "G**"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(gr_rect
		(start 20 20)
		(end 74 72)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "PDXHackerspace Exit Poll\ngithub.com/romkey/pdxhackerspace-exit-poll\nv0.7\n11/7/2024\n"
		(at 67.564 41.656 0)
		(layer "B.SilkS")
	)
	(gr_text "+"
		(at 26.924 33.782 0)
		(layer "F.SilkS")
	)
	(gr_text "RX0"
		(at 67.564 58.928 0)
		(layer "F.SilkS")
	)
	(gr_text "nc"
		(at 68.58 45.974 0)
		(layer "F.SilkS")
	)
	(gr_text "4.7K"
		(at 22.86 60.452 0)
		(layer "F.SilkS")
	)
	(gr_text "4.7K"
		(at 27.432 60.452 0)
		(layer "F.SilkS")
	)
	(gr_text "BOOT/IO0"
		(at 64.77 51.308 0)
		(layer "F.SilkS")
	)
	(gr_text "nc"
		(at 68.58 48.768 0)
		(layer "F.SilkS")
	)
	(gr_text "SCL"
		(at 67.818 61.468 0)
		(layer "F.SilkS")
	)
	(gr_text "3V3"
		(at 67.818 38.354 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 69.342 29.972 -90)
		(layer "F.SilkS")
	)
	(gr_text "IO1"
		(at 68.072 40.894 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 68.326 35.814 0)
		(layer "F.SilkS")
	)
	(gr_text "PDX Hackerspace\nExit Poll"
		(at 66.294 67.056 90)
		(layer "F.SilkS")
	)
	(gr_text "STEMMAQT/Qwiic"
		(at 30.226 64.548 0)
		(layer "F.SilkS")
	)
	(gr_text "TX0"
		(at 67.818 56.388 0)
		(layer "F.SilkS")
	)
	(gr_text "IO37\n"
		(at 67.564 43.688 0)
		(layer "F.SilkS")
	)
	(gr_text "~{CPU_RST}"
		(at 65.024 53.848 0)
		(layer "F.SilkS")
	)
	(gr_text "SDA"
		(at 67.818 64.008 0)
		(layer "F.SilkS")
	)
	(gr_text "50mm x 54mm\nmounting holes m2\n2.5mm offset from edges\n"
		(at 90.17 71.374 0)
		(layer "User.1")
	)
	(zone
		(net 11)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 19.304 19.304) (xy 19.558 72.644) (xy 75.040343 72.707282) (xy 74.93 19.05)
			)
		)
	)
	(zone
		(net 3)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 19.304 19.05) (xy 74.93 19.05) (xy 74.93 72.39) (xy 19.558 72.39)
			)
		)
	)
)
