(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 23)
    (no_connects 0)
    (area 64.440999 78.283999 78.053001 88.594001)
    (thickness 1.6)
    (drawings 47)
    (tracks 47)
    (zones 0)
    (modules 12)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C2-Pad2)")
  (net 7 "Net-(C3-Pad2)")
  (net 8 "Net-(C4-Pad2)")
  (net 9 /Ground)
  (net 10 "Net-(J3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(J3-Pad1)")
  )
  (module sandwhich:Conn_01x04_Sandwhich_Small (layer B.Cu) (tedit 5ABE3D78)
    (at 76.327 79.629)
    (fp_text reference J3 (at 0 1.27) (layer B.SilkS))
    (fp_text value Conn_01x04_Male_Sandwhich (at 0 -3.81) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at 0 2.54) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J3-Pad1)"))
    (pad 3 smd rect (at 0 5.08) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J3-Pad1)"))
    (pad 4 smd rect (at 0 7.62) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J3-Pad1)"))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5ABE32CE)
    (at 69.596 85.471 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -2.0574 -1.778 180) (layer F.SilkS))
    (fp_text value 10p (at 0 0 450) (layer F.Fab))
    (fp_text user %R (at -2.0574 -1.778 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5ABE32B9)
    (at 69.596 87.249)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 2.0828 0.7366) (layer F.SilkS))
    (fp_text value 2M (at 0 0 270) (layer F.Fab))
    (fp_text user %R (at 2.0828 0.7366) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5ABE32F1)
    (at 72.898 83.566 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -3.0988 180) (layer F.SilkS))
    (fp_text value 10p (at 0 0 450) (layer F.Fab))
    (fp_text user %R (at 0 -3.0988 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5ABE3282)
    (at 69.596 81.534 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0.1524 1.9304 180) (layer F.SilkS))
    (fp_text value 10p (at 0 0 450) (layer F.Fab))
    (fp_text user %R (at 0.1524 1.9304 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5ABE322F)
    (at 72.898 79.629 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 2.286 0.6858 180) (layer F.SilkS))
    (fp_text value 10p (at 0 0 450) (layer F.Fab))
    (fp_text user %R (at 2.286 0.6858 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5ABE4198)
    (at 72.898 85.344)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0.0254 2.032) (layer F.SilkS))
    (fp_text value 2M (at 0 0 270) (layer F.Fab))
    (fp_text user %R (at 0.0254 2.032) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5ABE3286)
    (at 69.596 83.312)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -0.127 -3.0226) (layer F.SilkS))
    (fp_text value 2M (at 0 0 270) (layer F.Fab))
    (fp_text user %R (at -0.127 -3.0226) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5ABE3249)
    (at 72.898 81.407)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -2.2606 -1.778) (layer F.SilkS))
    (fp_text value 2M (at 0 0 270) (layer F.Fab))
    (fp_text user %R (at -2.2606 -1.778) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sandwhich:Conn_01x04_Sandwhich_Small (layer F.Cu) (tedit 5ABE32FA)
    (at 76.327 87.249)
    (fp_text reference J1 (at -2.2606 0.5334) (layer F.SilkS))
    (fp_text value Conn_01x04_Male_Sandwhich (at 0 3.81) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0 -2.54) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at 0 -5.08) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 4 smd rect (at 0 -7.62) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
  )
  (module sandwhich:Conn_01x04_Sandwhich_Small (layer F.Cu) (tedit 5ABE32A2)
    (at 66.167 79.629 180)
    (fp_text reference J2 (at -2.2352 0.508 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male_Sandwhich (at 0 3.81 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 0 -2.54 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C3-Pad2)"))
    (pad 3 smd rect (at 0 -5.08 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C2-Pad2)"))
    (pad 4 smd rect (at 0 -7.62 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module sandwhich:Conn_01x04_Sandwhich_Small (layer B.Cu) (tedit 5ABE3D74)
    (at 66.167 79.629)
    (fp_text reference J4 (at 0 1.27) (layer B.SilkS))
    (fp_text value Conn_01x04_Male_Sandwhich (at 0 -3.81) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at 0 2.54) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J3-Pad1)"))
    (pad 3 smd rect (at 0 5.08) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J3-Pad1)"))
    (pad 4 smd rect (at 0 7.62) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J3-Pad1)"))
  )
  (gr_text GND (at 76.2889 83.4898) (layer B.SilkS))
  (gr_text GND (at 66.1924 83.4644) (layer B.SilkS))
  (gr_text 3.0 (at 66.167 85.979) (layer B.SilkS))
  (gr_text Version (at 76.327 85.979) (layer B.SilkS))
  (gr_text 1.111 (at 70.485 86.614) (layer B.SilkS))
  (gr_text 2.5 (at 70.485 85.344) (layer B.SilkS))
  (gr_text 3.333 (at 70.485 84.074) (layer B.SilkS))
  (gr_text 18 (at 72.517 86.614) (layer B.SilkS))
  (gr_text 8 (at 72.517 85.344) (layer B.SilkS))
  (gr_text 6 (at 72.517 84.074) (layer B.SilkS))
  (gr_text 10 (at 73.914 86.614) (layer B.SilkS))
  (gr_text 5 (at 73.914 85.344) (layer B.SilkS))
  (gr_text 4 (at 73.914 84.074) (layer B.SilkS))
  (gr_text 5 (at 70.485 82.804) (layer B.SilkS))
  (gr_text 3 (at 73.914 82.804) (layer B.SilkS))
  (gr_text 4 (at 72.517 82.804) (layer B.SilkS))
  (gr_text 10 (at 70.485 81.534) (layer B.SilkS))
  (gr_text 2 (at 72.517 81.534) (layer B.SilkS))
  (gr_text 2 (at 73.914 81.534) (layer B.SilkS))
  (gr_text v (at 68.58 80.264) (layer B.SilkS))
  (gr_text X (at 73.914 80.264) (layer B.SilkS))
  (gr_text pF (at 70.485 80.264) (layer B.SilkS))
  (gr_text MΩ (at 72.517 80.264) (layer B.SilkS))
  (gr_text Reduc. (at 76.2762 83.4644) (layer F.SilkS))
  (gr_text Probe (at 76.327 85.979) (layer F.SilkS))
  (gr_text Saleae (at 66.294 80.899) (layer F.SilkS))
  (gr_text "Pro\n" (at 66.167 85.979) (layer F.SilkS))
  (gr_text "Gain Reduction" (at 71.247 78.994) (layer B.SilkS))
  (gr_text Gain (at 76.2 80.9244) (layer F.SilkS))
  (gr_text "Ryan Bahneman" (at 71.247 87.757) (layer B.SilkS))
  (gr_text "Logic\n" (at 66.167 83.439) (layer F.SilkS))
  (gr_line (start 64.516 88.519) (end 64.516 78.359) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.978 88.519) (end 64.516 88.519) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 64.516 78.359) (end 77.978 78.359) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.978 78.359) (end 77.978 88.519) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 10) (net_name "Net-(J3-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.1) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77.9272 78.359) (xy 77.9272 88.4936) (xy 64.516 88.4936) (xy 64.516 78.359)
      )
    )
  )
  (zone (net 9) (net_name /Ground) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.75) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 64.5668 78.3336) (xy 64.516 78.359) (xy 64.516 78.3336)
      )
    )
  )
)
