(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 51)
    (zones 0)
    (modules 3)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (grid_origin 107.95 118.745)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(B1-Pad22)")
  (net 2 "Net-(B1-Pad21)")
  (net 3 "Net-(B1-Pad19)")
  (net 4 "Net-(B1-Pad18)")
  (net 5 "Net-(B1-Pad15)")
  (net 6 "Net-(B1-Pad13)")
  (net 7 "Net-(B1-Pad11)")
  (net 8 "Net-(B1-Pad10)")
  (net 9 "Net-(B1-Pad7)")
  (net 10 "Net-(B1-Pad1)")
  (net 11 "Net-(J1-Pad4)")
  (net 12 "Net-(J1-Pad3)")
  (net 13 GND)
  (net 14 +5V)
  (net 15 "Net-(B1-Pad16)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.1524)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(B1-Pad1)")
    (add_net "Net-(B1-Pad10)")
    (add_net "Net-(B1-Pad11)")
    (add_net "Net-(B1-Pad13)")
    (add_net "Net-(B1-Pad15)")
    (add_net "Net-(B1-Pad16)")
    (add_net "Net-(B1-Pad18)")
    (add_net "Net-(B1-Pad19)")
    (add_net "Net-(B1-Pad21)")
    (add_net "Net-(B1-Pad22)")
    (add_net "Net-(B1-Pad7)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(XA1-Pad10)")
    (add_net "Net-(XA1-Pad11)")
    (add_net "Net-(XA1-Pad12)")
    (add_net "Net-(XA1-Pad13)")
    (add_net "Net-(XA1-Pad14)")
    (add_net "Net-(XA1-Pad15)")
    (add_net "Net-(XA1-Pad16)")
    (add_net "Net-(XA1-Pad17)")
    (add_net "Net-(XA1-Pad18)")
    (add_net "Net-(XA1-Pad6)")
    (add_net "Net-(XA1-Pad7)")
    (add_net "Net-(XA1-Pad8)")
    (add_net "Net-(XA1-Pad9)")
  )
  (module cole_library:ht16k33_breakout (layer B.Cu) (tedit 6028A1A0)
    (at 118.11 100.84)
    (fp_text reference XA1 (at 0 19.05) (layer B.SilkS) hide)
    (fp_text value ht16k33_breakout (at 0 -19.05) (layer B.Fab))
    (fp_text user GND (at -7.62 16.51) (layer B.SilkS))
    (fp_text user VDD (at 7.62 16.51) (layer B.SilkS))
    (fp_text user Adafruit (at 0 -16.77 180) (layer B.SilkS))
    (fp_text user HT16K33 (at 0 -14.865 180) (layer B.SilkS))
    (fp_text user Breakout (at 0 -12.96 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at -8.89 16.51) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 2 thru_hole circle (at -8.89 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(B1-Pad21)"))
    (pad 3 thru_hole circle (at -8.89 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(B1-Pad15)"))
    (pad 4 thru_hole circle (at -8.89 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(B1-Pad13)"))
    (pad 5 thru_hole circle (at -8.89 6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(B1-Pad16)"))
    (pad 6 thru_hole circle (at -8.89 3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -8.89 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -8.89 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -8.89 -3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -8.89 -6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at -8.89 -8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at -8.89 -11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at -8.89 -13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at -8.89 -16.51) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 8.89 -16.51) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 8.89 -13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 8.89 -11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at 8.89 -8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 8.89 -6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(B1-Pad11)"))
    (pad 20 thru_hole circle (at 8.89 -3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(B1-Pad10)"))
    (pad 21 thru_hole circle (at 8.89 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(B1-Pad7)"))
    (pad 22 thru_hole circle (at 8.89 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(B1-Pad18)"))
    (pad 23 thru_hole circle (at 8.89 3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(B1-Pad19)"))
    (pad 24 thru_hole circle (at 8.89 6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(B1-Pad1)"))
    (pad 25 thru_hole circle (at 8.89 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(B1-Pad22)"))
    (pad 26 thru_hole circle (at 8.89 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad3)"))
    (pad 27 thru_hole circle (at 8.89 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad4)"))
    (pad 28 thru_hole circle (at 8.89 16.51) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 +5V))
    (model W:/cole/KiCAD/proton_pack/cole_library.pretty/3d/ht16k33.wrl
      (offset (xyz 0 0 2.54))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cole_library:bargraph_bl28 (layer F.Cu) (tedit 6028A08E)
    (at 120.65 100.838)
    (fp_text reference B1 (at 0 17.018) (layer F.SilkS) hide)
    (fp_text value bargraph_bl28 (at 0 17.78) (layer F.Fab))
    (pad 22 thru_hole circle (at -2.54 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(B1-Pad22)"))
    (pad 21 thru_hole circle (at -2.54 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(B1-Pad21)"))
    (pad 19 thru_hole circle (at -2.54 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(B1-Pad19)"))
    (pad 18 thru_hole circle (at -2.54 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(B1-Pad18)"))
    (pad 16 thru_hole circle (at -2.54 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(B1-Pad16)"))
    (pad 15 thru_hole circle (at -2.54 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(B1-Pad15)"))
    (pad 13 thru_hole circle (at -2.54 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(B1-Pad13)"))
    (pad 11 thru_hole circle (at 2.54 -12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(B1-Pad11)"))
    (pad 10 thru_hole circle (at 2.54 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(B1-Pad10)"))
    (pad 7 thru_hole circle (at 2.54 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(B1-Pad7)"))
    (pad 1 thru_hole circle (at 2.54 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(B1-Pad1)"))
    (model W:/cole/KiCAD/proton_pack/cole_library.pretty/3d/bargraph_bl28.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 121.92 81.28 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 90) (layer B.SilkS) hide)
    (fp_text value Conn_01x04_Male (at 0 -9.95 90) (layer B.Fab))
    (fp_text user %R (at 0 -3.81 180) (layer B.Fab))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 20.32 (width 0.15) (layer Dwgs.User)
    (gr_text "0.8000 in" (at 118.11 74.265) (layer Dwgs.User))
    (feature1 (pts (xy 128.27 79.375) (xy 128.27 74.978579)))
    (feature2 (pts (xy 107.95 79.375) (xy 107.95 74.978579)))
    (crossbar (pts (xy 107.95 75.565) (xy 128.27 75.565)))
    (arrow1a (pts (xy 128.27 75.565) (xy 127.143496 76.151421)))
    (arrow1b (pts (xy 128.27 75.565) (xy 127.143496 74.978579)))
    (arrow2a (pts (xy 107.95 75.565) (xy 109.076504 76.151421)))
    (arrow2b (pts (xy 107.95 75.565) (xy 109.076504 74.978579)))
  )
  (dimension 39.37 (width 0.15) (layer Dwgs.User)
    (gr_text "1.5500 in" (at 104.11 99.06 90) (layer Dwgs.User))
    (feature1 (pts (xy 107.95 79.375) (xy 104.823579 79.375)))
    (feature2 (pts (xy 107.95 118.745) (xy 104.823579 118.745)))
    (crossbar (pts (xy 105.41 118.745) (xy 105.41 79.375)))
    (arrow1a (pts (xy 105.41 79.375) (xy 105.996421 80.501504)))
    (arrow1b (pts (xy 105.41 79.375) (xy 104.823579 80.501504)))
    (arrow2a (pts (xy 105.41 118.745) (xy 105.996421 117.618496)))
    (arrow2b (pts (xy 105.41 118.745) (xy 104.823579 117.618496)))
  )
  (gr_text "Barmeter \nBL28-3005SA04Y" (at 120.65 100.965 90) (layer F.SilkS))
  (gr_text SCL (at 116.84 83.185) (layer F.SilkS))
  (gr_text SDA (at 114.3 83.185) (layer F.SilkS))
  (gr_text GND (at 119.38 83.185) (layer F.SilkS))
  (gr_text +5V (at 121.92 83.185) (layer F.SilkS))
  (gr_arc (start 127 80.645) (end 128.27 80.645) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 109.22 80.645) (end 109.22 79.375) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 128.27 118.745) (end 107.95 118.745) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 128.27 80.645) (end 128.27 118.745) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 109.22 79.375) (end 127 79.375) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 107.95 118.745) (end 107.95 80.645) (layer Edge.Cuts) (width 0.05))
)
