(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~52~ubuntu17.04.1)
  (general
    (links 59)
    (no_connects 0)
    (area 45.644999 67.234999 104.215001 147.395001)
    (thickness 1.6)
    (drawings 17)
    (tracks 185)
    (zones 0)
    (modules 15)
    (nets 105)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.381)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 1.524)
    (user_trace_width 2.54)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 "Net-(D1-Pad2)")
  (net 3 GND)
  (net 4 BB_I2C2_SCL)
  (net 5 BB_I2C2_SDA)
  (net 6 "Net-(J2-Pad3)")
  (net 7 "Net-(J2-Pad1)")
  (net 8 "Net-(J2-Pad2)")
  (net 9 SYS_5V)
  (net 10 VDD_5V)
  (net 11 CSYNC_B)
  (net 12 "Net-(P2-Pad3)")
  (net 13 "Net-(P2-Pad4)")
  (net 14 "Net-(P2-Pad5)")
  (net 15 "Net-(P2-Pad6)")
  (net 16 CSYNC_A)
  (net 17 "Net-(P3-Pad3)")
  (net 18 "Net-(P3-Pad4)")
  (net 19 "Net-(P3-Pad5)")
  (net 20 "Net-(P3-Pad6)")
  (net 21 "Net-(P8-Pad3)")
  (net 22 "Net-(P8-Pad4)")
  (net 23 "Net-(P8-Pad5)")
  (net 24 "Net-(P8-Pad6)")
  (net 25 "Net-(P8-Pad7)")
  (net 26 "Net-(P8-Pad8)")
  (net 27 "Net-(P8-Pad9)")
  (net 28 "Net-(P8-Pad10)")
  (net 29 "Net-(P8-Pad11)")
  (net 30 "Net-(P8-Pad12)")
  (net 31 "Net-(P8-Pad13)")
  (net 32 "Net-(P8-Pad14)")
  (net 33 "Net-(P8-Pad15)")
  (net 34 "Net-(P8-Pad16)")
  (net 35 "Net-(P8-Pad17)")
  (net 36 "Net-(P8-Pad18)")
  (net 37 "Net-(P8-Pad19)")
  (net 38 "Net-(P8-Pad20)")
  (net 39 "Net-(P8-Pad21)")
  (net 40 "Net-(P8-Pad22)")
  (net 41 "Net-(P8-Pad23)")
  (net 42 "Net-(P8-Pad24)")
  (net 43 "Net-(P8-Pad25)")
  (net 44 BB_GPIO1_29)
  (net 45 BB_VSYNC)
  (net 46 "Net-(P8-Pad28)")
  (net 47 BB_HSYNC)
  (net 48 "Net-(P8-Pad30)")
  (net 49 "Net-(P8-Pad31)")
  (net 50 "Net-(P8-Pad32)")
  (net 51 "Net-(P8-Pad33)")
  (net 52 BB_LCD11)
  (net 53 "Net-(P8-Pad35)")
  (net 54 BB_LCD10)
  (net 55 BB_LCD8)
  (net 56 BB_LCD9)
  (net 57 "Net-(P8-Pad39)")
  (net 58 "Net-(P8-Pad40)")
  (net 59 "Net-(P8-Pad41)")
  (net 60 "Net-(P8-Pad42)")
  (net 61 BB_LCD2)
  (net 62 BB_LCD3)
  (net 63 BB_LCD0)
  (net 64 BB_LCD1)
  (net 65 +3V3)
  (net 66 "Net-(P9-Pad9)")
  (net 67 "Net-(P9-Pad10)")
  (net 68 "Net-(P9-Pad11)")
  (net 69 "Net-(P9-Pad12)")
  (net 70 "Net-(P9-Pad13)")
  (net 71 "Net-(P9-Pad14)")
  (net 72 "Net-(P9-Pad15)")
  (net 73 "Net-(P9-Pad16)")
  (net 74 "Net-(P9-Pad17)")
  (net 75 "Net-(P9-Pad18)")
  (net 76 "Net-(P9-Pad21)")
  (net 77 "Net-(P9-Pad22)")
  (net 78 "Net-(P9-Pad23)")
  (net 79 "Net-(P9-Pad24)")
  (net 80 "Net-(P9-Pad25)")
  (net 81 "Net-(P9-Pad26)")
  (net 82 "Net-(P9-Pad27)")
  (net 83 "Net-(P9-Pad28)")
  (net 84 "Net-(P9-Pad29)")
  (net 85 "Net-(P9-Pad30)")
  (net 86 "Net-(P9-Pad31)")
  (net 87 "Net-(P9-Pad32)")
  (net 88 "Net-(P9-Pad33)")
  (net 89 "Net-(P9-Pad34)")
  (net 90 "Net-(P9-Pad35)")
  (net 91 "Net-(P9-Pad36)")
  (net 92 "Net-(P9-Pad37)")
  (net 93 "Net-(P9-Pad38)")
  (net 94 "Net-(P9-Pad39)")
  (net 95 "Net-(P9-Pad40)")
  (net 96 "Net-(P9-Pad41)")
  (net 97 "Net-(P9-Pad42)")
  (net 98 "Net-(P9-Pad43)")
  (net 99 "Net-(P9-Pad44)")
  (net 100 "Net-(P9-Pad45)")
  (net 101 "Net-(P9-Pad46)")
  (net 102 "Net-(Q1-Pad1)")
  (net 103 "Net-(U2-Pad8)")
  (net 104 "Net-(U2-Pad11)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net BB_GPIO1_29)
    (add_net BB_HSYNC)
    (add_net BB_I2C2_SCL)
    (add_net BB_I2C2_SDA)
    (add_net BB_LCD0)
    (add_net BB_LCD1)
    (add_net BB_LCD10)
    (add_net BB_LCD11)
    (add_net BB_LCD2)
    (add_net BB_LCD3)
    (add_net BB_LCD8)
    (add_net BB_LCD9)
    (add_net BB_VSYNC)
    (add_net CSYNC_A)
    (add_net CSYNC_B)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P3-Pad6)")
    (add_net "Net-(P8-Pad10)")
    (add_net "Net-(P8-Pad11)")
    (add_net "Net-(P8-Pad12)")
    (add_net "Net-(P8-Pad13)")
    (add_net "Net-(P8-Pad14)")
    (add_net "Net-(P8-Pad15)")
    (add_net "Net-(P8-Pad16)")
    (add_net "Net-(P8-Pad17)")
    (add_net "Net-(P8-Pad18)")
    (add_net "Net-(P8-Pad19)")
    (add_net "Net-(P8-Pad20)")
    (add_net "Net-(P8-Pad21)")
    (add_net "Net-(P8-Pad22)")
    (add_net "Net-(P8-Pad23)")
    (add_net "Net-(P8-Pad24)")
    (add_net "Net-(P8-Pad25)")
    (add_net "Net-(P8-Pad28)")
    (add_net "Net-(P8-Pad3)")
    (add_net "Net-(P8-Pad30)")
    (add_net "Net-(P8-Pad31)")
    (add_net "Net-(P8-Pad32)")
    (add_net "Net-(P8-Pad33)")
    (add_net "Net-(P8-Pad35)")
    (add_net "Net-(P8-Pad39)")
    (add_net "Net-(P8-Pad4)")
    (add_net "Net-(P8-Pad40)")
    (add_net "Net-(P8-Pad41)")
    (add_net "Net-(P8-Pad42)")
    (add_net "Net-(P8-Pad5)")
    (add_net "Net-(P8-Pad6)")
    (add_net "Net-(P8-Pad7)")
    (add_net "Net-(P8-Pad8)")
    (add_net "Net-(P8-Pad9)")
    (add_net "Net-(P9-Pad10)")
    (add_net "Net-(P9-Pad11)")
    (add_net "Net-(P9-Pad12)")
    (add_net "Net-(P9-Pad13)")
    (add_net "Net-(P9-Pad14)")
    (add_net "Net-(P9-Pad15)")
    (add_net "Net-(P9-Pad16)")
    (add_net "Net-(P9-Pad17)")
    (add_net "Net-(P9-Pad18)")
    (add_net "Net-(P9-Pad21)")
    (add_net "Net-(P9-Pad22)")
    (add_net "Net-(P9-Pad23)")
    (add_net "Net-(P9-Pad24)")
    (add_net "Net-(P9-Pad25)")
    (add_net "Net-(P9-Pad26)")
    (add_net "Net-(P9-Pad27)")
    (add_net "Net-(P9-Pad28)")
    (add_net "Net-(P9-Pad29)")
    (add_net "Net-(P9-Pad30)")
    (add_net "Net-(P9-Pad31)")
    (add_net "Net-(P9-Pad32)")
    (add_net "Net-(P9-Pad33)")
    (add_net "Net-(P9-Pad34)")
    (add_net "Net-(P9-Pad35)")
    (add_net "Net-(P9-Pad36)")
    (add_net "Net-(P9-Pad37)")
    (add_net "Net-(P9-Pad38)")
    (add_net "Net-(P9-Pad39)")
    (add_net "Net-(P9-Pad40)")
    (add_net "Net-(P9-Pad41)")
    (add_net "Net-(P9-Pad42)")
    (add_net "Net-(P9-Pad43)")
    (add_net "Net-(P9-Pad44)")
    (add_net "Net-(P9-Pad45)")
    (add_net "Net-(P9-Pad46)")
    (add_net "Net-(P9-Pad9)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad8)")
    (add_net SYS_5V)
    (add_net VCC)
    (add_net VDD_5V)
  )
  (module Diodes_THT:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 5921392E)
    (at 86.36 144.78 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 5.08 -2.06 90) (layer F.SilkS))
    (fp_text value 1N4148 (at 5.08 2.06 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x03_Pitch2.54mm (layer F.Cu) (tedit 595D4967)
    (at 72.39 76.2 90)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at -1.27 -2.54 90) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 4.315 7.35 90) (layer F.Fab))
    (fp_text user %R (at 4.315 -2.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 BB_I2C2_SCL))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 BB_I2C2_SDA))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-3pol (layer F.Cu) (tedit 5630081E)
    (at 52.07 143.51 90)
    (descr "3-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J2 (at 5 5.9 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x03 (at 5 -6.6 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 10 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad2)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-3pol.wrl
      (at (xyz 0.1968 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 58613494)
    (at 57.15 77.47 180)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J3 (at -1.7 0 270) (layer F.SilkS))
    (fp_text value GS3 (at 1.8 0 270) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 9 SYS_5V))
    (pad 2 smd rect (at 0 0 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0 1.27 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 10 VDD_5V))
  )
  (module Pin_Headers:Pin_Header_Angled_1x06_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 63.5 123.19 180)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference P2 (at 4.315 -2.27 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 4.315 14.97 180) (layer F.Fab))
    (fp_text user %R (at 4.315 -2.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 CSYNC_B))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(P2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(P2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(P2-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x06_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 83.82 110.49)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference P3 (at 4.315 -2.27) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 4.315 14.97) (layer F.Fab))
    (fp_text user %R (at 4.315 -2.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 CSYNC_A))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(P3-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(P3-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(P3-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x23_Pitch2.54mm (layer F.Cu) (tedit 595D495F)
    (at 96.52 69.85)
    (descr "Through hole straight pin header, 2x23, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x23 2.54mm double row")
    (fp_text reference P8 (at -2.54 -0.635) (layer F.SilkS))
    (fp_text value CONN_02X23 (at 1.27 58.21) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(P8-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(P8-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(P8-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(P8-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(P8-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(P8-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(P8-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(P8-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(P8-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(P8-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(P8-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(P8-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(P8-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(P8-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(P8-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(P8-Pad19)"))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(P8-Pad20)"))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(P8-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P8-Pad22)"))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(P8-Pad23)"))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(P8-Pad24)"))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(P8-Pad25)"))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 BB_GPIO1_29))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 BB_VSYNC))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(P8-Pad28)"))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 BB_HSYNC))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(P8-Pad30)"))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(P8-Pad31)"))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(P8-Pad32)"))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(P8-Pad33)"))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 BB_LCD11))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(P8-Pad35)"))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 BB_LCD10))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 BB_LCD8))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 BB_LCD9))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(P8-Pad39)"))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(P8-Pad40)"))
    (pad 41 thru_hole oval (at 0 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(P8-Pad41)"))
    (pad 42 thru_hole oval (at 2.54 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(P8-Pad42)"))
    (pad 43 thru_hole oval (at 0 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 BB_LCD2))
    (pad 44 thru_hole oval (at 2.54 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 BB_LCD3))
    (pad 45 thru_hole oval (at 0 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 BB_LCD0))
    (pad 46 thru_hole oval (at 2.54 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 BB_LCD1))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x23_Pitch2.54mm.wrl
      (at (xyz 0.05 -1.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x23_Pitch2.54mm (layer F.Cu) (tedit 595D4952)
    (at 48.26 69.85)
    (descr "Through hole straight pin header, 2x23, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x23 2.54mm double row")
    (fp_text reference P9 (at 5.08 -0.635) (layer F.SilkS))
    (fp_text value CONN_02X23 (at 1.27 58.21) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 +3V3))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 +3V3))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 VDD_5V))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 VDD_5V))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 SYS_5V))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 SYS_5V))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(P9-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(P9-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(P9-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(P9-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(P9-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(P9-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(P9-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(P9-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(P9-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(P9-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 BB_I2C2_SCL))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 BB_I2C2_SDA))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "Net-(P9-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(P9-Pad22)"))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(P9-Pad23)"))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(P9-Pad24)"))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(P9-Pad25)"))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P9-Pad26)"))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(P9-Pad27)"))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(P9-Pad28)"))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(P9-Pad29)"))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(P9-Pad30)"))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(P9-Pad31)"))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(P9-Pad32)"))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(P9-Pad33)"))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(P9-Pad34)"))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(P9-Pad35)"))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(P9-Pad36)"))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(P9-Pad37)"))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 "Net-(P9-Pad38)"))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 "Net-(P9-Pad39)"))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(P9-Pad40)"))
    (pad 41 thru_hole oval (at 0 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 "Net-(P9-Pad41)"))
    (pad 42 thru_hole oval (at 2.54 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 "Net-(P9-Pad42)"))
    (pad 43 thru_hole oval (at 0 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 "Net-(P9-Pad43)"))
    (pad 44 thru_hole oval (at 2.54 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 "Net-(P9-Pad44)"))
    (pad 45 thru_hole oval (at 0 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 "Net-(P9-Pad45)"))
    (pad 46 thru_hole oval (at 2.54 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 "Net-(P9-Pad46)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x23_Pitch2.54mm.wrl
      (at (xyz 0.05 -1.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 91.44 134.62 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value Q_NMOS_GSD (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 96.52 140.97 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 -2.31 90) (layer F.SilkS))
    (fp_text value 1K (at 3.81 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 BB_GPIO1_29))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 102 "Net-(Q1-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 595D146E)
    (at 67.31 85.09)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 7.62 2.54) (layer F.SilkS))
    (fp_text value 4.7K (at 3.81 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 +3V3))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 BB_I2C2_SCL))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 595D1465)
    (at 71.12 81.28)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 7.62 2.54) (layer F.SilkS))
    (fp_text value 4.7K (at 3.81 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 +3V3))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 BB_I2C2_SDA))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relays_THT:Relay_SPDT_OMRON-G5Q (layer F.Cu) (tedit 58FA2D90)
    (at 81.28 135.89 180)
    (descr "Relay SPDT Omron Serie G5Q")
    (tags "Relay SPDT Omron Serie G5Q")
    (fp_text reference RL1 (at 9.5 -10.5 360) (layer F.SilkS))
    (fp_text value G5Q-1 (at 9 3 360) (layer F.Fab))
    (fp_text user %R (at 8.89 -3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.52 1.52) (drill 0.76) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad1)"))
    (pad 3 thru_hole circle (at 17.78 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad2)"))
    (pad 4 thru_hole circle (at 15.24 -7.62) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad3)"))
    (pad 5 thru_hole circle (at 0 -7.62) (size 1.52 1.52) (drill 0.76) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Relays_THT.3dshapes/Relay_SPDT_OMRON-G5Q.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-20_W7.62mm_LongPads (layer F.Cu) (tedit 58CC8E2D)
    (at 69.85 105.41)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U1 (at 3.81 -2.39) (layer F.SilkS))
    (fp_text value 74LS244 (at 3.81 25.25) (layer F.Fab))
    (fp_text user %R (at 3.81 11.43) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 BB_LCD11))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 BB_LCD3))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(P3-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(P2-Pad6)"))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 BB_LCD10))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 BB_LCD2))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(P3-Pad5)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(P2-Pad5)"))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 BB_LCD9))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 BB_LCD1))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(P3-Pad4)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(P2-Pad4)"))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 BB_LCD8))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 BB_LCD0))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad3)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(P2-Pad3)"))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 20 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-20_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm_LongPads (layer F.Cu) (tedit 58CC8E2C)
    (at 66.04 99.06 90)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U2 (at 3.81 -2.39 90) (layer F.SilkS))
    (fp_text value 74LS32 (at 3.81 17.63 90) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 BB_HSYNC))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 "Net-(U2-Pad8)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 BB_VSYNC))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 CSYNC_B))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 BB_VSYNC))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 "Net-(U2-Pad11)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 BB_HSYNC))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 CSYNC_A))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "BBB CRT\nbreakout\n(2 CRTs,\n4b depth)" (at 87.63 83.185) (layer F.SilkS))
  (gr_line (start 45.72 147.32) (end 45.72 67.31) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 96.52 147.32) (end 45.72 147.32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.33 143.51) (end 96.52 147.32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.33 135.89) (end 100.33 143.51) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.14 132.08) (end 100.33 135.89) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.14 101.6) (end 104.14 132.08) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.6 99.06) (end 104.14 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.6 67.31) (end 101.6 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.71 67.31) (end 101.6 67.31) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.71 69.85) (end 92.71 67.31) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.17 72.39) (end 92.71 69.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.9 72.39) (end 90.17 72.39) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 57.15 72.39) (end 88.9 72.39) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 54.61 69.85) (end 57.15 72.39) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 54.61 67.31) (end 54.61 69.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 45.72 67.31) (end 54.61 67.31) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 59.055 74.93) (xy 88.9 74.93) (xy 94.615 68.58) (xy 100.33 68.58) (xy 100.33 71.12)
        (xy 94.615 71.12) (xy 94.615 146.05) (xy 76.2 146.05) (xy 73.025 143.51) (xy 73.025 135.255)
        (xy 70.485 133.35) (xy 60.96 133.35) (xy 52.705 125.095) (xy 52.07 71.12) (xy 46.99 71.12)
        (xy 46.99 68.58) (xy 52.705 68.58)
      )
    )
  )
)
