(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 6)
    (no_connects 0)
    (area 128.194999 111.684999 144.855001 126.313001)
    (thickness 1.6)
    (drawings 7)
    (tracks 17)
    (zones 0)
    (modules 5)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 128.016 111.506)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(Q1-Pad2)")
  (net 4 GND)
  (net 5 +3V3)
  (net 6 /GPIO)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3V3)
    (add_net /GPIO)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(Q1-Pad2)")
  )
  (module Project:Pin_Header_Straight_1x03_Pitch2.54mm (layer B.Cu) (tedit 58D3DADC)
    (at 130.556 121.92)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference P1 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -7.41) (layer B.Fab) hide)
    (fp_text user %R (at 0 2.33) (layer B.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /GPIO))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Project:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 58D3DA36)
    (at 142.24 113.792 180)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 6.35 -2.66 180) (layer F.SilkS) hide)
    (fp_text value 10K (at 6.35 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 12.7 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /GPIO))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Project:OldSowjetaera_Transistor_Type-I_SmallPads (layer B.Cu) (tedit 58D3DA51)
    (at 137.668 119.126 90)
    (fp_text reference Q1 (at 0 2.54 90) (layer B.SilkS))
    (fp_text value PN2222A (at 8.89 -1.27 90) (layer B.Fab) hide)
    (pad 2 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole circle (at -2 0 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at 2 0 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model Transistors_OldSowjetAera.3dshapes/OldSowjetaera_Transistor_Type-I_SmallPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Project:LED_D5.0mm (layer F.Cu) (tedit 58D3DA68)
    (at 140.208 119.126)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -3.96) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 3.96) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Project:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 58D3DA83)
    (at 129.794 124.46)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 6.35 -2.66) (layer F.SilkS) hide)
    (fp_text value 200 (at 6.35 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 144.78 111.76) (end 128.27 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 126.238) (end 144.78 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 126.238) (end 144.78 126.238) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 111.76) (end 128.27 126.238) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text +3V3 (at 128.778 121.666 90) (layer B.SilkS))
  (gr_text GND (at 128.778 119.126 90) (layer B.SilkS))
  (gr_text GPIO (at 128.778 116.586 90) (layer B.SilkS))
)
