<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.2">
<drawing>
<board>
<plain>
<wire x1="-11.43" y1="-5.25500625" x2="-8.42771875" y2="-8.255" width="0" layer="20" curve="90"/>
<wire x1="-8.42771875" y1="-8.255" x2="62" y2="-8.255" width="0" layer="20"/>
<wire x1="62" y1="-8.255" x2="65" y2="-5.25500625" width="0" layer="20" curve="90"/>
<wire x1="65" y1="-5.25500625" x2="65" y2="54.3716" width="0" layer="20"/>
<wire x1="65" y1="54.3716" x2="62" y2="57.27" width="0" layer="20" curve="90"/>
<wire x1="62" y1="57.27" x2="-8.42771875" y2="57.27" width="0" layer="20"/>
<wire x1="-8.42771875" y1="57.27" x2="-11.43" y2="54.3716" width="0" layer="20" curve="90"/>
<wire x1="-11.43" y1="54.3716" x2="-11.43" y2="-5.25500625" width="0" layer="20"/>
<hole x="3.5" y="3.5" drill="2.8"/>
<hole x="3.5" y="52.5" drill="2.8"/>
<hole x="61.5" y="52.5" drill="2.8"/>
<hole x="61.5" y="3.5" drill="2.8"/>
<text>SOFT-SPI</text>
<text>HW-SPI</text>
<text>GND</text>
<text>3v3</text>
<text>GND</text>
<text>5V</text>
<text>1-Wire + 12-BIT ADC Hat</text>
<text>DS2482 + MCP3208</text>
<text>rev 4</text>
<text>HW CE
SELECT</text>
<text>*CE0</text>
<text>CE1</text>
<text>https://www.tindie.com/stores/cburgess129</text>
<text>Soft-SPI:</text>
<text>clk</text>
<text>miso</text>
<text>mosi</text>
<text>ce</text>
<text>GPIO05</text>
<text>GPIO06</text>
<text>GPIO13</text>
<text>GPIO19</text>
<text>Max Voltage
per ADC
Channel:</text>
<text>VREF+.25V</text>
<text>12-BIT ADC Channels</text>
<text>2A MAX
Output</text>
<text>500ma
MAX Output</text>
<text>JLCJLCJLCJLC</text>
<text>clk</text>
<text>miso</text>
<text>mosi</text>
<text>ce</text>
<text>1-Wire Channels</text>
<text>+</text>
<text>IO4</text>
<text>ADC
VREF
SOURCE</text>
<text>*5V</text>
<text>3v3</text>
<text>0x19</text>
<text>*0x18</text>
<text>1-Wire
I2C
Address</text>
<text>MAX Voltage
Per 1-Wire
Channel:</text>
<hole x="21.9964" y="17.2212" drill="2.2"/>
<hole x="45.0596" y="17.2212" drill="2.2"/>
<text>GND</text>
<text>5V</text>
<text>SCL</text>
<text>SDA</text>
<text>I2C OLED (.96-inch)</text>
<text>VCC+.25</text>
<text>1-WIRE
VCC
SOURCE</text>
<text>5V</text>
<text>3v3*</text>
<text>MCP3208 - SPI (CE0)</text>
<text>DS2482  - I2C (0x18)</text>
<text>OLED - I2C (0x78)</text>
<text>SW1 - GPIO12</text>
<circle x="11.303" y="-6.35" radius="1.204825" width="0.1524" layer="46"/>
<circle x="11.303" y="-4.445" radius="1.204825" width="0.1524" layer="46"/>
<rectangle x1="10.033" y1="-6.477" x2="12.573" y2="-4.318" layer="46"/>
<circle x="30.48" y="-6.35" radius="1.204825" width="0.1524" layer="46"/>
<circle x="30.48" y="-4.445" radius="1.204825" width="0.1524" layer="46"/>
<rectangle x1="29.21" y1="-6.477" x2="31.75" y2="-4.318" layer="46"/>
<circle x="49.657" y="-6.35" radius="1.204825" width="0.1524" layer="46"/>
<circle x="49.657" y="-4.318" radius="1.204825" width="0.1524" layer="46"/>
<rectangle x1="48.387" y1="-6.477" x2="50.927" y2="-4.318" layer="46"/>
<circle x="-7.62" y="44.704" radius="1.204825" width="0.1524" layer="46"/>
<circle x="-9.525" y="44.704" radius="1.204825" width="0.1524" layer="46"/>
<rectangle x1="-9.8425" y1="43.6245" x2="-7.3025" y2="45.7835" layer="46" rot="R90"/>
<circle x="-7.62" y="25.527" radius="1.204825" width="0.1524" layer="46"/>
<circle x="-9.525" y="25.527" radius="1.204825" width="0.1524" layer="46"/>
<rectangle x1="-9.8425" y1="24.4475" x2="-7.3025" y2="26.6065" layer="46" rot="R90"/>
<circle x="-7.62" y="6.35" radius="1.204825" width="0.1524" layer="46"/>
<circle x="-9.525" y="6.35" radius="1.204825" width="0.1524" layer="46"/>
<rectangle x1="-9.8425" y1="5.2705" x2="-7.3025" y2="7.4295" layer="46" rot="R90"/>
<text>-</text>
<text>+</text>
<text>IO0</text>
<text>-</text>
<text>+</text>
<text>IO1</text>
<text>-</text>
<text>+</text>
<text>IO2</text>
<text>-</text>
<text>+</text>
<text>IO3</text>
<text>-</text>
<text>+</text>
<text>IO5</text>
<text>-</text>
<text>+</text>
<text>IO6</text>
<text>-</text>
<text>+</text>
<text>IO7</text>
<text>-</text>
<text>+</text>
<text>CH0</text>
<text>-</text>
<text>+</text>
<text>CH1</text>
<text>-</text>
<text>+</text>
<text>CH2</text>
<text>-</text>
<text>+</text>
<text>CH3</text>
<text>-</text>
<text>+</text>
<text>CH4</text>
<text>-</text>
<text>+</text>
<text>CH5</text>
<text>-</text>
<text>+</text>
<text>CH6</text>
<text>-</text>
<text>+</text>
<text>CH7</text>
<text>-</text>
</plain>
<libraries>
<library name="resistor">
<packages>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
</packages>
</library>
<library name="my-custom-lib">
<packages>
<package name="BWCE">
</package>
<package name="MICROBUILDER_TERMBLOCK_1X2-5.08MM">
</package>
<package name="MA04-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA03-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_3_1-NC_TRACE_SILK">
</package>
</packages>
</library>
<library name="Seeed-Fuse-2016">
<packages>
<package name="F1812">
<description>http://www.fuse-china.com/1812smdfuses.htm</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="MCP3008-I_SL">
<packages>
<package name="SOIC127P600X175-16N">
</package>
</packages>
</library>
<library name="RasPi-BplusHAT_CamSlot">
<description>Generated from &lt;b&gt;RasPi-BplusHAT_CamSlot.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="PIN_20X2">
</package>
</packages>
</library>
<library name="1wire">
<description>&lt;h1&gt;Dallas/Maxim 1-Wire/iButton devices&lt;/h1&gt;
&lt;p&gt;Onewire is a simple, low-cost bus system working with hundreds of devices on an up to 300m long one-wire (plus GND) bus system. It is relative slow (~16kBaud) but electrically undemanding, too. The onewire is hotplug-capable, if the host software supports it. The bus can be controlled by a single &amp;mu;C port pin or by special host adapter chips, which are available for RS232, Parallel, I&lt;sup&gt;2&lt;/sup&gt;C, and USB to onewire conversion. They are available as ready-to-run host adapter devices, too.&lt;/p&gt;
&lt;p&gt;The chips on the bus can be powered through the bus line, this is called "parasite power". All neccesary circuit and capacities for parasite power are on chip. Some chips need an additional power source to provide all features.&lt;/p&gt;
&lt;p&gt;iButton is an application for onewire devices, using special packaged onewire devices as keys or for data storage. All onewire chips have a unique serial number for technical reasons, and together with the hot-plug capability this makes them useable as unique keys. In addition, many onewire chips have additional memory (EPROM, EEPROM, RAM) on the chip, which can be used to store cryptographic keys. iButtons come in various packages which are protected against corrosive agents and weather influences.&lt;/p&gt;
&lt;p&gt;Get more info at &lt;tt&gt;http://www.maxim-ic.com/1-Wire.cfm&lt;/tt&gt;&lt;/p&gt;
&lt;p&gt;Linux driver at &lt;tt&gt;http://owfs.sf.net&lt;/tt&gt;&lt;/p&gt;
&lt;h3&gt;Copyright notice:&lt;/h3&gt;
&lt;p&gt;The devices in this library are copyrighted by various authors &amp;mdash; permission to use, distribute and modify this library is given to you at the terms of the LGPL. Copyright holders are&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Jan Kandziora &amp;lt;jjj@gmx.de&amp;gt;&lt;/li&gt;
&lt;li&gt;Giovanni Varasano &amp;lt;giovanni.varasano@fastwebnet.it&amp;gt;&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;The authorship for each device is given in the device notes.&lt;/p&gt;</description>
<packages>
<package name="SO16">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Arduino-Teensy-v44_PLUS_ESP-12E_4LAYER">
<description>Generated from &lt;b&gt;Arduino-Teensy-v44_PLUS_ESP-12E_4LAYER.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="PTC-1206">
</package>
</packages>
</library>
<library name="Adafruit Feather 328P">
<description>Generated from &lt;b&gt;Adafruit Feather 328P.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="EVQ-Q2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="resistor" package="C0805K" value="1uf">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="resistor" package="M0805" value="1k">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="resistor" package="M0805" value="2k">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="my-custom-lib" package="MICROBUILDER_TERMBLOCK_1X2-5.08MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="my-custom-lib" package="MICROBUILDER_TERMBLOCK_1X2-5.08MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="Seeed-Fuse-2016" package="F1812" value="MF-MSMF250">
<attribute name="MPN" value="MF-MSMF050-2"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="resistor" package="C0805K" value="1uF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PWR" library="adafruit" package="CHIPLED_0805" value="green_led, 35MCD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="resistor" package="M0805" value="1k">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="my-custom-lib" package="BWCE" value=""/>
<element name="JP1" library="SparkFun-Jumpers" package="SMT-JUMPER_3_1-NC_TRACE_SILK" value="JUMPER-SMT_3_1-NC_TRACE_SILK">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Jumpers" package="SMT-JUMPER_3_1-NC_TRACE_SILK" value="JUMPER-SMT_3_1-NC_TRACE_SILK">
<attribute name="NAME"/>
</element>
<element name="JP3" library="SparkFun-Jumpers" package="SMT-JUMPER_3_1-NC_TRACE_SILK" value="JUMPER-SMT_3_1-NC_TRACE_SILK">
<attribute name="NAME"/>
</element>
<element name="JP4" library="SparkFun-Jumpers" package="SMT-JUMPER_3_1-NC_TRACE_SILK" value="JUMPER-SMT_3_1-NC_TRACE_SILK">
<attribute name="NAME"/>
</element>
<element name="JP5" library="SparkFun-Jumpers" package="SMT-JUMPER_3_1-NC_TRACE_SILK" value="JUMPER-SMT_3_1-NC_TRACE_SILK">
<attribute name="NAME"/>
</element>
<element name="U1" library="MCP3008-I_SL" package="SOIC127P600X175-16N" value="MCP3008-I/SL">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Eight Channel SPI Serial Interface 2.7 V 10-Bit A/D Converter SMT - SOIC-16 "/>
<attribute name="MF" value="Microchip"/>
<attribute name="MP" value="MCP3008-I/SL"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOIC-16 Microchip"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="GPIO" library="RasPi-BplusHAT_CamSlot" package="PIN_20X2" value="PIN20X2">
<attribute name="NAME"/>
</element>
<element name="C1" library="resistor" package="C0805K" value="100nf">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Jumpers" package="SMT-JUMPER_3_1-NC_TRACE_SILK" value="JUMPER-SMT_3_1-NC_TRACE_SILK">
<attribute name="NAME"/>
</element>
<element name="I2C_OLED" library="my-custom-lib" package="MA04-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="1wire" package="SO16" value="DS2482-800+">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="resistor" package="M0805" value="1k2">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="resistor" package="M0805" value="1k2">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="JP10" library="SparkFun-Jumpers" package="SMT-JUMPER_3_1-NC_TRACE_SILK" value="JUMPER-SMT_3_1-NC_TRACE_SILK">
<attribute name="NAME"/>
</element>
<element name="F2" library="Arduino-Teensy-v44_PLUS_ESP-12E_4LAYER" package="PTC-1206" value="500MA HOLD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F3" library="Arduino-Teensy-v44_PLUS_ESP-12E_4LAYER" package="PTC-1206" value="500MA HOLD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun-Jumpers" package="SMT-JUMPER_3_1-NC_TRACE_SILK" value="JUMPER-SMT_3_1-NC_TRACE_SILK">
<attribute name="NAME"/>
</element>
<element name="SW1" library="Adafruit Feather 328P" package="EVQ-Q2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="resistor" package="M0805" value="1k">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="SV1" library="my-custom-lib" package="MA03-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV2" library="my-custom-lib" package="MA03-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV3" library="my-custom-lib" package="MA03-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV4" library="my-custom-lib" package="MA03-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV5" library="my-custom-lib" package="MA03-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV6" library="my-custom-lib" package="MA03-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV7" library="my-custom-lib" package="MA03-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV8" library="my-custom-lib" package="MA03-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV13" library="my-custom-lib" package="MA03-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV14" library="my-custom-lib" package="MA03-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV15" library="my-custom-lib" package="MA03-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV16" library="my-custom-lib" package="MA03-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV9" library="my-custom-lib" package="MA03-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV10" library="my-custom-lib" package="MA03-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV11" library="my-custom-lib" package="MA03-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV12" library="my-custom-lib" package="MA03-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$28">
</signal>
<signal name="S$33">
</signal>
<signal name="S$39">
</signal>
<signal name="S$40">
</signal>
<signal name="S$60">
</signal>
<signal name="S$61">
</signal>
<signal name="S$213">
</signal>
<signal name="S$234">
</signal>
<signal name="GND">
<contactref element="R5" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="J7" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="U1" pad="9"/>
<contactref element="U1" pad="14"/>
<contactref element="C2" pad="2"/>
<contactref element="GPIO" pad="9"/>
<contactref element="GPIO" pad="25"/>
<contactref element="GPIO" pad="39"/>
<contactref element="GPIO" pad="6"/>
<contactref element="GPIO" pad="14"/>
<contactref element="GPIO" pad="20"/>
<contactref element="GPIO" pad="30"/>
<contactref element="GPIO" pad="34"/>
<contactref element="U2" pad="13"/>
<contactref element="C1" pad="2"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="7"/>
<contactref element="JP10" pad="3"/>
<contactref element="I2C_OLED" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="SV13" pad="3"/>
<contactref element="SV14" pad="3"/>
<contactref element="SV15" pad="3"/>
<contactref element="SV16" pad="3"/>
<contactref element="SV9" pad="3"/>
<contactref element="SV10" pad="3"/>
<contactref element="SV11" pad="3"/>
<contactref element="SV12" pad="3"/>
<contactref element="SV1" pad="3"/>
<contactref element="SV2" pad="3"/>
<contactref element="SV3" pad="3"/>
<contactref element="SV4" pad="3"/>
<contactref element="SV5" pad="3"/>
<contactref element="SV6" pad="3"/>
<contactref element="SV7" pad="3"/>
<contactref element="SV8" pad="3"/>
</signal>
<signal name="+3V3">
<contactref element="J1" pad="2"/>
<contactref element="PWR" pad="A"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="JP10" pad="1"/>
<contactref element="JP6" pad="1"/>
<contactref element="F2" pad="1"/>
<contactref element="JP7" pad="3"/>
</signal>
<signal name="+5V">
<contactref element="F1" pad="1"/>
<contactref element="GPIO" pad="2"/>
<contactref element="GPIO" pad="4"/>
<contactref element="F3" pad="1"/>
</signal>
<signal name="CLK">
<contactref element="JP1" pad="2"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="CS">
<contactref element="JP4" pad="2"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="DOUT">
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="DIN">
<contactref element="JP3" pad="2"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="HW_SPI_CLK">
<contactref element="JP1" pad="3"/>
<contactref element="GPIO" pad="23"/>
</signal>
<signal name="SOFT_SPI_CLK/GPIO05">
<contactref element="JP1" pad="1"/>
<contactref element="GPIO" pad="29"/>
</signal>
<signal name="HW_SPI_CE0">
<contactref element="JP5" pad="3"/>
<contactref element="GPIO" pad="24"/>
</signal>
<signal name="SOFT_SPI_CE/GPIO19">
<contactref element="JP4" pad="1"/>
<contactref element="GPIO" pad="35"/>
</signal>
<signal name="CH0">
<contactref element="U1" pad="1"/>
<contactref element="SV1" pad="2"/>
</signal>
<signal name="CH1">
<contactref element="U1" pad="2"/>
<contactref element="SV2" pad="2"/>
</signal>
<signal name="CH2">
<contactref element="U1" pad="3"/>
<contactref element="SV3" pad="2"/>
</signal>
<signal name="CH3">
<contactref element="U1" pad="4"/>
<contactref element="SV4" pad="2"/>
</signal>
<signal name="CH4">
<contactref element="U1" pad="5"/>
<contactref element="SV5" pad="2"/>
</signal>
<signal name="CH5">
<contactref element="U1" pad="6"/>
<contactref element="SV6" pad="2"/>
</signal>
<signal name="CH6">
<contactref element="U1" pad="7"/>
<contactref element="SV7" pad="2"/>
</signal>
<signal name="CH7">
<contactref element="U1" pad="8"/>
<contactref element="SV8" pad="2"/>
</signal>
<signal name="HW_SPI_CE">
<contactref element="JP4" pad="3"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="HW_SPI_CE1">
<contactref element="JP5" pad="1"/>
<contactref element="GPIO" pad="26"/>
</signal>
<signal name="SOFT_SPI_MOSI/GPIO13">
<contactref element="JP3" pad="1"/>
<contactref element="GPIO" pad="33"/>
</signal>
<signal name="HW_SPI_MOSI">
<contactref element="JP3" pad="3"/>
<contactref element="GPIO" pad="19"/>
</signal>
<signal name="HW_SPI_MISO">
<contactref element="JP2" pad="3"/>
<contactref element="GPIO" pad="21"/>
</signal>
<signal name="SOFT_SPI_MISO/GPIO06">
<contactref element="JP2" pad="1"/>
<contactref element="GPIO" pad="31"/>
</signal>
<signal name="HW_SPI_CE2">
</signal>
<signal name="HW_SPI_CE3">
</signal>
<signal name="HW_SPI_CE4">
</signal>
<signal name="DOUT_DIVIDED">
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="5V_TAP">
<contactref element="J7" pad="1"/>
<contactref element="F1" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="PWR" pad="C"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="VREF">
<contactref element="U1" pad="15"/>
<contactref element="JP6" pad="2"/>
<contactref element="SV5" pad="1"/>
<contactref element="SV1" pad="1"/>
<contactref element="SV4" pad="1"/>
<contactref element="SV3" pad="1"/>
<contactref element="SV2" pad="1"/>
<contactref element="SV8" pad="1"/>
<contactref element="SV7" pad="1"/>
<contactref element="SV6" pad="1"/>
</signal>
<signal name="1W7">
<contactref element="U2" pad="9"/>
<contactref element="SV16" pad="2"/>
</signal>
<signal name="1W6">
<contactref element="U2" pad="10"/>
<contactref element="SV15" pad="2"/>
</signal>
<signal name="1W5">
<contactref element="U2" pad="11"/>
<contactref element="SV14" pad="2"/>
</signal>
<signal name="1W4">
<contactref element="U2" pad="12"/>
<contactref element="SV13" pad="2"/>
</signal>
<signal name="1W3">
<contactref element="U2" pad="1"/>
<contactref element="SV12" pad="2"/>
</signal>
<signal name="1W2">
<contactref element="U2" pad="16"/>
<contactref element="SV11" pad="2"/>
</signal>
<signal name="1W1">
<contactref element="U2" pad="15"/>
<contactref element="SV10" pad="2"/>
</signal>
<signal name="1W0">
<contactref element="U2" pad="14"/>
<contactref element="SV9" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="GPIO" pad="3"/>
<contactref element="U2" pad="3"/>
<contactref element="R3" pad="2"/>
<contactref element="I2C_OLED" pad="4"/>
</signal>
<signal name="SCL">
<contactref element="GPIO" pad="5"/>
<contactref element="R2" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="I2C_OLED" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="JP10" pad="2"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="1WIRE_VCC">
<contactref element="U2" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="JP7" pad="2"/>
<contactref element="SV13" pad="1"/>
<contactref element="SV14" pad="1"/>
<contactref element="SV9" pad="1"/>
<contactref element="SV10" pad="1"/>
<contactref element="SV11" pad="1"/>
<contactref element="SV12" pad="1"/>
<contactref element="SV15" pad="1"/>
<contactref element="SV16" pad="1"/>
</signal>
<signal name="3V3_PRE-FUSE">
<contactref element="GPIO" pad="1"/>
<contactref element="F2" pad="2"/>
</signal>
<signal name="5V_FUS">
<contactref element="JP6" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="16"/>
<contactref element="F3" pad="2"/>
<contactref element="JP7" pad="1"/>
<contactref element="I2C_OLED" pad="2"/>
</signal>
<signal name="GPIO12">
<contactref element="GPIO" pad="32"/>
<contactref element="SW1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="SW1" pad="B'"/>
<contactref element="R1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
