(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(gr_line
		(start 100.866 68.01)
		(end 195.866 68.01)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 199.866 94.51)
		(mid 198.694427 97.338427)
		(end 195.866 98.51)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 96.865999 72.01)
		(mid 98.037572 69.181573)
		(end 100.866 68.01)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 100.856 94.52)
		(end 102.748 94.52)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 195.876 72)
		(end 197.768 72)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 173.766 83.26)
		(end 176.766 83.26)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 122.966 83.26)
		(end 125.966 83.26)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.866 72.01)
		(end 199.866 94.51)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 195.866 98.51)
		(end 100.866 98.51)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 148.3 83.26)
		(end 151.8 83.26)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 186.466 83.26)
		(end 189.566 83.26)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 100.866 98.51)
		(mid 98.037573 97.338427)
		(end 96.866 94.51)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 195.876 94.52)
		(end 197.768 94.52)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 96.866 94.51)
		(end 96.866 72.01)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 110.266 83.26)
		(end 113.366 83.26)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 195.866 68.01)
		(mid 198.694427 69.181573)
		(end 199.866 72.01)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 100.856 72)
		(end 102.748 72)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "Power"
		(at 180 72 0)
		(layer "F.SilkS")
	)
	(gr_text "Stereo Width Controller"
		(at 148.3 95 0)
		(layer "F.SilkS")
	)
	(gr_text "Width"
		(at 148.3 72 0)
		(layer "F.SilkS")
	)
	(gr_text "Process"
		(at 116.9 72 0)
		(layer "F.SilkS")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 199.95 98.59) (xy 199.98 67.84) (xy 96.74 67.86) (xy 96.72 98.59) (xy 199.95 98.59)
			)
		)
	)
)
